**PIC32MM0256GPM064 FAMILY**

1. **Bit Flash Microcontroller with MIPS32® microAptiv™ UC Core, Low Power and USB**

### Operating Conditions

* 2.0V to 3.6V, -40ºC to +85ºC, DC to 25 MHz

### Low-Power Modes

* Low-Power modes:
  + Idle – CPU off, peripherals run from system clock
  + Sleep – CPU and peripherals off:
    - Fast wake-up Sleep with retention
    - Low-power Sleep with retention
* 0.65 μA Sleep current for RAM Retention

Regulator mode and 5 μA for Regulator Standby mode

* On-Chip 1.8V Voltage Regulator (VREG)
* On-Chip Ultra Low-Power Retention Regulator

### High-Performance 32-Bit RISC CPU

* microAptiv™ UC 32-Bit Core with 5-Stage Pipeline
* microMIPS™ Instruction Set for 35% Smaller Code and 98% Performance compared to MIPS32 Instructions
* 1.53 DMIPS/MHz (37 DMIPS) (Dhrystone 2.1) Performance
* 3.17 CoreMark®/MHz (79 CoreMark) Performance
* 16-Bit/32-Bit Wide Instructions with 32-Bit Wide Data Path
* Two Sets of 32 Core Register Files (32-bit) to Reduce Interrupt Latency
* Single-Cycle 32x16 Multiply and Two-Cycle 32x32 Multiply
* 64-Bit, Zero Wait State Flash with ECC to Maximize Endurance/Retention

### Microcontroller Features

* Up to 256K Flash Memory
  + 20,000 Erase/Write Cycle Endurance
  + 20 Years Minimum Data Retention
  + Self-Programmable under Software Control
* Up to 32K SRAM Memory
* Multiple Interrupt Vectors with Individually Programmable Priority
* Fail-Safe Clock Monitor mode
* Configurable Watchdog Timer with On-Chip, Low-Power RC Oscillator
* Programmable Code Protection
* Selectable Oscillator Options Including:
  + High-precision, 8 MHz (FRC) internal RC oscillator – 2x/3x/4x/6x/12x/24x PLL, which can be clocked from FRC or the Primary Oscillator
  + Primary high-speed, crystal/resonator oscillator or external clock

### Peripheral Features

* USB 2.0 Compliant Full-Speed and Low-Speed Device, Host and On-The-Go (OTG) Controller:
  + Dedicated DMA
  + Device mode operation from FRC oscillator; no crystal oscillator required
* Atomic Set, Clear and Invert Operation on Select Peripheral Registers
* High-Current Sink/Source
* Independent, Low-Power 32 kHz Timer Oscillator
* Three 4-Wire SPI modules:
  + 16-byte FIFO
  + Variable width
  + I2S mode
* Three I2C Master and Slave w/Address Masking and IPMI Support
* Three Enhanced Addressable UARTs:
  + RS-232, RS-485 and LIN/J2602 support
  + IrDA® with on-chip hardware encoder and decoder
* External Edge and Level Change Interrupt on All Ports
* Hardware Real-Time Clock and Calendar (RTCC)
* Up to 24 Peripheral Pin Select (PPS) Remappable Pins
* 21 Total 16-Bit Timers:
  + Three dedicated 16-bit timers/counters
  + Two can be concatenated to form a 32-bit timer
  + Two additional 16-bit timers in each MCCP and SCCP module, totaling 18
* Capture/Compare/PWM/Timer modules:
  + Two 16-bit timers or one 32-bit timer in each module
  + PWM resolution down to 21 ns
  + Three Multiple Output (MCCP) modules:
    - Flexible configuration as PWM, input capture, output compare or timers
    - Six PWM outputs
    - Programmable dead time
    - Auto-shutdown
  + Six Single Output (SCCP) modules:
    - Flexible configuration as PWM, input capture, output compare or timers
    - Single PWM output
* Reference Clock Output (REFO)
* Four Configurable Logic Cells (CLC) with Internal Connections to Select Peripherals and PPS
* 4-Channel Hardware DMA with Automatic Data Size Detection and CRC Engine

### Debug Features

* Two Programming and Debugging Interfaces:
  + 2-wire ICSP™ interface with non-intrusive access and real-time data exchange with application
  + 4-wire MIPS® standard Enhanced JTAG interface
* IEEE Standard 1149.2 Compatible (JTAG) Boundary Scan

### Analog Features

* Three Analog Comparators with Input Multiplexing
* Programmable High/Low-Voltage Detect (HLVD)
* 5-Bit Comparator Voltage Reference DAC with Pin Output
* Up to 24-Channel, Software-Selectable 10/12-Bit SAR Analog-to-Digital Converter (ADC):
  + 12-bit 200K samples/second conversion rate (single Sample-and-Hold)
  + 10-bit 300k samples/second conversion rate (single Sample-and-Hold)
  + Sleep mode operation
  + Low-voltage boost for input
  + Band gap reference input feature
  + Windowed threshold compare feature
  + Auto-scan feature
* Brown-out Reset (BOR)

TABLE 1: PIC32MM0256GPM064 FAMILY DEVICES

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Device** | **Pins** | **Program Memory (Kbytes)** | **Data Memory (Kbytes)** | **General Purpose I/O/PPS** | **16-Bit Timers Maximum** | **PWM Outputs Maximum** | **Remappable Peripherals** | | | | | | **10/12-Bit ADC (External Channels)** | **Comparators** | **CRC** | **RTCC** | **I2C** | **USB** | **Packages** |
| **Dedicated 16-Bit Timers** | **UART(1)/LIN/J2602** | **MCCP(4)** | **SCCP(3)** | **CLC** | **SPI(2)/I2S** |
| PIC32MM0064GPM028 | 28 | 64 | 16 | 21/18 | 21 | 18 | 3 | 3 | 3 | 6 | 4 | 3 | 12 | 3 | Yes | Yes | 3 | Yes | SSOP/QFN/ UQFN |
| PIC32MM0128GPM028 | 28 | 128 | 16 | 21/18 | 21 | 18 | 3 | 3 | 3 | 6 | 4 | 3 | 12 | 3 | Yes | Yes | 3 | Yes | SSOP/QFN/ UQFN |
| PIC32MM0256GPM028 | 28 | 256 | 32 | 21/18 | 21 | 18 | 3 | 3 | 3 | 6 | 4 | 3 | 12 | 3 | Yes | Yes | 3 | Yes | SSOP/QFN/ UQFN |
| PIC32MM0064GPM036 | 36/40 | 64 | 16 | 27/20 | 21 | 20 | 3 | 3 | 3 | 6 | 4 | 3 | 15 | 3 | Yes | Yes | 3 | Yes | VQFN/UQFN |
| PIC32MM0128GPM036 | 36/40 | 128 | 16 | 27/20 | 21 | 20 | 3 | 3 | 3 | 6 | 4 | 3 | 15 | 3 | Yes | Yes | 3 | Yes | VQFN/UQFN |
| PIC32MM0256GPM036 | 36/40 | 256 | 32 | 27/20 | 21 | 20 | 3 | 3 | 3 | 6 | 4 | 3 | 15 | 3 | Yes | Yes | 3 | Yes | VQFN/UQFN |
| PIC32MM0064GPM048 | 48 | 64 | 16 | 38/24 | 21 | 24 | 3 | 3 | 3 | 6 | 4 | 3 | 17 | 3 | Yes | Yes | 3 | Yes | UQFN/TQFP |
| PIC32MM0128GPM048 | 48 | 128 | 16 | 38/24 | 21 | 24 | 3 | 3 | 3 | 6 | 4 | 3 | 17 | 3 | Yes | Yes | 3 | Yes | UQFN/TQFP |
| PIC32MM0256GPM048 | 48 | 256 | 32 | 38/24 | 21 | 24 | 3 | 3 | 3 | 6 | 4 | 3 | 17 | 3 | Yes | Yes | 3 | Yes | UQFN/TQFP |
| PIC32MM0064GPM064 | 64 | 64 | 16 | 52/24 | 21 | 24 | 3 | 3 | 3 | 6 | 4 | 3 | 20 | 3 | Yes | Yes | 3 | Yes | QFN/TQFP |
| PIC32MM0128GPM064 | 64 | 128 | 16 | 52/24 | 21 | 24 | 3 | 3 | 3 | 6 | 4 | 3 | 20 | 3 | Yes | Yes | 3 | Yes | QFN/TQFP |
| PIC32MM0256GPM064 | 64 | 256 | 32 | 52/24 | 21 | 24 | 3 | 3 | 3 | 6 | 4 | 3 | 20 | 3 | Yes | Yes | 3 | Yes | QFN/TQFP |

**Note 1:** UART1 has assigned pins. UART2 and UART3 are remappable.

**2:** SPI1 and SPI3 have assigned pins. SPI2 is remappable.

**3:** SCCP can be configured as a PWM with 1 output, input capture, output compare, 2 x 16-bit timers or 1 x 32-bit timer.

**4:** MCCP can be configured as a PWM with up to 6 outputs, input capture, output compare, 2 x 16-bit timers or 1 x 32-bit timer.

**PIC32MM0256GPM028**

### Pin Diagrams



**28-Pin SSOP**

MCLR 1

PGEC2/**RP1**/RA0 2

PGED2/**RP2**/RA1 3

PGED1/**RP6**/RB0 4

PGEC1/**RP7**/RB1 5

**RP8**/RB2 6

TDI/**RP9**/RB3 7

VSS 8

OSC1/**RP3**/RA2 9

OSC2/**RP4**/RA3**(1)** 10

SOSCI/**RP10**/RB4 11

SOSCO/**RP5**/RA4 12

VDD 13

PGED3/**RP11**/RB5 14

28 AVDD/VDD

27 AVSS/VSS

26 **RP17**/RB15**(1)**

25 **RP16**/RB14

24 **RP15**/RB13**(1)**

23 VUSB3V3

22 D+/RB11

21 D-/RB10

20 VCAP

19 PGEC3/TDO/**RP18**/RC9**(1)** 18 TMS/**RP14**/RB9**(1)**

17 TCK/**RP13**/RB8**(1)**

16 **RP12**/RB7

15 VBUS/RB6

**Legend:** Shaded pins are up to 5V tolerant.

**Note 1:** High drive strength pin.

TABLE 2: COMPLETE PIN FUNCTION DESCRIPTIONS FOR 28-PIN SSOP DEVICES

|  |  |  |  |
| --- | --- | --- | --- |
| **Pin** | **Function** | **Pin** | **Function** |
| 1 | MCLR | 15 | VBUS/RB6 |
| 2 | PGEC2/VREF+/CVREF+/AN0/**RP1**/OCM1E/INT3/RA0 | 16 | **RP12**/SDA3/SDI3/OCM3F/RB7 |
| 3 | PGED2/VREF-/AN1/**RP2**/OCM1F/RA1 | 17 | TCK/**RP13**/SCL1/U1CTS/SCK1/OCM1A/RB8**(**[**1**](#_bookmark8)**)** |
| 4 | PGED1/AN2/C1IND/C2INB/C3INC/**RP6**/OCM2C/RB0 | 18 | TMS/REFCLKI/**RP14**/SDA1/T1CK/T1G/T2CK/T2G/U1RTS/U1BCLK/SDO1/OCM1B/ INT2/RB9**(**[**1**](#_bookmark8)**)** |
| 5 | PGEC1/AN3/C1INC/C2INA/**RP7**/OCM2D/RB1 | 19 | PGEC3/TDO/**RP18**/ASCL1**(**[**2**](#_bookmark9)**)/**T3CK/T3G/USBOEN/SDO3/OCM2A/RC9**(**[**1**](#_bookmark8)**)** |
| 6 | AN4/C1INB/**RP8**/SDA2/OCM2E/RB2 | 20 | VCAP |
| 7 | TDI/AN11/C1INA/**RP9**/SCL2/OCM2F/RB3 | 21 | D-/RB10 |
| 8 | VSS | 22 | D+/RB11 |
| 9 | OSC1/CLKI/AN5/**RP3**/OCM1C/RA2 | 23 | VUSB3V3 |
| 10 | OSC2/CLKO/AN6/C3IND/**RP4**/OCM1D/RA3**(**[**1**](#_bookmark8)**)** | 24 | AN8/LVDIN/**RP15**/SCL3/SCK3/OCM3A/RB13**(**[**1**](#_bookmark8)**)** |
| 11 | SOSCI/AN7/**RP10**/OCM3C/RB4 | 25 | CVREF/AN9/C3INB/**RP16**/RTCC/U1TX/VBUSON/SDI1/OCM3B/INT1/RB14 |
| 12 | SOSCO/SCLKI/**RP5**/PWRLCLK/OCM3D/RA4 | 26 | AN10/C3INA/REFCLKO/**RP17**/U1RX/SS1/FSYNC1/OCM2B/INT0/RB15**(**[**1**](#_bookmark8)**)** |
| 13 | VDD | 27 | AVSS/VSS |
| 14 | PGED3/**RP11**/ASDA1**(**[**2**](#_bookmark9)**)**/USBID/SS3/FSYNC3/ OCM3E/RB5 | 28 | AVDD/VDD |

**Note 1:** High drive strength pin.

**2:** Alternate pin assignments for I2C1 as determined by the I2C1SEL Configuration bit.



### Pin Diagrams (Continued)

**28-Pin QFN/UQFN**

28 27 26 25 24 23 22

PGED1/**RP6**/RB0 1 

PGEC1/**RP7**/RB1 2

**RP8**/RB2 3

TDI/**RP9**/RB3 4 **PIC32MM0256GPM028**

Vss 5

OSC1/**RP3**/RA2 6

OSC2/**RP4**/RA3**(1)** 7

21

20

19

18

17

16

15

**RP15**/RB13**(1)** VUSB3V3 D+/RB11

D-/RB10 VCAP

PGEC3/TDO/**RP18**/RC9**(1)**

TMS/**RP14**/RB9**(1)**

8 9 10 11 12 13 14

**Legend:** Shaded pins are up to 5V tolerant.

**Note 1:** High drive strength pin.

PGED2/**RP2**/RA1 PGEC2/**RP1**/RA0 MCLR

AVDD/VDD

AVSS/VSS

**RP17**/RB15**(1) RP16**/RB14

TABLE 3: COMPLETE PIN FUNCTION DESCRIPTIONS FOR 28-PIN QFN/UQFN DEVICES

SOSCI/**RP10**/RB4 SOSCO/**RP5**/RA4

VDD

PGED3/**RP11**/RB5

VBUS/RB6

**RP12**/RB7 TCK/**RP13**/RB8**(1)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Pin** | **Function** | **Pin** | **Function** |
| 1 | PGED1/AN2/C1IND/C2INB/C3INC/**RP6**/OCM2C/RB0 | 15 | TMS/REFCLKI/**RP14**/SDA1/T1CK/T1G/T2CK/T2G/U1RTS/U1BCLK/SDO1/ OCM1B/INT2/RB9**(**[**1**](#_bookmark10)**)** |
| 2 | PGEC1/AN3/C1INC/C2INA/**RP7**/OCM2D/RB1 | 16 | PGEC3/TDO/**RP18**/ASCL1**(**[**2**](#_bookmark11)**)**/T3CK/T3G/USBOEN/SDO3/OCM2A/RC9**(**[**1**](#_bookmark10)**)** |
| 3 | AN4/C1INB/**RP8**/SDA2/OCM2E/RB2 | 17 | VCAP |
| 4 | TDI/AN11/C1INA/**RP9**/SCL2/OCM2F/RB3 | 18 | D-/RB10 |
| 5 | VSS | 19 | D+/RB11 |
| 6 | OSC1/CLKI/AN5/**RP3**/OCM1C/RA2 | 20 | VUSB3V3 |
| 7 | OSC2/CLKO/AN6/C3IND/**RP4**/OCM1D/RA3**(**[**1**](#_bookmark10)**)** | 21 | AN8/LVDIN/**RP15**/SCL3/SCK3/OCM3A/RB13**(**[**1**](#_bookmark10)**)** |
| 8 | SOSCI/AN7/**RP10**/OCM3C/RB4 | 22 | CVREF/AN9/C3INB/**RP16**/RTCC/U1TX/VBUSON/SDI1/OCM3B/INT1/RB14 |
| 9 | SOSCO/SCLKI/**RP5**/PWRLCLK/OCM3D/RA4 | 23 | AN10/C3INA/REFCLKO/**RP17**/U1RX/SS1/FSYNC1/OCM2B/INT0/RB15**(**[**1**](#_bookmark10)**)** |
| 10 | VDD | 24 | AVSS/VSS |
| 11 | PGED3/**RP11**/ASDA1**(**[**2**](#_bookmark11)**)**/USBID/SS3/FSYNC3/OCM3E/RB5 | 25 | AVDD/VDD |
| 12 | VBUS/RB6 | 26 | MCLR |
| 13 | **RP12**/SDA3/SDI3/OCM3F/RB7 | 27 | PGEC2/VREF+/CVREF+/AN0/**RP1**/OCM1E/INT3/RA0 |
| 14 | TCK/**RP13**/SCL1/U1CTS/SCK1/OCM1A/RB8**(**[**1**](#_bookmark10)**)** | 28 | PGED2/VREF-/AN1/**RP2**/OCM1F/RA1 |

**Note 1:** High drive strength pin.

**2:** Alternate pin assignments for I2C1 as determined by the I2C1SEL Configuration bit.

10

11

12

13

14

15

16

17

18

### Pin Diagrams (Continued)



**36-Pin QFN**

**RP8**/RB2 TDI/**RP9**/RB3

RC0 RC1 **RP19**/RC2

VSS OSC1/**RP3**/RA2 OSC2/**RP4**/RA3**(1)**

SOSCI/**RP10**/RB4

1

2

3

4

5

6

7

8

9

**PIC32MM0256GPM036**

27 **RP15**/RB13**(1)**

26 VUSB3V3

25 D+/RB11

24 D-/RB10

23 VDD

22 VCAP

21 PGEC3/TDO/**RP18**/RC9**(1)**

20 RC8

19 TMS/**RP14**/RB9**(1)**

**Legend:** Shaded pins are up to 5V tolerant.

**Note 1:** High drive strength pin.

36

35

34

33

32

31

30

29

28

PGEC1/**RP7**/RB1 PGED1/**RP6**/RB0 PGED2/**RP2**/RA1 PGEC2/**RP1**/RA0 MCLR AVDD/VDD AVSS/VSS **RP17**/RB15**(1)**

**RP16**/RB14

TABLE 4: COMPLETE PIN FUNCTION DESCRIPTIONS FOR 36-PIN QFN DEVICES

SOSCO/**RP5**/RA4

**RP24**/RA9

VSS VDD RC3

PGED3/**RP11**/RB5

VBUS/RB6

**RP12**/RB7 TCK/**RP13**/RB8**(1)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Pin** | **Function** | **Pin** | **Function** |
| 1 | AN4/C1INB/**RP8**/SDA2/OCM2E/RB2 | 19 | TMS/REFCLKI/**RP14**/SDA1/T1CK/T1G/U1RTS/U1BCLK/SDO1/OCM1B/INT2/RB9**(**[**1**](#_bookmark12)**)** |
| 2 | TDI/AN11/C1INA/**RP9**/SCL2/OCM2F/RB3 | 20 | AN14/LVDIN/C2INC/RC8 |
| 3 | AN12/C2IND/T2CK/T2G/RC0 | 21 | PGEC3/TDO/**RP18**/ASCL1**(**[**2**](#_bookmark13)**)**/USBOEN/SDO3/RC9**(**[**1**](#_bookmark12)**)** |
| 4 | AN13/T3CK/T3G/RC1 | 22 | VCAP |
| 5 | **RP19**/OCM2A/RC2 | 23 | VDD |
| 6 | VSS | 24 | D-/RB10 |
| 7 | OSC1/CLKI/AN5/**RP3**/OCM1C/RA2 | 25 | D+/RB11 |
| 8 | OSC2/CLKO/AN6/C3IND/**RP4**/OCM1D/RA3**(**[**1**](#_bookmark12)**)** | 26 | VUSB3V3 |
| 9 | SOSCI/AN7/**RP10**/OCM3C/RB4 | 27 | AN8/**RP15**/SCL3/SCK3/RB13**(**[**1**](#_bookmark12)**)** |
| 10 | SOSCO/SCLKI/**RP5**/PWRLCLK/OCM3D/RA4 | 28 | CVREF/AN9/C3INB/**RP16**/RTCC/U1TX/VBUSON/SDI1/OCM3B/INT1/RB14 |
| 11 | **RP24**/OCM3A/RA9 | 29 | AN10/C3INA/REFCLKO/**RP17**/U1RX/SS1/FSYNC1/OCM2B/INT0/RB15**(**[**1**](#_bookmark12)**)** |
| 12 | VSS | 30 | AVSS/VSS |
| 13 | VDD | 31 | AVDD/VDD |
| 14 | RC3 | 32 | MCLR |
| 15 | PGED3/**RP11**/ASDA1**(**[**2**](#_bookmark13)**)**/USBID/SS3/FSYNC3/OCM3E/RB5 | 33 | PGEC2/VREF+/CVREF+/AN0/**RP1**/OCM1E/INT3/RA0 |
| 16 | VBUS/RB6 | 34 | PGED2/VREF-/AN1/**RP2**/OCM1F/RA1 |
| 17 | **RP12**/SDA3/SDI3/OCM3F/RB7 | 35 | PGED1/AN2/C1IND/C2INB/C3INC/**RP6**/OCM2C/RB0 |
| 18 | TCK/**RP13**/SCL1/U1CTS/SCK1/OCM1A/RB8**(1)** | 36 | PGEC1/AN3/C1INC/C2INA/**RP7**/OCM2D/RB1 |

**Note 1:** High drive strength pin.

**2:** Alternate pin assignments for I2C1 as determined by the I2C1SEL Configuration bit.

11

12

13

14

15

16

17

18

19

20

### Pin Diagrams (Continued)

40 39 38 37 36 35 34 33 32 31

30

29

28

27

26

25

24

23

22

10

11 12 13 14 15 16 17 18 19 20

**40-Pin UQFN(1)**

**RP8**/RB2 TDI/**RP9**/RB3

RC0 RC1 **RP19**/RC2

VSS

OSC1/**RP3**/RA2 OSC2/**RP4**/RA3**(1)** SOSCI/**RP10**/RB4

SOSCO/**RP5**/RA4

1

2

3

4

5

6

7

8

9

10

**PIC32MM0256GPM036**

30 **RP15**/RB13**(1)**

29 VUSB3V3

28 D+/RB11

27 D-/RB10

26 VDD

25 N/C

24 VCAP

23 N/C

22 PGEC3/TDO/**RP18**/RC9**(1)**

21 RC8

**Legend:** Shaded pins are up to 5V tolerant.

**Note 1:** High drive strength pin.

40

39

38

37

36

35

34

33

32

31

N/C PGEC1/**RP7**/RB1 PGED1/**RP6**/RB0 PGED2/**RP2**/RA1 PGEC2/**RP1**/RA0 MCLR

AVDD/VDD AVSS/VSS **RP17**/RB15**(1) RP16**/RB14

TABLE 5: COMPLETE PIN FUNCTION DESCRIPTIONS FOR 40-PIN UQFN DEVICES

**RP24**/RA9

VSS VDD RC3

PGED3/**RP11**/RB5

VBUS/RB6 **RP12**/RB7 TCK/**RP13**/RB8**(1)**

N/C

TMS/**RP14**/RB9**(1)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Pin** | **Function** | **Pin** | **Function** |
| 1 | AN4/C1INB/**RP8**/SDA2/OCM2E/RB2 | 21 | AN14/LVDIN/C2INC/RC8 |
| 2 | TDI/AN11/C1INA/**RP9**/SCL2/OCM2F/RB3 | 22 | PGEC3/TDO/**RP18**/ASCL1**(**[**2**](#_bookmark15)**)**/SDO3/USBOEN/RC9**(**[**1**](#_bookmark14)**)** |
| 3 | AN12/C2IND/T2CK/T2G/RC0 | 23 | N/C |
| 4 | AN13/T3CK/T3G/RC1 | 24 | VCAP |
| 5 | **RP19**/OCM2A/RC2 | 25 | N/C |
| 6 | VSS | 26 | VDD |
| 7 | OSC1/CLKI/AN5/**RP3**/OCM1C/RA2 | 27 | D-/RB10 |
| 8 | OSC2/CLKO/AN6/C3IND/**RP4**/OCM1D/RA3**(**[**1**](#_bookmark14)**)** | 28 | D+/RB11 |
| 9 | SOSCI/AN7/**RP10**/OCM3C/RB4 | 29 | VUSB3V3 |
| 10 | SOSCO/SCLKI/**RP5**/PWRLCLK/OCM3D/RA4 | 30 | AN8/**RP15**/SCL3/SCK3/RB13**(**[**1**](#_bookmark14)**)** |
| 11 | **RP24**/OCM3A/RA9 | 31 | CVREF/AN9/C3INB/**RP16**/RTCC/U1TX/VBUSON/SDI1/OCM3B/INT1/RB14 |
| 12 | VSS | 32 | AN10/C3INA/REFCLKO/**RP17**/U1RX/SS1/FSYNC1/OCM2B/INT0/RB15**(**[**1**](#_bookmark14)**)** |
| 13 | VDD | 33 | AVSS/VSS |
| 14 | RC3 | 34 | AVDD/VDD |
| 15 | PGED3/**RP11**/ASDA1**(**[**2**](#_bookmark15)**)**/USBID/SS3/FSYNC3/OCM3E/RB5 | 35 | MCLR |
| 16 | VBUS/RB6 | 36 | PGEC2/VREF+/CVREF+/AN0/**RP1**/OCM1E/INT3/RA0 |
| 17 | **RP12**/SDA3/SDI3/OCM3F/RB7 | 37 | PGED2/VREF-/AN1/**RP2**/OCM1F/RA1 |
| 18 | TCK/**RP13**/SCL1/U1CTS/SCK1/OCM1A/RB8**(**[**1**](#_bookmark14)**)** | 38 | PGED1/AN2/C1IND/C2INB/C3INC/**RP6**/OCM2C/RB0 |
| 19 | N/C | 39 | PGEC1/AN3/C1INC/C2INA/**RP7**/OCM2D/RB1 |
| 20 | TMS/REFCLKI/**RP14**/SDA1/T1CK/T1G/U1RTS/U1BCLK/ SDO1/OCM1B/INT2/RB9**(**[**1**](#_bookmark14)**)** | 40 | N/C |

**Note 1:** High drive strength pin.

**2:** Alternate pin assignments for I2C1 as determined by the I2C1SEL Configuration bit.



**RP22**/RA10**(1) RP21**/RA7 **RP16**/RB14 **RP17**/RB15**(1)**

AVSS/VSS

AVDD/VDD

MCLR RA6 PGEC2/**RP1**/RA0 PGED2/**RP2**/RA1 PGED1/**RP6**/RB0 PGEC1/**RP7**/RB1

13

14

15

16

17

18

19

20

21

22

23

24

48

47

46

45

44

43

42

41

40

39

38

37

### Pin Diagrams (Continued)

**48-Pin UQFN, TQFP(1)**

TMS/**RP14**/RB9**(1)**

**RP23**/RC6 **RP20**/RC7

RC8 PGEC3/TDO/**RP18**/RC9**(1)**

VSS VCAP RA15

D-/RB10 D+/RB11 VUSB3V3

**RP15**/RB13**(1)**

1

2

3

4

5

6

7

8

9

10

11

12

**PIC32MM0256GPM048**

36

35

34

33

32

31

30

29

28

27

26

25

SOSCO/**RP5**/RA4 SOSCI/**RP10**/RB4 RA8**(1)** OSC2/**RP4**/RA3**(1)** OSC1/**RP3**/RA2

VSS VDD

**RP19**/RC2 RC1

RC0 TDI/**RP9**/RB3

**RP8**/RB2

**Legend:** Shaded pins are up to 5V tolerant.

**Note 1:** High drive strength pin.

TCK/**RP13**/RB8**(1) RP12**/RB7 VBUS/RB6 PGED3/**RP11**/RB5 RC12

VDD VSS RC5 RC4 RC3 RD0**(1)**

**RP24**/RA9

TABLE 6: COMPLETE PIN FUNCTION DESCRIPTIONS FOR 48-PIN UQFN/TQFP DEVICES

|  |  |  |  |
| --- | --- | --- | --- |
| **Pin** | **Function** | **Pin** | **Function** |
| 1 | TMS/**RP14**/SDA1/OCM1B/INT2/RB9**(**[**1**](#_bookmark16)**)** | 25 | AN4/C1INB/**RP8**/SDA2/OCM2E/RB2 |
| 2 | **RP23**/RC6 | 26 | TDI/AN11/C1INA/**RP9**/SCL2/OCM2F/RB3 |
| 3 | **RP20**/RC7 | 27 | AN12/C2IND/T2CK/T2G/RC0 |
| 4 | AN14/LVDIN/C2INC/RC8 | 28 | AN13/T3CK/T3G/RC1 |
| 5 | PGEC3/TDO/**RP18**/ASCL1**(**[**2**](#_bookmark17)**)**/USBOEN/RC9**(**[**1**](#_bookmark16)**)** | 29 | **RP19**/OCM2A/RC2 |
| 6 | VSS | 30 | VDD |
| 7 | VCAP | 31 | VSS |
| 8 | RTCC/RA15 | 32 | OSC1/CLKI/AN5/**RP3**/OCM1C/RA2 |
| 9 | D-/RB10 | 33 | OSC2/CLKO/AN6/C3IND/**RP4**/RA3**(**[**1**](#_bookmark16)**)** |
| 10 | D+/RB11 | 34 | SDO3/RA8**(**[**1**](#_bookmark16)**)** |
| 11 | VUSB3V3 | 35 | SOSCI/AN7/**RP10**/OCM3C/RB4 |
| 12 | AN8/**RP15**/SCL3/RB13**(**[**1**](#_bookmark16)**)** | 36 | SOSCO/SCLKI/**RP5**/PWRLCLK/OCM3D/RA4 |
| 13 | **RP22**/SCK3/RA10**(**[**1**](#_bookmark16)**)** | 37 | **RP24**/OCM3A/RA9 |
| 14 | **RP21**/SDI3/RA7 | 38 | REFCLKI/T1CK/T1G/U1RTS/U1BCLK/SDO1/RD0**(**[**1**](#_bookmark16)**)** |
| 15 | CVREF/AN9/C3INB/**RP16**/VBUSON/SDI1/OCM3B/INT1/RB14 | 39 | OCM2B/RC3 |
| 16 | AN10/C3INA/REFCLKO/**RP17**/SS1/FSYNC1/INT0/RB15**(**[**1**](#_bookmark16)**)** | 40 | OCM1E/INT3/RC4 |
| 17 | AVSS/VSS | 41 | AN15/OCM1D/RC5 |
| 18 | AVDD/VDD | 42 | VSS |
| 19 | MCLR | 43 | VDD |
| 20 | AN19/U1RX/RA6 | 44 | U1TX/RC12 |
| 21 | PGEC2/VREF+/CVREF+/AN0/**RP1**/RA0 | 45 | PGED3/**RP11**/ASDA1**(**[**2**](#_bookmark17)**)**/USBID/SS3/FSYNC3/OCM3E/RB5 |
| 22 | PGED2/VREF-/AN1/**RP2**/OCM1F/RA1 | 46 | VBUS/RB6 |
| 23 | PGED1/AN2/C1IND/C2INB/C3INC/**RP6**/OCM2C/RB0 | 47 | **RP12**/SDA3/OCM3F/RB7 |
| 24 | PGEC1/AN3/C1INC/C2INA/**RP7**/OCM2D/RB1 | 48 | TCK/**RP13**/SCL1/U1CTS/SCK1/OCM1A/RB8**(**[**1**](#_bookmark16)**)** |

**Note 1:** High drive strength pin.

**2:** Alternate pin assignments for I2C1 as determined by the I2C1SEL Configuration bit.

VDD VSS RC0 RC1

**RP19**/RC2

RC11 VDD VSS

OSC1/**RP3**/RA2 OSC2/**RP4**/RA3**(1)**

RA8**(1)**

SOSCI/**RP10**/RB4 SOSCO/**RP5**/RA4

**RP24**/RA9

RD4 RD2

17

18

19

20

21

22

23

24

25

26

27

28

29

30

31

32

64

63

62

61

60

59

58

57

56

55

54

53

52

51

50

49

### Pin Diagrams (Continued)

**64-Pin QFN, TQFP(1)**

**RP21**/RA7 **RP16**/RB14 **RP17**/RB15**(1)**

AVSS/VSS

AVDD/VDD

RA13 RA12

RA11 MCLR RA6

PGEC2/**RP1**/RA0 PGED2/**RP2**/RA1 PGED1/**RP6**/RB0 PGEC1/**RP7**/RB1

**RP8**/RB2 TDI/**RP9**/RB3

1

2

3

4

5

6

7

8

9

10

11

12

13

14

15

16

**PIC32MM0256GPM064**

48

47

46

45

44

43

42

41

40

39

38

37

36

35

34

33

TCK/**RP13**/RB8**(1)** RC13**(1) RP12**/RB7

RC10 VBUS/RB6

PGED3/**RP11**/RB5 RC15

RC14 RC12 VDD VSS RC5 RC4 RC3 RD0**(1)** RD3

**Legend:** Shaded pins are up to 5V tolerant.

**Note 1:** High drive strength pin.

**RP22**/RA10**(1) RP15**/RB13**(1)** VUSB3V3 D+/RB11

D-/RB10 RA14 RA15 VDD VCAP

PGEC3/TDO/**RP18**/RC9**(1)** RA5

RD1 RC8

**RP20**/RC7

**RP23**/RC6 TMS/**RP14**/RB9**(1)**

TABLE 7: COMPLETE PIN FUNCTION DESCRIPTIONS FOR 64-PIN QFN/TQFP DEVICES

|  |  |  |  |
| --- | --- | --- | --- |
| **Pin** | **Function** | **Pin** | **Function** |
| 1 | **RP21**/SDI3/RA7 | 33 | OCM3B/RD3 |
| 2 | CVREF/AN9/C3INB/**RP16**/VBUSON/RB14 | 34 | REFCLKI/T1CK/T1G/U1RTS/U1BCLK/SDO1/RD0**(**[**1**](#_bookmark18)**)** |
| 3 | AN10/C3INA/REFCLKO/**RP17**/RB15**(**[**1**](#_bookmark18)**)** | 35 | OCM2B/RC3 |
| 4 | AVSS | 36 | OCM1E/INT3/RC4 |
| 5 | AVDD | 37 | AN15/OCM1D/RC5 |
| 6 | AN16/U1CTS/RA13 | 38 | VSS |
| 7 | AN17/OCM1A/RA12 | 39 | VDD |
| 8 | AN18/RA11 | 40 | U1TX/RC12 |
| 9 | MCLR | 41 | OCM3D/RC14 |
| 10 | AN19/U1RX/RA6 | 42 | OCM3E/RC15 |
| 11 | PGEC2/VREF+/CVREF+/AN0/**RP1**/RA0 | 43 | PGED3/**RP11**/ASDA1**(**[**2**](#_bookmark19)**)**/USBID/RB5 |
| 12 | PGED2/VREF-/AN1/**RP2**/OCM1F/RA1 | 44 | VBUS/RB6 |
| 13 | PGED1/AN2/C1IND/C2INB/C3INC/**RP6**/OCM2C/RB0 | 45 | OCM3F/RC10 |
| 14 | PGEC1/AN3/C1INC/C2INA/**RP7**/OCM2D/RB1 | 46 | **RP12**/SDA3/RB7 |
| 15 | AN4/C1INB/**RP8**/SDA2/OCM2E/RB2 | 47 | SCK1/RC13**(**[**1**](#_bookmark18)**)** |
| 16 | TDI/AN11/C1INA/**RP9**/SCL2/OCM2F/RB3 | 48 | TCK/**RP13**/SCL1/RB8**(**[**1**](#_bookmark18)**)** |
| 17 | VDD | 49 | TMS/**RP14**/SDA1/INT2/RB9**(**[**1**](#_bookmark18)**)** |
| 18 | VSS | 50 | **RP23**/RC6 |
| 19 | AN12/C2IND/T2CK/T2G/RC0 | 51 | **RP20**/RC7 |
| 20 | AN13/T3CK/T3G/RC1 | 52 | AN14/LVDIN/C2INC/RC8 |
| 21 | **RP19**/OCM2A/RC2 | 53 | OCM1B/RD1 |
| 22 | SS3/FSYNC3/RC11 | 54 | OCM3A/RA5 |
| 23 | VDD | 55 | PGEC3/TDO/**RP18**/ASCL1**(**[**2**](#_bookmark19)**)**/USBOEN/RC9**(**[**1**](#_bookmark18)**)** |
| 24 | VSS | 56 | VCAP |
| 25 | OSC1/CLKI/AN5/**RP3**/OCM1C/RA2 | 57 | VDD |
| 26 | OSC2/CLKO/AN6/C3IND/**RP4**/RA3**(**[**1**](#_bookmark18)**)** | 58 | RTCC/RA15 |
| 27 | SDO3/RA8**(**[**1**](#_bookmark18)**)** | 59 | OCM3C/RA14 |
| 28 | SOSCI/AN7/**RP10**/RB4 | 60 | D-/RB10 |
| 29 | SOSCO/SCLKI/**RP5**/PWRLCLK/RA4 | 61 | D+/RB11 |
| 30 | **RP24**/RA9 | 62 | VUSB3V3 |
| 31 | SDI1/INT1/RD4 | 63 | AN8/**RP15**/SCL3/RB13**(**[**1**](#_bookmark18)**)** |
| 32 | SS1/FSYNC1/INT0/RD2 | 64 | **RP22**/SCK3/RA10**(**[**1**](#_bookmark18)**)** |

**Note 1:** High drive strength pin.

**2:** Alternate pin assignments for I2C1 as determined by the I2C1SEL Configuration bit.

### Table of Contents

1.0 Device Overview 15

[2.0 Guidelines for Getting Started with 32-Bit Microcontrollers 23](#_bookmark29)

[3.0 CPU 29](#_bookmark57)

[4.0 Memory Organization 39](#_bookmark78)

[5.0 Flash Program Memory 45](#_bookmark100)

[6.0 Resets 53](#_bookmark120)

[7.0 CPU Exceptions and Interrupt Controller 59](#_bookmark146)

[8.0 Direct Memory Access (DMA) Controller 77](#_bookmark168)

[9.0 Oscillator Configuration 97](#_bookmark205)

[10.0 I/O Ports 113](#_bookmark246)

[11.0 Timer1 127](#_bookmark304)

[12.0 Timer2 and Timer3 131](#_bookmark311)

[13.0 Watchdog Timer (WDT) 137](#_bookmark325)

[14.0 Capture/Compare/PWM/Timer Modules (MCCP and SCCP) 141](#_bookmark333)

[15.0 Serial Peripheral Interface (SPI) and Inter-IC Sound (I](#_bookmark356)2S) 159

[16.0 Inter-Integrated Circuit (I](#_bookmark372)2C) 167

[17.0 Universal Asynchronous Receiver Transmitter (UART) 175](#_bookmark381)

[18.0 USB On-The-Go (OTG) 181](#_bookmark391)

[19.0 Real-Time Clock and Calendar (RTCC) 209](#_bookmark456)

[20.0 12-Bit ADC Converter with Threshold Detect 217](#_bookmark471)

[21.0 Configurable Logic Cell (CLC) 229](#_bookmark507)

[22.0 Comparator 243](#_bookmark523)

[23.0 Voltage Reference (](#_bookmark534)CVREF) 249

[24.0 High/Low-Voltage Detect (HLVD) 253](#_bookmark541)

[25.0 Power-Saving Features 257](#_bookmark549)

[26.0 Special Features 263](#_bookmark563)

[27.0 Instruction Set 281](#_bookmark618)

[28.0 Development Support 283](#_bookmark620)

[29.0 Electrical Characteristics 287](#_bookmark635)

[30.0 Packaging Information 319](#_bookmark778)

[Appendix A: Revision History 347](#_bookmark783)

[Index 349](#_bookmark785)

[The Microchip Web Site 353](#_bookmark786)

[Customer Change Notification Service 353](#_bookmark788)

[Customer Support 353](#_bookmark790)

[Product Identification System 355](#_bookmark792)

**TO OUR VALUED CUSTOMERS**

It is our intention to provide our valued customers with the best documentation possible to ensure successful use of your Microchip products. To this end, we will continue to improve our publications to better suit your needs. Our publications will be refined and enhanced as new volumes and updates are introduced.

If you have any questions or comments regarding this publication, please contact the Marketing Communications Department via E-mail at [**docerrors@microchip.com**](mailto:docerrors@microchip.com). We welcome your feedback.

**Most Current Data Sheet**

To obtain the most up-to-date version of this data sheet, please register at our Worldwide Web site at:

[**http://www.microchip.com**](http://www.microchip.com/)

You can determine the version of a data sheet by examining its literature number found on the bottom outside corner of any page. The last character of the literature number is the version number, (e.g., DS30000000A is version A of document DS30000000).

**Errata**

An errata sheet, describing minor operational differences from the data sheet and recommended workarounds, may exist for current devices. As device/documentation issues become known to us, we will publish an errata sheet. The errata will specify the revision of silicon and revision of document to which it applies.

To determine if an errata sheet exists for a particular device, please check with one of the following:

* Microchip’s Worldwide Web site; [**h**](http://www.microchip.com/)**ttp:/**[**/w**](http://www.microchip.com/)**w**[**w.microchip.com**](http://www.microchip.com/)
* Your local Microchip sales office (see last page)

When contacting a sales office, please specify which device, revision of silicon and data sheet (include literature number) you are using.

**Customer Notification System**

Register on our web site at [**www.microchip.com**](http://www.microchip.com/) to receive the most current information on all of our products.

### Referenced Sources

This device data sheet is based on the following individual sections of the *“PIC32 Family Reference Manual”*. These documents should be considered as the general reference for the operation of a particular module or device feature.

**Note:** [To access the documents listed below,](http://www.microchip.com/) [browse the documentation section of the](http://www.microchip.com/) [Microchip web site (](http://www.microchip.com/)www.microchip.com).

* **Section 1. “Introduction”** (DS60001127)
* **Section 5. “Flash Programming”** (DS60001121)
* **Section 7. “Resets”** (DS60001118)
* **Section 8. “Interrupts”** (DS61108)
* **Section 10. “Power-Saving Modes”** (DS60001130)
* **Section 12. “I/O Ports”** (DS60001120)
* **Section 14. “Timers”** (DS60001105)
* **Section 19. “Comparator”** (DS60001110)
* **Section 20. “Comparator Voltage Reference”** (DS61109)
* **Section 21. “UART”** (DS61107)
* **Section 23. “Serial Peripheral Interface (SPI)”** (DS61106)
* **Section 24. “Inter-Integrated Circuit™ (I2C™)”** (DS61116)
* **Section 25. “12-Bit Analog-to-Digital Converter (ADC) with Threshold Detect”** (DS60001359)
* **Section 27. “USB On-The-Go (OTG)”** (DS61126)
* **Section 28. “RTCC with Timestamp”** (DS60001362)
* **Section 30. “Capture/Compare/PWM/Timer (MCCP and SCCP)”** (DS60001381)
* **Section 31. “DMA Controller”** (DS60001117)
* **Section 33. “Programming and Diagnostics”** (DS61129)
* **Section 36. “Configurable Logic Cell”** (DS60001363)
* **Section 48. “Memory Organization and Permissions”** (DS60001214)
* **Section 50. “CPU for Devices with MIPS32® microAptiv™ and M-Class Cores”** (DS60001192)
* **Section 59. “Oscillators with DCO”** (DS60001329)
* **Section 62. “Dual Watchdog Timer”** (DS60001365)

NOTES:



Peripheral Bus Clocked by PBCLK

32

Flash Controller (write)

32

32

32

32

32

32

32

64

Flash Controller

64-Bit Wide Program Flash Memory

Flash Line Buffer

HLVD

PORTD

Comparators

RTCC

UART1,2,3

PORTC

12-Bit ADC

I2C1,2,3

SPI1,2,3

PORTB

SCCP4-9

MCCP1,2,3

Timer1,2,3

PORTA

ICD

I/O Change Notification



Priority Interrupt Controller



JTAG BSCAN

32

Bus Matrix

USB

DMA with CRC

32

RAM

32

Peripheral Bridge



Peripheral Bus Clocked by PBCLK

**1.0 DEVICE** **OVERVIEW** This data sheet contains device-specific information for the PIC32MM0256GPM064 family devices.

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a compre- hensive reference source. To complement the information in this data sheet, refer to the *“PIC32 Family Reference Manual”*, which is available from the Microchip web site ([www.microchip.com/PIC32](http://www.microchip.com/PIC32)). The information in this data sheet supersedes the information in the FRM.

[Figure 1-1](#_bookmark23) illustrates a general block diagram of the core and peripheral modules in the PIC32MM0256GPM064 family of devices.

[Table 1-1](#_bookmark26) lists the pinout I/O descriptions for the pins shown in the device pin tables.

FIGURE 1-1: PIC32MM0256GPM064 FAMILY BLOCK DIAGRAM



AVDD, AVSS

OSC2/CLKO OSC1/CLKI

VDD,VSS

MCLR

SOSCO, SCLKI,

SOSCI

VCAP

SYSCLK

PBCLK (1:1 with SYSCLK)

|  |  |
| --- | --- |
| Primary Oscillator |  |
| FRC/LPRC  Oscillators |
| Secondary Oscillator |
| Dividers |
| PLL |
| Timing Generation |
|  |
|  |

|  |
| --- |
| Power-up Timer |
| Oscillator Start-up Timer |
| Power-on Reset |
| Watchdog Timer |
| Brown-out Reset |
| Voltage Regulator |
| Precision Band Gap Reference |

|  |  |
| --- | --- |
| INT | EJTAG |
| MIPS32® microAptiv™ UC CPU Core | |
| DS | IS |

TABLE 1-1: PIC32MM0256GPM064 FAMILY PINOUT DESCRIPTION

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin Name** | **Pin Number** | | | | | | **Pin Type** | **Buffer Type** | **Description** |
| **28-Pin SSOP** | **28-Pin QFN/ UQFN** | **36-Pin QFN** | **40-Pin UQFN** | **48-Pin QFN/ TQFP** | **64-Pin QFN/ TQFP** |
| AN0 | 2 | 27 | 33 | 36 | 21 | 11 | I | ANA | Analog-to-Digital Converter input channels |
| AN1 | 3 | 28 | 34 | 37 | 22 | 12 | I | ANA |
| AN2 | 4 | 1 | 35 | 38 | 23 | 13 | I | ANA |
| AN3 | 5 | 2 | 36 | 39 | 24 | 14 | I | ANA |
| AN4 | 6 | 3 | 1 | 1 | 25 | 15 | I | ANA |
| AN5 | 9 | 6 | 7 | 7 | 32 | 25 | I | ANA |
| AN6 | 10 | 7 | 8 | 8 | 33 | 26 | I | ANA |
| AN7 | 11 | 8 | 9 | 9 | 35 | 28 | I | ANA |
| AN8 | 24 | 21 | 27 | 30 | 12 | 63 | I | ANA |
| AN9 | 25 | 22 | 28 | 31 | 15 | 2 | I | ANA |
| AN10 | 26 | 23 | 29 | 32 | 16 | 3 | I | ANA |
| AN11 | 7 | 4 | 2 | 2 | 26 | 16 | I | ANA |
| AN12 | — | — | 3 | 3 | 27 | 19 | I | ANA |
| AN13 | — | — | 4 | 4 | 28 | 20 | I | ANA |
| AN14 | — | — | 20 | 21 | 4 | 52 | I | ANA |
| AN15 | — | — | — | — | 41 | 37 | I | ANA |
| AN16 | — | — | — | — | — | 6 | I | ANA |
| AN17 | — | — | — | — | — | 7 | I | ANA |
| AN18 | — | — | — | — | — | 8 | I | ANA |
| AN19 | — | — | — | — | — | 10 | I | ANA |
| AVDD | 28 | 25 | 31 | 34 | 18 | 5 | P | — | Analog modules power supply |
| AVSS | 27 | 24 | 30 | 33 | 17 | 4 | P | — | Analog modules ground |
| C1INA | 7 | 4 | 2 | 2 | 26 | 16 | I | ANA | Comparator 1 Input A |
| C1INB | 6 | 3 | 1 | 1 | 25 | 15 | I | ANA | Comparator 1 Input B |
| C1INC | 5 | 2 | 36 | 39 | 24 | 14 | I | ANA | Comparator 1 Input C |
| C1IND | 4 | 1 | 35 | 38 | 23 | 13 | I | ANA | Comparator 1 Input D |
| C2INA | 5 | 2 | 36 | 39 | 24 | 14 | I | ANA | Comparator 2 Input A |
| C2INB | 4 | 1 | 35 | 38 | 23 | 13 | I | ANA | Comparator 2 Input B |
| C2INC | — | — | 20 | 21 | 4 | 52 | I | ANA | Comparator 2 Input C |
| C2IND | — | — | 3 | 3 | 27 | 19 | I | ANA | Comparator 2 Input D |
| C3INA | 26 | 23 | 29 | 32 | 16 | 3 | I | ANA | Comparator 3 Input A |
| C3INB | 25 | 22 | 28 | 31 | 15 | 2 | I | ANA | Comparator 3 Input B |
| C3INC | 4 | 1 | 35 | 38 | 23 | 13 | I | ANA | Comparator 3 Input C |
| C3IND | 10 | 7 | 8 | 8 | 33 | 26 | I | ANA | Comparator 3 Input D |
| CLKI | 9 | 6 | 7 | 7 | 32 | 25 | I | ST | External Clock source input (EC mode) |
| CLKO | 10 | 7 | 8 | 8 | 33 | 26 | O | DIG | System clock output |
| CVREF | 25 | 22 | 28 | 31 | 15 | 2 | O | ANA | Comparator voltage reference output |
| CVREF+ | 2 | 27 | 33 | 36 | 21 | 11 | I | ANA | Positive comparator voltage reference input |
| D+ | 22 | 19 | 25 | 28 | 10 | 61 | I/O | — | USB transceiver differential plus line |
| D- | 21 | 18 | 24 | 27 | 9 | 60 | I/O | — | USB transceiver differential minus line |
| FSYNC1 | 26 | 23 | 29 | 32 | 16 | 32 | I/O | ST/DIG | SPI1 frame signal input or output |
| FSYNC3 | 14 | 11 | 15 | 15 | 45 | 22 | I/O | ST/DIG | SPI3 frame signal input or output |

|  |  |  |  |
| --- | --- | --- | --- |
| **Legend:** | ST = Schmitt Trigger input buffer | DIG = Digital input/output | P = Power |
|  | I2C = I2C/SMBus input buffer | ANA = Analog level input/output |  |

TABLE 1-1: PIC32MM0256GPM064 FAMILY PINOUT DESCRIPTION (CONTINUED)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin Name** | **Pin Number** | | | | | | **Pin Type** | **Buffer Type** | **Description** |
| **28-Pin SSOP** | **28-Pin QFN/ UQFN** | **36-Pin QFN** | **40-Pin UQFN** | **48-Pin QFN/ TQFP** | **64-Pin QFN/ TQFP** |
| INT0 | 26 | 23 | 29 | 32 | 16 | 32 | I | ST | External Interrupt 0 |
| INT1 | 25 | 22 | 28 | 31 | 15 | 31 | I | ST | External Interrupt 1 |
| INT2 | 18 | 15 | 19 | 20 | 1 | 49 | I | ST | External Interrupt 2 |
| INT3 | 2 | 27 | 33 | 36 | 40 | 36 | I | ST | External Interrupt 3 |
| LVDIN | 24 | 21 | 20 | 21 | 4 | 52 | I | ANA | High/Low-Voltage Detect input |
| MCLR | 1 | 26 | 32 | 35 | 19 | 9 | I | ST | Master Clear (device Reset) |
| OCM1A | 17 | 14 | 18 | 18 | 48 | 7 | O | DIG | MCCP1 Output A |
| OCM1B | 18 | 15 | 19 | 20 | 1 | 53 | O | DIG | MCCP1 Output B |
| OCM1C | 9 | 6 | 7 | 7 | 32 | 25 | O | DIG | MCCP1 Output C |
| OCM1D | 10 | 7 | 8 | 8 | 41 | 37 | O | DIG | MCCP1 Output D |
| OCM1E | 2 | 27 | 33 | 36 | 40 | 36 | O | DIG | MCCP1 Output E |
| OCM1F | 3 | 28 | 34 | 37 | 22 | 12 | O | DIG | MCCP1 Output F |
| OCM2A | 19 | 16 | 5 | 5 | 29 | 21 | O | DIG | MCCP2 Output A |
| OCM2B | 26 | 23 | 29 | 32 | 39 | 35 | O | DIG | MCCP2 Output B |
| OCM2C | 4 | 1 | 35 | 38 | 23 | 13 | O | DIG | MCCP2 Output C |
| OCM2D | 5 | 2 | 36 | 39 | 24 | 14 | O | DIG | MCCP2 Output D |
| OCM2E | 6 | 3 | 1 | 1 | 25 | 15 | O | DIG | MCCP2 Output E |
| OCM2F | 7 | 4 | 2 | 2 | 26 | 16 | O | DIG | MCCP2 Output F |
| OCM3A | 24 | 21 | 11 | 11 | 37 | 54 | O | DIG | MCCP3 Output A |
| OCM3B | 25 | 22 | 28 | 31 | 15 | 33 | O | DIG | MCCP3 Output B |
| OCM3C | 11 | 8 | 9 | 9 | 35 | 59 | O | DIG | MCCP3 Output C |
| OCM3D | 12 | 9 | 10 | 10 | 36 | 41 | O | DIG | MCCP3 Output D |
| OCM3E | 14 | 11 | 15 | 15 | 45 | 42 | O | DIG | MCCP3 Output E |
| OCM3F | 16 | 13 | 17 | 17 | 47 | 45 | O | DIG | MCCP3 Output F |
| OSC1 | 9 | 6 | 7 | 7 | 32 | 25 | — | — | Primary Oscillator crystal |
| OSC2 | 10 | 7 | 8 | 8 | 33 | 26 | — | — | Primary Oscillator crystal |
| PGEC1 | 5 | 2 | 36 | 39 | 24 | 14 | I | ST | ICSP™ Port 1 programming clock input |
| PGEC2 | 2 | 27 | 33 | 36 | 21 | 11 | I | ST | ICSP Port 2 programming clock input |
| PGEC3 | 19 | 16 | 21 | 22 | 5 | 55 | I | ST | ICSP Port 3 programming clock input |
| PGED1 | 4 | 1 | 35 | 38 | 23 | 13 | I/O | ST/DIG | ICSP Port 1 programming data |
| PGED2 | 3 | 28 | 34 | 37 | 22 | 12 | I/O | ST/DIG | ICSP Port 2 programming data |
| PGED3 | 14 | 11 | 15 | 15 | 45 | 43 | I/O | ST/DIG | ICSP Port 3 programming data |
| PWRLCLK | 12 | 9 | 10 | 10 | 36 | 29 | I | ST | Real-Time Clock 50/60 Hz clock input |

|  |  |  |  |
| --- | --- | --- | --- |
| **Legend:** | ST = Schmitt Trigger input buffer | DIG = Digital input/output | P = Power |
|  | I2C = I2C/SMBus input buffer | ANA = Analog level input/output |  |

TABLE 1-1: PIC32MM0256GPM064 FAMILY PINOUT DESCRIPTION (CONTINUED)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin Name** | **Pin Number** | | | | | | **Pin Type** | **Buffer Type** | **Description** |
| **28-Pin SSOP** | **28-Pin QFN/ UQFN** | **36-Pin QFN** | **40-Pin UQFN** | **48-Pin QFN/ TQFP** | **64-Pin QFN/ TQFP** |
| RA0 | 2 | 27 | 33 | 36 | 21 | 11 | I/O | ST/DIG | PORTA digital I/Os |
| RA1 | 3 | 28 | 34 | 37 | 22 | 12 | I/O | ST/DIG |
| RA2 | 9 | 6 | 7 | 7 | 32 | 25 | I/O | ST/DIG |
| RA3 | 10 | 7 | 8 | 8 | 33 | 26 | I/O | ST/DIG |
| RA4 | 12 | 9 | 10 | 10 | 36 | 29 | I/O | ST/DIG |
| RA5 | — | — | — | — | — | 54 | I/O | ST/DIG |
| RA6 | — | — | — | — | 20 | 10 | I/O | ST/DIG |
| RA7 | — | — | — | — | 14 | 1 | I/O | ST/DIG |
| RA8 | — | — | — | — | 34 | 27 | I/O | ST/DIG |
| RA9 | — | — | 11 | 11 | 37 | 30 | I/O | ST/DIG |
| RA10 | — | — | — | — | 13 | 64 | I/O | ST/DIG |
| RA11 | — | — | — | — | — | 8 | I/O | ST/DIG |
| RA12 | — | — | — | — | — | 7 | I/O | ST/DIG |
| RA13 | — | — | — | — | — | 6 | I/O | ST/DIG |
| RA14 | — | — | — | — | — | 59 | I/O | ST/DIG |
| RA15 | — | — | — | — | 8 | 58 | I/O | ST/DIG |
| RB0 | 4 | 1 | 35 | 38 | 23 | 13 | I/O | ST/DIG | PORTB digital I/Os |
| RB1 | 5 | 2 | 36 | 39 | 24 | 14 | I/O | ST/DIG |  |
| RB2 | 6 | 3 | 1 | 1 | 25 | 15 | I/O | ST/DIG |  |
| RB3 | 7 | 4 | 2 | 2 | 26 | 16 | I/O | ST/DIG |  |
| RB4 | 11 | 8 | 9 | 9 | 35 | 28 | I/O | ST/DIG |  |
| RB5 | 14 | 11 | 15 | 15 | 45 | 43 | I/O | ST/DIG |  |
| RB6 | 15 | 12 | 16 | 16 | 46 | 44 | I/O | ST/DIG |  |
| RB7 | 16 | 13 | 17 | 17 | 47 | 46 | I/O | ST/DIG |  |
| RB8 | 17 | 14 | 18 | 18 | 48 | 48 | I/O | ST/DIG |  |
| RB9 | 18 | 15 | 19 | 20 | 1 | 49 | I/O | ST/DIG |  |
| RB10 | 21 | 18 | 24 | 27 | 9 | 60 | I/O | ST/DIG |  |
| RB11 | 22 | 19 | 25 | 28 | 10 | 61 | I/O | ST/DIG |  |
| RB13 | 24 | 21 | 27 | 30 | 12 | 63 | I/O | ST/DIG |  |
| RB14 | 25 | 22 | 28 | 31 | 15 | 2 | I/O | ST/DIG |  |
| RB15 | 26 | 23 | 29 | 32 | 16 | 3 | I/O | ST/DIG |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Legend:** | ST = Schmitt Trigger input buffer | DIG = Digital input/output | P = Power |
|  | I2C = I2C/SMBus input buffer | ANA = Analog level input/output |  |

TABLE 1-1: PIC32MM0256GPM064 FAMILY PINOUT DESCRIPTION (CONTINUED)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin Name** | **Pin Number** | | | | | | **Pin Type** | **Buffer Type** | **Description** |
| **28-Pin SSOP** | **28-Pin QFN/ UQFN** | **36-Pin QFN** | **40-Pin UQFN** | **48-Pin QFN/ TQFP** | **64-Pin QFN/ TQFP** |
| RC0 | — | — | 3 | 3 | 27 | 19 | I/O | ST/DIG | PORTC digital I/Os |
| RC1 | — | — | 4 | 4 | 28 | 20 | I/O | ST/DIG |
| RC2 | — | — | 5 | 5 | 29 | 21 | I/O | ST/DIG |
| RC3 | — | — | 14 | 14 | 39 | 35 | I/O | ST/DIG |
| RC4 | — | — | — | — | 40 | 36 | I/O | ST/DIG |
| RC5 | — | — | — | — | 41 | 37 | I/O | ST/DIG |
| RC6 | — | — | — | — | 2 | 50 | I/O | ST/DIG |
| RC7 | — | — | — | — | 3 | 51 | I/O | ST/DIG |
| RC8 | — | — | 20 | 21 | 4 | 52 | I/O | ST/DIG |
| RC9 | 19 | 16 | 21 | 22 | 5 | 55 | I/O | ST/DIG |
| RC10 | — | — | — | — | — | 45 | I/O | ST/DIG |
| RC11 | — | — | — | — | — | 22 | I/O | ST/DIG |
| RC12 | — | — | — | — | 44 | 40 | I/O | ST/DIG |
| RC13 | — | — | — | — | — | 47 | I/O | ST/DIG |
| RC14 | — | — | — | — | — | 41 | I/O | ST/DIG |
| RC15 | — | — | — | — | — | 42 | I/O | ST/DIG |
| RD0 | — | — | — | — | 38 | 34 | I/O | ST/DIG | PORTD digital I/Os |
| RD1 | — | — | — | — | — | 53 | I/O | ST/DIG |
| RD2 | — | — | — | — | — | 32 | I/O | ST/DIG |
| RD3 | — | — | — | — | — | 33 | I/O | ST/DIG |
| RD4 | — | — | — | — | — | 31 | I/O | ST/DIG |
| REFCLKI | 18 | 15 | 19 | 20 | 38 | 34 | I | ST | External reference clock input |
| REFCLKO | 26 | 23 | 29 | 32 | 16 | 3 | O | ST | External reference clock output |
| RP1 | 2 | 27 | 33 | 36 | 21 | 11 | I/O | ST/DIG | Remappable peripherals (input or output) |
| RP2 | 3 | 28 | 34 | 37 | 22 | 12 | I/O | ST/DIG |
| RP3 | 9 | 6 | 7 | 7 | 32 | 25 | I/O | ST/DIG |
| RP4 | 10 | 7 | 8 | 8 | 33 | 26 | I/O | ST/DIG |
| RP5 | 12 | 9 | 10 | 10 | 36 | 29 | I/O | ST/DIG |
| RP6 | 4 | 1 | 35 | 38 | 23 | 13 | I/O | ST/DIG |
| RP7 | 5 | 2 | 36 | 39 | 24 | 14 | I/O | ST/DIG |
| RP8 | 6 | 3 | 1 | 1 | 25 | 15 | I/O | ST/DIG |
| RP9 | 7 | 4 | 2 | 2 | 26 | 16 | I/O | ST/DIG |
| RP10 | 11 | 8 | 9 | 9 | 35 | 28 | I/O | ST/DIG |
| RP11 | 14 | 11 | 15 | 15 | 45 | 43 | I/O | ST/DIG |
| RP12 | 16 | 13 | 17 | 17 | 47 | 46 | I/O | ST/DIG |
| RP13 | 17 | 14 | 18 | 18 | 48 | 48 | I/O | ST/DIG |
| RP14 | 18 | 15 | 19 | 20 | 1 | 49 | I/O | ST/DIG |
| RP15 | 24 | 21 | 27 | 30 | 12 | 63 | I/O | ST/DIG |
| RP16 | 25 | 22 | 28 | 31 | 15 | 2 | I/O | ST/DIG |
| RP17 | 26 | 23 | 29 | 32 | 16 | 3 | I/O | ST/DIG |
| RP18 | 19 | 16 | 21 | 22 | 5 | 55 | I/O | ST/DIG |
| RP19 | — | — | 5 | 5 | 29 | 21 | I/O | ST/DIG |
| RP20 | — | — | — | — | 3 | 51 | I/O | ST/DIG |

|  |  |  |  |
| --- | --- | --- | --- |
| **Legend:** | ST = Schmitt Trigger input buffer | DIG = Digital input/output | P = Power |
|  | I2C = I2C/SMBus input buffer | ANA = Analog level input/output |  |

TABLE 1-1: PIC32MM0256GPM064 FAMILY PINOUT DESCRIPTION (CONTINUED)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin Name** | **Pin Number** | | | | | | **Pin Type** | **Buffer Type** | **Description** |
| **28-Pin SSOP** | **28-Pin QFN/ UQFN** | **36-Pin QFN** | **40-Pin UQFN** | **48-Pin QFN/ TQFP** | **64-Pin QFN/ TQFP** |
| RP21 | — | — | — | — | 14 | 1 | I/O | ST/DIG | Remappable peripherals (input or output) |
| RP22 | — | — | — | — | 13 | 64 | I/O | ST/DIG |
| RP23 | — | — | — | — | 2 | 50 | I/O | ST/DIG |
| RP24 | — | — | 11 | 11 | 37 | 30 | I/O | ST/DIG |
| RTCC | 25 | 22 | 28 | 31 | 8 | 58 | O | DIG | Real-Time Clock/Calendar alarm/seconds output |
| SCK1 | 17 | 14 | 18 | 18 | 48 | 47 | I/O | ST/DIG | SPI1 clock (input or output) |
| SCK3 | 24 | 21 | 27 | 30 | 13 | 64 | I/O | ST/DIG | SPI3 clock (input or output) |
| SCL1 | 17 | 14 | 18 | 18 | 48 | 48 | I/O | I2C | I2C1 synchronous serial clock input/output |
| ASCL1 | 19 | 16 | 21 | 22 | 5 | 55 | I/O | I2C | Alternate I2C1 synchronous serial clock input/ output |
| SCL2 | 7 | 4 | 2 | 2 | 26 | 16 | I/O | I2C | I2C2 synchronous serial clock input/output |
| SCL3 | 24 | 21 | 27 | 30 | 12 | 63 | I/O | I2C | I2C3 synchronous serial clock input/output |
| SCLKI | 12 | 9 | 10 | 10 | 36 | 29 | I | ST | Secondary Oscillator digital clock input |
| SDA1 | 18 | 15 | 19 | 20 | 1 | 49 | I/O | I2C | I2C1 data input/output |
| ASDA1 | 14 | 11 | 15 | 15 | 45 | 43 | I/O | I2C | Alternate I2C1 data input/output |
| SDA2 | 6 | 3 | 1 | 1 | 25 | 15 | I/O | I2C | I2C2 data input/output |
| SDA3 | 16 | 13 | 17 | 17 | 47 | 46 | I/O | I2C | I2C3 data input/output |
| SDI1 | 25 | 22 | 28 | 31 | 15 | 31 | I | ST | SPI1 data input |
| SDI3 | 16 | 13 | 17 | 17 | 14 | 1 | I | ST | SPI3 data input |
| SDO1 | 18 | 15 | 19 | 20 | 38 | 34 | O | DIG | SPI1 data output |
| SDO3 | 19 | 16 | 21 | 22 | 34 | 27 | O | DIG | SPI3 data output |
| SOSCI | 11 | 8 | 9 | 9 | 35 | 28 | — | — | Secondary Oscillator crystal |
| SOSCO | 12 | 9 | 10 | 10 | 36 | 29 | — | — | Secondary Oscillator crystal |
| SS1 | 26 | 23 | 29 | 32 | 16 | 32 | I | ST | SPI1 slave select input |
| SS3 | 14 | 11 | 15 | 15 | 45 | 22 | I | ST | SPI3 slave select input |
| T1CK | 18 | 15 | 19 | 20 | 38 | 34 | I | ST | Timer1 external clock input |
| T2CK | 18 | 15 | 3 | 3 | 27 | 19 | I | ST | Timer2 external clock input |
| T3CK | 19 | 16 | 4 | 4 | 28 | 20 | I | ST | Timer3 external clock input |
| T1G | 18 | 15 | 19 | 20 | 38 | 34 | I | ST | Timer1 clock gate input |
| T2G | 18 | 15 | 3 | 3 | 27 | 19 | I | ST | Timer2 clock gate input |
| T3G | 19 | 16 | 4 | 4 | 28 | 20 | I | ST | Timer3 clock gate input |
| TCK | 17 | 14 | 18 | 18 | 48 | 48 | I | ST | JTAG clock input |
| TDI | 7 | 4 | 2 | 2 | 26 | 16 | I | ST | JTAG data input |
| TDO | 19 | 16 | 21 | 22 | 5 | 55 | O | DIG | JTAG data output |
| TMS | 18 | 15 | 19 | 20 | 1 | 49 | I | ST | JTAG mode select input |

|  |  |  |  |
| --- | --- | --- | --- |
| **Legend:** | ST = Schmitt Trigger input buffer | DIG = Digital input/output | P = Power |
|  | I2C = I2C/SMBus input buffer | ANA = Analog level input/output |  |

TABLE 1-1: PIC32MM0256GPM064 FAMILY PINOUT DESCRIPTION (CONTINUED)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Pin Name** | **Pin Number** | | | | | | **Pin Type** | **Buffer Type** | **Description** |
| **28-Pin SSOP** | **28-Pin QFN/ UQFN** | **36-Pin QFN** | **40-Pin UQFN** | **48-Pin QFN/ TQFP** | **64-Pin QFN/ TQFP** |
| U1BCLK | 18 | 15 | 19 | 20 | 38 | 34 | O | DIG | UART1 IrDA® 16x baud clock output |
| U1CTS | 17 | 14 | 18 | 18 | 48 | 6 | I | ST | UART1 Clear-to-Send |
| U1RTS | 18 | 15 | 19 | 20 | 38 | 34 | O | DIG | UART1 Ready-to-Send |
| U1RX | 26 | 23 | 29 | 32 | 20 | 10 | I | ST | UART1 receive data input |
| U1TX | 25 | 22 | 28 | 31 | 44 | 40 | O | DIG | UART1 transmit data output |
| USBID | 14 | 11 | 15 | 15 | 45 | 43 | I | ST | USB OTG ID (OTG mode only) |
| USBOEN | 19 | 16 | 21 | 22 | 5 | 55 | O | — | USB transceiver output enable flag |
| VBUSON | 25 | 22 | 28 | 31 | 15 | 2 | O | — | USB host and On-The-Go (OTG) bus power control output |
| VBUS | 15 | 12 | 16 | 16 | 46 | 44 | P | — | USB VBUS connection (5V nominal) |
| VUSB3V3 | 23 | 20 | 26 | 29 | 11 | 62 | P | — | USB transceiver power input (3.3V nominal) |
| VCAP | 20 | 17 | 22 | 24 | 7 | 56 | P | — | Core voltage regulator filter capacitor connection |
| VDD | 13,28 | 10,25 | 13,23,31 | 13,26,  34 | 18,30,  43 | 17,23,  39,57 | P | — | Digital modules power supply |
| VREF- | 3 | 28 | 34 | 37 | 22 | 12 | I | ANA | Analog-to-Digital Converter negative reference |
| VREF+ | 2 | 27 | 33 | 36 | 21 | 11 | I | ANA | Analog-to-Digital Converter positive reference |
| VSS | 8,27 | 5,24 | 6,12,30 | 6,12,33 | 6,17,31,  42 | 18,24,  38 | P | — | Digital modules ground |

|  |  |  |  |
| --- | --- | --- | --- |
| **Legend:** | ST = Schmitt Trigger input buffer | DIG = Digital input/output | P = Power |
|  | I2C = I2C/SMBus input buffer | ANA = Analog level input/output |  |

NOTES:

# GUIDELINES FOR GETTING STARTED WITH 32-BIT MICROCONTROLLERS

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a compre- hensive reference source. To complement the information in this data sheet, refer to the *“PIC32 Family Reference Manual”*, which is available from the Microchip web site ([www.microchip.com/PIC32](http://www.microchip.com/PIC32)). The information in this data sheet supersedes the information in the FRM.

### Basic Connection Requirements

Getting started with the PIC32MM0256GPM064 family of 32-bit Microcontrollers (MCUs) requires attention to a minimal set of device pin connections before pro- ceeding with development. The following is a list of pin names, which must always be connected:

* All VDD and VSS pins

(see [**Section 2.2 “Decoupling Capacitors”**](#_bookmark32))

* All AVDD and AVSS pins, even if the ADC module is not used (see [**Section 2.2 “Decoupling Capacitors”**](#_bookmark32))
* MCLR pin (see [**Section 2.3 “Master Clear (MCLR) Pin”**](#_bookmark36))
* VCAP pin (see [**Section 2.4 “Voltage Regulator Pin (VCAP)”**](#_bookmark44))
* PGECx/PGEDx pins, used for In-Circuit Serial Programming™ (ICSP™) and debugging purposes (see [**Section 2.5 “ICSP Pins”**](#_bookmark49))
* OSC1 and OSC2 pins, when external oscillator source is used (see [**Section 2.7 “External Oscillator Pins”**](#_bookmark54))
* VUSB3V3 pin, this pin must be powered for USB operation (see [**Section 18.4 “Powering the USB Transceiver”**](#_bookmark397))

The following pin(s) may be required as well:

VREF+/VREF- pins, used when external voltage reference for the ADC module is implemented.

### Decoupling Capacitors

The use of decoupling capacitors on power supply pins, such as VDD, VSS, AVDD and AVSS, is required. See [Figure 2-1](#_bookmark34).

Consider the following criteria when using decoupling capacitors:

• **Value and type of capacitor:** A value of 0.1 µF (100 nF), 10-20V is recommended. The capacitor should be a low Equivalent Series Resistance

(low-ESR) capacitor and have resonance frequency in the range of 20 MHz and higher. It is further recommended that ceramic capacitors be used.

• **Placement on the printed circuit board:** The decoupling capacitors should be placed as close to the pins as possible. It is recommended that the capacitors be placed on the same side of the board as the device. If space is constricted, the capacitor can be placed on another layer on the PCB using a via; however, ensure that the trace length from the pin to the capacitor is within one-quarter inch

(6 mm) in length.

• **Handling high-frequency noise:** If the board is experiencing high-frequency noise, upward of tens of MHz, add a second ceramic-type capacitor in parallel to the above described decoupling capaci- tor. The value of the second capacitor can be in the range of 0.01 µF to 0.001 µF. Place this second capacitor next to the primary decoupling capacitor. In high-speed circuit designs, consider implement- ing a decade pair of capacitances, as close to the power and ground pins as possible. For example,

0.1 µF in parallel with 0.001 µF.

* **Maximizing performance:** On the board layout from the power supply circuit, run the power and return traces to the decoupling capacitors first, and then to the device pins. This ensures that the decoupling capacitors are first in the power chain. Equally important is to keep the trace length between the capacitor and the power pins to a minimum, thereby reducing PCB track inductance.

**Note:** The AVDD and AVSS pins must be connected, regardless of ADC use and the ADC voltage reference source.

FIGURE 2-1: RECOMMENDED

MINIMUM CONNECTION



VDD

10 µF

CEFC

0.1 µF Ceramic

R

R1

MCLR

C

VUSB3V3

USB

**(1)**

Power

**PIC32**

VDD

VSS

VSS

VDD

0.1 µF Ceramic

0.1 µF Ceramic

0.1 µF Ceramic

0.1 µF Ceramic

**Note 1:** Refer to [**Section 18.4 “Powering the USB**](#_bookmark397)[**Transceiver”**](#_bookmark397) for requirements of this pin.

VCAP/VCORE

VDD

VSS

2.2.1 BULK CAPACITORS

AVDD

AVSS

VDD

VSS

The use of a bulk capacitor is recommended to improve power supply stability. Typical values range from 4.7 µF to 47 µF. This capacitor should be located as close to the device as possible.

### Master Clear (MCLR) Pin

The MCLR pin provides for two specific device functions:

* Device Reset
* Device Programming and Debugging

Pulling The MCLR pin low generates a device Reset. [Figure 2-2](#_bookmark39) illustrates a typical MCLR circuit. During device programming and debugging, the resistance and capacitance that can be added to the pin must be considered. Device programmers and debuggers drive the MCLR pin. Consequently, specific voltage levels (VIH and VIL) and fast signal transitions must not be adversely affected. Therefore, specific values of R and C will need to be adjusted based on the application and PCB requirements.

For example, as illustrated in [Figure 2-2](#_bookmark39), it is recommended that the capacitor, C, be isolated from the MCLR pin during programming and debugging operations.

Place the components illustrated in [Figure 2-2](#_bookmark39) within one-quarter inch (6 mm) from the MCLR pin.

FIGURE 2-2: EXAMPLE OF MCLR PIN

**CONNECTIONS(**[**1**](#_bookmark41)**,**[**2**](#_bookmark42)**,**[**3**](#_bookmark43)**)**

VDD

R 10k

0.1 µF**(2)** C

R1**(1)**

1 k

MCLR

**PIC32**

1

5

4

2 VDD

PGECx**(3)** PGEDx**(3)**

3 VSS

6 NC

**Note 1:** 470  R1  1 k will limit any current flowing into MCLR from the external capacitor, C, in the event of MCLR pin breakdown, due to Electrostatic Discharge (ESD) or Electrical Overstress (EOS). Ensure that the MCLR pin VIH and VIL specifications are met without interfering with the debugger/programmer tools.

**2:** The capacitor can be sized to prevent unintentional Resets from brief glitches or to extend the device Reset period during POR.

**3:** No pull-ups or bypass capacitors are allowed on active debug/program PGECx/PGEDx pins.

ICSP™

**Note:** When MCLR is used to wake the device from Retention Sleep, a POR Reset will occur.

### Voltage Regulator Pin (VCAP)

A low-ESR (< 5Ω) capacitor is required on the VCAP pin to stabilize the output voltage of the on-chip voltage regulator. The VCAP pin must not be connected to VDD and must use a capacitor of 10 µF connected to ground. The type can be ceramic or tantalum. Suitable examples of capacitors are shown in [Table 2-1](#_bookmark47). Capacitors with equivalent specification can be used.

**ESR (****)**

The placement of this capacitor should be close to VCAP. It is recommended that the trace length not exceed

0.25 inch (6 mm). Refer to [**Section 29.0 “Electrical Characteristics”**](#_bookmark636) for additional information.

Designers may use [Figure 2-3](#_bookmark46) to evaluate ESR equivalence of candidate devices.

FIGURE 2-3: FREQUENCY vs. ESR

PERFORMANCE FOR SUGGESTED VCAP

10

1

0.1

0.01


0.001

0.01 0.1 1

10 100 1000 10,000

**Frequency (MHz)**

**Note:** Typical data measurement at +25°C, 0V DC bias.



.

TABLE 2-1: SUITABLE CAPACITOR EQUIVALENTS

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Make** | **Part #** | **Nominal Capacitance** | **Base Tolerance** | **Rated Voltage** | **Temp. Range** |
| TDK | C3216X7R1C106K | 10 µF | ±10% | 16V | -55 to +125ºC |
| TDK | C3216X5R1C106K | 10 µF | ±10% | 16V | -55 to +85ºC |
| Panasonic | ECJ-3YX1C106K | 10 µF | ±10% | 16V | -55 to +125ºC |
| Panasonic | ECJ-4YB1C106K | 10 µF | ±10% | 16V | -55 to +85ºC |
| Murata | GRM319R61C106KE15D | 10 µF | ±10% | 16V | -55 to +85ºC |

2.4.1 CONSIDERATIONS FOR CERAMIC CAPACITORS

In recent years, large value, low-voltage, surface-mount ceramic capacitors have become very cost effective in sizes up to a few tens of microfarad. The low-ESR, small physical size and other properties make ceramic capacitors very attractive in many types of applications.

Ceramic capacitors are suitable for use with the inter- nal voltage regulator of this microcontroller. However, some care is needed in selecting the capacitor to ensure that it maintains sufficient capacitance over the intended operating range of the application.

Typical low-cost, 10 F ceramic capacitors are available in X5R, X7R and Y5V dielectric ratings (other types are also available, but are less common). The initial tolerance specifications for these types of capacitors are often specified as ±10% to ±20% (X5R and X7R) or -20%/+80% (Y5V). However, the effective capaci- tance that these capacitors provide in an application circuit will also vary based on additional factors, such as the applied DC bias voltage and the temperature. The total in-circuit tolerance is, therefore, much wider than the initial tolerance specification.

The X5R and X7R capacitors typically exhibit satis- factory temperature stability (ex: ±15% over a wide temperature range, but consult the manufacturer’s data sheets for exact specifications). However, Y5V capaci- tors typically have extreme temperature tolerance specifications of +22%/-82%. Due to the extreme temperature tolerance, a 10 F nominal rated Y5V type capacitor may not deliver enough total capacitance to meet minimum internal voltage regulator stability and transient response requirements. Therefore, Y5V capacitors are not recommended for use with the internal regulator.

In addition to temperature tolerance, the effective capacitance of large value ceramic capacitors can vary substantially, based on the amount of DC voltage applied to the capacitor. This effect can be very significant, but is often overlooked or is not always documented.

Typical DC bias voltage vs. capacitance graph for X7R type capacitors is shown in [Figure 2-4](#_bookmark48).

FIGURE 2-4: DC BIAS VOLTAGE vs.

CAPACITANCE CHARACTERISTICS

10

0

-10

-20

-30

16V Capacitor

-40

-50

-60

-70

-80

10V Capacitor

6.3V Capacitor

0 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17

DC Bias Voltage (VDC)

**Capacitance Change (%)**

When selecting a ceramic capacitor to be used with the internal voltage regulator, it is suggested to select a high-voltage rating, so that the operating voltage is a small percentage of the maximum rated capacitor voltage. The minimum DC rating for the ceramic capacitor on VCAP is 16V. Suggested capacitors are shown in [Table 2-1](#_bookmark47).

### ICSP Pins

The PGECx and PGEDx pins are used for In-Circuit Serial Programming™ (ICSP™) and debugging pur- poses. It is recommended to keep the trace length between the ICSP connector and the ICSP pins on the device as short as possible. If the ICSP connec- tor is expected to experience an ESD event, a series resistor is recommended, with the value in the range of a few tens of Ohms, not to exceed 100 Ohms.

Pull-up resistors, series diodes and capacitors on the PGECx and PGEDx pins are not recommended as they will interfere with the programmer/debugger communi- cations to the device. If such discrete components are an application requirement, they should be removed from the circuit during programming and debugging. Alternatively, refer to the AC/DC characteristics and timing requirements information in the respective device Flash programming specification for information on capacitive loading limits and pin Input Voltage High (VIH) and Input Voltage Low (VIL) requirements.


Ensure that the “Communication Channel Select” (i.e., PGECx/PGEDx pins) programmed into the device

matches the physical connections for the ICSP to MPLAB® ICD 3 or MPLAB REAL ICE™ In-Circuit Emulator.

For more information on MPLAB® ICD 3 and REAL ICE connection requirements, refer to the following documents that are available from the Microchip web site.

* *“Using MPLAB® ICD 3”* (poster) (DS51765)
* *“Development Tools Design Advisory”* (DS51764)
* *“MPLAB® REAL ICE™ In-Circuit Emulator User’s Guide” (*DS51616)
* *“Using MPLAB® REAL ICE™ In-Circuit Emulator”*

(poster) (DS51749)



### JTAG

The TMS, TDO, TDI and TCK pins are used for testing and debugging according to the Joint Test Action Group (JTAG) standard. It is recommended to keep the trace length between the JTAG connector, and the JTAG pins on the device, as short as possible. If the JTAG connector is expected to experience an ESD event, a series resistor is recommended, with the value in the range of a few tens of Ohms, not to exceed 100 Ohms.

Pull-up resistors, series diodes and capacitors on the TMS, TDO, TDI and TCK pins are not recommended as they will interfere with the programmer/debugger com- munications to the device. If such discrete components are an application requirement, they should be removed from the circuit during programming and debugging. Alternatively, refer to the AC/DC characteristics and timing requirements information in the respective device Flash programming specification for information on capacitive loading limits, and pin Input Voltage High (VIH) and Input Voltage Low (VIL) requirements.

For additional information and design guidance on oscillator circuits, please refer to these Microchip Application Notes, available at the corporate web site: (www.microchip.com).

* AN826, *“Crystal Oscillator Basics and Crystal Selection for rfPIC™ and PICmicro® Devices”*
* AN849, *“Basic PICmicro® Oscillator Design”*
* AN943, *“Practical PICmicro® Oscillator Analysis and Design”*
* AN949, *“Making Your Oscillator Work”*

FIGURE 2-5: SUGGESTED OSCILLATOR

CIRCUIT PLACEMENT

Oscillator

Secondary Guard Trace

Guard Ring

Main Oscillator

### External Oscillator Pins

This family of devices has options for two external oscillators: a high-frequency Primary Oscillator and a low-frequency Secondary Oscillator (refer to [**Section 9.0 “Oscillator Configuration”**](#_bookmark207) for details).

The oscillator circuit should be placed on the same side of the board as the device. Also, place the oscillator



### Unused I/Os

circuit close to the respective oscillator pins, not exceeding one-half inch (12 mm) distance between them. The load capacitors should be placed next to the oscillator itself, on the same side of the board. Use a grounded copper pour around the oscillator circuit to isolate them from surrounding circuits. The grounded copper pour should be routed directly to the MCU ground. Do not run any signal traces or power traces inside the ground pour. Also, if using a two-sided board, avoid any traces on the other side of the board where the crystal is placed. A suggested layout is illustrated in [Figure 2-5](#_bookmark52).

To minimize power consumption, unused I/O pins should not be allowed to float as inputs. They can be configured as outputs and driven to a logic low or logic high state.

Alternatively, inputs can be reserved by ensuring the pin is always configured as an input and externally con- necting the pin to VSS or VDD. A current-limiting resistor may be used to create this connection if there is any risk of inadvertently configuring the pin as an output with the logic output state opposite of the chosen power rail.

NOTES:

# CPU

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To complement the information in this data

sheet, refer to **Section 50. “CPU for Devices with MIPS32® microAptiv™ and M-Class Cores”** (DS60001192) in the

*“PIC32 Family Reference Manual”*, which is available from the Microchip web site ([www.microchip.com/PIC32).](http://www.microchip.com/PIC32)) MIPS32®

[microAptiv™ UC microprocessor core](http://www.imgtec.com/) [resources are available at: www.imgtec.com.](http://www.imgtec.com/) The information in this data sheet supersedes the information in the FRM.

The MIPS32® microAptiv™ UC microprocessor core is the heart of the PIC32MM0256GPM064 family devices. The CPU fetches instructions, decodes each instruction, fetches source operands, executes each instruction and writes the results of the instruction execution to the proper destinations.

### Features

The PIC32MM0256GPM064 family processor core key features include:

* 5-Stage Pipeline
* 32-Bit Address and Data Paths
* MIPS32 Enhanced Architecture:
  + Multiply-add and multiply-subtract instructions.
  + Targeted multiply instruction.
  + Zero and one detect instructions.
  + WAIT instruction.
  + Conditional move instructions.
  + Vectored interrupts.
  + Atomic interrupt enable/disable.
  + One GPR shadow set to minimize latency of interrupts.
  + Bit field manipulation instructions.
* microMIPS™ Instruction Set:
  + microMIPS allows improving the code size density over MIPS32, while maintaining MIPS32 performance.
  + microMIPS supports all MIPS32 instructions (except for branch-likely instructions) with new optimized 32-bit encoding. Frequent MIPS32 instructions are available as 16-bit instructions.
  + Added seventeen new and thirty-five MIPS32® corresponding, commonly used instructions in 16-bit opcode format.
  + Stack Pointer implicit in instruction.
  + MIPS32 assembly and ABI compatible.
* Memory Management Unit with Simple Fixed Mapping Translation (FMT) Mechanism
* Multiply/Divide Unit (MDU):
  + Configurable using high-performance multiplier array.
  + Maximum issue rate of one 32x16 multiply per clock.
  + Maximum issue rate of one 32x32 multiply every other clock.
  + Early-in iterative divide. Minimum 11 and maximum 33 clock latency (dividend (rs) sign extension dependent).
* Power Control:
  + No minimum frequency: 0 MHz.
  + Power-Down mode (triggered by WAIT

instruction).

* EJTAG Debug/Profiling:
  + CPU control with start, stop and single stepping.
  + Software breakpoints via the SDBBP

instruction.

* + Simple hardware breakpoints on virtual addresses, 4 instruction and

2 data breakpoints.

* + PC and/or load/store address sampling for profiling.
  + Performance counters.
  + Supports Fast Debug Channel (FDC).

A block diagram of the PIC32MM0256GPM064 family processor core is shown in [Figure 3-1](#_bookmark59).





EJTAG

**Debug/Profiling**

Breakpoints Fast Debug Channel

Performance Counters

FIGURE 3-1: PIC32MM0256GPM064 FAMILY MICROPROCESSOR CORE BLOCK DIAGRAM

**MIPS32® microAptiv™ UC Microprocessor Core**

SYSCLK

MMU

System Interface

Interrupt Interface

2-Wire Debug



Enhanced MDU

**Execution Unit**

ALU/Shift Atomic/LdSt MCU ASE

GPR

(2 sets)



Power Management

System Coprocessor

System Bus



Decode (microMIPS™)

### Architecture Overview

The MIPS32® microAptiv™ UC microprocessor core in the PIC32MM0256GPM064 family devices contains several logic blocks, working together in parallel, pro- viding an efficient high-performance computing engine. The following blocks are included with the core:

* Execution Unit
* General Purpose Register (GPR)
* Multiply/Divide Unit (MDU)
* System Control Coprocessor (CP0)
* Memory Management Unit (MMU)
* Power Management
* microMIPS Instructions Decoder
* Enhanced JTAG (EJTAG) Controller
  + 1. EXECUTION UNIT

The processor core execution unit implements a load/ store architecture with single-cycle ALU operations (logical, shift, add, subtract) and an autonomous Multiply/ Divide Unit (MDU). The core contains thirty-two 32-bit General Purpose Registers (GPRs) used for integer operations and address calculation. One additional register file shadow set (containing thirty-two registers) is added to minimize context switching overhead during interrupt/exception processing. The register file consists of two read ports and one write port, and is fully bypassed to minimize operation latency in the pipeline.

The execution unit includes:

* 32-bit adder used for calculating the data address
* Address unit for calculating the next instruction address
* Logic for branch determination and branch target address calculation
* Load aligner
* Bypass multiplexers used to avoid Stalls when executing instruction streams where data produc- ing instructions are followed closely by consumers for their results
* Leading zero/one detect unit for implementing the

CLZ and CLO instructions

* Arithmetic Logic Unit (ALU) for performing arithmetic and bitwise logical operations
* Shifter and store aligner
  + 1. MULTIPLY/DIVIDE UNIT (MDU)

The microAptiv UC core includes a Multiply/Divide Unit (MDU) that contains a separate pipeline for multiply and divide operations. This pipeline operates in parallel with the Integer Unit (IU) pipeline and does not stall when the IU pipeline stalls. This allows the long- running MDU operations to be partially masked by system Stalls and/or other Integer Unit instructions.

The high-performance MDU consists of a 32x16 booth recoded multiplier, Result/Accumulation registers (HI and LO), a divide state machine, and the necessary multiplexers and control logic. The first number shown (‘32’ of 32x16) represents the rs operand. The second number (‘16’ of 32x16) represents the rt operand. The microAptiv UC core only checks the value of the rt operand to determine how many times the operation must pass through the multiplier. The 16x16 and 32x16 operations pass through the multiplier once. A 32x32 operation passes through the multiplier twice.

The MDU supports execution of one 16x16 or 32x16 multiply operation every clock cycle; 32x32 multiply operations can be issued every other clock cycle. Appro- priate interlocks are implemented to stall the issuance of back-to-back, 32x32 multiply operations. The multiply operand size is automatically determined by logic built into the MDU. Divide operations are implemented with a simple 1-bit-per-clock iterative algorithm. An early-in detection checks the sign extension of the dividend (rs) operand. If rs is 8 bits wide, 23 iterations are skipped. For a 16-bit wide rs, 15 iterations are skipped, and for a 24-bit wide rs, 7 iterations are skipped. Any attempt to issue a subsequent MDU instruction while a divide is still active causes an IU pipeline Stall until the divide operation has completed.

[Table 3-1](#_bookmark62) lists the repeat rate (peak issue rate of cycles until the operation can be re-issued), and latency (number of cycles until a result is available) for the microAptiv UC core multiply and divide instructions. The approximate latency and repeat rates are listed in terms of pipeline clocks.

TABLE 3-1: MULTIPLY/DIVIDE UNIT LATENCIES AND REPEAT RATES

|  |  |  |  |
| --- | --- | --- | --- |
| **Opcode** | **Operand Size (mul *rt*) (div *rs*)** | **Latency** | **Repeat Rate** |
| MULT/MULTU, MADD/MADDU, MSUB/MSUBU | 16 bits | 1 | 1 |
| 32 bits | 2 | 2 |
| MUL (GPR destination) | 16 bits | 2 | 1 |
| 32 bits | 3 | 2 |
| DIV/DIVU | 8 bits | 12 | 11 |
| 16 bits | 19 | 18 |
| 24 bits | 26 | 25 |
| 32 bits | 33 | 32 |

The MIPS® architecture defines that the result of a multiply or divide operation be placed in the HI and LO registers. Using the Move-From-HI (MFHI) and Move- From-LO (MFLO) instructions, these values can be transferred to the general purpose register file.

In addition to the HI/LO targeted operations, the MIPS architecture also defines a Multiply instruction, MUL, which places the least significant results in the primary register file instead of the HI/LO register pair. By avoid- ing the explicit MFLO instruction, required when using the LO register, and by supporting multiple destination registers, the throughput of multiply-intensive operations is increased.

Two other instructions, Multiply-Add (MADD) and Multiply-Subtract (MSUB), are used to perform the multiply-accumulate and multiply-subtract operations. The MADD instruction multiplies two numbers and then adds the product to the current contents of the HI and LO registers. Similarly, the MSUB instruction multiplies two operands and then subtracts the product from the HI and LO registers. The MADD and MSUB operations are commonly used in DSP algorithms.

* + 1. SYSTEM CONTROL

COPROCESSOR (CP0)

In the MIPS architecture, CP0 is responsible for the virtual-to-physical address translation, the exception control system, the processor’s diagnostics capability, the operating modes (Kernel, User and Debug) and whether interrupts are enabled or disabled. These configuration options and other system information are available by accessing the CP0 registers listed in [Table 3-2](#_bookmark64).

TABLE 3-2: COPROCESSOR 0 REGISTERS

|  |  |  |
| --- | --- | --- |
| **Register Number** | **Register Name** | **Function** |
| 0-3 | Reserved | Reserved in the microAptiv™ UC. |
| 4 | UserLocal | User information that can be written by privileged software and read via  RDHWR Register 29. |
| 5-6 | Reserved | Reserved in the microAptiv UC. |
| 7 | HWREna | Enables access via the RDHWR instruction to selected hardware registers in Non-Privileged mode. |
| 8 | BadVAddr**(**[**1**](#_bookmark66)**)** | Reports the address for the most recent address related exception. |
| 9 | Count**(**[**1**](#_bookmark66)**)** | Processor cycle count. |
| 10 | Reserved | Reserved in the microAptiv UC. |
| 11 | Compare**(**[**1**](#_bookmark66)**)** | Timer interrupt control. |
| 12 | Status/ IntCtl/ SRSCtl/ SRSMap1/ View\_IPL/ SRSMAP2 | Processor status and control; interrupt control and shadow set control. |
| 13 | Cause**(**[**1**](#_bookmark66)**)**/ View\_RIPL | Cause of last exception. |
| 14 | EPC**(**[**1**](#_bookmark66)**)** | Program Counter at last exception. |
| 15 | PRId/ EBase/ CDMMBase | Processor identification and revision; exception base address; Common Device Memory Map Base register. |
| 16 | CONFIG/ CONFIG1/ CONFIG2/ CONFIG3/ CONFIG7 | Configuration registers. |
| 7-22 | Reserved | Reserved in the microAptiv UC. |
| 23 | Debug/ Debug2/ TraceControl/ TraceControl2/  UserTraceData1/ TraceBPC**(**[**2**](#_bookmark67)**)** | EJTAG Debug register. EJTAG Debug Register 2. EJTAG Trace Control register.  EJTAG Trace Control Register 2. EJTAG User Trace Data 1 register. EJTAG Trace Breakpoint register. |
| 24 | DEPC**(**[**2**](#_bookmark67)**)**/  UserTraceData2 | Program Counter at last debug exception. EJTAG User Trace Data 2 register. |
| 25 | PerfCtl0/ PerfCnt0/ PerfCtl1/ PerfCnt1 | Performance Counter 0 control. Performance Counter 0.  Performance Counter 1 control. Performance Counter 1. |
| 26 | ErrCtl | Software parity check enable. |
| 27 | CacheErr | Records information about SRAM parity errors. |
| 28-29 | Reserved | Reserved in the PIC32 core. |
| 30 | ErrorEPC**(**[**1**](#_bookmark66)**)** | Program Counter at last error. |
| 31 | DeSAVE**(**[**2**](#_bookmark67)**)** | Debug Handler Scratchpad register. |

**Note 1:** Registers used in exception processing.

**2:** Registers used in debug.

### Power Management

The processor core offers a number of power management features, including low-power design, active power management and Power-Down modes of operation. The core is a static design that supports slowing or halting of the clocks, which reduces system power consumption during Idle periods.

The mechanism for invoking Power-Down mode is implemented through execution of the WAIT instruction, used to initiate Sleep or Idle. The majority of the power consumed by the processor core is in the clock tree and clocking registers. The PIC32MM family makes extensive use of local gated clocks to reduce this dynamic power consumption.

### EJTAG Debug Support

The microAptiv UC core has an Enhanced JTAG (EJTAG) interface for use in the software debug. In addition to the standard mode of operation, the microAptiv UC core provides a Debug mode that is entered after a debug exception (derived from a hard- ware breakpoint, single-step exception, etc.) is taken and continues until a Debug Exception Return (DERET) instruction is executed. During this time, the processor executes the debug exception handler routine.

The EJTAG interface operates through the Test Access Port (TAP), a serial communication port used for trans- ferring test data in and out of the microAptiv UC core. In addition to the standard JTAG instructions, special instructions defined in the EJTAG specification specify which registers are selected and how they are used.

### MIPS32® microAptiv™ UC Core Configuration

[Register 3-1](#_bookmark71) through [Register 3-4](#_bookmark76) show the default configuration of the microAptiv UC core, which is included on PIC32MM0256GPM064 family devices.

REGISTER 3-1: CONFIG: CONFIGURATION REGISTER; CP0 REGISTER 16, SELECT 0

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | r-1 | R/W-0 | R/W-1 | R/W-0 | R/W-0 | R/W-1 | R/W-0 | r-0 |
| — | K23<2:0> | | | KU<2:0>**(**[**1**](#_bookmark73)**)** | | | — |
| 23:16 | r-0 | R-0 | R-1 | R-0 | r-0 | r-0 | r-0 | R-1 |
| — | UDI | SB | MDU | — | — | — | DS |
| 15:8 | R-0 | R-0 | R-0 | R-0 | R-0 | R-1 | R-0 | R-1 |
| BE | AT<1:0> | | AR<2:0> | | | MT<2:1> | |
| 7:0 | R-1 | r-0 | r-0 | r-0 | r-0 | R/W-0 | R/W-1 | R/W-0 |
| MT<0> | — | — | — | — | K0<2:0> | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** | r = Reserved bit |  |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **Reserved:** This bit is hardwired to ‘1’ to indicate the presence of the CONFIG1 register bit 30-28 **K23<2:0>:** Cacheability of the kseg2 and kseg3 Segments bits

010 = Cache is not implemented

bit 27-25 **KU<2:0>:** Cacheability of the kuseg and useg Segments bits**(**[**1**](#_bookmark73)**)**

010 = Cache is not implemented

bit 24-23 **Reserved:** Must be written as zeros; returns zeros on reads bit 22 **UDI:** User-Defined bit

0 = CorExtend user-defined instructions are not implemented

bit 21 **SB:** SimpleBE bit

1 = Only Simple Byte Enables are allowed on the internal bus interface bit 20 **MDU:** Multiply/Divide Unit bit

0 = Fast, high-performance MDU

bit 19-17 **Reserved:** Must be written as zeros; returns zeros on reads bit 16 **DS:** Dual SRAM Interface bit

1 = Dual instruction/data SRAM interface

bit 15 **BE:** Endian Mode bit

0 = Little-endian

bit 14-13 **AT<1:0>:** Architecture Type bits

00 = MIPS32®

bit 12-10 **AR<2:0>:** Architecture Revision Level bits

001 = MIPS32 Release 2 bit 9-7 **MT<2:0>:** MMU Type bits

011 = Fixed mapping

bit 6-3 **Reserved:** Must be written as zeros; returns zeros on reads bit 2-0 **K0<2:0>:** kseg0 Coherency Algorithm bits

010 = Cache is not implemented

**Note 1:** The KU<2:0> bits are not usable as this device does not support User mode.

REGISTER 3-2: CONFIG1: CONFIGURATION REGISTER 1; CP0 REGISTER 16, SELECT 1

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | r-1 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | U-0 | U-0 | U-0 | R-1 | R-0 | R-0 | R-1 | R-0 |
| — | — | — | PC | WR | CA | EP | FP |

|  |  |  |
| --- | --- | --- |
| **Legend:** | r = Reserved bit |  |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **Reserved:** This bit is hardwired to ‘1’ to indicate the presence of the CONFIG2 register bit 30-5 **Unimplemented:** Read as ‘0’

bit 4 **PC:** Performance Counter bit

1 = The processor core contains performance counters bit 3 **WR:** Watch Register Presence bit

0 = No Watch registers are present

bit 2 **CA:** Code Compression Implemented bit

0 = No MIPS16e® are present bit 1 **EP:** EJTAG Present bit

1 = Core implements EJTAG bit 0 **FP:** Floating Point Unit bit

0 = Floating point unit is not implemented

REGISTER 3-3: CONFIG3: CONFIGURATION REGISTER 3; CP0 REGISTER 16, SELECT 3

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | r-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | R-0 | R-1 | R-0 | R-0 | R-0 | R-1 | R-1 |
| — | IPLW<1:0> | | MMAR<2:0> | | | MCU | ISAONEXC |
| 15:8 | R-0 | R-1 | R-1 | R-1 | U-0 | U-0 | U-0 | R-0 |
| ISA<1:0> | | ULRI | RXI | — | — | — | ITL |
| 7:0 | U-0 | R-1 | R-1 | R-0 | R-1 | U-0 | U-0 | R-0 |
| — | VEIC | VINT | SP | CDMM | — | — | TL |

|  |  |  |
| --- | --- | --- |
| **Legend:** | r = Reserved bit | y = Value set from Configuration bits on POR |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **Reserved:** This bit is hardwired as ‘0’ bit 30-23 **Unimplemented:** Read as ‘0’

bit 22-21 **IPLW<1:0>:** Width of the Status IPL and Cause RIPL bits

01 = IPL and RIPL bits are 8 bits in width

bit 20-18 **MMAR<2:0>:** microMIPS™ Architecture Revision Level bits

000 = Release 1

bit 17 **MCU:** MIPS® MCU ASE Implemented bit

1 = MCU ASE is implemented

bit 16 **ISAONEXC:** ISA on Exception bit

1 = microMIPS is used on entrance to an exception vector bit 15-14 **ISA<1:0>:** Instruction Set Availability bits

01 = Only microMIPS is implemented

bit 13 **ULRI:** UserLocal Register Implemented bit

1 = UserLocal Coprocessor 0 register is implemented bit 12 **RXI:** RIE and XIE Implemented in PageGrain bit

1 = RIE and XIE bits are implemented bit 11-9 **Unimplemented:** Read as ‘0’

bit 8 **ITL:** Indicates that iFlowtrace™ Hardware is Present bit

0 = The iFlowtrace hardware is not implemented in the core bit 7 **Unimplemented:** Read as ‘0’

bit 6 **VEIC:** External Vector Interrupt Controller bit

1 = Support for an external interrupt controller is implemented. bit 5 **VINT:** Vector Interrupt bit

1 = Vector interrupts are implemented bit 4 **SP:** Small Page bit

0 = 4-Kbyte page size

bit 3 **CDMM:** Common Device Memory Map bit

1 = CDMM is implemented bit 2-1 **Unimplemented:** Read as ‘0’ bit 0 **TL:** Trace Logic bit

0 = Trace logic is not implemented

REGISTER 3-4: CONFIG5: CONFIGURATION REGISTER 5; CP0 REGISTER 16, SELECT 5

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | R-1 |
| — | — | — | — | — | — | — | NF |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-1 **Unimplemented:** Read as ‘0’ bit 0 **NF:** Nested Fault bit

1 = Nested Fault feature is implemented

# MEMORY ORGANIZATION

PIC32MM microcontrollers provide 4 GBytes of unified virtual memory address space. All memory regions, including program memory, data memory, SFRs and Configuration registers, reside in this address space at their respective unique addresses. The data memory can be made executable, allowing the CPU to execute code from data memory.

Key features include:

* 32-Bit Native Data Width
* Separate Boot Flash Memory (BFM) for Protected Code
* Robust Bus Exception Handling to Intercept Runaway Code
* Simple Memory Mapping with Fixed Mapping Translation (FMT) Unit

The PIC32MM0256GPM064 family devices implement two address spaces: virtual and physical. All hardware resources, such as program memory, data memory and peripherals, are located at their respective physical addresses. Virtual addresses are exclusively used by the CPU to fetch and execute instructions. Physical addresses are used by peripherals, such as Flash controllers, that access memory independently of the CPU.

The virtual address space is divided into two segments of 512 Mbytes each, labeled kseg0 and kseg1. The Program Flash Memory (PFM) and Data RAM Memory (DRM) are accessible from either kseg0 or kseg1, while the Boot Flash Memory (BFM) and peripheral SFRs are accessible only from kseg1.

The Fixed Mapping Translation (FMT) unit translates the memory segments into corresponding physical address regions. [Figure 4-1](#_bookmark86) through [Figure 4-3](#_bookmark95) illus- trate the fixed mapping scheme, implemented by the PIC32MM0256GPM064 family core, between the virtual and physical address space.

The mapping of the memory segments depends on the CPU error level, set by the ERL bit in the CPU STATUS register. Error level is set (ERL = 1) by the CPU on a Reset, Soft Reset or Non-Maskable Interrupt (NMI). In this mode, the CPU can access memory by the physi- cal address. This mode is provided for compatibility with other MIPS processor cores that use a TLB-based MMU. The C start-up code clears the ERL bit to zero, so that when application software starts up, it sees the proper virtual to physical memory mapping.

### Alternate Configuration Bits Space

Every Configuration Word has an associated Alternate Word (designated by the letter A as the first letter in the name of the word). During device start-up, Primary Words are read, and if uncorrectable ECC errors are found, the BCFGERR (RCON<27>) flag is set and Alternate Words are used. If uncorrectable ECC errors are found in Primary and Alternate Words, the BCFGFAIL (RCON<26>) flag is set, and the default configuration is used. The Primary Configuration bits’ area is located at the address range, from 0x1FC01780 to 0x1FC017E8. The Alternate Configuration bits’ area is located at the address range, from 0x1FC01700 to 0x1FC01768.

### Bus Matrix (BMX)

The BMX is a switch fabric that connects the system bus initiators (Flash controller, CPU instruction, CPU data, system DMA and USB) to bus targets (RAM, Flash and peripherals without integrated DMA). All data and instructions are transferred through this bus. Only one initiator can connect to a given target at a time. Multiple initiators can be active at one time provided each one has a separate target. Multiple priority modes (Round Robin, Fixed CPU Highest and Fixed CPU Lowest) are available to allow the priority to be tailored to the application needs. Mode 0 is a Fixed Priority mode with the CPU having the highest priority (refer to [Table 4-1](#_bookmark84)). For most applications, this mode should be sufficient; however, it is possible for the CPU to generate sufficient bus traffic to ‘starve’ the other initiators attempting to access Flash memory, preventing them from performing transfers in the required time limit. If this ‘starvation’ occurs, the Round Robin or CPU Lowest mode should be chosen.

Mode 1 is a Fixed Priority mode with the CPU having the lowest priority (refer to [Table 4-1](#_bookmark84)). This mode can reduce the latency of DMA transfers because the DMA engines have a higher priority than the CPU.

Mode 2 is a Round Robin or Rotating Priority mode. The initiator’s priority for each target rotates with every access. This ensures, not that the initiator is starved, but the latency for accesses changes with every access; this makes the latency variable.

The Arbitration mode is selected by the BMXARB<1:0> bits (CFGCON<25:24>).

**Note:** The CPU has two initiators: one for data and the other for instructions. In all Arbitra- tion modes, the CPU data initiator has higher priority than the CPU instruction initiator.

TABLE 4-1: FIXED MODES ORDER OF PRIORITY

|  |  |
| --- | --- |
| **Mode 1** | **Mode 0** |
| **CPU Lowest** | **CPU Highest** |
| Highest Priority | |
| Flash Controller | Flash Controller |
| DMA | CPU |
| USB | USB |
| CPU | DMA |
| Lowest Priority | |

Refer to **Section 48. “Memory Organization and Permissions”** (DS60001214) in the *“PIC32 Family Reference Manual”*, which is available from the Microchip web site ([www.microchip.com/PIC32)](http://www.microchip.com/PIC32)) for more information regarding Bus Matrix operation.

### Flash Line Buffer

The Flash line buffer is a buffer that resides between the Bus Matrix and the Flash memory. When a Flash fetch is generated, an aligned double word (64 bits) is read. This is then placed in the Flash line buffer. If the next initiator requested address’s data is contained in the Flash line buffer, it is read directly without requiring another Flash fetch; if it is not in the Flash line buffer, a Flash fetch is generated.

**Note:** The Arbitration mode chosen only has an effect on system performance when a contention for a target occurs.

The Flash controller, when programming memory, always has the highest priority regardless of the priority mode setting.

**kseg1**

**kseg0**

|  |
| --- |
| 16 Kbytes RAM |
| Reserved |
| 64 Kbytes Flash |
| Reserved |
| SFRs |
| Reserved |
| Boot Flash |
| Configuration Bits**(**[**3**](#_bookmark90)**)** |
| Reserved |

FIGURE 4-1: MEMORY MAP FOR DEVICES WITH 64 Kbytes OF PROGRAM MEMORY([1](#_bookmark88))



**Virtual Memory Map**

0x00000000

0x7FFFFFFF

0x80000000

0x80003FFF

0x80004000

0x9CFFFFFF

0x9D000000

0x9D00FFFF

0x9D010000

0x9F7FFFFF

0x9F800000

0x9F80FFFF

0x9F810000

0x9FBFFFFF

0x9FC00000

0x9FC016FF

0x9FC01700

0x9FC017FF

0x9FC01800

0x9FFFFFFF

0xA0000000

0xA0003FFF

0xA0004000

0xBCFFFFFF

0xBD000000

0xBD00FFFF

0xBD010000

0xBF7FFFFF

0xBF800000

0xBF80FFFF

0xBF810000

0xBFBFFFFF

0xBFC00000

0xBFC016FF

0xBFC01700

0xBFC017FF

0xBFC01800

0xFFFFFFFF

**Physical Memory Map**

0x00000000

0x00003FFF

0x00004000

0x1CFFFFFF

0x1D000000

0x1D00FFFF

0x1D010000

0x1F7FFFFF

0x1F800000

0x1F80FFFF

0x1F810000

0x1FBFFFFF

0x1FC00000

0x1FC016FF

0x1FC01700

0x1FC017FF

0x1FC01800

0xFFFFFFFF

**Note 1:** Memory areas are not shown to scale.

**2:** This region should be accessed from kseg1 space only.

**3:** Primary Configuration bits’ area is located at the address range, from 0x1FC01780 to 0x1FC017E8. Alternate Configuration bits’ area is located at the address range, from 0x1FC01700 to 0x1FC01768. Refer to [**Section 4.1 “Alternate Configuration Bits Space”**](#_bookmark80) for more information.

|  |
| --- |
| Reserved |
| 16 Kbytes RAM |
| Reserved |
| 64 Kbytes Flash |
| Reserved |
| SFRs**(**[**2**](#_bookmark89)**)** |
| Reserved |
| Boot Flash**(**[**2**](#_bookmark89)**)** |
| Configuration Bits**(**[**2**](#_bookmark89)**,**[**3**](#_bookmark90)**)** |
| Reserved |
| 16 Kbytes RAM |
| Reserved |
| 64 Kbytes Flash |
| Reserved |
| SFRs |
| Reserved |
| Boot Flash |
| Configuration Bits**(**[**3**](#_bookmark90)**)** |
| Reserved |

**kseg1**

**kseg0**

|  |
| --- |
| 16 Kbytes RAM |
| Reserved |
| 128 Kbytes Flash |
| Reserved |
| SFRs |
| Reserved |
| Boot Flash |
| Configuration Bits**(**[**3**](#_bookmark94)**)** |
| Reserved |

FIGURE 4-2: MEMORY MAP FOR DEVICES WITH 128 Kbytes OF PROGRAM MEMORY([1](#_bookmark92))



**Virtual Memory Map**

0x00000000

0x7FFFFFFF

0x80000000

0x80003FFF

0x80004000

0x9CFFFFFF

0x9D000000

0x9D01FFFF

0x9D020000

0x9F7FFFFF

0x9F800000

0x9F80FFFF

0x9F810000

0x9FBFFFFF

0x9FC00000

0x9FC016FF

0x9FC01700

0x9FC017FF

0x9FC01800

0x9FFFFFFF

0xA0000000

0xA0003FFF

0xA0004000

0xBCFFFFFF

0xBD000000

0xBD01FFFF

0xBD020000

0xBF7FFFFF

0xBF800000

0xBF80FFFF

0xBF810000

0xBFBFFFFF

0xBFC00000

0xBFC016FF

0xBFC01700

0xBFC017FF

0xBFC01800

0xFFFFFFFF

**Physical Memory Map**

0x00000000

0x80003FFF

0x80004000

0x1CFFFFFF

0x1D000000

0x1D01FFFF

0x1D020000

0x1F7FFFFF

0x1F800000

0x1F80FFFF

0x1F810000

0x1FBFFFFF

0x1FC00000

0x1FC016FF

0x1FC01700

0x1FC017FF

0x1FC01800

0xFFFFFFFF

**Note 1:** Memory areas are not shown to scale.

**2:** This region should be accessed from kseg1 space only.

**3:** Primary Configuration bits’ area is located at the address range, from 0x1FC01780 to 0x1FC017E8. Alternate Configuration bits’ area is located at the address range, from 0x1FC01700 to 0x1FC01768. Refer to [**Section 4.1 “Alternate Configuration Bits Space”**](#_bookmark80) for more information.

|  |
| --- |
| Reserved |
| 16 Kbytes RAM |
| Reserved |
| 128 Kbytes Flash |
| Reserved |
| SFRs**(**[**2**](#_bookmark93)**)** |
| Reserved |
| Boot Flash**(**[**2**](#_bookmark93)**)** |
| Configuration Bits**(**[**2**](#_bookmark93)**,**[**3**](#_bookmark94)**)** |
| Reserved |
| 16 Kbytes RAM |
| Reserved |
| 128 Kbytes Flash |
| Reserved |
| SFRs |
| Reserved |
| Boot Flash |
| Configuration Bits**(**[**3**](#_bookmark94)**)** |
| Reserved |

**kseg0**

**kseg1**

|  |
| --- |
| 32 Kbytes RAM |
| Reserved |
| 256 Kbytes Flash |
| Reserved |
| SFRs |
| Reserved |
| Boot Flash |
| Configuration Bits**(**[**3**](#_bookmark99)**)** |
| Reserved |

FIGURE 4-3: MEMORY MAP FOR DEVICES WITH 256 Kbytes OF PROGRAM MEMORY([1](#_bookmark97))



**Virtual Memory Map**

0x00000000

0x7FFFFFFF

0x80000000

0x80007FFF

0x80008000

0x9CFFFFFF

0x9D000000

0x9D003FFF

0x9D004000

0x9F7FFFFF

0x9F800000

0x9F80FFFF

0x9F810000

0x9FBFFFFF

0x9FC00000

0x9FC016FF

0x9FC01700

0x9FC017FF

0x9FC01800

0x9FFFFFFF

0xA0000000

0xA0007FFF

0xA0008000

0xBCFFFFFF

0xBD000000

0xBD03FFFF

0xBD040000

0xBF7FFFFF

0xBF800000

0xBF80FFFF

0xBF810000

0xBFBFFFFF

0xBFC00000

0xBFC016FF

0xBFC01700

0xBFC017FF

0xBFC01800

0xFFFFFFFF

**Physical Memory Map**

0x00000000

0x00007FFF

0x00008000

0x1CFFFFFF

0x1D000000

0x1D03FFFF

0x1D040000

0x1F7FFFFF

0x1F800000

0x1F80FFFF

0x1F810000

0x1FBFFFFF

0x1FC00000

0x1FC016FF

0x1FC01700

0x1FC017FF

0x1FC01800

0xFFFFFFFF

**Note 1:** Memory areas are not shown to scale.

**2:** This region should be accessed from kseg1 space only.

**3:** Primary Configuration bits’ area is located at the address range, from 0x1FC01780 to 0x1FC017E8.

Alternate Configuration bits’ area is located at the address range, from 0x1FC01700 to 0x1FC01768. Refer to [**Section 4.1 “Alternate Configuration Bits Space”**](#_bookmark80) for more information.

|  |
| --- |
| Reserved |
| 32 Kbytes RAM |
| Reserved |
| 256 Kbytes Flash |
| Reserved |
| SFRs**(**[**2**](#_bookmark98)**)** |
| Reserved |
| Boot Flash**(**[**2**](#_bookmark98)**)** |
| Configuration Bits**(**[**2**](#_bookmark98)**,**[**3**](#_bookmark99)**)** |
| Reserved |
| 32 Kbytes RAM |
| Reserved |
| 256 Kbytes Flash |
| Reserved |
| SFRs |
| Reserved |
| Boot Flash |
| Configuration Bits**(**[**3**](#_bookmark99)**)** |
| Reserved |

NOTES:

# FLASH PROGRAM MEMORY

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To com- plement the information in this data sheet, refer to **Section 5. “Flash Programming”** (DS60001121) in the *“PIC32 Family Refer- ence Manual”*, which [is available from the](http://www.microchip.com/PIC32) [Microchip web site (](http://www.microchip.com/PIC32)[www.microchip.com/](http://www.microchip.com/) PIC32). The information in this data sheet supersedes the information in the FRM.

PIC32MM0256GPM064 family devices contain an internal Flash program memory for executing user code. The program and Boot Flash can be write- protected. The erase page size is 512 32-bit words. The program row size is 64 32-bit words. The memory can be programmed by rows or by two 32-bit words, called double-words.

**Note:** Double-words must be 64-bit aligned.

The devices implement a 6-bit Error Correcting Code (ECC). The memory control block contains a logic to write and read ECC bits to and from the Flash memory. The Flash is programmed at the same time as the cor- responding ECC bits. The ECC provides improved resistance to Flash errors. The ECC single-bit error generates an interrupt and can be transparently corrected. The ECC double-bit error results in a bus error exception.

There are three methods by which the user can program this memory:

* Run-Time Self-Programming (RTSP)
* EJTAG Programming
* In-Circuit Serial Programming™ (ICSP™)

RTSP is performed by software executing from either Flash or RAM memory. Information about RTSP techniques is described in **Section 5. “Flash Program- ming”** (DS60001121) in the *“PIC32 Family Reference Manual”*. EJTAG programming is performed using the JTAG port of the device. ICSP programming requires fewer connections than for EJTAG programming. The EJTAG and ICSP methods are described in the *“PIC32 Flash Programming Specification”* (DS60001145), which is available for download from the Microchip web site.

### Flash Controller Registers Write Protection

The NVMPWP and NVMBWP registers, and the WR bit in the NVMCON register are protected (locked) from an accidental write. Each time a special unlock sequence is required to modify the content of these registers or bits. To unlock, the following steps should be done:

1. Disable interrupts prior to the unlock sequence.
2. Execute the system unlock sequence by writing the key values of 0xAA996655 and 0x556699AA to the NVMKEY register.
3. Write the new value to the required bits.
4. Re-enable interrupts.
5. Relock the system. Refer to [Example 5-1](#_bookmark104).

EXAMPLE 5-1:

// unlock sequence NVMKEY = AA996655; NVMKEY = 556699AA;

// relock NVMKEY = 0;

### Flash Control Registers

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 46

TABLE 5-1: FLASH CONTROLLER REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2930 | NVMCON**(**[**1**](#_bookmark106)**)** | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | WR | WREN | WRERR | LVDERR | r | — | — | — | — | — | — | — | NVMOP<3:0> | | | | 0000 |
| 2940 | NVMKEY | 31:16 | NVMKEY<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2950 | NVMADDR**(**[**1**](#_bookmark106)**)** | 31:16 | NVMADDR<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2960 | NVMDATA0 | 31:16 | NVMDATA0<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2970 | NVMDATA1 | 31:16 | NVMDATA1<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2980 | NVMSRCADDR | 31:16 | NVMSRCADDR<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2990 | NVMPWP**(**[**1**](#_bookmark106)**)** | 31:16 | PWPULOCK | — | — | — | — | — | — | — | PWP<23:16> | | | | | | | | 8000 |
| 15:0 | PWP<15:0> | | | | | | | | | | | | | | | | 0000 |
| 29A0 | NVMBWP**(**[**1**](#_bookmark106)**)** | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | BWPULOCK | — | — | — | — | BWP2 | BWP1 | BWP0 | — | — | — | — | — | — | — | — | 8700 |

**Legend:** — = unimplemented, read as ‘0’; r = Reserved bit. Reset values are shown in hexadecimal.

**Note 1:** These registers have corresponding CLR, SET and INV registers at their virtual addresses, plus offsets of 0x4, 0x8 and 0xC, respectively.

REGISTER 5-1: NVMCON: PROGRAMMING CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0, HC | R/W-0 | R-0, HS, HC | R-0, HS, HC | r-0 | U-0 | U-0 | U-0 |
| WR**(**[**1**](#_bookmark109)**,**[**3**](#_bookmark111)**)** | WREN**(**[**1**](#_bookmark109)**)** | WRERR**(**[**1**](#_bookmark109)**,**[**2**](#_bookmark110)**)** | LVDERR**(**[**1**](#_bookmark109)**,**[**2**](#_bookmark110)**)** | — | — | — | — |
| 7:0 | U-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | — | NVMOP<3:0> | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** | HS = Hardware Settable bit | HC = Hardware Clearable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared r = Reserved bit |

bit 31-16 **Unimplemented:** Read as ‘0’ bit 15 **WR:** Write Control bit**(**[**1**](#_bookmark109)**,**[**3**](#_bookmark111)**)**

This bit cannot be cleared and can be set only when WREN = 1, and the unlock sequence has been performed.

1 = Initiates a Flash operation

0 = Flash operation is complete or inactive bit 14 **WREN:** Write Enable bit**(**[**1**](#_bookmark109)**)**

1 = Enables writes to the WR bit and disables writes to the NVMOP<3:0> bits

0 = Disables writes to the WR bit and enables writes to the NVMOP<3:0> bits bit 13 **WRERR:** Write Error bit**(**[**1**](#_bookmark109)**,**[**2**](#_bookmark110)**)**

This bit can be cleared only by setting the NVMOP<3:0> bits = 0000 and initiating a Flash operation.

1 = Program or erase sequence did not complete successfully

0 = Program or erase sequence completed normally bit 12 **LVDERR:** Low-Voltage Detect Error bit**(**[**1**](#_bookmark109)**,**[**2**](#_bookmark110)**)**

This bit can be cleared only by setting the NVMOP<3:0> bits = 0000 and initiating a Flash operation.

1 = Low-voltage is detected (possible data corruption if WRERR is set)

0 = Voltage level is acceptable for programming bit 11 **Reserved:** Maintain as ‘0’

bit 10-4 **Unimplemented:** Read as ‘0’

**Note 1:** These bits are only reset by a Power-on Reset (POR) and are not affected by other Reset sources. **2:** These bits are cleared by setting NVMOP<3:0> = 0000 and initiating a Flash operation (i.e., WR). **3:** This bit is only writable when the NVMKEY unlock sequence is followed. Refer to [Example 5-1](#_bookmark104).

REGISTER 5-1: NVMCON: PROGRAMMING CONTROL REGISTER (CONTINUED)

bit 3-0 **NVMOP<3:0>:** NVM Operation bits

These bits are only writable when WREN = 0. 1111 = Reserved

•

•

•

1000 = Reserved

0111 = Program Erase Operation: Erases all of Program Flash Memory (all pages must be unprotected, PWP<23:0> = 0x000000, Boot Flash Memory is not erased)

0110 = Reserved

0101 = Reserved

0100 = Page Erase Operation: Erases page selected by NVMADDR if it is not write-protected

0011 = Row Program Operation: Programs row selected by NVMADDR if it is not write-protected

0010 = Double-Word Program Operation: Programs two words to address selected by NVMADDR if it is not write-protected

0001 = Reserved

0000 = No operation (clears the WRERR and LVDERR status bits when executed)

**Note 1:** These bits are only reset by a Power-on Reset (POR) and are not affected by other Reset sources. **2:** These bits are cleared by setting NVMOP<3:0> = 0000 and initiating a Flash operation (i.e., WR). **3:** This bit is only writable when the NVMKEY unlock sequence is followed. Refer to Example 5-1.

REGISTER 5-2: NVMKEY: PROGRAMMING UNLOCK REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 |
| NVMKEY<31:24> | | | | | | | |
| 23:16 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 |
| NVMKEY<23:16> | | | | | | | |
| 15:8 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 |
| NVMKEY<15:8> | | | | | | | |
| 7:0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 |
| NVMKEY<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-0 **NVMKEY<31:0>:** Programming Unlock Register bits These bits are write-only and read as ‘0’ on any read.

**Note:** This register is used as part of the unlock sequence to prevent inadvertent writes to the PFM. Refer to [Example 5-1](#_bookmark104).

REGISTER 5-3: NVMADDR: FLASH ADDRESS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NVMADDR<31:24>**(**[**1**](#_bookmark114)**)** | | | | | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NVMADDR<23:16>**(**[**1**](#_bookmark114)**)** | | | | | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NVMADDR<15:8>**(**[**1**](#_bookmark114)**)** | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NVMADDR<7:0>**(**[**1**](#_bookmark114)**)** | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-0 **NVMADDR<31:0>:** Flash Address bits**(**[**1**](#_bookmark114)**)**

|  |  |
| --- | --- |
| **NVMOP<3:0>**  **Selection** | **Flash Address Bits (NVMADDR<31:0>)** |
| Page Erase | Address identifies the page to erase (NVMADDR<10:0> are ignored). |
| Row Program | Address identifies the row to program (NVMADDR<7:0> are ignored). |
| Double-Word Program | Address identifies the double-word (64-bit) to program (NVMADDR<2:0> bits are ignored). **Note:** Must be 64-bit aligned. |

**Note 1:** For all other NVMOP<3:0> bits settings, the Flash address is ignored. See the NVMCON register ([Register 5-1](#_bookmark107)) for additional information on these bits.

**Note:** The bits in this register are only reset by a Power-on Reset (POR) and are not affected by other Reset sources.

REGISTER 5-4: NVMDATAx: FLASH DATA x REGISTER (x = 0-1)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NVMDATAx<31:24> | | | | | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NVMDATAx<23:16> | | | | | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NVMDATAx<15:8> | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NVMDATAx<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-0 **NVMDATAx<31:0>:** Flash Data x bits

Double-Word Program: Writes NVMDATA1:NVMDATA0 to the target Flash address defined in NVMADDR. NVMDATA0 contains the least significant instruction word.

**Note:** The bits in this register are only reset by a Power-on Reset (POR) and are not affected by other Reset sources.

REGISTER 5-5: NVMSRCADDR: SOURCE DATA ADDRESS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NVMSRCADDR<31:24> | | | | | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NVMSRCADDR<23:16> | | | | | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NVMSRCADDR<15:8> | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NVMSRCADDR<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-0 **NVMSRCADDR<31:0>:** Source Data Address bits

The system physical address of the data to be programmed into the Flash when the NVMOP<3:0> bits (NVMCON<3:0>) are set to perform row programming.

**Note:** The bits in this register are only reset by a Power-on Reset (POR) and are not affected by other Reset sources.

REGISTER 5-6: NVMPWP: PROGRAM FLASH WRITE-PROTECT REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-1 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| PWPULOCK | — | — | — | — | — | — | — |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| PWP<23:16> | | | | | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| PWP<15:8> | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| PWP<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **PWPULOCK:** Program Flash Memory Page Write-Protect Unlock bit

1 = Register is not locked and can be modified

0 = Register is locked and cannot be modified

This bit is only clearable and cannot be set except by any Reset. bit 30-24 **Unimplemented:** Read as ‘0’

bit 23-0 **PWP<23:0>:** Flash Program Write-Protect (Page) Address bits

Physical memory below address, 0x1DXXXXXX, is write-protected, where ‘XXXXXX’ is specified by PWP<23:0>. When the PWP<23:0> bits have a value of ‘0’, write protection is disabled for the entire Program Flash Memory. If the specified address falls within the page, the entire page and all pages below the current page will be protected.

**Note:** The bits in this register are only writable when the NVMKEY unlock sequence is followed. Refer to [Example 5-1](#_bookmark104).

REGISTER 5-7: NVMBWP: BOOT FLASH (PAGE) WRITE-PROTECT REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-1 | U-0 | U-0 | U-0 | U-0 | R/W-1 | R/W-1 | R/W-1 |
| BWPULOCK | — | — | — | — | BWP2**(**[**1**](#_bookmark119)**)** | BWP1**(**[**1**](#_bookmark119)**)** | BWP0**(**[**1**](#_bookmark119)**)** |
| 7:0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’

bit 15 **BWPULOCK:** Boot Alias Write-Protect Unlock bit

1 = BWPx bits are not locked and can be modified

0 = BWPx bits are locked and cannot be modified

This bit is only clearable and cannot be set except by any Reset. bit 14-11 **Unimplemented:** Read as ‘0’

bit 10 **BWP2:** Boot Alias Page 2 Write-Protect bit**(**[**1**](#_bookmark119)**)**

1 = Write protection for physical address, 0x01FC08000 through 0x1FC0BFFF, is enabled

0 = Write protection for physical address, 0x01FC08000 through 0x1FC0BFFF, is disabled bit 9 **BWP1:** Boot Alias Page 1 Write-Protect bit**(**[**1**](#_bookmark119)**)**

1 = Write protection for physical address, 0x01FC04000 through 0x1FC07FFF, is enabled

0 = Write protection for physical address, 0x01FC04000 through 0x1FC07FFF, is disabled bit 8 **BWP0:** Boot Alias Page 0 Write-Protect bit**(**[**1**](#_bookmark119)**)**

1 = Write protection for physical address, 0x01FC00000 through 0x1FC03FFF, is enabled

0 = Write protection for physical address, 0x01FC00000 through 0x1FC03FFF, is disabled bit 7-0 **Unimplemented:** Read as ‘0’

**Note 1:** These bits are only available when the NVMKEY unlock sequence is performed and the associated Lock bit (BWPULOCK) is set.

**Note:** The bits in this register are only writable when the NVMKEY unlock sequence is followed. Refer to [Example 5-1](#_bookmark104).

* 1. **RESETS** The Reset module combines all Reset sources and controls the device Master Reset Signal, SYSRST. The

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To com- plement the information in this data sheet, refer to **Section 7. “Resets”** (DS60001118) in the *“PIC32 Family Reference Manual”*, which [is available from the Microchip](http://www.microchip.com/PIC32) [web site (](http://www.microchip.com/PIC32)[www.microchip.com/PIC32).](http://www.microchip.com/PIC32)) The information in this data sheet supersedes the information in the FRM.

device Reset sources are as follows:

* + - Power-on Reset (POR)
    - Master Clear Reset Pin (MCLR)
    - Software Reset (SWR)
    - Watchdog Timer Reset (WDTR)
    - Brown-out Reset (BOR)
    - Configuration Mismatch Reset (CMR)

A simplified block diagram of the Reset module is illustrated in [Figure 6-1](#_bookmark128).

FIGURE 6-1: SYSTEM RESET BLOCK DIAGRAM

MCLR

Glitch Filter

MCLR

Sleep or Idle

WDT

Time-out

WDTR

NMI

Time-out

Voltage Regulator Enabled

POR

SYSRST

VDD

VDD Rise Detect

Brown-out Reset

BOR

Configuration Mismatch Reset

Software Reset

CMR

SWR



### Reset Control Registers

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 54

TABLE 6-1: RESETS REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 26E0 | RCON | 31:16 | PORIO | PORCORE | — | — | BCFGERR | BCFGFAIL | — | — | — | — | — | — | — | — | — | — | C000 |
| 15:0 | — | — | — | — | — | — | CMR | — | EXTR | SWR | — | WDTO | SLEEP | IDLE | BOR | POR | 0003 |
| 26F0 | RSWRST | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | SWRST | 0000 |
| 2700 | RNMICON | 31:16 | — | — | — | — | — | — | — | WDTR | SWNMI | — | — | — | GNMI | — | CF | WDTS | 0000 |
| 15:0 | NMICNT<15:0> | | | | | | | | | | | | | | | | 0000 |
| 2710 | PWRCON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | SBOREN | RETEN | VREGS | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual addresses, plus offsets of 0x4, 0x8 and 0xC, respectively.

REGISTER 6-1: RCON: RESET CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-1, HS | R/W-1, HS | U-0 | U-0 | R/W-0, HS | R/W-0, HS | U-0 | U-0 |
| PORIO | PORCORE | — | — | BCFGERR | BCFGFAIL | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | R/W-0, HS | U-0 |
| — | — | — | — | — | — | CMR | — |
| 7:0 | R/W-0, HS | R/W-0, HS | U-0 | R/W-0, HS | R/W-0, HS | R/W-0, HS | R/W-1, HS | R/W-1, HS |
| EXTR**(**[**1**](#_bookmark133)**)** | SWR**(**[**1**](#_bookmark133)**)** | — | WDTO**(**[**1**](#_bookmark133)**)** | SLEEP**(**[**1**](#_bookmark133)**)** | IDLE**(**[**1**](#_bookmark133)**,**[**2**](#_bookmark134)**)** | BOR**(**[**1**](#_bookmark133)**)** | POR**(**[**1**](#_bookmark133)**)** |

|  |  |  |
| --- | --- | --- |
| **Legend:** | HS = Hardware Settable bit |  |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **PORIO:** VDD POR Flag bit

Set by hardware at detection of a VDD POR event.

1 = A Power-on Reset has occurred due to VDD voltage

0 = A Power-on Reset has not occurred due to VDD voltage bit 30 **PORCORE:** Core Voltage POR Flag bit

Set by hardware at detection of a core POR event.

1 = A Power-on Reset has occurred due to core voltage

0 = A Power-on Reset has not occurred due to core voltage bit 29-28 **Unimplemented:** Read as ‘0’

bit 27 **BCFGERR:** Primary Configuration Registers Error Flag bit

1 = An error occurred during a read of the Primary Configuration registers

0 = No error occurred during a read of the Primary Configuration registers bit 26 **BCFGFAIL:** Primary/Alternate Configuration Registers Error Flag bit

1 = An error occurred during a read of the Primary and Alternate Configuration registers

0 = No error occurred during a read of the Primary and Alternate Configuration registers bit 25-10 **Unimplemented:** Read as ‘0’

bit 9 **CMR:** Configuration Mismatch Reset Flag bit

1 = A Configuration Mismatch Reset has occurred

0 = A Configuration Mismatch Reset has not occurred bit 8 **Unimplemented:** Read as ‘0’

bit 7 **EXTR:** External Reset (MCLR) Pin Flag bit**(**[**1**](#_bookmark133)**)**

1 = Master Clear (pin) Reset has occurred

0 = Master Clear (pin) Reset has not occurred bit 6 **SWR:** Software Reset Flag bit**(**[**1**](#_bookmark133)**)**

1 = Software Reset was executed

0 = Software Reset was not executed bit 5 **Unimplemented:** Read as ‘0’

bit 4 **WDTO:** Watchdog Timer Time-out Flag bit**(**[**1**](#_bookmark133)**)**

1 = WDT time-out has occurred

0 = WDT time-out has not occurred

**Note 1:** User software must clear these bits to view the next detection.

**2:** The IDLE bit will also be set when the device wakes from Sleep.

REGISTER 6-1: RCON: RESET CONTROL REGISTER (CONTINUED)

bit 3 **SLEEP:** Wake from Sleep Flag bit**(**[**1**](#_bookmark133)**)**

1 = Device was in Sleep mode

0 = Device was not in Sleep mode bit 2 **IDLE:** Wake from Idle Flag bit**(**[**1**](#_bookmark133)**,**[**2**](#_bookmark134)**)**

1 = Device was in Idle mode

0 = Device was not in Idle mode bit 1 **BOR:** Brown-out Reset Flag bit**(**[**1**](#_bookmark133)**)**

1 = Brown-out Reset has occurred

0 = Brown-out Reset has not occurred bit 0 **POR:** Power-on Reset Flag bit**(**[**1**](#_bookmark133)**)**

1 = Power-on Reset has occurred

0 = Power-on Reset has not occurred

**Note 1:** User software must clear these bits to view the next detection.

**2:** The IDLE bit will also be set when the device wakes from Sleep.

REGISTER 6-2: RSWRST: SOFTWARE RESET REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | W-0, HC |
| — | — | — | — | — | — | — | SWRST**(**[**1**](#_bookmark136)**,**[**2**](#_bookmark137)**)** |

**Legend:**

R = Readable bit

-n = Value at POR

HC = Hardware Clearable bit

W = Writable bit

‘1’ = Bit is set

U = Unimplemented bit, read as ‘0’

‘0’ = Bit is cleared

x = Bit is unknown

bit 31-1 **Unimplemented:** Read as ‘0’

bit 0 **SWRST:** Software Reset Trigger bit**(**[**1**](#_bookmark136)**,**[**2**](#_bookmark137)**)**

1 = Enables Software Reset event

0 = No effect

**Note 1:** The system unlock sequence must be performed before the SWRST bit can be written. Refer to

[**Section 26.4 “System Registers Write Protection”**](#_bookmark570) for details.

**2:** Once this bit is set, any read of the RSWRST register will cause a Reset to occur.

REGISTER 6-3: RNMICON: NON-MASKABLE INTERRUPT (NMI) CONTROL REGISTER([2](#_bookmark140))

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | R/W-0 |
| — | — | — | — | — | — | — | WDTR |
| 23:16 | R/W-0 | U-0 | U-0 | U-0 | R/W-0 | U-0 | R/W-0 | R/W-0 |
| SWNMI | — | — | — | GNMI | — | CF | WDTS |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NMICNT<15:8> | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| NMICNT<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-25 **Unimplemented:** Read as ‘0’

bit 24 **WDTR:** Watchdog Timer Time-out Flag bit

1 = A Run mode WDT time-out has occurred and caused an NMI

0 = WDT time-out has not occurred

Setting this bit will cause a WDT NMI event and NMICNT will begin counting. bit 23 **SWNMI:** Software NMI Trigger bit

1 = An NMI has been generated

0 = An NMI has not been generated bit 22-20 **Unimplemented:** Read as ‘0’

bit 19 **GNMI:** Software General NMI Trigger bit

1 = A general NMI has been generated

0 = A general NMI has not been generated bit 18 **Unimplemented:** Read as ‘0’

bit 17 **CF:** Clock Fail Detect bit

1 = FSCM has detected clock failure and caused an NMI

0 = FSCM has not detected clock failure

Setting this bit will cause a CF NMI event, but will not cause a clock switch to the FRC. bit 16 **WDTS:** Watchdog Timer Time-out in Sleep Mode Flag bit

1 = WDT time-out has occurred during Sleep mode and caused a wake-up from Sleep

0 = WDT time-out has not occurred during Sleep mode Setting this bit will cause a WDT NMI.

bit 15-0 **NMICNT<15:0>:** NMI Reset Counter Value bits

These bits specify the reload value used by the NMI Reset counter.

0xFFFF-0x0001 = Number of SYSCLK cycles before a device Reset occurs**(**[**1**](#_bookmark139)**)** 0x0000 = No delay between NMI assertion and device Reset event

**Note 1:** If a Watchdog Timer NMI event (when not in Sleep or Idle mode) is cleared before this counter reaches ‘0’, no device Reset is asserted. This NMI Reset counter is only applicable to the Watchdog Timer NMI event.

**2:** The system unlock sequence must be performed before the RNMICON register can be written. Refer to

[**Section 26.4 “System Registers Write Protection”**](#_bookmark570) for details.

REGISTER 6-4: PWRCON: POWER CONTROL REGISTER([2](#_bookmark144))

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | U-0 | U-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | — | — | SBOREN | RETEN**(**[**1**](#_bookmark143)**)** | VREGS |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-3 **Unimplemented:** Read as ‘0’ bit 2 **SBOREN:** BOR Enable bit

Enables the BOR for select BOREN Configuration bit settings.

1 = Writing a ‘1’ to this bit enables the BOR for select BOREN configuration values

0 = Writing a ‘0’ to this bit enables the BOR for select BOREN configuration values bit 1 **RETEN:** Output Level of the Regulator During Sleep Selection bit**(**[**1**](#_bookmark143)**)**

1 = Writing a ‘1’ to this bit will cause the main regulator to be put in a low-power state during Sleep mode**(**[**3**](#_bookmark145)**)**

0 = Writing a ‘0’ to this bit will have no effect bit 0 **VREGS:** Voltage Regulator Standby Enable bit

1 = Voltage regulator will remain active during Sleep mode

0 = Voltage regulator will go into Standby mode during Sleep mode

**Note 1:** Refer to [**Section 25.0 “Power-Saving Features”**](#_bookmark550) for details.

**2:** The SYSKEY register is used to unlock this register.

**3:** The RETEN bit in the device configuration must also be set to enable this mode.

# CPU EXCEPTIONS AND INTERRUPT CONTROLLER

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To com- plement the information in this data sheet, refer to **Section 8. “Interrupts”** (DS61108) and **Section 50. “CPU for Devices with**

**MIPS32® microAptiv™ and M-Class**

**Cores”** (DS60001192) in the *“PIC32 Family Reference Manual”*, which [is](http://www.microchip.com/PIC32) [available from the Microchip web site](http://www.microchip.com/PIC32) [(](http://www.microchip.com/PIC32)[www.microchip.com/PIC32).](http://www.microchip.com/PIC32)) The infor- mation in this data sheet supersedes the information in the FRM.

PIC32MM0256GPM064 family devices generate inter- rupt requests in response to interrupt events from peripheral modules. The interrupt control module exists externally to the CPU logic and prioritizes the interrupt events before presenting them to the CPU.

The CPU handles interrupt events as part of the excep- tion handling mechanism, which is described in [**Section 7.1 “CPU Exceptions”**](#_bookmark149).

The PIC32MM0256GPM064 family device interrupt module includes the following features:

* Single Vector or Multivector Mode Operation
* Five External Interrupts with Edge Polarity Control
* Interrupt Proximity Timer
* Module Freeze in Debug mode
* Seven User-Selectable Priority Levels for Each Vector
* Four User-Selectable Subpriority Levels within Each Priority
* One Shadow Register Set that can be Used for Any Priority Level, Eliminating Software Context Switch and Reducing Interrupt Latency
* Software can Generate any Interrupt
* User-Configurable Interrupt Vectors’ Offset and Vector Table Location

[Figure 7-1](#_bookmark147) shows the block diagram for the interrupt controller and CPU exceptions.





FIGURE 7-1: CPU EXCEPTIONS AND INTERRUPT CONTROLLER MODULE BLOCK DIAGRAM



CPU Core (Exception Handling)

SYSCLK

Interrupt Requests

|  |  |
| --- | --- |
| Interrupt Controller | Vector Number and Offset |
| Priority Level |
| Shadow Set Number |
|  |

### CPU Exceptions

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 60

CPU Coprocessor 0 contains the logic for identifying and managing exceptions. Exceptions can be caused by a variety of sources, including boundary cases in data, external events or program errors. [Table 7-1](#_bookmark150) lists the exception types in order of priority.

TABLE 7-1: MIPS32® microAptiv™ UC MICROPROCESSOR CORE EXCEPTION TYPES

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Exception Type (In Order of Priority)** | **Description** | **Branches to** | **Status Bits Set** | **Debug Bits Set** | **EXCCODE** | **XC32 Function Name** |
| Highest Priority | | | | | | |
| Reset | Assertion of MCLR. | 0xBFC0\_0000 | BEV, ERL | — | — | \_on\_reset |
| Soft Reset | Execution of a RESET instruction. | 0xBFC0\_0000 | BEV, SR, ERL | — | — | \_on\_reset |
| DSS | EJTAG debug single step. | 0xBFC0\_0480  (ProbEn = 0 in ECR) 0xBFC0\_0200  (ProbEn = 1 in ECR) | — | DSS | — | — |
| DINT | EJTAG debug interrupt. Caused by setting the EjtagBrk bit in the ECR register. | 0xBFC0\_0480  (ProbEn = 0 in ECR) 0xBFC0\_0200  (ProbEn = 1 in ECR) | — | DINT | — | — |
| NMI | Non-Maskable Interrupt. | 0xBFC0\_0000 | BEV, NMI, ERL | — | — | \_nmi\_handler |
| Interrupt | Assertion of unmasked hardware or software interrupt signal. | See [Table 7-2](#_bookmark152) | IPL<2:0> | — | Int (0x00) | See [Table 7-2](#_bookmark152) |
| DIB | EJTAG debug hardware instruction break matched. | 0xBFC0\_0480  (ProbEn = 0 in ECR) 0xBFC0\_0200  (ProbEn = 1 in ECR) | — | DIB | — | — |
| AdEL | Load address alignment error. | EBASE + 0x180 | EXL | — | ADEL (0x04) | \_general\_exception\_handler |
| IBE | Instruction fetch bus error. | EBASE + 0x180 | EXL | — | IBE (0x06) | \_general\_exception\_handler |
| DBp | EJTAG breakpoint (execution of SDBBP  instruction). | 0xBFC0\_0480  (ProbEn = 0 in ECR) 0xBFC0\_0200  (ProbEn = 1 in ECR) | DBp | — | — | — |
| Sys | Execution of SYSCALL instruction. | EBASE + 0x180 | EXL | — | Sys (0x08) | \_general\_exception\_handler |
| Bp | Execution of BREAK instruction. | EBASE + 0x180 | EXL | — | Bp (0x09) | \_general\_exception\_handler |

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 61

TABLE 7-1: MIPS32® microAptiv™ UC MICROPROCESSOR CORE EXCEPTION TYPES (CONTINUED)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Exception Type (In Order of Priority)** | **Description** | **Branches to** | **Status Bits Set** | **Debug Bits Set** | **EXCCODE** | **XC32 Function Name** |
| CpU | Execution of a coprocessor instruction for a coprocessor that is not enabled. | EBASE + 0x180 | CU, EXL | — | CpU (0x0B) | \_general\_exception\_handler |
| RI | Execution of a reserved instruction. | EBASE + 0x180 | EXL | — | RI (0x0A) | \_general\_exception\_handler |
| Ov | Execution of an arithmetic instruction that overflowed. | EBASE + 0x180 | EXL | — | Ov (0x0C) | \_general\_exception\_handler |
| Tr | Execution of a trap (when trap condition is true). | EBASE + 0x180 | EXL | — | Tr (0x0D) | \_general\_exception\_handler |
| DDBL | EJTAG data address break (address only) or EJTAG data value break on load (address and value). | 0xBFC0\_0480  (ProbEn = 0 in ECR) 0xBFC0\_0200  (ProbEn = 1 in ECR) | — | DDBL for a load instruction or DDBS for a store  instruction | — | — |
| DDBS | EJTAG data address break (address only) or EJTAG data value break on store (address and value). | 0xBFC0\_0480  (ProbEn = 0 in ECR) 0xBFC0\_0200  (ProbEn = 1 in ECR) | — | DDBL for a load instruction or DDBS for a store  instruction | — | — |
| AdES | Store address alignment error. | EBASE + 0x180 | EXL | — | ADES (0x05) | \_general\_exception\_handler |
| DBE | Load or store bus error. | EBASE + 0x180 | EXL | — | DBE (0x07) | \_general\_exception\_handler |
| CBrk | EJTAG complex breakpoint. | 0xBFC0\_0480  (ProbEn = 0 in ECR) 0xBFC0\_0200  (ProbEn = 1 in ECR) | — | DIBImpr, DDBLImpr and/or DDBSImpr | — | — |
| Lowest Priority | | | | | | |

### Interrupts

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 62

The PIC32MM0256GPM064 family uses fixed offset for vector spacing. For details, refer to **Section 8. “Interrupts”** (DS61108) in the *“PIC32 Family Reference Manual”*. [Table 7-2](#_bookmark152) provides the interrupt related vectors and bits information.

TABLE 7-2: INTERRUPTS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Interrupt Source** | **MPLAB® XC32 Vector Name** | **Vector Number** | **Interrupt Related Bits Location** | | | | **Persistent Interrupt** |
| **Flag** | **Enable** | **Priority** | **Subpriority** |
| Core Timer | \_CORE\_TIMER\_VECTOR | 0 | IFS0<0> | IEC0<0> | IPC0<4:2> | IPC0<1:0> | No |
| Core Software 0 | \_CORE\_SOFTWARE\_0\_VECTOR | 1 | IFS0<1> | IEC0<1> | IPC0<12:10> | IPC0<9:8> | No |
| Core Software 1 | \_CORE\_SOFTWARE\_1\_VECTOR | 2 | IFS0<2> | IEC0<2> | IPC0<20:18> | IPC0<17:16> | No |
| External 0 | \_EXTERNAL\_0\_VECTOR | 3 | IFS0<3> | IEC0<3> | IPC0<28:26> | IPC0<25:24> | No |
| External 1 | \_EXTERNAL\_1\_VECTOR | 4 | IFS0<4> | IEC0<4> | IPC1<4:2> | IPC1<1:0> | No |
| External 2 | \_EXTERNAL\_2\_VECTOR | 5 | IFS0<5> | IEC0<5> | IPC1<12:10> | IPC1<9:8> | No |
| External 3 | \_EXTERNAL\_3\_VECTOR | 6 | IFS0<6> | IEC0<6> | IPC1<20:18> | IPC1<17:16> | No |
| External 4 | \_EXTERNAL\_4\_VECTOR | 7 | IFS0<7> | IEC0<7> | IPC1<28:26> | IPC1<25:24> | No |
| PORTA Change Notification | \_CHANGE\_NOTICE\_A\_VECTOR | 8 | IFS0<8> | IEC0<8> | IPC2<4:2> | IPC2<1:0> | No |
| PORTB Change Notification | \_CHANGE\_NOTICE\_B\_VECTOR | 9 | IFS0<9> | IEC0<9> | IPC2<12:10> | IPC2<9:8> | No |
| PORTC Change Notification | \_CHANGE\_NOTICE\_C\_VECTOR | 10 | IFS0<10> | IEC0<10> | IPC2<20:18> | IPC2<17:16> | No |
| PORTD Change Notification | \_CHANGE\_NOTICE\_D\_VECTOR | 11 | IFS0<11> | IEC0<11> | IPC2<28:26> | IPC2<25:24> | No |
| RESERVED |  | 12 | IFS0<12> | IEC0<12> | IPC3<4:2> | IPC3<1:0> | No |
| RESERVED |  | 13 | IFS0<13> | IEC0<13> | IPC3<12:10> | IPC3<9:8> | No |
| RESERVED |  | 14 | IFS0<14> | IEC0<14> | IPC3<20:18> | IPC3<17:16> | No |
| RESERVED |  | 15 | IFS0<15> | IEC0<15> | IPC3<28:26> | IPC3<25:24> | No |
| RESERVED |  | 16 | IFS0<16> | IEC0<16> | IPC4<4:2> | IPC4<1:0> | No |
| Timer1 | \_TIMER\_1\_VECTOR | 17 | IFS0<17> | IEC0<17> | IPC4<12:10> | IPC4<9:8> | No |
| Timer2 | \_TIMER\_2\_VECTOR | 18 | IFS0<18> | IEC0<18> | IPC4<20:18> | IPC4<17:16> | No |
| Timer3 | \_TIMER\_3\_VECTOR | 19 | IFS0<19> | IEC0<19> | IPC4<28:26> | IPC4<25:24> | No |
| RESERVED |  | 20 | IFS0<20> | IEC0<20> | IPC5<4:2> | IPC5<1:0> | No |
| RESERVED |  | 21 | IFS0<21> | IEC0<21> | IPC5<12:10> | IPC5<9:8> | No |
| RESERVED |  | 22 | IFS0<22> | IEC0<22> | IPC5<20:18> | IPC5<17:16> | No |
| Comparator 1 | \_COMPARATOR\_1\_VECTOR | 23 | IFS0<23> | IEC0<23> | IPC5<28:26> | IPC5<25:24> | No |
| Comparator 2 | \_COMPARATOR\_2\_VECTOR | 24 | IFS0<24> | IEC0<24> | IPC6<4:2> | IPC6<1:0> | No |
| Comparator 3 | \_COMPARATOR\_3\_VECTOR | 25 | IFS0<25> | IEC0<25> | IPC6<12:10> | IPC6<9:8> | No |

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 63

TABLE 7-2: INTERRUPTS (CONTINUED)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Interrupt Source** | **MPLAB® XC32 Vector Name** | **Vector Number** | **Interrupt Related Bits Location** | | | | **Persistent Interrupt** |
| **Flag** | **Enable** | **Priority** | **Subpriority** |
| RESERVED |  | 26 | IFS0<26> | IEC0<26> | IPC6<20:18> | IPC6<17:16> | No |
| RESERVED |  | 27 | IFS0<27> | IEC0<27> | IPC6<28:26> | IPC6<25:24> | No |
| RESERVED |  | 28 | IFS0<28> | IEC0<28> | IPC7<4:2> | IPC7<1:0> | No |
| USB | \_USB\_VECTOR | 29 | IFS0<29> | IEC0<29> | IPC7<12:10> | IPC7<9:8> | No |
| RESERVED |  | 30 | IFS0<30> | IEC0<30> | IPC7<20:18> | IPC7<17:16> | No |
| RESERVED |  | 31 | IFS0<31> | IEC0<31> | IPC7<28:26> | IPC7<25:24> | No |
| Real-Time Clock Alarm | \_RTCC\_VECTOR | 32 | IFS1<0> | IEC1<0> | IPC8<4:2> | IPC8<1:0> | No |
| ADC Conversion | \_ADC\_VECTOR | 33 | IFS1<1> | IEC1<1> | IPC8<12:10> | IPC8<9:8> | No |
| RESERVED |  | 34 | IFS1<2> | IEC1<2> | IPC8<20:18> | IPC8<17:16> | No |
| RESERVED |  | 35 | IFS1<3> | IEC1<3> | IPC8<28:26> | IPC8<25:24> | No |
| High/Low-Voltage Detect | \_HLVD\_VECTOR | 36 | IFS1<4> | IEC1<4> | IPC9<4:2> | IPC9<1:0> | Yes |
| Logic Cell 1 | \_CLC1\_VECTOR | 37 | IFS1<5> | IEC1<5> | IPC9<12:10> | IPC9<9:8> | No |
| Logic Cell 2 | \_CLC2\_VECTOR | 38 | IFS1<6> | IEC1<6> | IPC9<20:18> | IPC9<17:16> | No |
| Logic Cell 3 | \_CLC3\_VECTOR | 39 | IFS1<7> | IEC1<7> | IPC9<28:26> | IPC9<25:24> | No |
| Logic Cell 4 | \_CLC4\_VECTOR | 40 | IFS1<8> | IEC1<8> | IPC10<4:2> | IPC10<1:0> | No |
| SPI1 Error | \_SPI1\_ERR\_VECTOR | 41 | IFS1<9> | IEC1<9> | IPC10<12:10> | IPC10<9:8> | Yes |
| SPI1 Transmission | \_SPI1\_TX\_VECTOR | 42 | IFS1<10> | IEC1<10> | IPC10<20:18> | IPC10<17:16> | Yes |
| SPI1 Reception | \_SPI1\_RX\_VECTOR | 43 | IFS1<11> | IEC1<11> | IPC10<28:26> | IPC10<25:24> | Yes |
| SPI2 Error | \_SPI2\_ERR\_VECTOR | 44 | IFS1<12> | IEC1<12> | IPC11<4:2> | IPC11<1:0> | Yes |
| SPI2 Transmission | \_SPI2\_TX\_VECTOR | 45 | IFS1<13> | IEC1<13> | IPC11<12:10> | IPC11<9:8> | Yes |
| SPI2 Reception | \_SPI2\_RX\_VECTOR | 46 | IFS1<14> | IEC1<14> | IPC11<20:18> | IPC11<17:16> | Yes |
| SPI3 Error | \_SPI3\_ERR\_VECTOR | 47 | IFS1<15> | IEC1<15> | IPC11<28:26> | IPC11<25:24> | Yes |
| SPI3 Transmission | \_SPI3\_TX\_VECTOR | 48 | IFS1<16> | IEC1<16> | IPC12<4:2> | IPC12<1:0> | Yes |
| SPI3 Reception | \_SPI3\_RX\_VECTOR | 49 | IFS1<17> | IEC1<17> | IPC12<12:10> | IPC12<9:8> | Yes |
| RESERVED |  | 50 | IFS1<18> | IEC1<18> | IPC12<20:18> | IPC12<17:16> | No |
| RESERVED |  | 51 | IFS1<19> | IEC1<19> | IPC12<28:26> | IPC12<25:24> | No |
| RESERVED |  | 52 | IFS1<20> | IEC1<20> | IPC13<4:2> | IPC13<1:0> | No |
| UART1 Reception | \_UART1\_RX\_VECTOR | 53 | IFS1<21> | IEC1<21> | IPC13<12:10> | IPC13<9:8> | Yes |
| UART1 Transmission | \_UART1\_TX\_VECTOR | 54 | IFS1<22> | IEC1<22> | IPC13<20:18> | IPC13<17:16> | Yes |
| UART1 Error | \_UART1\_ERR\_VECTOR | 55 | IFS1<23> | IEC1<23> | IPC13<28:26> | IPC13<25:24> | Yes |

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 64

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Interrupt Source** | **MPLAB® XC32 Vector Name** | **Vector Number** | **Interrupt Related Bits Location** | | | | **Persistent Interrupt** |
| **Flag** | **Enable** | **Priority** | **Subpriority** |
| UART2 Reception | \_UART2\_RX\_VECTOR | 56 | IFS1<24> | IEC1<24> | IPC14<4:2> | IPC14<1:0> | Yes |
| UART2 Transmission | \_UART2\_TX\_VECTOR | 57 | IFS1<25> | IEC1<25> | IPC14<12:10> | IPC14<9:8> | Yes |
| UART2 Error | \_UART2\_ERR\_VECTOR | 58 | IFS1<26> | IEC1<26> | IPC14<20:18> | IPC14<17:16> | Yes |
| UART3 Reception | \_UART3\_RX\_VECTOR | 59 | IFS1<27> | IEC1<27> | IPC14<28:26> | IPC14<25:24> | Yes |
| UART3 Transmission | \_UART3\_TX\_VECTOR | 60 | IFS1<28> | IEC1<28> | IPC15<4:2> | IPC15<1:0> | Yes |
| UART3 Error | \_UART3\_ERR\_VECTOR | 61 | IFS1<29> | IEC1<29> | IPC15<12:10> | IPC15<9:8> | Yes |
| RESERVED |  | 62 | IFS1<30> | IEC1<30> | IPC15<20:18> | IPC15<17:16> | No |
| RESERVED |  | 63 | IFS1<31> | IEC1<31> | IPC15<28:26> | IPC15<25:24> | No |
| RESERVED |  | 64 | IFS2<0> | IEC2<0> | IPC16<4:2> | IPC16<1:0> | No |
| I2C1 Slave | \_I2C1\_SLAVE\_VECTOR | 65 | IFS2<1> | IEC2<1> | IPC16<12:10> | IPC16<9:8> | Yes |
| I2C1 Master | \_I2C1\_MASTER\_VECTOR | 66 | IFS2<2> | IEC2<2> | IPC16<20:18> | IPC16<17:16> | Yes |
| I2C1 Bus Collision | \_I2C1\_BUS\_VECTOR | 67 | IFS2<3> | IEC2<3> | IPC16<28:26> | IPC16<25:24> | Yes |
| I2C2 Slave | \_I2C2\_SLAVE\_VECTOR | 68 | IFS2<4> | IEC2<4> | IPC17<4:2> | IPC17<1:0> | Yes |
| I2C2 Master | \_I2C2\_MASTER\_VECTOR | 69 | IFS2<5> | IEC2<5> | IPC17<12:10> | IPC17<9:8> | Yes |
| I2C2 Bus Collision | \_I2C2\_BUS\_VECTOR | 70 | IFS2<6> | IEC2<6> | IPC17<20:18> | IPC17<17:16> | Yes |
| I2C3 Slave | \_I2C3\_SLAVE\_VECTOR | 71 | IFS2<7> | IEC2<7> | IPC17<28:26> | IPC17<25:24> | Yes |
| I2C3 Master | \_I2C3\_MASTER\_VECTOR | 72 | IFS2<8> | IEC2<8> | IPC18<4:2> | IPC18<1:0> | Yes |
| I2C3 Bus Collision | \_I2C3\_BUS\_VECTOR | 73 | IFS2<9> | IEC2<9> | IPC18<12:10> | IPC18<9:8> | Yes |
| CCP1 Input Capture or Output Compare | \_CCP1\_VECTOR | 74 | IFS2<10> | IEC2<10> | IPC18<20:18> | IPC18<17:16> | No |
| CCP1 Timer | \_CCT1\_VECTOR | 75 | IFS2<11> | IEC2<11> | IPC18<28:26> | IPC18<25:24> | No |
| CCP2 Input Capture or Output Compare | \_CCP2\_VECTOR | 76 | IFS2<12> | IEC2<12> | IPC19<4:2> | IPC19<1:0> | No |
| CCP2 Timer | \_CCT2\_VECTOR | 77 | IFS2<13> | IEC2<13> | IPC19<12:10> | IPC19<9:8> | No |
| CCP3 Input Capture or Output Compare | \_CCP3\_VECTOR | 78 | IFS2<14> | IEC2<14> | IPC19<20:18> | IPC19<17:16> | No |
| CCP3 Timer | \_CCT3\_VECTOR | 79 | IFS2<15> | IEC2<15> | IPC19<28:26> | IPC19<25:24> | No |
| CCP4 Input Capture or Output Compare | \_CCP4\_VECTOR | 80 | IFS2<16> | IEC2<16> | IPC20<4:2> | IPC20<1:0> | No |
| CCP4 Timer | \_CCT4\_VECTOR | 81 | IFS2<17> | IEC2<17> | IPC20<12:10> | IPC20<9:8> | No |
| CCP5 Input Capture or Output Compare | \_CCP5\_VECTOR | 82 | IFS2<18> | IEC2<18> | IPC20<20:18> | IPC20<17:16> | No |
| CCP5 Timer | \_CCT5\_VECTOR | 83 | IFS2<19> | IEC2<19> | IPC20<28:26> | IPC20<25:24> | No |
| CCP6 Input Capture or Output Compare | \_CCP6\_VECTOR | 84 | IFS2<20> | IEC2<20> | IPC21<4:2> | IPC21<1:0> | No |
| CCP6 Timer | \_CCT6\_VECTOR | 85 | IFS2<21> | IEC2<21> | IPC21<12:10> | IPC21<9:8> | No |
| CCP7 Input Capture or Output Compare | \_CCP7\_VECTOR | 86 | IFS2<22> | IEC2<22> | IPC21<20:18> | IPC21<17:16> | No |
| CCP7 Timer | \_CCT7\_VECTOR | 87 | IFS2<23> | IEC2<23> | IPC21<28:26> | IPC21<25:24> | No |

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 65

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Interrupt Source** | **MPLAB® XC32 Vector Name** | **Vector Number** | **Interrupt Related Bits Location** | | | | **Persistent Interrupt** |
| **Flag** | **Enable** | **Priority** | **Subpriority** |
| CCP8 Input Capture or Output Compare | \_CCP8\_VECTOR | 88 | IFS2<24> | IEC2<24> | IPC22<4:2> | IPC22<1:0> | No |
| CCP8 Timer | \_CCT8\_VECTOR | 89 | IFS2<25> | IEC2<25> | IPC22<12:10> | IPC22<9:8> | No |
| CCP9 Input Capture or Output Compare | \_CCP9\_VECTOR | 90 | IFS2<26> | IEC2<26> | IPC22<20:18> | IPC22<17:16> | No |
| CCP9 Timer | \_CCT9\_VECTOR | 91 | IFS2<27> | IEC2<27> | IPC22<28:26> | IPC22<25:24> | No |
| FRC Auto-Tune | \_FRC\_TUNE | 92 | IFS2<28> | IEC2<28> | IPC23<4:2> | IPC23<1:0> | No |
| NVM Program or Erase Complete | \_NVM\_VECTOR | 94 | IFS2<30> | IEC2<30> | IPC23<20:18> | IPC23<17:16> | Yes |
| Core Performance Counter | \_PERFORMANCE\_COUNTER\_VECTOR | 95 | IFS2<31> | IEC2<31> | IPC23<28:26> | IPC23<25:24> | No |
| RESERVED |  | 96 | IFS3<0> | IEC3<0> | IPC24<4:2> | IPC24<1:0> | No |
| Single-Bit ECC Error | \_ECCSB\_ERR\_VECTOR | 97 | IFS3<1> | IEC3<1> | IPC24<12:10> | IPC24<9:8> | No |
| DMA Channel 0 | \_DMA0\_VECTOR | 98 | IFS3<2> | IEC3<2> | IPC24<20:18> | IPC24<17:16> | No |
| DMA Channel 1 | \_DMA1\_VECTOR | 99 | IFS3<3> | IEC3<3> | IPC24<28:26> | IPC24<25:24> | No |
| DMA Channel 2 | \_DMA2\_VECTOR | 100 | IFS3<4> | IEC3<4> | IPC25<4:2> | IPC25<1:0> | No |
| DMA Channel 3 | \_DMA3\_VECTOR | 101 | IFS3<5> | IEC3<5> | IPC25<12:10> | IPC25<9:8> | No |

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 66

**Name(1)**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| F000 | INTCON | 31:16 | — | — | — | — | — | — | — | — | — |  | | VS<6:0> | | | | | 0000 |
| 15:0 | — | — | — | MVEC | — | TPC<2:0> | | | — | — | — | INT4EP | INT3EP | INT2EP | INT1EP | INT0EP | 0000 |
| F010 | PRISS | 31:16 | PRI7SS<3:0> | | | | PRI6SS<3:0> | | | | PRI5SS<3:0> | | | | PRI4SS<3:0> | | | | 0000 |
| 15:0 | PRI3SS<3:0> | | | | PRI2SS<3:0> | | | | PRI1SS<3:0> | | | | — | — | — | SS0 | 0000 |
| F020 | INTSTAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | SRIPL<2:0> | | | SIRQ<7:0> | | | | | | | | 0000 |
| F030 | IPTMR | 31:16 | IPTMR<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| F040 | IFS0 | 31:16 | — | USBIF | — | — | — | — | CMP3IF | CMP2IF | CMP1IF | — | — | — | T3IF | T2IF | T1IF | — | 0000 |
| 15:0 | — | — | — | — | CNDIF | CNCIF | CNBIF | CNAIF | INT4IF | INT3IF | INT2IF | INT1IF | INT0IF | CS1IF | CS0IF | CTIF | 0000 |
| F050 | IFS1 | 31:16 | — | — | U3EIF | U3TXIF | U3RXIF | U2EIF | U2TXIF | U2RXIF | U1EIF | U1TXIF | U1RXIF | — | — | — | SPI3RXIF | SPI3TXIF | 0000 |
| 15:0 | SPI3EIF | SPI2RXIF | SPI2TXIF | SPI2EIF | SPI1RXIF | SPI1TXIF | SPI1EIF | CLC4IF | CLC3IF | CLC2IF | CLC1IF | LVDIF | — | — | AD1IF | RTCCIF | 0000 |
| F060 | IFS2 | 31:16 | CPCIF | NVMIF | — | FSTIF | CCT9IF | CCP9IF | CCT8IF | CCP8IF | CCT7IF | CCP7IF | CCT6IF | CCP6IF | CCT5IF | CCP5IF | CCT4IF | CCP4IF | 0000 |
| 15:0 | CCT3IF | CCP3IF | CCT2IF | CCP2IF | CCT1IF | CCP1IF | I2C3BCIF | I2C3MIF | I2C3SIF | I2C2BCIF | I2C2MIF | I2C2SIF | I2C1BCIF | I2C1MIF | I2C1SIF | — | 0000 |
| F070 | IFS3 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | DMA3IF | DMA2IF | DMA1IF | DMA0IF | ECCBEIF | — | 0000 |
| F080 | IEC0 | 31:16 | — | USBIE | — | — | — | — | CMP3IE | CMP2IE | CMP1IE | — | — | — | T3IE | T2IE | T1IE | — | 0000 |
| 15:0 | — | — | — | — | CNDIE | CNCIE | CNBIE | CNAIE | INT4IE | INT3IE | INT2IE | INT1IE | INT0IE | CS1IE | CS0IE | CTIE | 0000 |
| F090 | IEC1 | 31:16 | — | — | U3EIE | U3TXIE | U3RXIE | U2EIE | U2TXIE | U2RXIE | U1EIE | U1TXIE | U1RXIE | — | — | — | SPI3RXIE | SPI3TXIE | 0000 |
| 15:0 | SPI3EIE | SPI2RXIE | SPI2TXIE | SPI2EIE | SPI1RXIE | SPI1TXIE | SPI1EIE | CLC4IE | CLC3IE | CLC2IE | CLC1IE | LVDIE | — | — | AD1IE | RTCCIE | 0000 |
| F0A0 | IEC2 | 31:16 | CPCIE | NVMIE | — | FSTIE | CCT9IE | CCP9IE | CCT8IE | CCP8IE | CCT7IE | CCP7IE | CCT6IE | CCP6IE | CCT5IE | CCP5IE | CCT4IE | CCP4IE | 0000 |
| 15:0 | CCT3IE | CCP3IE | CCT2IE | CCP2IE | CCT1IE | CCP1IE | I2C3BCIE | I2C3MIE | I2C3SIE | I2C2BCIE | I2C2MIE | I2C2SIE | I2C1BCIE | I2C1MIE | I2C1SIE | — | 0000 |
| F0B0 | IEC3 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | DMA3IE | DMA2IE | DMA1IE | DMA0IE | ECCBEIE | — | 0000 |
| F0C0 | IPC0 | 31:16 | — | — | — | INT0IP<2:0> | | | INT0IS<1:0> | | — | — | — | CS1IP<2:0> | | | CS1IS<1:0> | | 0000 |
| 15:0 | — | — | — | CS0IP<2:0> | | | CS0IS<1:0> | | — | — | — | CTIP<2:0> | | | CTIS<1:0> | | 0000 |
| F0D0 | IPC1 | 31:16 | — | — | — | INT4IP<2:0> | | | INT4IS<1:0> | | — | — | — | INT3IP<2:0> | | | INT3IS<1:0> | | 0000 |
| 15:0 | — | — | — | INT2IP<2:0> | | | INT2IS<1:0> | | — | — | — | INT1IP<2:0> | | | INT1IS<1:0> | | 0000 |
| F0E0 | IPC2 | 31:16 | — | — | — | CNDIP<2:0> | | | CNDIS<1:0> | | — | — | — | CNCIP<2:0> | | | CNCIS<1:0> | | 0000 |
| 15:0 | — | — | — | CNBIP<2:0> | | | CNBIS<1:0> | | — | — | — | CNAIP<2:0> | | | CNAIS<1:0> | | 0000 |
| F0F0 | IPC3 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 67

**Name(1)**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| F100 | IPC4 | 31:16 | — | — | — | T3IP<2:0> | | | T3IS<1:0> | | — | — | — | T2IP<2:0> | | | T2IS<1:0> | | 0000 |
| 15:0 | — | — | — | T1IP<2:0> | | | T1IS<1:0> | | — | — | — | — | — | — | — | — | 0000 |
| F110 | IPC5 | 31:16 | — | — | — | CMP1IP<2:0> | | | CMP1IS<1:0> | | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| F120 | IPC6 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | CMP3IP<2:0> | | | CMP3IS<1:0> | | — | — | — | CMP2IP<2:0> | | | CMP2IS<1:0> | | 0000 |
| F130 | IPC7 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | USBIP<2:0> | | | USBIS<1:0> | | — | — | — | — | — | — | — | — | 0000 |
| F140 | IPC8 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | AD1IP<2:0> | | | AD1IS<1:0> | | — | — | — | RTCCIP<2:0> | | | RTCCIS<1:0> | | 0000 |
| F150 | IPC9 | 31:16 | — | — | — | CLC3IP<2:0> | | | CLC3IS<1:0> | | — | — | — | CLC2IP<2:0> | | | CLC2IS<1:0> | | 0000 |
| 15:0 | — | — | — | CLC1IP<2:0> | | | CLC1IS<1:0> | | — | — | — | LVDIP<2:0> | | | LVDIS<1:0> | | 0000 |
| F160 | IPC10 | 31:16 | — | — | — | SPI1RXIP<2:0> | | | SPI1RXIS<1:0> | | — | — | — | SPI1TXIP<2:0> | | | SPI1TXIS<1:0> | | 0000 |
| 15:0 | — | — | — | SPI1EIP<2:0> | | | SPI1EIS<1:0> | | — | — | — | CLC4IP<2:0> | | | CLC4IS<1:0> | | 0000 |
| F170 | IPC11 | 31:16 | — | — | — | SPI3EIP<2:0> | | | SPI3EIS<1:0> | | — | — | — | SPI2RXIP<2:0> | | | SPI2RXIS<1:0> | | 0000 |
| 15:0 | — | — | — | SPI2TXIP<2:0> | | | SPI2TXIS<1:0> | | — | — | — | SPI2EIP<2:0> | | | SPI2EIS<1:0> | | 0000 |
| F180 | IPC12 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | SPI3RXIP<2:0> | | | SPI3RXIS<1:0> | | — | — | — | SPI3TXIP<2:0> | | | SPI3TXIS<1:0> | | 0000 |
| F190 | IPC13 | 31:16 | — | — | — | U1EIP<2:0> | | | U1EIS<1:0> | | — | — | — | U1TXIP<2:0> | | | U1TXIS<1:0> | | 0000 |
| 15:0 | — | — | — | U1RXIP<2:0> | | | U1RXIS<1:0> | | — | — | — | — | — | — | — | — | 0000 |
| F1A0 | IPC14 | 31:16 | — | — | — | U3RXIP<2:0> | | | U3RXIS<1:0> | | — | — | — | U2EIP<2:0> | | | U2EIS<1:0> | | 0000 |
| 15:0 | — | — | — | U2TXIP<2:0> | | | U2TXIS<1:0> | | — | — | — | U2RXIP<2:0> | | | U2RXIS<1:0> | | 0000 |
| F1B0 | IPC15 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | U3EIP<2:0> | | | U3EIS<1:0> | | — | — | — | U3TXIP<2:0> | | | U3TXIS<1:0> | | 0000 |
| F1C0 | IPC16 | 31:16 | — | — | — | I2C1BCIP<2:0> | | | I2C1BCIS<1:0> | | — | — | — | I2C1MIP<2:0> | | | I2C1MIS<1:0> | | 0000 |
| 15:0 | — | — | — | I2C1SIP<2:0> | | | I2C1SIS<1:0> | | — | — | — | — | — | — | — | — | 0000 |
| F1D0 | IPC17 | 31:16 | — | — | — | I2C3SIP<2:0> | | | I2C3SIS<1:0> | | — | — | — | I2C2BCIP<2:0> | | | I2C2BCIS<1:0> | | 0000 |
| 15:0 | — | — | — | I2C2MIP<2:0> | | | I2C2MIS<1:0> | | — | — | — | I2C2SIP<2:0> | | | I2C2SIS<1:0> | | 0000 |
| F1E0 | IPC18 | 31:16 | — | — | — | CCT1IP<2:0> | | | CCT1IS<1:0> | | — | — | — | CCP1IP<2:0> | | | CCP1IS<1:0> | | 0000 |
| 15:0 | — | — | — | I2C3BCIP<2:0> | | | I2C3BCIS<1:0> | | — | — | — | I2C3MIP<2:0> | | | I2C3MIS<1:0> | | 0000 |
| F1F0 | IPC19 | 31:16 | — | — | — | CCT3IP<2:0> | | | CCT3IS<1:0> | | — | — | — | CCP3IP<2:0> | | | CCP3IS<1:0> | | 0000 |
| 15:0 | — | — | — | CCT2IP<2:0> | | | CCT2IS<1:0> | | — | — | — | CCP2IP<2:0> | | | CCP2IS<1:0> | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 68

**Name(1)**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| F200 | IPC20 | 31:16 | — | — | — | CCT5IP<2:0> | | | CCT5IS<1:0> | | — | — | — | CCP5IP<2:0> | | | CCP5IS<1:0> | | 0000 |
| 15:0 | — | — | — | CCT4IP<2:0> | | | CCT4IS<1:0> | | — | — | — | CCP4IP<2:0> | | | CCP4IS<1:0> | | 0000 |
| F210 | IPC21 | 31:16 | — | — | — | CCT7IP<2:0> | | | CCT7IS<1:0> | | — | — | — | CCP7IP<2:0> | | | CCP7IS<1:0> | | 0000 |
| 15:0 | — | — | — | CCT6IP<2:0> | | | CCT6IS<1:0> | | — | — | — | CCP6IP<2:0> | | | CCP6IS<1:0> | | 0000 |
| F220 | IPC22 | 31:16 | — | — | — | CCT9IP<2:0> | | | CCT9IS<1:0> | | — | — | — | CCP9IP<2:0> | | | CCP9IS<1:0> | | 0000 |
| 15:0 | — | — | — | CCT8IP<2:0> | | | CCT8IS<1:0> | | — | — | — | CCP8IP<2:0> | | | CCP8IS<1:0> | | 0000 |
| F230 | IPC23 | 31:16 | — | — | — | CPCIP<2:0> | | | CPCIS<1:0> | | — | — | — | NVMIP<2:0> | | | NVMIS<1:0> | | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | FSTIP<2:0> | | | FSTIS<1:0> | | 0000 |
| F240 | IPC24 | 31:16 | — | — | — | DMA1IP<2:0> | | | DMA1IS<1:0> | | — | — | — | DMA0IP<2:0> | | | DMA0IS<1:0> | | 0000 |
| 15:0 | — | — | — | ECCBEIP<2:0> | | | ECCBEIS<1:0> | | — | — | — | — | — | — | — | — | 0000 |
| F250 | IPC25 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | DMA3IP<2:0> | | | DMA3IS<1:0> | | — | — | — | DMA2IP<2:0> | | | DMA2IS<1:0> | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

REGISTER 7-1: INTCON: INTERRUPT CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | VS<6:0> | | | | | | |
| 15:8 | U-0 | U-0 | U-0 | R/W-0 | U-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | MVEC | — | TPC<2:0> | | |
| 7:0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | INT4EP | INT3EP | INT2EP | INT1EP | INT0EP |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-23 **Unimplemented:** Read as ‘0’ bit 22-16 **VS<6:0>**: Vector Spacing bits

Spacing Between Vectors:

0000000 = 0 Bytes

0000001 = 8 Bytes

0000010 = 16 Bytes

0000100 = 32 Bytes

0001000 = 64 Bytes

0010000 = 128 Bytes

0100000 = 256 Bytes

1000000 = 512 Bytes

All other values are reserved. The operation of this device is undefined if a reserved value is written to this field. If MVEC = 0, this field is ignored.

bit 15-13 **Unimplemented:** Read as ‘0’

bit 12 **MVEC:** Multivector Configuration bit

1 = Interrupt controller is configured for Multivectored mode

0 = Interrupt controller is configured for Single Vectored mode bit 11 **Unimplemented:** Read as ‘0’

bit 10-8 **TPC<2:0>:** Interrupt Proximity Timer Control bits

111 = Interrupts of Group Priority 7 or lower start the interrupt proximity timer 110 = Interrupts of Group Priority 6 or lower start the interrupt proximity timer 101 = Interrupts of Group Priority 5 or lower start the interrupt proximity timer 100 = Interrupts of Group Priority 4 or lower start the interrupt proximity timer 011 = Interrupts of Group Priority 3 or lower start the interrupt proximity timer 010 = Interrupts of Group Priority 2 or lower start the interrupt proximity timer 001 = Interrupts of Group Priority 1 start the interrupt proximity timer

000 = Disables interrupt proximity timer bit 7-5 **Unimplemented:** Read as ‘0’

bit 4 **INT4EP:** External Interrupt 4 Edge Polarity Control bit

1 = Rising edge

0 = Falling edge

bit 3 **INT3EP:** External Interrupt 3 Edge Polarity Control bit

1 = Rising edge

0 = Falling edge

REGISTER 7-1: INTCON: INTERRUPT CONTROL REGISTER (CONTINUED)

bit 2 **INT2EP:** External Interrupt 2 Edge Polarity Control bit

1 = Rising edge

0 = Falling edge

bit 1 **INT1EP:** External Interrupt 1 Edge Polarity Control bit

1 = Rising edge

0 = Falling edge

bit 0 **INT0EP:** External Interrupt 0 Edge Polarity Control bit

1 = Rising edge

0 = Falling edge

REGISTER 7-2: PRISS: PRIORITY SHADOW SELECT REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| PRI7SS<3:0>**(**[**1**](#_bookmark161)**)** | | | | PRI6SS<3:0>**(**[**1**](#_bookmark161)**)** | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| PRI5SS<3:0>**(**[**1**](#_bookmark161)**)** | | | | PRI4SS<3:0>**(**[**1**](#_bookmark161)**)** | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| PRI3SS<3:0>**(**[**1**](#_bookmark161)**)** | | | | PRI2SS<3:0>**(**[**1**](#_bookmark161)**)** | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | U-0 | U-0 | R/W-0 |
| PRI1SS<3:0>**(**[**1**](#_bookmark161)**)** | | | | — | — | — | SS0 |

|  |  |  |  |
| --- | --- | --- | --- |
| **Legend:**  R = Readable bit  -n = Value at POR | | W = Writable bit ‘1’ = Bit is set | U = Unimplemented bit, read as ‘0’  ‘0’ = Bit is cleared x = Bit is unknown |
| bit 31-28 | **PRI7SS<3:0>:** Interrupt with Priority Level 7 Shadow Set bits**(**[**1**](#_bookmark161)**)** | | |
|  | 1111 = Reserved  • | | |
|  | • | | |
|  | • | | |
|  | 0010 = Reserved  0001 = Interrupt with a priority level of 7 uses Shadow Set 1  0000 = Interrupt with a priority level of 7 uses Shadow Set 0 | | |
| bit 27-24 | **PRI6SS<3:0>:** Interrupt with Priority Level 6 Shadow Set bits**(**[**1**](#_bookmark161)**)** | | |
|  | 1111 = Reserved  • | | |
|  | • | | |
|  | • | | |
|  | 0010 = Reserved  0001 = Interrupt with a priority level of 6 uses Shadow Set 1  0000 = Interrupt with a priority level of 6 uses Shadow Set 0 | | |

**Note 1:** These bits are ignored if the MVEC bit (INTCON<12>) = 0.

REGISTER 7-2: PRISS: PRIORITY SHADOW SELECT REGISTER (CONTINUED)

bit 23-20 **PRI5SS<3:0>:** Interrupt with Priority Level 5 Shadow Set bits**(**[**1**](#_bookmark161)**)**

1111 = Reserved

•

•

•

0010 = Reserved

0001 = Interrupt with a priority level of 5 uses Shadow Set 1

0000 = Interrupt with a priority level of 5 uses Shadow Set 0 bit 19-16 **PRI4SS<3:0>:** Interrupt with Priority Level 4 Shadow Set bits**(**[**1**](#_bookmark161)**)**

1111 = Reserved

•

•

•

0010 = Reserved

0001 = Interrupt with a priority level of 4 uses Shadow Set 1

0000 = Interrupt with a priority level of 4 uses Shadow Set 0 bit 15-12 **PRI3SS<3:0>:** Interrupt with Priority Level 3 Shadow Set bits**(**[**1**](#_bookmark161)**)**

1111 = Reserved

•

•

•

0010 = Reserved

0001 = Interrupt with a priority level of 3 uses Shadow Set 1

0000 = Interrupt with a priority level of 3 uses Shadow Set 0 bit 11-8 **PRI2SS<3:0>:** Interrupt with Priority Level 2 Shadow Set bits**(**[**1**](#_bookmark161)**)**

1111 = Reserved

•

•

•

0010 = Reserved

0001 = Interrupt with a priority level of 2 uses Shadow Set 1

0000 = Interrupt with a priority level of 2 uses Shadow Set 0 bit 7-4 **PRI1SS<3:0>:** Interrupt with Priority Level 1 Shadow Set bits**(**[**1**](#_bookmark161)**)**

1111 = Reserved

•

•

•

0010 = Reserved

0001 = Interrupt with a priority level of 1 uses Shadow Set 1

0000 = Interrupt with a priority level of 1 uses Shadow Set 0 bit 3-1 **Unimplemented:** Read as ‘0’

bit 0 **SS0:** Single Vector Shadow Register Set bit

1 = Single vector is presented with a shadow set

0 = Single vector is not presented with a shadow set

**Note 1:** These bits are ignored if the MVEC bit (INTCON<12>) = 0.

REGISTER 7-3: INTSTAT: INTERRUPT STATUS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC |
| — | — | — | — | — | SRIPL<2:0>**(**[**1**](#_bookmark163)**)** | | |
| 7:0 | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC |
| SIRQ<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** | HS = Hardware Settable bit | HC = Hardware Clearable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-11 **Unimplemented:** Read as ‘0’

bit 10-8 **SRIPL<2:0>:** Requested Priority Level for Single Vector Mode bits**(**[**1**](#_bookmark163)**)**

111-000 = The priority level of the latest interrupt presented to the CPU bit 7-0 **SIRQ<7:0>:** Last Interrupt Request Serviced Status bits

11111111-00000000 = The last interrupt request number serviced by the CPU

**Note 1:** This value should only be used when the interrupt controller is configured for Single Vector mode.

REGISTER 7-4: IPTMR: INTERRUPT PROXIMITY TIMER REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| IPTMR<31:24> | | | | | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| IPTMR<23:16> | | | | | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| IPTMR<15:8> | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| IPTMR<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-0 **IPTMR<31:0>:** Interrupt Proximity Timer Reload bits

Used by the interrupt proximity timer as a reload value when the interrupt proximity timer is triggered by an interrupt event.

REGISTER 7-5: IFSx: INTERRUPT FLAG STATUS REGISTER x

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| IFS<31:24> | | | | | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| IFS<23:16> | | | | | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| IFS<15:8> | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| IFS<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-0 **IFS<31:0>:** Interrupt Flag Status bits

1 = Interrupt request has occurred

0 = No interrupt request has occurred

**Note:** This register represents a generic definition of the IFSx register. Refer to [Table 7-3](#_bookmark155) for the exact bit definitions.

REGISTER 7-6: IECx: INTERRUPT ENABLE CONTROL REGISTER x

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| IEC<31:24> | | | | | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| IEC<23:16> | | | | | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| IEC<15:8> | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| IEC<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-0 **IEC<31-0>:** Interrupt Enable bits

1 = Interrupt is enabled

0 = Interrupt is disabled

**Note:** This register represents a generic definition of the IECx register. Refer to [Table 7-3](#_bookmark155) for the exact bit definitions.

REGISTER 7-7: IPCx: INTERRUPT PRIORITY CONTROL REGISTER x

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | IP3<2:0> | | | IS3<1:0> | |
| 23:16 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | IP2<2:0> | | | IS2<1:0> | |
| 15:8 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | IP1<2:0> | | | IS1<1:0> | |
| 7:0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | IP0<2:0> | | | IS0<1:0> | |

**Legend:**

R = Readable bit

-n = Value at POR

W = Writable bit

‘1’ = Bit is set

U = Unimplemented bit, read as ‘0’

‘0’ = Bit is cleared

x = Bit is unknown

bit 31-29 **Unimplemented:** Read as ‘0’

bit 28-26 **IP3<2:0>:** Interrupt Priority 3 bits

111 = Interrupt priority is 7

•

•

•

010 = Interrupt priority is 2

001 = Interrupt priority is 1

000 = Interrupt is disabled

bit 25-24 **IS3<1:0>:** Interrupt Subpriority 3 bits

11 = Interrupt subpriority is 3

10 = Interrupt subpriority is 2

01 = Interrupt subpriority is 1

00 = Interrupt subpriority is 0

bit 23-21 **Unimplemented:** Read as ‘0’

bit 20-18 **IP2<2:0>:** Interrupt Priority 2 bits

111 = Interrupt priority is 7

•

•

•

010 = Interrupt priority is 2

001 = Interrupt priority is 1

000 = Interrupt is disabled

bit 17-16 **IS2<1:0>:** Interrupt Subpriority 2 bits

11 = Interrupt subpriority is 3

10 = Interrupt subpriority is 2

01 = Interrupt subpriority is 1

00 = Interrupt subpriority is 0

bit 15-13 **Unimplemented:** Read as ‘0’

**Note:** This register represents a generic definition of the IPCx register. Refer to [Table 7-3](#_bookmark155) for the exact bit definitions.

REGISTER 7-7: IPCx: INTERRUPT PRIORITY CONTROL REGISTER x (CONTINUED)

bit 12-10 **IP1<2:0>:** Interrupt Priority 1 bits

111 = Interrupt priority is 7

•

•

•

010 = Interrupt priority is 2

001 = Interrupt priority is 1

000 = Interrupt is disabled

bit 9-8 **IS1<1:0>:** Interrupt Subpriority 1 bits

11 = Interrupt subpriority is 3

10 = Interrupt subpriority is 2

01 = Interrupt subpriority is 1

00 = Interrupt subpriority is 0

bit 7-5 **Unimplemented:** Read as ‘0’

bit 4-2 **IP0<2:0>:** Interrupt Priority 0 bits

111 = Interrupt priority is 7

•

•

•

010 = Interrupt priority is 2

001 = Interrupt priority is 1

000 = Interrupt is disabled

bit 1-0 **IS0<1:0>:** Interrupt Subpriority 0 bits

11 = Interrupt subpriority is 3

10 = Interrupt subpriority is 2

01 = Interrupt subpriority is 1

00 = Interrupt subpriority is 0

**Note:** This register represents a generic definition of the IPCx register. Refer to Table 7-3 for the exact bit definitions.

NOTES:

# DIRECT MEMORY ACCESS (DMA) CONTROLLER

**Note 1:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To complement the information in this data sheet, refer to **Section 31. “DMA Controller”** (DS60001117) in the *“PIC32 Family Reference Manual”*[, which is](http://www.microchip.com/PIC32) [available from the Microchip web site](http://www.microchip.com/PIC32) [(](http://www.microchip.com/PIC32)[www.microchip.com/PIC32).](http://www.microchip.com/PIC32))

The Direct Memory Access (DMA) Controller is a bus master module useful for data transfers between peripherals and memory without CPU intervention. The source and destination of a DMA transfer can be any of the memory-mapped modules, that do not have a ded- icated DMA, existent in the PIC32 (such as SPI, UART, PMP, etc.) or the memory itself.

The following are some of the key features of the DMA Controller module:

* Four Identical Channels, Each Featuring:
  + Auto-Increment Source and Destination Address registers
  + Source and Destination Pointers
  + Memory to memory and memory to peripheral transfers
* Automatic Word Size Detection:
  + Transfer granularity, down to byte level
  + Bytes need not be word-aligned at source and destination
* Fixed Priority Channel Arbitration
* Flexible DMA Channel Operating modes:
  + Manual (software) or automatic (interrupt) DMA requests
  + One-Shot or Auto-Repeat Block Transfer modes
  + Channel-to-channel chaining
* Flexible DMA Requests:
  + A DMA request can be selected from any of the peripheral interrupt sources
  + Each channel can select any (appropriate) observable interrupt as its DMA request source
  + A DMA transfer abort can be selected from any of the peripheral interrupt sources
  + Pattern (data) match transfer termination
* Multiple DMA Channel Status Interrupts:
  + DMA channel block transfer complete
  + Source empty or half empty
  + Destination full or half full
  + DMA transfer aborted due to an external event
  + Invalid DMA address generated
* DMA Debug Support Features:
  + Most recent address accessed by a DMA channel
  + Most recent DMA channel to transfer data
* CRC Generation module:
  + CRC module can be assigned to any of the available channels
  + CRC module is highly configurable
* User Selectable Bus Arbitration Priority (refer to

[**Section 4.2 “Bus Matrix (BMX)”**](#_bookmark82))

* 8 System Clocks Per Cell Transfer

FIGURE 8-1: DMA BLOCK DIAGRAM

Global Control (DMACON)

Channel 3 Control

Channel 1 Control

Bus Matrix

Channel 0 Control

INT Controller

System IRQ

Peripheral Bus Address Decoder

I0

I1 Y

I2 I3

Channel Priority Arbitration BMXARB<1:0>

### DMA Control Registers

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 78

TABLE 8-1: DMA CONTROLLER REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF88\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 8900 | DMACON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON | — | — | SUSPEND | DMABUSY | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 8910 | DMASTAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | RDWR | DMACH<2:0> | | | 0000 |
| 8920 | DMAADDR | 31:16 | DMAADDR<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 8930 | DCRCCON | 31:16 | — | — | BYTO<1:0> | | WBO | — | — | BITO | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | PLEN<4:0> | | | | | CRCEN | CRCAPP | CRCTYP | — | — | CRCCH<2:0> | | | 0000 |
| 8940 | DCRCDATA | 31:16 | DCRCDATA<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 8950 | DCRCXOR | 31:16 | DCRCXOR<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual addresses, plus offsets of 0x4, 0x8 and 0xC, respectively. See [**Section 10.1 “CLR, SET and INV Registers”**](#_bookmark250) for more information.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 79

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF88\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 8960 | DCH0CON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHBUSY | — | — | — | — | — | — | CHCHNS | CHEN | CHAED | CHCHN | CHAEN | — | CHEDET | CHPRI<1:0> | | 0000 |
| 8970 | DCH0ECON | 31:16 | — | — | — | — | — | — | — | — | CHAIRQ<7:0> | | | | | | | | 00FF |
| 15:0 | CHSIRQ<7:0> | | | | | | | | CFORCE | CABORT | PATEN | SIRQEN | AIRQEN | — | — | — | FF00 |
| 8980 | DCH0INT | 31:16 | — | — | — | — | — | — | — | — | CHSDIE | CHSHIE | CHDDIE | CHDHIE | CHBCIE | CHCCIE | CHTAIE | CHERIE | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | CHSDIF | CHSHIF | CHDDIF | CHDHIF | CHBCIF | CHCCIF | CHTAIF | CHERIF | 0000 |
| 8990 | DCH0SSA | 31:16 | CHSSA<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 89A0 | DCH0DSA | 31:16 | CHDSA<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 89B0 | DCH0SSIZ | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHSSIZ<15:0> | | | | | | | | | | | | | | | | 0000 |
| 89C0 | DCH0DSIZ | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHDSIZ<15:0> | | | | | | | | | | | | | | | | 0000 |
| 89D0 | DCH0SPTR | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHSPTR<15:0> | | | | | | | | | | | | | | | | 0000 |
| 89E0 | DCH0DPTR | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHDPTR<15:0> | | | | | | | | | | | | | | | | 0000 |
| 89F0 | DCH0CSIZ | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHCSIZ<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8A00 | DCH0CPTR | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHCPTR<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8A10 | DCH0DAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | CHPDAT<7:0> | | | | | | | | 0000 |
| 8A20 | DCH1CON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHBUSY | — | — | — | — | — | — | CHCHNS | CHEN | CHAED | CHCHN | CHAEN | — | CHEDET | CHPRI<1:0> | | 0000 |
| 8A30 | DCH1ECON | 31:16 | — | — | — | — | — | — | — | — | CHAIRQ<7:0> | | | | | | | | 00FF |
| 15:0 | CHSIRQ<7:0> | | | | | | | | CFORCE | CABORT | PATEN | SIRQEN | AIRQEN | — | — | — | FF00 |
| 8A40 | DCH1INT | 31:16 | — | — | — | — | — | — | — | — | CHSDIE | CHSHIE | CHDDIE | CHDHIE | CHBCIE | CHCCIE | CHTAIE | CHERIE | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | CHSDIF | CHSHIF | CHDDIF | CHDHIF | CHBCIF | CHCCIF | CHTAIF | CHERIF | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual addresses, plus offsets of 0x4, 0x8 and 0xC, respectively. See [**Section 10.1 “CLR, SET and INV Registers”**](#_bookmark250) for more information.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 80

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF88\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 8A50 | DCH1SSA | 31:16 | CHSSA<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 8A60 | DCH1DSA | 31:16 | CHDSA<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 8A70 | DCH1SSIZ | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHSSIZ<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8A80 | DCH1DSIZ | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHDSIZ<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8A90 | DCH1SPTR | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHSPTR<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8AA0 | DCH1DPTR | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHDPTR<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8AB0 | DCH1CSIZ | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHCSIZ<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8AC0 | DCH1CPTR | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHCPTR<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8AD0 | DCH1DAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | CHPDAT<7:0> | | | | | | | | 0000 |
| 8AE0 | DCH2CON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHBUSY | — | — | — | — | — | — | CHCHNS | CHEN | CHAED | CHCHN | CHAEN | — | CHEDET | CHPRI<1:0> | | 0000 |
| 8AF0 | DCH2ECON | 31:16 | — | — | — | — | — | — | — | — | CHAIRQ<7:0> | | | | | | | | 00FF |
| 15:0 | CHSIRQ<7:0> | | | | | | | | CFORCE | CABORT | PATEN | SIRQEN | AIRQEN | — | — | — | FF00 |
| 8B00 | DCH2INT | 31:16 | — | — | — | — | — | — | — | — | CHSDIE | CHSHIE | CHDDIE | CHDHIE | CHBCIE | CHCCIE | CHTAIE | CHERIE | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | CHSDIF | CHSHIF | CHDDIF | CHDHIF | CHBCIF | CHCCIF | CHTAIF | CHERIF | 0000 |
| 8B10 | DCH2SSA | 31:16 | CHSSA<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 8B20 | DCH2DSA | 31:16 | CHDSA<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 8B30 | DCH2SSIZ | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHSSIZ<15:0> | | | | | | | | | | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual addresses, plus offsets of 0x4, 0x8 and 0xC, respectively. See **Section 10.1 “CLR, SET and INV Registers”** for more information.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 81

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF88\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 8B40 | DCH2DSIZ | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHDSIZ<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8B50 | DCH2SPTR | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHSPTR<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8B60 | DCH2DPTR | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHDPTR<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8B70 | DCH2CSIZ | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHCSIZ<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8B80 | DCH2CPTR | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHCPTR<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8B90 | DCH2DAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | CHPDAT<7:0> | | | | | | | | 0000 |
| 8BA0 | DCH3CON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHBUSY | — | — | — | — | — | — | CHCHNS | CHEN | CHAED | CHCHN | CHAEN | — | CHEDET | CHPRI<1:0> | | 0000 |
| 8BB0 | DCH3ECON | 31:16 | — | — | — | — | — | — | — | — | CHAIRQ<7:0> | | | | | | | | 00FF |
| 15:0 | CHSIRQ<7:0> | | | | | | | | CFORCE | CABORT | PATEN | SIRQEN | AIRQEN | — | — | — | FF00 |
| 8BC0 | DCH3INT | 31:16 | — | — | — | — | — | — | — | — | CHSDIE | CHSHIE | CHDDIE | CHDHIE | CHBCIE | CHCCIE | CHTAIE | CHERIE | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | CHSDIF | CHSHIF | CHDDIF | CHDHIF | CHBCIF | CHCCIF | CHTAIF | CHERIF | 0000 |
| 8BD0 | DCH3SSA | 31:16 | CHSSA<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 8BE0 | DCH3DSA | 31:16 | CHDSA<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 8BF0 | DCH3SSIZ | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHSSIZ<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8C00 | DCH3DSIZ | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHDSIZ<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8C10 | DCH3SPTR | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHSPTR<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8C20 | DCH3DPTR | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHDPTR<15:0> | | | | | | | | | | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual addresses, plus offsets of 0x4, 0x8 and 0xC, respectively. See **Section 10.1 “CLR, SET and INV Registers”** for more information.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 82

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF88\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 8C30 | DCH3CSIZ | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHCSIZ<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8C40 | DCH3CPTR | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CHCPTR<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8C50 | DCH3DAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | CHPDAT<7:0> | | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual addresses, plus offsets of 0x4, 0x8 and 0xC, respectively. See **Section 10.1 “CLR, SET and INV Registers”** for more information.

REGISTER 8-1: DMACON: DMA CONTROLLER CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | U-0 | U-0 | R/W-0 | R/W-0 | U-0 | U-0 | U-0 |
| ON**(**[**1**](#_bookmark179)**)** | — | — | SUSPEND | DMABUSY | — | — | — |
| 7:0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’ bit 15 **ON:** DMA On bit**(**[**1**](#_bookmark179)**)**

1 = DMA module is enabled

0 = DMA module is disabled bit 14-13 **Unimplemented:** Read as ‘0’ bit 12 **SUSPEND:** DMA Suspend bit

1 = DMA transfers are suspended to allow CPU uninterrupted access to data bus

0 = DMA operates normally

bit 11 **DMABUSY:** DMA Module Busy bit

1 = DMA module is active

0 = DMA module is disabled and not actively transferring data bit 10-0 **Unimplemented:** Read as ‘0’

**Note 1:** The user’s software should not read/write the peripheral’s SFRs in the SYSCLK cycle immediately following the instruction that clears the module’s ON bit.

REGISTER 8-2: DMASTAT: DMA STATUS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | U-0 | U-0 | U-0 | U-0 | R-0 | R-0 | R-0 | R-0 |
| — | — | — | — | RDWR | DMACH<2:0> | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-4 **Unimplemented:** Read as ‘0’

bit 3 **RDWR:** DMA Read/Write Status bit

1 = Last DMA bus access was a read

0 = Last DMA bus access was a write bit 2-0 **DMACH<2:0>:** DMA Channel bits

These bits contain the value of the most recent active DMA channel.

REGISTER 8-3: DMAADDR: DMA ADDRESS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| DMAADDR<31:24> | | | | | | | |
| 23:16 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| DMAADDR<23:16> | | | | | | | |
| 15:8 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| DMAADDR<15:8> | | | | | | | |
| 7:0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| DMAADDR<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-0 **DMAADDR<31:0>:** DMA Module Address bits

These bits contain the address of the most recent DMA access.

REGISTER 8-4: DCRCCON: DMA CRC CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | U-0 | R/W-0 |
| — | — | BYTO<1:0> | | WBO**(**[**1**](#_bookmark183)**)** | — | — | BITO |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | PLEN<4:0> | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 |
| CRCEN | CRCAPP**(**[**1**](#_bookmark183)**)** | CRCTYP | — | — | CRCCH<2:0> | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-30 **Unimplemented:** Read as ‘0’

bit 29-28 **BYTO<1:0>:** CRC Byte Order Selection bits

11 = Endian byte swap on half-word boundaries (source half-word order with reverse source byte order per half-word)

10 = Swap half-words on word boundaries (reverse source half-word order with source byte order per half-word)

01 = Endian byte swap on word boundaries (reverse source byte order)

00 = No swapping (source byte order)

bit 27 **WBO:** CRC Write Byte Order Selection bit**(**[**1**](#_bookmark183)**)**

1 = Source data is written to the destination re-ordered, as defined by BYTO<1:0>

0 = Source data is written to the destination unaltered bit 26-25 **Unimplemented:** Read as ‘0’

bit 24 **BITO:** CRC Bit Order Selection bit

When CRCTYP (DCRCCON<5>) = 1 (CRC module is in IP Header mode):

1 = The IP header checksum is calculated Least Significant bit (LSb) first (reflected)

0 = The IP header checksum is calculated Most Significant bit (MSb) first (not reflected) When CRCTYP (DCRCCON<5>) = 0 (CRC module is in LFSR mode):

1 = The LFSR CRC is calculated Least Significant bit first (reflected)

0 = The LFSR CRC is calculated Most Significant bit first (not reflected) bit 23-13 **Unimplemented:** Read as ‘0’

bit 12-8 **PLEN<4:0>:** Polynomial Length bits

When CRCTYP (DCRCCON<5>) = 1 (CRC module is in IP Header mode): These bits are unused.

When CRCTYP (DCRCCON<5>) = 0 (CRC module is in LFSR mode):

Denotes the length of the polynomial – 1. bit 7 **CRCEN:** CRC Enable bit

1 = CRC module is enabled and channel transfers are routed through the CRC module

0 = CRC module is disabled and channel transfers proceed normally bit 6 **CRCAPP:** CRC Append Mode bit**(**[**1**](#_bookmark183)**)**

1 = The DMA transfers data from the source into the CRC but not to the destination; when a block transfer completes, the DMA writes the calculated CRC value to the location given by CHxDSA

0 = The DMA transfers data from the source through the CRC, obeying WBO as it writes the data to the destination

**Note 1:** When WBO = 1, unaligned transfers are not supported and the CRCAPP bit cannot be set.

REGISTER 8-4: DCRCCON: DMA CRC CONTROL REGISTER (CONTINUED)

bit 5 **CRCTYP:** CRC Type Selection bit

1 = The CRC module will calculate an IP header checksum

0 = The CRC module will calculate an LFSR CRC bit 4-3 **Unimplemented:** Read as ‘0’

bit 2-0 **CRCCH<2:0>:** CRC Channel Select bits

111 = CRC is assigned to Channel 7 110 = CRC is assigned to Channel 6 101 = CRC is assigned to Channel 5 100 = CRC is assigned to Channel 4 011 = CRC is assigned to Channel 3 010 = CRC is assigned to Channel 2 001 = CRC is assigned to Channel 1 000 = CRC is assigned to Channel 0

**Note 1:** When WBO = 1, unaligned transfers are not supported and the CRCAPP bit cannot be set.

REGISTER 8-5: DCRCDATA: DMA CRC DATA REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| DCRCDATA<31:24> | | | | | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| DCRCDATA<23:16> | | | | | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| DCRCDATA<15:8> | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| DCRCDATA<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-0 **DCRCDATA<31:0>:** CRC Data Register bits

Writing to this register will seed the CRC generator. Reading from this register will return the current value of the CRC. Bits greater than PLEN will return ‘0’ on any read.

When CRCTYP (DCRCCON<5>) = 1 (CRC module is in IP Header mode):

Only the lower 16 bits contain IP header checksum information. The upper 16 bits are always ‘0’. Data written to this register is converted and read back in ‘1’s complement form (current IP header checksum value).

When CRCTYP (DCRCCON<5>) = 0 (CRC module is in LFSR mode): Bits greater than PLEN will return ‘0’ on any read.

REGISTER 8-6: DCRCXOR: DMA CRCXOR ENABLE REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| DCRCXOR<31:24> | | | | | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| DCRCXOR<23:16> | | | | | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| DCRCXOR<15:8> | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| DCRCXOR<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-0 **DCRCXOR<31:0>:** CRC XOR Register bits

When CRCTYP (DCRCCON<5>) = 1 (CRC module is in IP Header mode): This register is unused.

When CRCTYP (DCRCCON<5>) = 0 (CRC module is in LFSR mode):

1 = Enables the XOR input to the Shift register

0 = Disables the XOR input to the Shift register; data is shifted in directly from the previous stage in the register

REGISTER 8-7: DCHxCON: DMA CHANNEL x CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | R/W-0 |
| CHBUSY | — | — | — | — | — | — | CHCHNS**(**[**1**](#_bookmark187)**)** |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | R-0 | R/W-0 | R/W-0 |
| CHEN**(**[**2**](#_bookmark188)**)** | CHAED | CHCHN | CHAEN | — | CHEDET | CHPRI<1:0> | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’ bit 15 **CHBUSY:** Channel Busy bit

1 = Channel is active or has been enabled

0 = Channel is inactive or has been disabled bit 14-9 **Unimplemented:** Read as ‘0’

bit 8 **CHCHNS:** Chain Channel Selection bit**(**[**1**](#_bookmark187)**)**

1 = Chain to channel lower in natural priority (CH1 will be enabled by CH2 transfer complete)

0 = Chain to channel higher in natural priority (CH1 will be enabled by CH0 transfer complete) bit 7 **CHEN:** Channel Enable bit**(**[**2**](#_bookmark188)**)**

1 = Channel is enabled

0 = Channel is disabled

bit 6 **CHAED:** Channel Allow Events if Disabled bit

1 = Channel start/abort events will be registered, even if the channel is disabled

0 = Channel start/abort events will be ignored if the channel is disabled bit **CHCHN:** Channel Chain Enable bit

1 = Allows channel to be chained

0 = Does not allow channel to be chained bit 4 **CHAEN:** Channel Automatic Enable bit

1 = Channel is continuously enabled and not automatically disabled after a block transfer is complete

0 = Channel is disabled on a block transfer complete bit 3 **Unimplemented:** Read as ‘0’

bit 2 **CHEDET:** Channel Event Detected bit

1 = An event has been detected

0 = No events have been detected bit 1-0 **CHPRI<1:0>:** Channel Priority bits

11 = Channel has Priority 3 (highest)

10 = Channel has Priority 2

01 = Channel has Priority 1

00 = Channel has Priority 0

**Note 1:** The chain selection bit takes effect when chaining is enabled (CHCHN = 1).

**2:** When the channel is suspended by clearing this bit, the user application should poll the CHBUSY bit (if available on the device variant) to see when the channel is suspended, as it may take some clock cycles to complete a current transaction before the channel is suspended.

REGISTER 8-8: DCHxECON: DMA CHANNEL x EVENT CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | R/W-1 | R/W-1 | R/W-1 | R/W-1 | R/W-1 | R/W-1 | R/W-1 | R/W-1 |
| CHAIRQ<7:0>**(**[**1**](#_bookmark190)**)** | | | | | | | |
| 15:8 | R/W-1 | R/W-1 | R/W-1 | R/W-1 | R/W-1 | R/W-1 | R/W-1 | R/W-1 |
| CHSIRQ<7:0>**(**[**1**](#_bookmark190)**)** | | | | | | | |
| 7:0 | S-0 | S-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | U-0 | U-0 |
| CFORCE | CABORT | PATEN | SIRQEN | AIRQEN | — | — | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** | S = Settable bit |  |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-24 **Unimplemented:** Read as ‘0’

bit 23-16 **CHAIRQ<7:0>:** Channel Transfer Abort IRQ bits**(**[**1**](#_bookmark190)**)**

11111111 = Interrupt 255 will abort any transfers in progress and sets the CHTAIF flag

•

•

•

00000001 = Interrupt 1 will abort any transfers in progress and sets the CHTAIF flag

00000000 = Interrupt 0 will abort any transfers in progress and sets the CHTAIF flag bit 15-8 **CHSIRQ<7:0>:** Channel Transfer Start IRQ bits**(**[**1**](#_bookmark190)**)**

11111111 = Interrupt 255 will initiate a DMA transfer

•

•

•

00000001 = Interrupt 1 will initiate a DMA transfer

00000000 = Interrupt 0 will initiate a DMA transfer bit 7 **CFORCE:** DMA Forced Transfer bit

1 = A DMA transfer is forced to begin when this bit is written to a ‘1’

0 = This bit always reads ‘0’

bit 6 **CABORT:** DMA Abort Transfer bit

1 = A DMA transfer is aborted when this bit is written to a ‘1’

0 = This bit always reads ‘0’

bit 5 **PATEN:** Channel Pattern Match Abort Enable bit

1 = Aborts transfer and clears CHEN on pattern match

0 = Pattern match is disabled

bit 4 **SIRQEN:** Channel Start IRQ Enable bit

1 = Starts channel cell transfer if an interrupt matching CHSIRQx occurs

0 = Interrupt number CHSIRQx is ignored and does not start a transfer bit 3 **AIRQEN:** Channel Abort IRQ Enable bit

1 = Channel transfer is aborted if an interrupt matching CHAIRQx occurs

0 = Interrupt number CHAIRQx is ignored and does not terminate a transfer bit 2-0 **Unimplemented:** Read as ‘0’

**Note 1:** See [Table 7-2](#_bookmark153) for the list of available interrupt IRQ sources.

REGISTER 8-9: DCHxINT: DMA CHANNEL x INTERRUPT CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHSDIE | CHSHIE | CHDDIE | CHDHIE | CHBCIE | CHCCIE | CHTAIE | CHERIE |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHSDIF | CHSHIF | CHDDIF | CHDHIF | CHBCIF | CHCCIF | CHTAIF | CHERIF |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-24 **Unimplemented:** Read as ‘0’

bit 23 **CHSDIE:** Channel Source Done Interrupt Enable bit

1 = Interrupt is enabled

0 = Interrupt is disabled

bit 22 **CHSHIE:** Channel Source Half Empty Interrupt Enable bit

1 = Interrupt is enabled

0 = Interrupt is disabled

bit 21 **CHDDIE:** Channel Destination Done Interrupt Enable bit

1 = Interrupt is enabled

0 = Interrupt is disabled

bit 20 **CHDHIE:** Channel Destination Half Full Interrupt Enable bit

1 = Interrupt is enabled

0 = Interrupt is disabled

bit 19 **CHBCIE:** Channel Block Transfer Complete Interrupt Enable bit

1 = Interrupt is enabled

0 = Interrupt is disabled

bit 18 **CHCCIE:** Channel Cell Transfer Complete Interrupt Enable bit

1 = Interrupt is enabled

0 = Interrupt is disabled

bit 17 **CHTAIE:** Channel Transfer Abort Interrupt Enable bit

1 = Interrupt is enabled

0 = Interrupt is disabled

bit 16 **CHERIE:** Channel Address Error Interrupt Enable bit

1 = Interrupt is enabled

0 = Interrupt is disabled

bit 15-8 **Unimplemented:** Read as ‘0’

bit 7 **CHSDIF:** Channel Source Done Interrupt Flag bit

1 = Channel Source Pointer has reached end of source (CHSPTRx = CHSSIZx)

0 = No interrupt is pending

bit 6 **CHSHIF:** Channel Source Half Empty Interrupt Flag bit

1 = Channel Source Pointer has reached midpoint of source (CHSPTRx = CHSSIZx/2)

0 = No interrupt is pending

REGISTER 8-9: DCHxINT: DMA CHANNEL x INTERRUPT CONTROL REGISTER (CONTINUED)

bit 5 **CHDDIF:** Channel Destination Done Interrupt Flag bit

1 = Channel Destination Pointer has reached end of destination (CHDPTRx = CHDSIZx)

0 = No interrupt is pending

bit 4 **CHDHIF:** Channel Destination Half Full Interrupt Flag bit

1 = Channel Destination Pointer has reached midpoint of destination (CHDPTRx = CHDSIZx/2)

0 = No interrupt is pending

bit 3 **CHBCIF:** Channel Block Transfer Complete Interrupt Flag bit

1 = A block transfer has been completed (the larger of CHSSIZx/CHDSIZx bytes has been transferred) or a pattern match event occurs

0 = No interrupt is pending

bit 2 **CHCCIF:** Channel Cell Transfer Complete Interrupt Flag bit

1 = A cell transfer has been completed (CHCSIZx bytes have been transferred)

0 = No interrupt is pending

bit 1 **CHTAIF:** Channel Transfer Abort Interrupt Flag bit

1 = An interrupt matching CHAIRQx has been detected and the DMA transfer has been aborted

0 = No interrupt is pending

bit 0 **CHERIF:** Channel Address Error Interrupt Flag bit

1 = A channel address error has been detected (either the source or the destination address is invalid)

0 = No interrupt is pending

REGISTER 8-10: DCHxSSA: DMA CHANNEL x SOURCE START ADDRESS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHSSA<31:24>**(**[**1**](#_bookmark193)**)** | | | | | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHSSA<23:16>**(**[**1**](#_bookmark193)**)** | | | | | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHSSA<15:8>**(**[**1**](#_bookmark193)**)** | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHSSA<7:0>**(**[**1**](#_bookmark193)**)** | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-0 **CHSSA<31:0>** Channel Source Start Address bits**(**[**1**](#_bookmark193)**)** Channel source start address.

**Note 1:** This must be the physical address of the source.

REGISTER 8-11: DCHxDSA: DMA CHANNEL x DESTINATION START ADDRESS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHDSA<31:24>**(**[**1**](#_bookmark195)**)** | | | | | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHDSA<23:16>**(**[**1**](#_bookmark195)**)** | | | | | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHDSA<15:8>**(**[**1**](#_bookmark195)**)** | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHDSA<7:0>**(**[**1**](#_bookmark195)**)** | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-0 **CHDSA<31:0>:** Channel Destination Start Address bits**(**[**1**](#_bookmark195)**)** Channel destination start address.

**Note 1:** This must be the physical address of the source.

REGISTER 8-12: DCHxSSIZ: DMA CHANNEL x SOURCE SIZE REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHSSIZ<15:8> | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHSSIZ<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’

bit 15-0 **CHSSIZ<15:0>:** Channel Source Size bits

1111111111111111 = 65,535-byte source size

•

•

•

0000000000000010 = 2-byte source size 0000000000000001 = 1-byte source size 0000000000000000 = 65,536-byte source size

REGISTER 8-13: DCHxDSIZ: DMA CHANNEL x DESTINATION SIZE REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHDSIZ<15:8> | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHDSIZ<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’

bit 15-0 **CHDSIZ<15:0>:** Channel Destination Size bits

1111111111111111 = 65,535-byte destination size

•

•

•

0000000000000010 = 2-byte destination size 0000000000000001 = 1-byte destination size 0000000000000000 = 65,536-byte destination size

REGISTER 8-14: DCHxSPTR: DMA CHANNEL x SOURCE POINTER REGISTER([1](#_bookmark199))

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| CHSPTR<15:8> | | | | | | | |
| 7:0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| CHSPTR<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’

bit 15-0 **CHSPTR<15:0>:** Channel Source Pointer bits

1111111111111111 = Points to Byte 65,535 of the source

•

•

•

0000000000000001 = Points to Byte 1 of the source

0000000000000000 = Points to Byte 0 of the source

**Note 1:** When in Pattern Detect mode, this register is reset on a pattern detect.

REGISTER 8-15: DCHxDPTR: DMA CHANNEL x DESTINATION POINTER REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| CHDPTR<15:8> | | | | | | | |
| 7:0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| CHDPTR<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’

bit 15-0 **CHDPTR<15:0>:** Channel Destination Pointer bits

1111111111111111 = Points to Byte 65,535 of the destination

•

•

•

0000000000000001 = Points to Byte 1 of the destination

0000000000000000 = Points to Byte 0 of the destination

REGISTER 8-16: DCHxCSIZ: DMA CHANNEL x CELL SIZE REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHCSIZ<15:8> | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHCSIZ<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’

bit 15-0 **CHCSIZ<15:0>:** Channel Cell Size bits

1111111111111111 = 65,535 bytes are transferred on an event

•

•

•

0000000000000010 = 2 bytes are transferred on an event 0000000000000001 = 1 byte is transferred on an event 0000000000000000 = 65,536 bytes are transferred on an event

REGISTER 8-17: DCHxCPTR: DMA CHANNEL x CELL POINTER REGISTER([1](#_bookmark203))

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| CHCPTR<15:8> | | | | | | | |
| 7:0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| CHCPTR<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’

bit 15-0 **CHCPTR<7:0>:** Channel Cell Progress Pointer bits

1111111111111111 = 65,535 bytes have been transferred since the last event

•

•

•

0000000000000001 = 1 byte has been transferred since the last event

0000000000000000 = 0 bytes have been transferred since the last event

**Note 1:** When in Pattern Detect mode, this register is reset on a pattern detect.

REGISTER 8-18: DCHxDAT: DMA CHANNEL x PATTERN DATA REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHPDAT<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7-0 **CHPDAT<7:0>:** Channel Data Register bits Pattern Terminate mode:

Data to be matched must be stored in this register to allow terminate on match.

All Other modes:

Unused.

* 1. **OSCILLATOR**

**CONFIGURATIO****N**

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To complement the information in this data sheet, refer to **Section 59. “Oscillators with DCO”** (DS60001329) in the *“PIC32*

*Family Reference Manual”*, which [is](http://www.microchip.com/PIC32) [available from the Microchip web site](http://www.microchip.com/PIC32) [(](http://www.microchip.com/PIC32)[www.microchip.com/PIC32).](http://www.microchip.com/PIC32)) The infor- mation in this data sheet supersedes the information in the FRM.

The PIC32MM0256GPM064 family oscillator system has the following modules and features:

* A Total of Five External and Internal Oscillator Options as Clock Sources
* On-Chip PLL with User-Selectable Multiplier and Output Divider to Boost Operating Frequency on Select Internal and External Oscillator Sources
* On-Chip User-Selectable Divisor Postscaler on Select Oscillator Sources
* Software-Controllable Switching between Various Clock Sources
* A Fail-Safe Clock Monitor (FSCM) that Detects Clock Failure and Permits Safe Application Recovery or Shutdown
* Flexible Reference Clock Output

A block diagram of the oscillator system is provided in [Figure 9-1](#_bookmark217).

### Fail-Safe Clock Monitor (FSCM)

The PIC32MM0256GPM064 family oscillator system includes a Fail-Safe Clock Monitor (FSCM). The FSCM monitors the SYSCLK for continuous operation. If it detects that the SYSCLK has failed, it switches the SYSCLK over to the FRC oscillator and triggers a Non- Maskable Interrupt (NMI). When the NMI is executed, software can attempt to restart the main oscillator or shut down the system.

In Sleep mode, both the SYSCLK and the FSCM halt, which prevents FSCM detection.

### Clock Switching Operation

With few limitations, applications are free to switch between any of the four clock sources (POSC, SOSC, FRC and LPRC) under software control and at any time. To limit the possible side effects that could result from this flexibility, PIC32 devices have a safeguard lock built into the switching process.

**Note:** The Primary Oscillator mode has three different submodes (XT, HS and EC), which are determined by the POSCMOD<1:0> Configuration bits. While an application can switch to and from Primary Oscillator mode in software, it cannot switch between the different primary submodes without reprogramming the device.

* + 1. ENABLING CLOCK SWITCHING

To enable clock switching, the FCKSM1 Configuration bit in FOSC must be programmed to ‘0’. (Refer to [**Section 26.1 “Configuration Bits”**](#_bookmark565) for further details.) If the FCKSM1 Configuration bit is unprogrammed (‘1’), the clock switching function and Fail-Safe Clock Monitor function are disabled; this is the default setting.

The NOSC<2:0> control bits (OSCCON<10:8>) do not control the clock selection when clock switching is disabled. However, the COSC<2:0> bits (OSCCON<14:12>) will reflect the clock source selected by the FNOSC<2:0> Configuration bits.

The OSWEN control bit (OSCCON<0>) has no effect when clock switching is disabled; it is held at ‘0’ at all times.

* + 1. OSCILLATOR SWITCHING SEQUENCE

At a minimum, performing a clock switch requires this basic sequence:

1. If desired, read the COSC<2:0> bits (OSCCON<14:12>) to determine the current oscillator source.
2. Perform the unlock sequence to allow a write to the OSCCON register.
3. Write the appropriate value to the NOSC<2:0> bits (OSCCON<10:8>) for the new oscillator source.
4. Set the OSWEN bit to initiate the oscillator switch.

Once the basic sequence is completed, the system clock hardware responds automatically as follows:

1. The clock switching hardware compares the COSCx bits with the new value of the NOSCx bits. If they are the same, then the clock switch is a redundant operation. In this case, the OSWEN bit is cleared automatically and the clock switch is aborted.
2. If a valid clock switch has been initiated, the LOCK (OSCTUN<11>) and CF (OSCCON<3>) bits are cleared.
3. The new oscillator is turned on by the hardware if it is not currently running. If a crystal oscillator must be turned on, the hardware will wait until the OST expires. If the new source is using the PLL, then the hardware waits until a PLL lock is detected (LOCK = 1).
4. The hardware waits for 10 clock cycles from the new clock source and then performs the clock switch.
5. The hardware clears the OSWEN bit to indicate a successful clock transition. In addition, the NOSC<2:0> bits values are transferred to the COSC<2:0> bits.
6. The old clock source is turned off if it is not being used by a peripheral, or enabled by device configuration or a control register.

A recommended code sequence for a clock switch includes the following:

1. Disable interrupts during the OSCCON register unlock and write sequence.
2. Execute the unlock sequence for OSCCON by writing 0xAA996655 and 0x556699AA to the SYSKEY register.
3. Write the new oscillator source to the NOSC<2:0> bits.
4. Set the OSWEN bit.
5. Relock the OSCCON register.
6. Continue to execute code that is not clock-sensitive (optional).

The core sequence for unlocking the OSCCON register and initiating a clock switch is shown in [Example 9-1](#_bookmark212).

EXAMPLE 9-1: BASIC CODE SEQUENCE

FOR CLOCK SWITCHING

SYSKEY = 0x00000000; SYSKEY = 0xAA996655; SYSKEY = 0x556699AA;

// force lock

// unlock

OSCCONbits.NOSC = 3;

// select the new clock source

OSCCONSET = 1;

// set the OSWEN bit

SYSKEY = 0x00000000;

// force lock

while (OSCCONbits.OSWEN); // optional wait for

switch operation

BSET OSCCON, #0

**Note 1:** The processor will continue to execute code throughout the clock switching sequence. Timing-sensitive code should not be executed during this time.

**2:** Direct clock switches between any Primary Oscillator mode with PLL and FRCPLL mode are not permitted. This applies to clock switches in either direc- tion. In these instances, the application must switch to FRC mode as a transi- tional clock source between the two PLL modes.

### FRC Active Clock Tuning

PIC32MM0256GPM064 family devices include an auto- matic mechanism to calibrate the FRC during run time. This system uses active clock tuning from a source of known accuracy to maintain the FRC within a very narrow margin of its nominal 8 MHz frequency. This allows for a frequency accuracy that is well within the requirements of the *“USB 2.0 Specification”* regarding full-speed USB devices.

**Note:** The self-tune feature maintains sufficient accuracy for operation in USB Device mode. For applications that function as a USB host, a high-accuracy clock source (±0.05%) is still required.

The self-tune system is controlled by the bits in the upper half of the OSCTUN register. Setting the ON bit (OSCTUN<15>) enables the self-tuning feature, allow- ing the hardware to calibrate to a source selected by the SRC bit (OSCTUN<12>). When SRC = 1, the system uses the Start-of-Frame (SOF) packets from an external USB host for its source. When SRC = 0, the system uses the crystal-controlled SOSC for its calibration source. Regardless of the source, the system uses the TUN<5:0> bits (OSCTUN<5:0>) to change the FRC Oscillator’s frequency. Frequency monitoring and adjustment is dynamic, occurring continuously during run time. While the system is active, the TUNx bits cannot be written to by software.

The self-tune system can generate a hardware interrupt, FSTIF. The interrupt can result from a drift of the FRC from the reference, by greater than 0.2% in either direc- tion, or whenever the frequency deviation is beyond the ability of the TUNx bits to correct (i.e., greater than 1.5%). The LOCK and ORNG status bits (OSCTUN<11,9>) are used to indicate these conditions.

The POL and ORPOL bits (OSCTUN<10,8>) configure the FSTIF interrupt to occur in the presence or the absence of the conditions. It is the user’s responsibility to monitor both the LOCK and ORNG bits to determine the exact cause of the interrupt.

**Note:** The POL and ORPOL bits should be ignored when the self-tune system is disabled (ON = 0).

**Note:** After exiting out of self-tune, 6 writes may be required to update the TUN<5:0> bits.

**Note:** To use the USB as a reference clock tuning source (SRC = 1), the microcontroller must be configured for USB device operation and connected to a non-suspended USB host or hub port.

If the SOSC is to be used as the reference clock tuning source (SRC = 0), the SOSC must also be enabled for clock tuning to occur.

FIGURE 9-1: PIC32MM0256GPM064 FAMILY OSCILLATOR DIAGRAM([1](#_bookmark220))

48 MHz to USB

 2

**Reference Clock**

REFO1CON REFO1TRIM

REFCLKI ROTRIM<8:0> (M) OE

**System PLL**

PLLODIV<2:0> (N)

POSC FRC LPRC

SPLLVCO SOSC

SYSCLK

 2  N + --M**-**



512

------ 

FIN**(1)**

REFCLKO

PLL x M

Fvco**(1)**

PLLICLK PLLMULT<6:0>

(M)

 N

FPLL**(1)**

RODIV<14:0> (N)

To MCCP, SCCP,

SPIx and UARTs

ROSEL<3:0>

**Primary Oscillator (POSC)**

SPLL

POSC (HS, EC)

OSC1/ CLKI

POSCMOD<1:0>

OSC2

To ADC, WDT, UART

and Flash Controller

FRC

Oscillator

8 MHz

Postscaler  N

FRCDIV

SYSCLK (FSYS)

TUN<5:0>

FRCDIV<2:0> (N)

LPRC

Oscillator

32 kHz

LPRC

PBCLK (FPB)

**Secondary Oscillator (SOSC)**

SOSC

SOSCO/ SCLKI

32.768 kHz SOSCEN

SOSCSEL

**Clock Control Logic**

SOSCI

FNOSC<2:0> NOSC<2:0>


COSC<2:0>

FCKSM<1:0> OSWEN

To Timer1, WDT, RTCC

To Timer1, RTCC, MCCP/SCCP and CLC

**Note 1:** Refer to [Table 29-19](#_bookmark701) in [**Section 29.0 “Electrical Characteristics”**](#_bookmark636) for frequency limitations.



Fail-Safe Clock Monitor

2 MHz ≤ FIN ≤ 24 MHz

16 MHz ≤ FVCO ≤ 96 MHz

FIGURE 9-2: REFERENCE OSCILLATOR

 2

48 MHz to USB

VCO

16-96 MHz

25 MHz Max**(**[**2**](#_bookmark223)**)**

 N

REFCLKO

**SPI Module**

RODIV<14:0>

ROTRIM<8:0>

OE

ROSEL<3:0>

**(**[**Note 1**](#_bookmark222)**)**

 N

SYSCLK PBCLK

25 MHz Max

50 MHz Max

SPI

Module

PLLMULT<6:0>

MCLKSEL

COSC<2:0>

PLLODIV<2:0>

PLLICLK

FRC

MCCP/SCCP

Module

CLKSEL<1:0>

**UART**

UART

Module

CLKSEL<1:0>

**Note 1:** Support circuitry for crystal is not shown.

**2:** In Retention mode, the maximum peripheral output frequency to an I/O pin must be limited to 33 kHz or less.



### Oscillator Control Registers

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 102

TABLE 9-1: OSCILLATOR CONFIGURATION REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(2)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets(1)** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2680 | OSCCON | 31:16 | — | — | — | — | — | FRCDIV<2:0> | | | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | COSC<2:0> | | | — | NOSC<2:0> | | | CLKLOCK | — | — | SLPEN | CF | — | SOSCEN | OSWEN | xx0x |
| 26A0 | SPLLCON | 31:16 | — | — | — | — | — | PLLODIV<2:0> | | | — | PLLMULT<6:0> | | | | | | | 0001 |
| 15:0 | — | — | — | — | — | — | — | — | PLLICLK | r | — | — | — | — | — | — | 0000 |
| 2720 | REFO1CON | 31:16 | — | RODIV<14:0> | | | | | | | | | | | | | | | 0000 |
| 15:0 | ON | — | SIDL | OE | RSLP | — | DIVSWEN | ACTIVE | — | — | — | — | ROSEL<3:0> | | | | 0000 |
| 2730 | REFO1TRIM | 31:16 | ROTRIM<8:0> | | | | | | | | | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 2770 | CLKSTAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | r | SPLLRDY | USBRDY | LPRCRDY | SOSCRDY | r | POSCRDY | SPDIVRDY | FRCRDY | 0000 |
| 2880 | OSCTUN | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON | r | SIDL | SRC | LOCK | POL | ORNG | ORPOL | — | — | TUN<5:0> | | | | | | 0000 |

**Legend:** x = unknown value on Reset; — = unimplemented, read as ‘0’; r = reserved bit. Reset values are shown in hexadecimal.

**Note 1:** Reset values are dependent on the FOSCSEL Configuration bits and the type of Reset.

**2:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

REGISTER 9-1: OSCCON: OSCILLATOR CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | — | — | FRCDIV<2:0> | | |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | R-y | R-y | R-y | U-0 | R/W-y | R/W-y | R/W-y |
| — | COSC<2:0> | | | — | NOSC<2:0> | | |
| 7:0 | R/W-0 | U-0 | U-0 | R/W-0 | R/W-0, HS | U-0 | R/W-y | R/W-y |
| CLKLOCK | — | — | SLPEN | CF | — | SOSCEN | OSWEN**(**[**1**](#_bookmark230)**)** |

|  |  |  |
| --- | --- | --- |
| **Legend:** | HS = Hardware Settable bit | y = Value set from Configuration bits on POR |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-27 **Unimplemented:** Read as ‘0’

bit 26-24 **FRCDIV<2:0>:** Internal Fast RC (FRC) Oscillator Clock Divider bits

111 = FRC divided by 256

110 = FRC divided by 64

101 = FRC divided by 32

100 = FRC divided by 16

011 = FRC divided by 8

010 = FRC divided by 4

001 = FRC divided by 2

000 = FRC divided by 1 (default setting) bit 23-15 **Unimplemented:** Read as ‘0’

bit 14-12 **COSC<2:0>:** Current Oscillator Selection bits

111-110 = Reserved (selects internal Fast RC (FRC) Oscillator divided by FRCDIV<2:0> bits (FRCDIV))

101 = Internal Low-Power RC (LPRC) Oscillator

100 = Secondary Oscillator (SOSC)

011 = Reserved

010 = Primary Oscillator (POSC) (XT, HS or EC)

001 = System PLL (SPLL)

000 = Internal Fast RC (FRC) Oscillator divided by FRCDIV<2:0> bits (FRCDIV) bit 11 **Unimplemented:** Read as ‘0’

bit 10-8 **NOSC<2:0>:** New Oscillator Selection bits

111-110 = Reserved (selects internal Fast RC (FRC) Oscillator divided by FRCDIV<2:0> bits (FRCDIV))

101 = Internal Low-Power RC (LPRC) Oscillator

100 = Secondary Oscillator (SOSC)

011 = Reserved

010 = Primary Oscillator (POSC) (XT, HS or EC)

001 = System PLL (SPLL)

000 = Internal Fast RC (FRC) Oscillator divided by FRCDIV<2:0> bits (FRCDIV)

On Reset, these bits are set to the value of the FNOSC<2:0> Configuration bits (FOSCSEL<2:0>).

**Note 1:** The Reset value for this bit depends on the setting of the IESO (FOSCSEL<7>) bit. When IESO = 1, the Reset value is ‘1’. When IESO = 0, the Reset value is ‘0’.

**Note:** Writes to this register require an unlock sequence. Refer to [**Section 26.4 “System Registers Write**](#_bookmark570)[**Protection”**](#_bookmark570) for details.

REGISTER 9-1: OSCCON: OSCILLATOR CONTROL REGISTER (CONTINUED)

bit 7 **CLKLOCK:** Clock Selection Lock Enable bit

1 = Clock and PLL selections are locked

0 = Clock and PLL selections are not locked and may be modified bit 6-5 **Unimplemented:** Read as ‘0’

bit 4 **SLPEN:** Sleep Mode Enable bit

1 = Device will enter Sleep mode when a WAIT instruction is executed

0 = Device will enter Idle mode when a WAIT instruction is executed bit 3 **CF:** Clock Fail Detect bit

1 = FSCM has detected a clock failure

0 = No clock failure has been detected bit 2 **Unimplemented:** Read as ‘0’

bit 1 **SOSCEN:** Secondary Oscillator (SOSC) Enable bit

1 = Enables the Secondary Oscillator

0 = Disables the Secondary Oscillator bit 0 **OSWEN:** Oscillator Switch Enable bit**(**[**1**](#_bookmark230)**)**

1 = Initiates an oscillator switch to a selection specified by the NOSC<2:0> bits

0 = Oscillator switch is complete

**Note 1:** The Reset value for this bit depends on the setting of the IESO (FOSCSEL<7>) bit. When IESO = 1, the Reset value is ‘1’. When IESO = 0, the Reset value is ‘0’.

**Note:** Writes to this register require an unlock sequence. Refer to **Section 26.4 “System Registers Write Protection”** for details.

REGISTER 9-2: SPLLCON: SYSTEM PLL CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | — | — | PLLODIV<2:0> | | |
| 23:16 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-1 |
| — | PLLMULT<6:0> | | | | | | |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-y | r-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| PLLICLK | — | — | — | — | — | — | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** | r = Reserved bit | y = Values set from Configuration bits on POR |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-27 **Unimplemented:** Read as ‘0’

bit 26-24 **PLLODIV<2:0>:** System PLL Output Clock Divider bits

111 = PLL divide-by-256 110 = PLL divide-by-64 101 = PLL divide-by-32 100 = PLL divide-by-16 011 = PLL divide-by-8 010 = PLL divide-by-4 001 = PLL divide-by-2

000 = PLL divide-by-1 (default setting) bit 23 **Unimplemented:** Read as ‘0’

bit 22-16 **PLLMULT<6:0>:** System PLL Multiplier bits

111111-0000111 = Reserved

0000110 = 24x

0000101 = 12x

0000100 = 8x

0000011 = 6x

0000010 = 4x

0000001 = 3x (default setting)

0000000 = 2x

bit 15-8 **Unimplemented:** Read as ‘0’

bit 7 **PLLICLK:** System PLL Input Clock Source bit

1 = FRC is selected as the input to the system PLL (not divided)

0 = POSC is selected as the input to the system PLL; the POR default value is specified by the PLLSRC bit The POR default value is specified by the PLLSRC Configuration bit in the FOSCSEL register. Refer to [Register 26-9](#_bookmark605) in [**Section 26.0 “Special Features”**](#_bookmark564) for more information.

bit 6 **Reserved:** Maintain as ‘0’

bit 5-0 **Unimplemented:** Read as ‘0’

**Note 1:** Writes to this register require an unlock sequence. Refer to [**Section 26.4 “System Registers Write**](#_bookmark570)[**Protection”**](#_bookmark570) for details.

REGISTER 9-3: REFO1CON: REFERENCE OSCILLATOR CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | RODIV<14:8> | | | | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| RODIV<7:0> | | | | | | | |
| 15:8 | R/W-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | R/W-0, HC | R-0, HS, HC |
| ON**(**[**1**](#_bookmark235)**)** | — | SIDL | OE | RSLP**(**[**2**](#_bookmark236)**)** | — | DIVSWEN | ACTIVE**(**[**1**](#_bookmark235)**)** |
| 7:0 | U-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | — | ROSEL<3:0>**(**[**3**](#_bookmark237)**)** | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** | HC = Hardware Clearable bit | HS = Hardware Settable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **Unimplemented:** Read as ‘0’

bit 30-16 **RODIV<14:0>:** Reference Clock Divider bits

The value selects the reference clock divider bits (see [Figure 9-1](#_bookmark217) for details). A value of ‘0’ selects no divider. bit 15 **ON:** Reference Oscillator Output Enable bit**(**[**1**](#_bookmark235)**)**

1 = Reference oscillator module is enabled

0 = Reference oscillator module is disabled bit 14 **Unimplemented:** Read as ‘0’

bit 13 **SIDL:** Peripheral Stop in Idle Mode bit

1 = Discontinues module operation when device enters Idle mode

0 = Continues module operation in Idle mode bit 12 **OE:** Reference Clock Output Enable bit

1 = Reference clock is driven out on the REFO1 pin

0 = Reference clock is not driven out on the REFO1 pin bit 11 **RSLP:** Reference Oscillator Module Run in Sleep bit**(**[**2**](#_bookmark236)**)**

1 = Reference oscillator module output continues to run in Sleep

0 = Reference oscillator module output is disabled in Sleep bit 10 **Unimplemented:** Read as ‘0’

bit 9 **DIVSWEN:** Divider Switch Enable bit

1 = Divider switch is in progress

0 = Divider switch is complete

bit 8 **ACTIVE:** Reference Clock Request Status bit**(**[**1**](#_bookmark235)**)**

1 = Reference clock request is active

0 = Reference clock request is not active bit 7-4 **Unimplemented:** Read as ‘0’

**Note 1:** Do not write to this register when the ON bit is not equal to the ACTIVE bit.

**2:** This bit is ignored when the ROSEL<3:0> bits = 0000.

**3:** The ROSEL<3:0> bits should not be written while the ACTIVE bit is ‘1’, as undefined behavior may result.

REGISTER 9-3: REFO1CON: REFERENCE OSCILLATOR CONTROL REGISTER (CONTINUED)

bit 3-0 **ROSEL<3:0>:** Reference Clock Source Select bits**(**[**3**](#_bookmark237)**)**

1111 = Reserved

•

•

•

0111 = System PLL VCO output (not divided)

0110 = Reserved

0101 = SOSC

0100 = LPRC

0011 = FRC

0010 = POSC

0001 = Reserved

0000 = SYSCLK

**Note 1:** Do not write to this register when the ON bit is not equal to the ACTIVE bit.

**2:** This bit is ignored when the ROSEL<3:0> bits = 0000.

**3:** The ROSEL<3:0> bits should not be written while the ACTIVE bit is ‘1’, as undefined behavior may result.

REGISTER 9-4: REFO1TRIM: REFERENCE OSCILLATOR TRIM REGISTER([1](#_bookmark239),[2](#_bookmark240),[3](#_bookmark241))

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| ROTRIM<8:1> | | | | | | | |
| 23:16 | R/W-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| ROTRIM<0> | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-23 **ROTRIM<8:0>:** Reference Oscillator Trim bits

111111111 = 511/512 divisor added to the RODIVx value

111111110 = 510/512 divisor added to the RODIVx value

•

•

•

100000000 = 256/512 divisor added to the RODIVx value

•

•

•

000000010 = 2/512 divisor added to the RODIVx value 000000001 = 1/512 divisor added to the RODIVx value 000000000 = 0 divisor added to the RODIVx value

bit 22-0 **Unimplemented:** Read as ‘0’

**Note 1:** While the ON bit (REFO1CON<15>) is ‘1’, writes to this register do not take effect until the DIVSWEN bit is also set to ‘1’.

**2:** Do not write to this register when the ON bit (REFO1CON<15>) is not equal to the ACTIVE bit (REFO1CON<8>).

**3:** Specified values in this register do not take effect if RODIV<14:0> (REFO1CON<30:16>) = 0.

REGISTER 9-5: CLKSTAT: CLOCK STATUS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | r-1 |
| — | — | — | — | — | — | — | — |
| 7:0 | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC | r-0 | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC |
| SPLLRDY | USBRDY | LPRCRDY | SOSCRDY | — | POSCRDY | SPDIVRDY | FRCRDY |

|  |  |  |
| --- | --- | --- |
| **Legend:** | HS = Hardware Settable bit | HC = Hardware Clearable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared r = Reserved bit |

bit 31-9 **Unimplemented:** Read as ‘0’

bit 8 **Reserved:** Read as ‘1’ bit 7 **SPLLRDY**: PLL Lock bit

1 = PLL is locked and ready

0 = PLL is not locked

bit 6 **USBRDY**: USB Oscillator Ready bit

1 = USB oscillator is running

0 = USB oscillator is not running

bit 5 **LPRCRDY:** LPRC Oscillator Ready bit

1 = LPRC oscillator is enabled

0 = LPRC oscillator is not enabled

bit 4 **SOSCRDY:** Secondary Oscillator (SOSC) Ready bit

1 = SOSC is enabled and the Oscillator Start-up Timer (OST) has expired

0 = SOSC is not enabled or the Oscillator Start-up Timer has not expired bit 3 **Reserved:** Read as ‘0’

bit 2 **POSCRDY:** Primary Oscillator (POSC) Ready bit

1 = POSC is enabled and the Oscillator Start-up Timer has expired

0 = POSC is not enabled or the Oscillator Start-up Timer has not expired

bit 1 **SPDIVRDY:** System PLL (with postscaler, SPLLDIV) Clock Ready Status bit

1 = SPLLDIV is enabled and the PLL start-up timer has expired

0 = SPLLDIV is not enabled or the PLL start-up timer has not expired bit 0 **FRCRDY:** Fast RC (FRC) Oscillator Ready bit

1 = FRC oscillator is enabled

0 = FRC oscillator is not enabled

REGISTER 9-6: OSCTUN: FRC TUNING REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | R-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | r-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| ON | — | SIDL | SRC | LOCK | POL | ORNG | ORPOL |
| 7:0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | TUN<5:0>**(**[**1**](#_bookmark245)**)** | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** | r = Reserved bit |  |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’ bit 15 **ON:** Self-Tune Enable bit

1 = FRC self-tuning is enabled; the TUNx bits are controlled by hardware

0 = FRC self-tuning is disabled; the TUNx bits are readable and writable bit 14 **Reserved:** Used by debugger

bit 13 **SIDL:** FRC Self-Tune Stop in Idle bit

1 = Self-tuning stops during Idle mode

0 = Self-tuning continues during Idle mode

bit 12 **SRC:** FRC Self-Tune Reference Clock Source bit

1 = The USB host clock is used to tune the FRC

0 = The 32.768 kHz SOSC clock is used to tune the FRC bit 11 **LOCK:** FRC Self-Tune Lock Status bit

1 = FRC accuracy is currently within ±0.2% of the SRC reference accuracy

0 = FRC accuracy may not be within ±0.2% of the SRC reference accuracy bit 10 **POL:** FRC Self-Tune Lock Interrupt Polarity bit

1 = A self-tune lock interrupt is generated when LOCK is ‘0’

0 = A self-tune lock interrupt is generated when LOCK is ‘1’ bit 9 **ORNG:** FRC Self-Tune Out of Range Status bit

1 = SRC reference clock error is beyond the range of TUN<5:0>; no tuning is performed

0 = SRC reference clock is within the tunable range; tuning is performed bit 8 **ORPOL:** FRC Self-Tune Out of Range Interrupt Polarity bit

1 = A self-tune out of range interrupt is generated when STOR is ‘0’

0 = A self-tune out of range interrupt is generated when STOR is ‘1’ bit 7-6 **Unimplemented:** Read as ‘0’

**Note 1:** OSCTUN functionality has been provided to help customers compensate for temperature effects on the FRC frequency over a wide range of temperatures. The tuning step-size is an approximation and is neither characterized, nor tested.

**Note:** Writes to this register require an unlock sequence. Refer to [**Section 26.4 “System Registers Write**](#_bookmark570)[**Protection”**](#_bookmark570) for details.

REGISTER 9-6: OSCTUN: FRC TUNING REGISTER (CONTINUED)

bit 5-0 **TUN<5:0>:** FRC Oscillator Tuning bits**(**[**1**](#_bookmark245)**)**

100000 = Center frequency – 1.50%

100001 =

•

•

•

111111 =

000000 = Center frequency; oscillator runs at a nominal frequency (8 MHz)

000001 =

•

•

•

011110 =

011111 = Center frequency + 1.453%

**Note 1:** OSCTUN functionality has been provided to help customers compensate for temperature effects on the FRC frequency over a wide range of temperatures. The tuning step-size is an approximation and is neither characterized, nor tested.

**Note:** Writes to this register require an unlock sequence. Refer to **Section 26.4 “System Registers Write Protection”** for details.

NOTES:

* 1. **I/O PORT****S** Many of the device pins are shared among the periph- erals and the Parallel I/O (PIO) ports. All I/O input ports

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a compre- hensive reference source. To complement the information in this data sheet, refer to **Section 12. “I/O Ports”** (DS60001120) in the *“PIC32 Family Reference Manual”*[,](http://www.microchip.com/PIC32) [which is available from the Microchip](http://www.microchip.com/PIC32) [web site (](http://www.microchip.com/PIC32)[www.microchip.com/PIC32).](http://www.microchip.com/PIC32)) The information in this data sheet supersedes the information in the FRM.

feature Schmitt Trigger inputs for improved noise immunity. Some pins in the devices are 5V tolerant pins. Some of the key features of the I/O ports are:

* + - Individual Output Pin Open-Drain Enable/Disable
    - Individual Input Pin Weak Pull-up and Pull-Down
    - Monitor Selective Inputs and Generate Interrupt when Change in Pin State is Detected
    - Operation during Sleep and Idle modes
    - Fast Bit Manipulation using the CLR, SET and INV Registers

[Figure 10-1](#_bookmark248) illustrates a block diagram of a typical multiplexed I/O port.

FIGURE 10-1: BLOCK DIAGRAM OF A TYPICAL SHARED PORT STRUCTURE

**Peripheral Module** Peripheral Input Data Peripheral Module Enable

Peripheral Output Enable

Peripheral Output Data

**Output Multiplexers**

**I/O**

1

0

Output Enable

**PIO Module**

Read TRISx

1

0

Output Data

Data Bus

D Q

I/O Pin

WR TRISx

CK

TRIS Latch

D Q

WR LATx + WR PORTx

CK

Data Latch

Read LATx

Input Data

Read PORTx



### CLR, SET and INV Registers

Every I/O module register has a corresponding CLR (Clear), SET (Set) and INV (Invert) register designed to provide fast atomic bit manipulations. As the name of the register implies, a value written to a SET, CLR or INV register effectively performs the implied operation, but only on the corresponding base register and only bits specified as ‘1’ are modified. Bits specified as ‘0’ are not modified.

Reading SET, CLR and INV registers returns undefined values. To see the effects of a write operation to a SET, CLR or INV register, the base register must be read.

### Parallel I/O (PIO) Ports

All port pins have 14 registers directly associated with their operation as digital I/Os. The Data Direction register (TRISx) determines whether the pin is an input or an out- put. If the data direction bit is a ‘1’, then the pin is an input. All port pins are defined as inputs after a Reset. The LATx register controls the pin level when it is configured as an output. Reads from the PORTx register read the port pins, while writes to the port pins write the latch, LATx.

### Open-Drain Configuration

In addition to the PORTx, LATx and TRISx registers for data control, the port pins can also be individually configured for either digital or open-drain outputs. This is controlled by the Open-Drain Control x register, ODCx, associated with each port. Setting any of the bits config- ures the corresponding pin to act as an open-drain output.

The open-drain feature allows the generation of outputs higher than VDD (e.g., 5V), on any desired 5V tolerant pins, by using external pull-up resistors. The maximum open-drain voltage allowed is the same as the maximum VIH specification.

### Configuring Analog and Digital Port Pins

When the PORTx register is read, all pins configured as analog input channels are read as cleared (a low level).

Pins configured as digital inputs do not convert an analog input. Analog levels on any pin defined as a digital input (including the ANx pins) can cause the input buffer to consume current that exceeds the device spec- ifications. The ANSELx register controls the operation of the analog port pins. The port pins that are to function as analog inputs must have their corresponding ANSELx and TRISx bits set. In order to use port pins for I/O func- tionality with digital modules, such as timers, UARTs, etc., the corresponding ANSELx bit must be cleared. The ANSELx register has a default value of 0xFFFF. Therefore, all pins that share analog functions are analog (not digital) by default. If the TRISx bit is cleared (output) while the ANSELx bit is set, the digital output level (VOH or VOL) is used by an analog peripheral, such as the ADC or comparator module.

### I/O Port Write/Read Timing

One instruction cycle is required between a port direction change or port write operation and a read operation of the same port. Typically, this instruction would be a NOP.

There is a three-instruction cycle delay in the port read synchronizer. When a port or port bit is read, the returned value is the value that was present on the port three system clocks prior.

### GPIO Port Merging

Port merging creates a 32-bit wide port from two GPIO ports. When the PORT32 bit is set, the next I/O port is mapped to the upper 16 bits of the lower port.

Only the next higher letter port can be merged to a given port (i.e., PORTA can only be merged with PORTB).

**Note:** All 32 pins may not be available. Refer to the pin diagrams for information regarding GPIO port pin availability.

### Input Change Notification (ICN)

The Input Change Notification function of the I/O ports allows the PIC32MM devices to generate interrupt requests to the processor in response to a Change-of- State (COS) on the input pins. This feature can detect input Change-of-States, even in Sleep mode, when the clocks are disabled. Every I/O port pin can be selected (enabled) for generating an interrupt request on a Change-of-State. Five control registers are associated with the Change Notification (CN) functionality of each I/O port. To enable the Change Notification feature for the port, the ON bit (CNCONx<15>) must be set.

The CNEN0x and CNEN1x registers contain the CN interrupt enable control bits for each of the input pins. The setting of these bits enables a CN interrupt for the corresponding pins. Also, these bits, in combination with the CNSTYLE bit (CNCONx<11>), define a type of transition when the interrupt is generated. Possible CN event options are listed in [Table 10-1](#_bookmark260).

TABLE 10-1: CHANGE NOTIFICATION

EVENT OPTIONS

|  |  |  |  |
| --- | --- | --- | --- |
| **CNSTYLE Bit (CNCONx<11>)** | **CNEN1x**  **Bit** | **CNEN0x**  **Bit** | **Change Notification Event Description** |
| 0 | Does not matter | 0 | Disabled |
| 0 | Does not matter | 1 | Detects a mismatch between the last read state and the current state of the pin |
| 1 | 0 | 0 | Disabled |
| 1 | 0 | 1 | Detects a positive transition only (from ‘0’ to ‘1’) |
| 1 | 1 | 0 | Detects a negative transition only (from ‘1’ to ‘0’) |
| 1 | 1 | 1 | Detects both positive and negative transitions |

The CNSTATx register indicates whether a change occurred on the corresponding pin since the last read of the PORTx bit. In addition to the CNSTATx register, the CNFx register is implemented for each port. This register contains flags for Change Notification events. These flags are set if the valid transition edge, selected in the CNEN0x and CNEN1x registers, is detected. CNFx stores the occurrence of the event. CNFx bits must be cleared in software to get the next Change Notification interrupt. The CN interrupt is generated only for the I/Os configured as inputs (corresponding TRISx bits must be set).

### Pin Pull-up and Pull-Down

Each I/O pin also has a weak pull-up and a weak pull- down connected to it. The pull-ups act as a current source, or sink source, connected to the pin and eliminate the need for external resistors when push button or keypad devices are connected. The pull-ups and pull-downs are enabled separately using the CNPUx and the CNPDx registers, which contain the control bits for each of the pins. Setting any of the control bits enables the weak pull-ups and/or pull-downs for the corresponding pins.

### Peripheral Pin Select (PPS)

A major challenge in general purpose devices is providing the largest possible set of peripheral features while mini- mizing the conflict of features on I/O pins. The challenge is even greater on low pin count devices. In an application where more than one peripheral needs to be assigned to a single pin, inconvenient work arounds in application code, or a complete redesign, may be the only option.

PPS configuration provides an alternative to these choices by enabling peripheral set selection and their placement on a wide range of I/O pins. By increasing the pinout options available on a particular device, users can better tailor the device to their entire application, rather than trimming the application to fit the device.

The PPS configuration feature operates over a fixed subset of digital I/O pins. Users may independently map the input and/or output of most digital peripherals to these I/O pins. PPS is performed in software and generally does not require the device to be reprogrammed. Hardware safeguards are included that prevent accidental or spurious changes to the peripheral mapping once it has been established.

* + 1. AVAILABLE PINS

The number of available pins is dependent on the particular device and its pin count. Pins that support the PPS feature include the designation, “RPn”, in their full pin designation, where “RP” designates a Remappable Peripheral and “n” is the remappable port number.

* + 1. AVAILABLE PERIPHERALS

The peripherals managed by the PPS are all digital only peripherals. These include general serial communica- tions (UART and SPI), general purpose timer clock inputs, timer-related peripherals (MCCP, SCCP) and others.

In comparison, some digital only peripheral modules are never included in the PPS feature. This is because the peripheral’s function requires special I/O circuitry on a specific port and cannot be easily connected to multiple

pins. These modules include I2C among others. A

similar requirement excludes all modules with analog inputs, such as the Analog-to-Digital Converter (ADC).

A key difference between remappable and non- remappable peripherals is that remappable peripherals are not associated with a default I/O pin. The peripheral must always be assigned to a specific I/O pin before it can be used. In contrast, non-remappable peripherals are always available on a default pin, assuming that the peripheral is active and not conflicting with another peripheral.

When a remappable peripheral is active on a given I/O pin, it takes priority over all other digital I/Os and digital communication peripherals associated with the pin. Priority is given regardless of the type of peripheral that is mapped. Remappable peripherals never take priority over any analog functions associated with the pin.

* + 1. CONTROLLING PPS

PPS features are controlled through two sets of SFRs: one to map peripheral inputs and one to map outputs. Because they are separately controlled, a particular peripheral’s input and output (if the peripheral has both) can be placed on any selectable function pin without constraint.

The association of a peripheral to a peripheral-selectable pin is handled in two different ways, depending on whether an input or output is being mapped.

* + 1. INPUT MAPPING

The inputs of the PPS options are mapped on the basis of the peripheral. That is, a control register associated with a peripheral dictates the pin it will be mapped to. The RPINRx registers (refer to the peripheral pins listed in [Table 10-2](#_bookmark270)) are used to configure peripheral input map- ping (see [Register 10-1](#_bookmark302)). Each register contains sets of 5-bit fields. Programming these bits with a number of the remappable pin will connect the peripheral to this RPn pin (refer to [Table 10-3](#_bookmark272)). For any given device, the valid range of values for any bit field is shown in [Table 10-2](#_bookmark270).

For example, [Figure 10-2](#_bookmark268) illustrates the remappable pin selection for the U2RX input.

FIGURE 10-2: REMAPPABLE INPUT

EXAMPLE FOR U2RX



U2RXR<4:0>

1

RP1

2

RP2

3

U2RX Input to Peripheral

RP3

n

RPn

**Note:** For input only, PPS functionality does not have priority over TRISx settings. Therefore, when configuring an RPn pin for input, the corresponding bit in the TRISx register must also be configured for input (set to ‘1’).

TABLE 10-2: INPUT PIN SELECTION

|  |  |  |  |
| --- | --- | --- | --- |
| **Input Name** | **Function Name** | **Register** | **Function Bits** |
| External Interrupt 4 | INT4 | RPINR1 | INT4R<4:0> |
| MCCP1 Input Capture | ICM1 | RPINR2 | ICM1R<4:0> |
| MCCP2 Input Capture | ICM2 | RPINR2 | ICM2R<4:0> |
| MCCP3 Input Capture | ICM3 | RPINR3 | ICM3R<4:0> |
| SCCP4 Input Capture | ICM4 | RPINR3 | ICM4R<4:0> |
| Output Compare Fault A | OCFA | RPINR5 | OCFAR<4:0> |
| Output Compare Fault B | OCFB | RPINR5 | OCFBR<4:0> |
| CCP Clock Input A | TCKIA | RPINR6 | TCKIAR<4:0> |
| CCP Clock Input B | TCKIB | RPINR6 | TCKIBR<4:0> |
| SCCP5 Input Capture | ICM5 | RPINR7 | ICM5R<4:0> |
| SCCP6 Input Capture | ICM6 | RPINR7 | ICM6R<4:0> |
| SCCP7 Input Capture | ICM7 | RPINR7 | ICM7R<4:0> |
| SCCP8 Input Capture | ICM8 | RPINR7 | ICM8R<4:0> |
| SCCP9 Input Capture | ICM9 | RPINR8 | ICM9R<4:0> |
| UART3 Receive | U3RX | RPINR8 | U3RXR<4:0> |
| UART2 Receive | U2RX | RPINR9 | U2RXR<4:0> |
| UART2 Clear-to-Send | U2CTS | RPINR9 | U2CTSR<4:0> |
| UART3 Clear-to-Send | U3CTS | RPINR10 | U3CTSR<4:0> |
| SPI2 Data Input | SDI2 | RPINR11 | SDI2R<4:0> |
| SPI2 Clock Input | SCK2IN | RPINR11 | SCK2INR<4:0> |
| SPI2 Slave Select Input | SS2IN | RPINR11 | SS2INR<4:0> |
| CLC Input A | CLCINA | RPINR12 | CLCINAR<4:0> |
| CLC Input B | CLCINB | RPINR12 | CLCINBR<4:0> |

TABLE 10-3: REMAPPABLE INPUT SOURCES PIN ASSIGNMENTS([1](#_bookmark274))

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Value** | **RPn Pins** | **Pin Assignment** |  | **Value** | **RPn Pins** | **Pin Assignment** |
| 00001 | RP1 | RA0 Pin | 01110 | RP14 | RB9 Pin |
| 00010 | RP2 | RA1 Pin | 01111 | RP15 | RB13 Pin |
| 00011 | RP3 | RA2 Pin | 10000 | RP16 | RB14 Pin |
| 00100 | RP4 | RA3 Pin | 10001 | RP17 | RB15 Pin |
| 00101 | RP5 | RA4 Pin | 10010 | RP18 | RC9 Pin |
| 00110 | RP6 | RB0 Pin | 10011 | RP19 | RC2 Pin |
| 00111 | RP7 | RB1 Pin | 10100 | RP20 | RC7 Pin |
| 01000 | RP8 | RB2 Pin | 10101 | RP21 | RA7 Pin |
| 01001 | RP9 | RB3 Pin | 10110 | RP22 | RA10 Pin |
| 01010 | RP10 | RB4 Pin | 10111 | RP23 | RC6 Pin |
| 01011 | RP11 | RB5 Pin | 11000 | RP24 | RA9 Pin |
| 01100 | RP12 | RB7 Pin | 11001-11111 | Reserved | |
| 01101 | RP13 | RB8 Pin |  | | | |

**Note 1:** All RPx pins are not available on all packages.

* + 1. OUTPUT MAPPING

In contrast to inputs, the outputs of the PPS options are mapped on the basis of the pin. In this case, a control register associated with a particular pin dictates the peripheral output to be mapped. The RPORx registers are used to control output mapping. Like the RPINRx registers, each register contains sets of 4-bit fields. The value of the bit field corresponds to one of the peripherals and that peripheral’s output is mapped to the pin (see [Table 10-4](#_bookmark279) and [Figure 10-3](#_bookmark276)).

A null output is associated with the output register Reset value of ‘0’. This is done to ensure that remap- pable outputs remain disconnected from all output pins by default.

FIGURE 10-3: EXAMPLE OF MULTIPLEXING

OF REMAPPABLE OUTPUT FOR RP0



RP1R<3:0>

Default 0

U2TX Output

1

SDO2 Output 2

Output Data

RP1

CLC2OUT 9

* + 1. CONTROLLING CONFIGURATION CHANGES

Because peripheral remapping can be changed during run time, some restrictions on peripheral remapping are needed to prevent accidental configuration changes. PIC32MM0256GPM064 family devices include two features to prevent alterations to the peripheral map:

* Control register lock sequence
* Configuration bit select lock
  + - 1. Control Register Lock

Under normal operation, writes to the RPORx and RPINRx registers are not allowed. Attempted writes appear to execute normally, but the contents of the registers remain unchanged. To change these regis- ters, they must be unlocked in hardware. The register lock is controlled by the IOLOCK bit in the RPCON register. Clearing IOLOCK prevents writes to the control registers; setting IOLOCK allows writes.

To set or clear the IOLOCK bit, an unlock sequence must be executed. Refer to [**Section 26.4 “System**](#_bookmark570)[**Registers Write Protection”**](#_bookmark570) for details.

TABLE 10-4: OUTPUT PIN SELECTION

|  |  |  |
| --- | --- | --- |
| **Output Function Number** | **Function** | **Output Name** |
| 0 | None | Not Connected |
| 1 | C1OUT | Comparator 1 Output |
| 2 | C2OUT | Comparator 2 Output |
| 3 | C3OUT | Comparator 3 Output |
| 4 | U2TX | UART2 Transmit |
| 5 | U2RTS | UART2 Request-to-Send |
| 6 | U3TX | UART3 Transmit |
| 7 | U3RTS | UART3 Request-to-Send |
| 8 | SDO2 | SPI2 Data Output |
| 9 | SCK2OUT | SPI2 Clock Output |
| 10 | SS2OUT | SPI2 Slave Select Output |
| 11 | OCM4 | SCCP4 Output Compare Output |
| 12 | OCM5 | SCCP5 Output Compare Output |
| 13 | OCM6 | SCCP6 Output Compare Output |
| 14 | OCM7 | SCCP7 Output Compare Output |
| 15 | OCM8 | SCCP8 Output Compare Output |
| 16 | OCM9 | SCCP9 Output Compare Output |
| 17 | CLC1OUT | CLC1 Output |
| 18 | CLC2OUT | CLC2 Output |
| 19 | CLC3OUT | CLC3 Output |
| 20 | CLC4OUT | CLC4 Output |

### I/O Ports Control Registers

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 120

TABLE 10-5: PORTA REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2BB0 | ANSELA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | ANSA<13:11>**(**[**2**](#_bookmark283)**)** | | | — | — | — | — | ANSA6**(**[**2**](#_bookmark283)**)** | — | — | ANSA<3:0> | | | | 000F |
| 2BC0 | TRISA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | TRISA<15:0>**(**[**3**](#_bookmark284)**)** | | | | | | | | | | | | | | | | 021F |
| 2BD0 | PORTA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | RA<15:0>**(**[**3**](#_bookmark284)**)** | | | | | | | | | | | | | | | | xxxx |
| 2BE0 | LATA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | LATA<15:0>**(**[**3**](#_bookmark284)**)** | | | | | | | | | | | | | | | | 0000 |
| 2BF0 | ODCA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ODCA<15:0>**(**[**3**](#_bookmark284)**)** | | | | | | | | | | | | | | | | 0000 |
| 2C00 | CNPUA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNPUA<15:0>**(**[**3**](#_bookmark284)**)** | | | | | | | | | | | | | | | | 0000 |
| 2C10 | CNPDA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNPDA<15:0>**(**[**4**](#_bookmark285)**)** | | | | | | | | | | | | | | | | 0000 |
| 2C20 | CNCONA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON | — | — | — | CNSTYLE | PORT32 | — | — | — | — | — | — | — | — | — | — | 0000 |
| 2C30 | CNEN0A | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNIE0A<15:0>**(**[**3**](#_bookmark284)**)** | | | | | | | | | | | | | | | | 0000 |
| 2C40 | CNSTATA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNSTATA<15:0>**(**[**3**](#_bookmark284)**)** | | | | | | | | | | | | | | | | 0000 |
| 2C50 | CNEN1A | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNIE1A<15:0>**(**[**3**](#_bookmark284)**)** | | | | | | | | | | | | | | | | 0000 |
| 2C60 | CNFA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNFA<15:0>**(**[**3**](#_bookmark284)**)** | | | | | | | | | | | | | | | | 0000 |

**Legend:** x = unknown value on Reset; — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

**2:** These bits are not available on 48, 36 or 28-pin devices.

**3:** Bits<14:11> are not available on 48-pin devices; bits<15:10> and bits<8:5> are not available on 36-pin devices.

**4:** Bits<15:5> are not available on 28-pin devices.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 121

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2CB0 | ANSELB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | ANSB<13:11>**(**[**2**](#_bookmark290)**)** | | | — | — | — | — | ANSB6**(**[**2**](#_bookmark290)**)** | — | ANSB<4:0> | | | | | E01F |
| 2CC0 | TRISB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | TRISB<15:0> | | | | | | | | | | | | | | | | FFFF |
| 2CD0 | PORTB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | RB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 2CE0 | LATB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | LATB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 2CF0 | ODCB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ODCB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 2D00 | CNPUB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNPUB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 2D10 | CNPDB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNPDB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 2D20 | CNCONB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON | — | — | — | CNSTYLE | PORT32 | — | — | — | — | — | — | — | — | — | — | 0000 |
| 2D30 | CNEN0B | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNIE0B<15:0> | | | | | | | | | | | | | | | | 0000 |
| 2D40 | CNSTATB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNSTATB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 2D50 | CNEN1B | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNIE1B<15:0> | | | | | | | | | | | | | | | | 0000 |
| 2D60 | CNFB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNFB<15:0> | | | | | | | | | | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

**2:** The ANSB<13:11> and ANSB6 bits are not available on 48, 36 or 28-pin devices.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 122

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2DB0 | ANSELC | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | ANSC8**(**[**2**](#_bookmark293)**)** | — | — | ANSC5**(**[**2**](#_bookmark293)**)** | — | — | — | ANSC<1:0>**(**[**2**](#_bookmark293)**)** | | 0003 |
| 2DC0 | TRISC | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | TRISC<15:0>**(**[**3**](#_bookmark294)**)** | | | | | | | | | | | | | | | | FFFF |
| 2DD0 | PORTC | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | RC<15:0>**(**[**3**](#_bookmark294)**)** | | | | | | | | | | | | | | | | 0000 |
| 2DE0 | LATC | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | LATC<15:0>**(**[**3**](#_bookmark294)**)** | | | | | | | | | | | | | | | | 0000 |
| 2DF0 | ODCC | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ODCC<15:0>**(**[**3**](#_bookmark294)**)** | | | | | | | | | | | | | | | | 0000 |
| 2E00 | CNPUC | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNPUC<15:0>**(**[**3**](#_bookmark294)**)** | | | | | | | | | | | | | | | | 0000 |
| 2E10 | CNPDC | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNPDC<15:0>**(**[**3**](#_bookmark294)**)** | | | | | | | | | | | | | | | | 0000 |
| 2E20 | CNCONC | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON | — | — | — | CNSTYLE | PORT32 | — | — | — | — | — | — | — | — | — | — | 0000 |
| 2E30 | CNEN0C | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNIE0C<15:0>**(**[**3**](#_bookmark294)**)** | | | | | | | | | | | | | | | | 0000 |
| 2E40 | CNSTATC | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNSTATC<15:0>**(**[**3**](#_bookmark294)**)** | | | | | | | | | | | | | | | | 0000 |
| 2E50 | CNEN1C | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNIE1C<15:0>**(**[**3**](#_bookmark294)**)** | | | | | | | | | | | | | | | | 0000 |
| 2E60 | CNFC | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CNFC<15:0>**(**[**3**](#_bookmark294)**)** | | | | | | | | | | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

**2:** Bit<8> is not available on 28-pin devices; bit<5> is not available on 36 or 28-pin devices; bits<1:0> are not available on 28-pin devices.

**3:** Bits<15:13> and bits<11:10> are not available on 48-pin devices; bits<15:10> and bits<7:5> are not available on 36-pin devices; bits<15:10> and bits<8:0> are not available on 28-pin devices.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 123

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(2)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2EB0 | ANSELD | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 2EC0 | TRISD | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | TRISD<3:0>**(**[**1**](#_bookmark298)**)** | | | | 030F |
| 2ED0 | PORTD | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | RD<3:0>**(**[**1**](#_bookmark298)**)** | | | | 0000 |
| 2EE0 | LATD | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | LATD<3:0>**(**[**1**](#_bookmark298)**)** | | | | 0000 |
| 2EF0 | ODCD | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | ODCD<3:0>**(**[**1**](#_bookmark298)**)** | | | | 0000 |
| 2F00 | CNPUD | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | CNPUD<3:0>**(**[**1**](#_bookmark298)**)** | | | | 0000 |
| 2F10 | CNPDD | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | CNPDD<3:0>**(**[**1**](#_bookmark298)**)** | | | | 0000 |
| 2F20 | CNCOND | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON | — | — | — | CNSTYLE | PORT32 | — | — | — | — | — | — | — | — | — | — | 0000 |
| 2F30 | CNEN0D | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | CNIE0D<3:0>**(**[**1**](#_bookmark298)**)** | | | | 0000 |
| 2F40 | CNSTATD | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | CNSTATD<3:0>**(**[**1**](#_bookmark298)**)** | | | | 0000 |
| 2F50 | CNEN1D | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | CNIE1D<3:0>**(**[**1**](#_bookmark298)**)** | | | | 0000 |
| 2F60 | CNFD | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | CNFD<3:0>**(**[**1**](#_bookmark298)**)** | | | | 0000 |
| 2F70 | SR0D | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | SR0D<3:0>**(**[**1**](#_bookmark298)**)** | | | | 0000 |
| 2F80 | SR1D | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | SR1D<3:0>**(**[**1**](#_bookmark298)**)** | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** Bits<3:1> are not available on 48-pin devices; bits are not available on 36 and 28-pin devices.

**2:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 124

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2A00 | RPCON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | IOLOCK | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 2A20 | RPINR1 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 |  |  |  |  |  |  |  |  |  |  |  | INT4R<4:0> | | | | | 0000 |
| 2A30 | RPINR2 | 31:16 | — | — | — | ICM2R<4:0> | | | | | — | — | — | ICM1R<4:0> | | | | | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 2A40 | RPINR3 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | ICM3R<4:0> | | | | | 0000 |
| 2A60 | RPINR5 | 31:16 | — | — | — | OCFBR<4:0> | | | | | — | — | — | OCFAR<4:0> | | | | | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 2A70 | RPINR6 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | TCKIBR<4:0> | | | | | — | — | — | TCKIAR<4:0> | | | | | 0000 |
| 2A80 | RPINR7 | 31:16 | — | — | — | ICM8R<4:0> | | | | | — | — | — | ICM7R<4:0> | | | | | 0000 |
| 15:0 | — | — | — | ICM6R<4:0> | | | | | — | — | — | ICM5R<4:0> | | | | | 0000 |
| 2A90 | RPINR8 | 31:16 | — | — | — | U3RXR<4:0> | | | | | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | ICM9R<4:0> | | | | | 0000 |
| 2AA0 | RPINR9 | 31:16 | — | — | — | U2CTSR<4:0> | | | | | — | — | — | U2RXR<4:0> | | | | | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 2AB0 | RPINR10 | 31:16 | — | — | — | U3RTSR<4:0> | | | | | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 2AC0 | RPINR11 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | SS2INR<4:0> | | | | | 0000 |
| 15:0 | — | — | — | SCK2INR<4:0> | | | | | — | — | — | SDI2R<4:0> | | | | | 0000 |
| 2AD0 | RPINR12 | 31:16 | — | — | — | CLCINBR<4:0> | | | | | — | — | — | CLCINAR<4:0> | | | | | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 2B10 | RPOR0 | 31:16 | — | — | — | RP4R<4:0> | | | | | — | — | — | RP3R<4:0> | | | | | 0000 |
| 15:0 | — | — | — | RP2R<4:0> | | | | | — | — | — | RP1R<4:0> | | | | | 0000 |
| 2B20 | RPOR1 | 31:16 | — | — | — | RP8R<4:0> | | | | | — | — | — | RP7R<4:0> | | | | | 0000 |
| 15:0 | — | — | — | RP6R<4:0> | | | | | — | — | — | RP5R<4:0> | | | | | 0000 |
| 2B30 | RPOR2 | 31:16 | — | — | — | RP12R<4:0> | | | | | — | — | — | RP11R<4:0> | | | | | 0000 |
| 15:0 | — | — | — | RP10R<4:0> | | | | | — | — | — | RP9R<4:0> | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 125

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2B40 | RPOR3 | 31:16 | — | — | — | RP16R<4:0> | | | | | — | — | — | RP15R<4:0> | | | | | 0000 |
| 15:0 | — | — | — | RP14R<4:0> | | | | | — | — | — | RP13R<4:0> | | | | | 0000 |
| 2B50 | RPOR4 | 31:16 | — | — | — | RP20R<4:0> | | | | | — | — | — | RP19R<4:0> | | | | | 0000 |
| 15:0 | — | — | — | RP18R<4:0> | | | | | — | — | — | RP17R<4:0> | | | | | 0000 |
| 2B60 | RPOR5 | 31:16 | — | — | — | RP24R<4:0> | | | | | — | — | — | RP23R<4:0> | | | | | 0000 |
| 15:0 | — | — | — | RP22R<4:0> | | | | | — | — | — | — | — | — | — | — | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

**PIC32MM0256GPM064 FAMILY**

REGISTER 10-1: CNCONx: CHANGE NOTIFICATION CONTROL FOR PORTx REGISTER (x = A-D)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | U-0 | U-0 |
| ON | — | — | — | CNSTYLE | PORT32 | — | — |
| 7:0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’

bit 15 **ON:** Change Notification (CN) Control On bit

1 = CN is enabled

0 = CN is disabled

bit 14-12 **Unimplemented:** Read as ‘0’

bit 11 **CNSTYLE:** Change Notification Style Selection bit

1 = Edge style (detects edge transitions, CNFx bits are used for a Change Notice event)

0 = Mismatch style (detects change from last port read, CNSTATx bits are used for a Change Notification event) bit 10 **PORT32:** Merge Ports bit

Maps the next higher GPIO’s control and status registers to the upper half, bits<31:16>, of this port.

1 = Merging of this port and the next port is enabled

0 = Merging is disabled; all ports are accessed through their registers bit 9-0 **Unimplemented:** Read as ‘0’

DS60001387C-page 126  2016-2017 Microchip Technology Inc.

* 1. **TIMER****1** PIC32MM0256GPM064 family devices feature one synchronous/asynchronous 16-bit timer that can operate

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To complement the information in this data sheet, refer to **Section 14. “Timers”** (DS60001105) in the *“PIC32 Family Refer- ence Manual”*, which is available from the Microchip web site ([www.microchip.com/](http://www.microchip.com/PIC32) [PIC32](http://www.microchip.com/PIC32)). The information in this data sheet supersedes the information in the FRM.

as a free-running interval timer for various timing applications and counting external events. This timer can be clocked from different sources, such as the Peripheral Bus Clock (PBCLK), Secondary Oscillator (SOSC), T1CK pin or LPRC oscillator.

The following modes are supported by Timer1:

* + - Synchronous Internal Timer
    - Synchronous Internal Gated Timer
    - Synchronous External Timer
    - Asynchronous External Timer

The timer has a selectable clock prescaler and can operate in Sleep and Idle modes.

FIGURE 11-1: TIMER1 BLOCK DIAGRAM

Trigger to ADC

Equal

16-Bit Comparator

TSYNC

1 Sync

TMR1

Reset

0

0

T1IF

Event Flag

1

Q

Q

D

TGATE

TGATE

TCS

ON

SOSC T1CK

LPRC

00

x1

01

10

Gate Sync

10

Prescaler

1, 8, 64, 256

TECS<1:0>

PBCLK

00

2

TCKPS<1:0>



PR1

### Timer1 Control Register

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 128

TABLE 11-1: TIMER1 REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 8000 | T1CON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON | — | SIDL | TWDIS | TWIP | — | TECS<1:0> | | TGATE | — | TCKPS<1:0> | | — | TSYNC | TCS | — | 0000 |
| 8010 | TMR1 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | TMR1<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8020 | PR1 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | PR1<15:0>**(**[**2**](#_bookmark309)**)** | | | | | | | | | | | | | | | | FFFF |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual addresses, plus offsets of 0x4, 0x8 and 0xC, respectively.

**2:** PR1 values of ‘0’ and ‘1’ are reserved.

REGISTER 11-1: T1CON: TIMER1 CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | U-0 | R/W-0 | R/W-0 | R-0 | U-0 | R/W-0 | R/W-0 |
| ON | — | SIDL | TWDIS | TWIP | — | TECS<1:0> | |
| 7:0 | R/W-0 | U-0 | R/W-0 | R/W-0 | U-0 | R/W-0 | R/W-0 | U-0 |
| TGATE | — | TCKPS<1:0> | | — | TSYNC | TCS | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’ bit 15 **ON:** Timer1 On bit

1 = Timer1 is enabled

0 = Timer1 is disabled

bit 14 **Unimplemented:** Read as ‘0’

bit 13 **SIDL:** Timer1 Stop in Idle Mode bit

1 = Discontinues operation when device enters Idle mode

0 = Continues operation even in Idle mode

bit 12 **TWDIS:** Asynchronous Timer1 Write Disable bit

1 = Writes to TMR1 are ignored until pending write operation completes

0 = Back-to-back writes are enabled (Legacy Asynchronous Timer mode functionality) bit 11 **TWIP:** Asynchronous Timer1 Write in Progress bit

In Asynchronous Timer1 mode:

1 = Asynchronous write to TMR1 register is in progress 0 = Asynchronous write to TMR1 register is complete In Synchronous Timer1 mode:

This bit is read as ‘0’.

bit 10 **Unimplemented:** Read as ‘0’

bit 9-8 **TECS<1:0>:** Timer1 External Clock Selection bits

11 = Reserved

10 = External clock comes from the LPRC

01 = External clock comes from the T1CK Pin

00 = External clock comes from the Secondary Oscillator (SOSC) bit 7 **TGATE:** Timer1 Gated Time Accumulation Enable bit

When TCS = 1:

This bit is ignored. When TCS = 0:

1 = Gated time accumulation is enabled

0 = Gated time accumulation is disabled bit 6 **Unimplemented:** Read as ‘0’

bit 5-4 **TCKPS<1:0>:** Timer1 Input Clock Prescale Select bits

11 = 1:256 prescale value

10 = 1:64 prescale value

01 = 1:8 prescale value

00 = 1:1 prescale value

**PIC32MM0256GPM064 FAMILY**

REGISTER 11-1: T1CON: TIMER1 CONTROL REGISTER (CONTINUED)

bit 3 **Unimplemented:** Read as ‘0’

bit 2 **TSYNC:** Timer1 External Clock Input Synchronization Selection bit When TCS = 1:

1 = External clock input is synchronized

0 = External clock input is not synchronized When TCS = 0:

This bit is ignored.

bit 1 **TCS:** Timer1 Clock Source Select bit

1 = External clock is defined by the TECS<1:0> bits

0 = Internal peripheral clock bit 0 **Unimplemented:** Read as ‘0’

**PIC32MM0256GPM064 FAMILY**

# TIMER2 AND TIMER3

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To complement the information in this data sheet, refer to **Section 14. “Timers”** (DS60001105) in the *“PIC32 Family Refer- ence Manual”*, which is available from the Microchip web site ([www.microchip.com/](http://www.microchip.com/PIC32) [PIC32](http://www.microchip.com/PIC32)). The information in this data sheet supersedes the information in the FRM.

This family of PIC32 devices features four synchronous 16-bit timers (default) that can operate as a free- running interval timer for various timing applications and counting external events. The following modes are supported:

* + - * + Synchronous Internal 16-Bit Timer
        + Synchronous Internal 16-Bit Gated Timer
        + Synchronous External 16-Bit Timer

A single 32-bit synchronous timer is available by combining Timer2 with Timer3. The resulting 32-bit timer can operate in three modes:

* + - * + Synchronous Internal 32-Bit Timer
        + Synchronous Internal 32-Bit Gated Timer
        + Synchronous External 32-Bit

### Additional Supported Features

* + - * + Selectable Clock Prescaler
        + Timers Operational during CPU Idle
        + ADC Event Trigger (only Timer3)
        + Fast Bit Manipulation using CLR, SET and INV Registers

FIGURE 12-1: TIMER2 AND TIMER3 BLOCK DIAGRAM (TYPE A, 16-BIT)



PRx

TMRx

Sync

ADC Event Trigger**(1)**

Comparator x 16

Equal

Reset

TxIF

Event Flag

0

1

Q

Q

D

TGATE (TxCON<7>)

TGATE (TxCON<7>)

TCS (TxCON<1>)

ON (TxCON<15>)

TxCK

x 1

Gate

Sync

1 0

Prescaler 1, 2, 4, 8, 16,

32, 64, 256

PBCLK

0 0

3

TCKPS (TxCON<6:4>)

**Note 1:** ADC Event Trigger is only available on Timer3.

FIGURE 12-2: TIMER2/3 BLOCK DIAGRAM (TYPE B, 32-BIT)

Data Bus<31:0>

<31:0>

Reset

TMRy

(Timer3 Only)

Most Significant Half-Word

TMRx

Least Significant Half-Word

Sync

ADC Event Trigger

Equal

Comparator x 32

TyIF Event 0

Flag

1

Q

Q

D

TGATE (TxCON<7>)

TGATE (TxCON<7>)

TCS (TxCON<1>)

(Type B Timers Only)

ON (TxCON<15>)

TxCK

x 1

Gate

Sync

1 0

Prescaler 1, 2, 4, 8, 16,

32, 64, 256

TPBCLK

0 0

3

TCKPS (TxCON<6:4>)

**Note:** The timer configuration bit, T32 (T2CON<3>), must be set to ‘1’ for a 32-bit timer/counter operation. All control bits are respective to the T2CON register and interrupt bits are respective to the T3CON register.



PRy PRx

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 133

### Timer2/3 Control Registers

TABLE 12-1: TIMER2/3 REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 8040 | T2CON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON | — | SIDL | — | — | — | — | — | TGATE | TCKPS<2:0> | | | T32 | — | TCS | — | 0000 |
| 8050 | TMR2 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | TMR2<15:0> | | | | | | | | | | | | | | | | 0000 |
| 8060 | PR2 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | PR2<15:0>**(**[**2**](#_bookmark317)**)** | | | | | | | | | | | | | | | | FFFF |
| 8080 | T3CON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON | — | SIDL | — | — | — | — | — | TGATE | TCKPS<2:0> | | | — | — | TCS | — | 0000 |
| 8090 | TMR3 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | TMR3<15:0> | | | | | | | | | | | | | | | | 0000 |
| 80A0 | PR3 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | PR3<15:0>**(**[**2**](#_bookmark317)**)** | | | | | | | | | | | | | | | | FFFF |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual addresses, plus offsets of 0x4, 0x8 and 0xC, respectively.

**2:** PR2 and PR3 values of ‘0’ and ‘1’ are reserved.

### Control Register

REGISTER 12-1: T2CON: TIMER2 CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | U-0 | R/W-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| ON**(**[**1**](#_bookmark320)**,**[**3**](#_bookmark322)**)** | — | SIDL**(**[**4**](#_bookmark323)**)** | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | R/W-0 | U-0 |
| TGATE**(**[**3**](#_bookmark322)**)** | TCKPS<2:0>**(**[**3**](#_bookmark322)**)** | | | T32**(**[**2**](#_bookmark321)**)** | — | TCS**(**[**3**](#_bookmark322)**)** | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’ bit 15 **ON:** Timer2 On bit**(**[**1**](#_bookmark320)**,**[**3**](#_bookmark322)**)**

1 = Module is enabled

0 = Module is disabled

bit 14 **Unimplemented:** Read as ‘0’

bit 13 **SIDL:** Timer2 Stop in Idle Mode bit**(**[**4**](#_bookmark323)**)**

1 = Discontinues operation when device enters Idle mode

0 = Continues operation when device is in Idle mode bit 12-8 **Unimplemented:** Read as ‘0’

bit 7 **TGATE:** Timer Gated Time Accumulation Enable bit**(**[**3**](#_bookmark322)**)**

When TCS = 1:

This bit is ignored and is read as ‘0’. When TCS = 0:

1 = Gated time accumulation is enabled

0 = Gated time accumulation is disabled

bit 6-4 **TCKPS<2:0>:** Timer Input Clock Prescale Select bits**(**[**3**](#_bookmark322)**)**

111 = 1:256 prescale value

110 = 1:64 prescale value

101 = 1:32 prescale value

100 = 1:16 prescale value

011 = 1:8 prescale value

010 = 1:4 prescale value

001 = 1:2 prescale value

000 = 1:1 prescale value

**Note 1:** The user’s software should not read/write the peripheral SFRs in the SYSCLK cycle immediately following the instruction that clears the module’s ON bit.

**2:** This bit is only available on even numbered timers (Timer2).

**3:** While operating in 32-bit mode, this bit has no effect for odd numbered timers (Timer1). All timer functions are set through the even numbered timers.

**4:** While operating in 32-bit mode, this bit must be cleared on odd numbered timers to enable the 32-bit timer in Idle mode.

**PIC32MM0256GPM064 FAMILY**

REGISTER 12-1: T2CON: TIMER2 CONTROL REGISTER (CONTINUED)

bit 3 **T32:** 32-Bit Timer Mode Select bit**(**[**2**](#_bookmark321)**)**

1 = Odd numbered and even numbered timers form a 32-bit timer

0 = Odd numbered and even numbered timers form a separate 16-bit timer bit 2 **Unimplemented:** Read as ‘0’

bit 1 **TCS:** Timer Clock Source Select bit**(**[**3**](#_bookmark322)**)**

1 = External clock from T2CK pin

0 = Internal peripheral clock bit 0 **Unimplemented:** Read as ‘0’

**Note 1:** The user’s software should not read/write the peripheral SFRs in the SYSCLK cycle immediately following the instruction that clears the module’s ON bit.

**2:** This bit is only available on even numbered timers (Timer2).

**3:** While operating in 32-bit mode, this bit has no effect for odd numbered timers (Timer1). All timer functions are set through the even numbered timers.

**4:** While operating in 32-bit mode, this bit must be cleared on odd numbered timers to enable the 32-bit timer in Idle mode.

REGISTER 12-2: T3CON: TIMER3 CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | U-0 | R/W-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| ON | — | SIDL | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | U-0 | R/W-0 | U-0 |
| TGATE | TCKPS<2:0> | | | — | — | TCS | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’ bit 15 **ON:** Timer3 On bit

1 = Timer3 is enabled

0 = Timer3 is disabled

bit 14 **Unimplemented:** Read as ‘0’

bit 13 **SIDL:** Timer3 Stop in Idle Mode bit

1 = Discontinues operation when device enters Idle mode

0 = Continues operation even in Idle mode bit 12-8 **Unimplemented:** Read as ‘0’

bit 7 **TGATE:** Timer3 Gated Time Accumulation Enable bit

When TCS = 1:

This bit is ignored. When TCS = 0:

1 = Gated time accumulation is enabled

0 = Gated time accumulation is disabled

bit 6-4 **TCKPS<2:0>:** Timer3 Input Clock Prescale Select bits

111 = 1:256 prescale value

110 = 1:64 prescale value

101 = 1:32 prescale value

100 = 1:16 prescale value

011 = 1:8 prescale value

010 = 1:4 prescale value

001 = 1:2 prescale value

000 = 1:1 prescale value

bit 3-2 **Unimplemented:** Read as ‘0’

bit 1 **TCS:** Timer3 Clock Source Select bit

1 = External clock is from the T3CK pin

0 = Internal peripheral clock bit 0 **Unimplemented:** Read as ‘0’



* 1. **WATCHDOG** **TIMER (WDT)** When enabled, the Watchdog Timer (WDT) can be

used to detect system software malfunctions by

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To com- plement the information in this data sheet, refer to **Section 62. “Dual Watchdog Timer”** (DS60001365) in the *“PIC32 Family Reference Manual”*, which [is](http://www.microchip.com/PIC32) [available from the Microchip web site](http://www.microchip.com/PIC32) [(](http://www.microchip.com/PIC32)[www.microchip.com/PIC32).](http://www.microchip.com/PIC32)) The informa- tion in this data sheet supersedes the information in the FRM.

resetting the device if the WDT is not cleared periodically in software. Various WDT time-out periods can be selected using the WDT postscaler. The WDT can also be used to wake the device from Sleep or Idle mode.

Some of the key features of the WDT module are:

* + - Configuration or Software Controlled
    - User-Configurable Time-out Period
    - Different Time-out Periods for Run and Sleep/Idle modes
    - Operates from LPRC Oscillator in Sleep/Idle modes
    - Different Clock Sources for Run mode
    - Can Wake the Device from Sleep or Idle

FIGURE 13-1: WATCHDOG TIMER BLOCK DIAGRAM



Comparator

Comparator

Power Save Mode WDT

LPRC Oscillator

Power Save

25-Bit Counter

Wake-up and NMI

CLKSEL<1:0>

ON

Power Save

Reset

SLPDIV<4:0>

SYSCLK

Run Mode WDT

00

Reserved

FRC Oscillator

01

Power Save

25-Bit Counter

NMI and Start NMI Counter

10

LPRC Oscillator

11

Reset

RUNDIV<4:0>

WDTCLRKEY<15:0> = 5743h

ON

All Resets Any System Clock Switch

### Watchdog Timer Control Registers

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 138

TABLE 13-1: WATCHDOG TIMER REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 3990 | WDTCON**(**[**1**](#_bookmark329)**)** | 31:16 | WDTCLRKEY<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | ON | — | — | RUNDIV<4:0> | | | | | CLKSEL<1:0> | | SLPDIV<4:0> | | | | | WDTWINEN | xxxx |

**Legend:** x = unknown value on Reset; — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** This register has corresponding CLR, SET and INV registers at its virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

REGISTER 13-1: WDTCON: WATCHDOG TIMER CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 |
| WDTCLRKEY<15:8> | | | | | | | |
| 23:16 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 |
| WDTCLRKEY<7:0> | | | | | | | |
| 15:8 | R/W-0 | U-0 | U-0 | R-y | R-y | R-y | R-y | R-y |
| ON**(**[**1**](#_bookmark332)**)** | — | — | RUNDIV<4:0> | | | | |
| 7:0 | R-y | R-y | R-y | R-y | R-y | R-y | R-y | R/W-y |
| CLKSEL<1:0> | | SLPDIV<4:0> | | | | | WDTWINEN |

**Legend:**

R = Readable bit

-n = Value at POR

y = Values set from Configuration bits on Reset

W = Writable bit

‘1’ = Bit is set

U = Unimplemented bit, read as ‘0’

‘0’ = Bit is cleared

x = Bit is unknown

bit 31-16 **WDTCLRKEY<15:0>:** Watchdog Timer Clear Key bits

To clear the Watchdog Timer to prevent a time-out, software must write the value, 0x5743, to the upper 16 bits of this register address using a single 16-bit write.

bit 15 **ON:** Watchdog Timer Enable bit**(**[**1**](#_bookmark332)**)**

1 = The WDT is enabled

0 = The WDT is disabled

bit 14-13 **Unimplemented:** Read as ‘0’

bit 12-8 **RUNDIV<4:0>:** Shadow Copy of Watchdog Timer Postscaler Value for Run Mode from Configuration bits On Reset, these bits are set to the values of the RWDTPS<4:0> Configuration bits in FWDT.

bit 7-6 **CLKSEL<1:0>:** Shadow Copy of Watchdog Timer Clock Selection Value for Run Mode from Configuration bits On Reset, these bits are set to the values of the RCLKSEL<1:0> Configuration bits in FWDT.

bit 5-1 **SLPDIV<4:0>:** Shadow Copy of Watchdog Timer Postscaler Value for Sleep/Idle Mode from Configuration bits On Reset, these bits are set to the values of the SWDTPS<4:0> Configuration bits in FWDT.

bit 0 **WDTWINEN:** Watchdog Timer Window Enable bit

On Reset, this bit is set to the inverse of the value of the WINDIS Configuration bit in FWDT.

1 = Windowed mode is enabled

0 = Windowed mode is disabled

**Note 1:** This bit only has control when FWDTEN (FWDT<15>) = 0.

NOTES:

# CAPTURE/COMPARE/PWM/ TIMER MODULES (MCCP AND SCCP)

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a compre- hensive reference source. To complement the information in this data sheet, refer to **Section 30. “Capture/Compare/PWM/ Timer (MCCP and SCCP)”** (DS60001381)

in the *“PIC32 Family Reference Manual”*, which [is available from the Microchip](http://www.microchip.com/PIC32) [web site (](http://www.microchip.com/PIC32)[www.microchip.com/PIC32).](http://www.microchip.com/PIC32)) The information in this data sheet supersedes the information in the FRM.

### Introduction

PIC32MM0256GPM064 family devices include nine Capture/Compare/PWM/Timer (CCP) modules. These modules are similar to the multipurpose timer modules found on many other 32-bit microcontrollers. They also provide the functionality of the comparable input capture, output compare and general purpose timer peripherals found in all earlier PIC32 devices.

CCP modules can operate in one of three major modes:

* + - * + General Purpose Timer
        + Input Capture
        + Output Compare/PWM

There are two different forms of the module, distinguished by the number of PWM outputs that the module can gen- erate. Single Capture/Compare/PWM/Timer (SCCPs) output modules provide only one PWM output. Multiple Capture/Compare/PWM/Timer (MCCPs) output modules can provide up to six outputs and an extended range of output control features, depending on the pin count of the particular device.

All modules (SCCP and MCCP) include these features:

* + - * + User-Selectable Clock Inputs, including System Clock and External Clock Input Pins
        + Input Clock Prescaler for Time Base
        + Output Postscaler for module Interrupt Events or Triggers
        + Synchronization Output Signal for coordinating other MCCP/SCCP modules with

User-Configurable Alternate and Auxiliary Source Options

* + - * + Fully Asynchronous Operation in all modes and in Low-Power Operation
        + Special Output Trigger for ADC Conversions
        + 16-Bit and 32-Bit General Purpose Timer modes with Optional Gated Operation for Simple Time Measurements
        + Capture modes:

Backward compatible with previous input capture peripherals of the PIC32 family

16-bit or 32-bit capture of time base on external event

Up to four-level deep FIFO capture buffer

Capture source input multiplexer

Gated capture operation to reduce noise-induced false captures

* + - * + Output Compare/PWM modes:

Backward compatible with previous output compare peripherals of the PIC32 family

Single Edge and Dual Edge Compare modes

Center-Aligned Compare mode

Variable Frequency Pulse mode

External Input mode

MCCP modules also include these extended PWM features:

* + - * + Single Output Steerable mode
        + Brush DC Motor (Forward and Reverse) modes
        + Half-Bridge with Dead-Time Delay mode
        + Push-Pull PWM mode
        + Output Scan mode
        + Auto-Shutdown with Programmable Source and Shutdown State
        + Programmable Output Polarity

The SCCP and MCCP modules can be operated in only one of the three major modes (Capture, Compare or Timer) at any time. The other modes are not available unless the module is reconfigured.

A conceptual block diagram for the module is shown in [Figure 14-1](#_bookmark335). All three modes use the time base gener- ator and the common Timer register pair (CCPxTMR). Other shared hardware components, such as comparators and buffer registers, are activated and used as a particular mode requires.

FIGURE 14-1: MCCP/SCCP CONCEPTUAL BLOCK DIAGRAM

CCPxIF

CCTxIF

External Capture

Input

CCP Sync Out

Special Event Trigger Out (ADC) Auxiliary Output

Clock Sources

CCPxTMR

T32

CCSEL MOD<3:0>

Compare/PWM Output(s)

Output Compare/

Sync and Gating Sources

PWM

OCFA/OCFB



Input Capture

### Registers



16/32-Bit Timer

Time Base Generator

Each MCCP/SCCP module has up to seven control and status registers:

* CCPxCON1 ([Register 14-1](#_bookmark340)) controls many of the features common to all modes, including input clock selection, time base prescaling, timer synchronization, Trigger mode operations and postscaler selection for all modes. The module is also enabled and the operational mode is selected from this register.
* CCPxCON2 ([Register 14-2](#_bookmark346)) controls auto- shutdown and restart operation, primarily for PWM operations, and also configures other input capture and output compare features, and configures auxiliary output operation.
* CCPxCON3 ([Register 14-3](#_bookmark350)) controls multiple output PWM dead time, controls the output of the output compare and PWM modes, and configures the PWM Output mode for the MCCP modules.
* CCPxSTAT ([Register 14-4](#_bookmark353)) contains read-only status bits showing the state of module operations.

Each module also includes eight buffer/counter registers that serve as Timer Value registers or data holding buffers:

* CCPxTMR is the 32-Bit Timer/Counter register
* CCPxPR is the 32-Bit Timer Period register
* CCPxR is the 32-bit primary data buffer for output compare operations
* CCPxBUF(H/L) is the 32-Bit Buffer register pair, which is used in input capture FIFO operations

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 143

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 0100 | CCP1CON1 | 31:16 | OPSSRC | RTRGEN | — | — | OPS<3:0> | | | | TRIGEN | ONESHOT | ALTSYNC | SYNC<4:0> | | | | | 0000 |
| 15:0 | ON | — | SIDL | CCPSLP | TMRSYNC | CLKSEL<2:0> | | | TMRPS<1:0> | | T32 | CCSEL | MOD<3:0> | | | | 0000 |
| 0110 | CCP1CON2 | 31:16 | OENSYNC | — | OCFEN | OCEEN | OCDEN | OCCEN | OCBEN | OCAEN | ICGSM<1:0> | | — | AUXOUT<1:0> | | ICS<2:0> | | | 0100 |
| 15:0 | PWMRSEN | ASDGM | — | SSDG | — | — | — | — | ASDG<7:0> | | | | | | | | 0000 |
| 0120 | CCP1CON3 | 31:16 | OETRIG | OSCNT<2:0> | | | — | OUTM<2:0> | | | — | — | POLACE | POLBDF | PSSACE<1:0> | | PSSBDF<1:0> | | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | DT<5:0> | | | | | | 0000 |
| 0130 | CCP1STAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | PRLWIP | TMRHWIP | TMRLWIP | RBWIP | RAWIP | 0000 |
| 15:0 | — | — | — | — | — | ICGARM | — | — | CCPTRIG | TRSET | TRCLR | ASEVT | SCEVT | ICDIS | ICOV | ICBNE | 0000 |
| 0140 | CCP1TMR | 31:16 | TMRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | TMRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0150 | CCP1PR | 31:16 | PRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | PRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0160 | CCP1RA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPA<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0170 | CCP1RB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0180 | CCP1BUF | 31:16 | BUFH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | BUFL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0200 | CCP2CON1 | 31:16 | OPSSRC | RTRGEN | — | — | OPS<3:0> | | | | TRIGEN | ONESHOT | ALTSYNC | SYNC<4:0> | | | | | 0000 |
| 15:0 | ON | — | SIDL | CCPSLP | TMRSYNC | CLKSEL<2:0> | | | TMRPS<1:0> | | T32 | CCSEL | MOD<3:0> | | | | 0000 |
| 0210 | CCP2CON2 | 31:16 | OENSYNC | — | OCFEN | OCEEN | OCDEN | OCCEN | OCBEN | OCAEN | ICGSM<1:0> | | — | AUXOUT<1:0> | | ICS<2:0> | | | 0100 |
| 15:0 | PWMRSEN | ASDGM | — | SSDG | — | — | — | — | ASDG<7:0> | | | | | | | | 0000 |
| 0220 | CCP2CON3 | 31:16 | OETRIG | OSCNT<2:0> | | | — | OUTM<2:0> | | | — | — | POLACE | POLBDF | PSSACE<1:0> | | PSSBDF<1:0> | | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | DT<5:0> | | | | | | 0000 |
| 0230 | CCP2STAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | PRLWIP | TMRHWIP | TMRLWIP | RBWIP | RAWIP | 0000 |
| 15:0 | — | — | — | — | — | ICGARM | — | — | CCPTRIG | TRSET | TRCLR | ASEVT | SCEVT | ICDIS | ICOV | ICBNE | 0000 |
| 0240 | CCP2TMR | 31:16 | TMRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | TMRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0250 | CCP2PR | 31:16 | PRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | PRL<15:0> | | | | | | | | | | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 144

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 0260 | CCP2RA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPA<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0270 | CCP2RB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0280 | CCP2BUF | 31:16 | BUFH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | BUFL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0300 | CCP3CON1 | 31:16 | OPSSRC | RTRGEN | — | — | OPS<3:0> | | | | TRIGEN | ONESHOT | ALTSYNC | SYNC<4:0> | | | | | 0000 |
| 15:0 | ON | — | SIDL | CCPSLP | TMRSYNC | CLKSEL<2:0> | | | TMRPS<1:0> | | T32 | CCSEL | MOD<3:0> | | | | 0000 |
| 0310 | CCP3CON2 | 31:16 | OENSYNC | — | OCFEN | OCEEN | OCDEN | OCCEN | OCBEN | OCAEN | ICGSM<1:0> | | — | AUXOUT<1:0> | | ICS<2:0> | | | 0100 |
| 15:0 | PWMRSEN | ASDGM | — | SSDG | — | — | — | — | ASDG<7:0> | | | | | | | | 0000 |
| 0320 | CCP3CON3 | 31:16 | OETRIG | OSCNT<2:0> | | | — | OUTM<2:0> | | | — | — | POLACE | POLBDF | PSSACE<1:0> | | PSSBDF<1:0> | | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | DT<5:0> | | | | | | 0000 |
| 0330 | CCP3STAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | PRLWIP | TMRHWIP | TMRLWIP | RBWIP | RAWIP | 0000 |
| 15:0 | — | — | — | — | — | ICGARM | — | — | CCPTRIG | TRSET | TRCLR | ASEVT | SCEVT | ICDIS | ICOV | ICBNE | 0000 |
| 0340 | CCP3TMR | 31:16 | TMRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | TMRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0350 | CCP3PR | 31:16 | PRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | PRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0360 | CCP3RA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPA<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0370 | CCP3RB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0380 | CCP3BUF | 31:16 | BUFH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | BUFL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0400 | CCP4CON1 | 31:16 | OPSSRC | RTRGEN | — | — | OPS<3:0> | | | | TRIGEN | ONESHOT | ALTSYNC | SYNC | | | | | 0000 |
| 15:0 | ON | — | SIDL | CCPSLP | TMRSYNC | CLKSEL<2:0> | | | TMRPS<1:0> | | T32 | CCSEL | MOD<3:0> | | | | 0000 |
| 0410 | CCP4CON2 | 31:16 | OENSYNC | — | — | — | — | — | — | OCAEN | ICGSM<1:0> | | — | AUXOUT<1:0> | | ICS<2:0> | | | 0100 |
| 15:0 | PWMRSEN | ASDGM | — | SSDG | — | — | — | — | ASDG<7:0> | | | | | | | | 0000 |
| 0420 | CCP4CON3 | 31:16 | OETRIG | OSCNT<2:0> | | | — | — | — | — | — | — | POLACE | — | PSSACE<1:0> | | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 145

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 0430 | CCP4STAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | PRLWIP | TMRHWIP | TMRLWIP | RBWIP | RAWIP | 0000 |
| 15:0 | — | — | — | — | — | ICGARM | — | — | CCPTRIG | TRSET | TRCLR | ASEVT | SCEVT | ICDIS | ICOV | ICBNE | 0000 |
| 0440 | CCP4TMR | 31:16 | TMRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | TMRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0450 | CCP4PR | 31:16 | PRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | PRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0460 | CCP4RA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPA<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0470 | CCP4RB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0480 | CCP4BUF | 31:16 | BUFH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | BUFL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0500 | CCP5CON1 | 31:16 | OPSSRC | RTRGEN | — | — | OPS<3:0> | | | | TRIGEN | ONESHOT | ALTSYNC | SYNC<4:0> | | | | | 0000 |
| 15:0 | ON | — | SIDL | CCPSLP | TMRSYNC | CLKSEL<2:0> | | | TMRPS<1:0> | | T32 | CCSEL | MOD<3:0> | | | | 0000 |
| 0510 | CCP5CON2 | 31:16 | OENSYNC | — | OCFEN | OCEEN | OCDEN | OCCEN | OCBEN | OCAEN | ICGSM<1:0> | | — | AUXOUT<1:0> | | ICS<2:0> | | | 0100 |
| 15:0 | PWMRSEN | ASDGM | — | SSDG | — | — | — | — | ASDG<7:0> | | | | | | | | 0000 |
| 0520 | CCP5CON3 | 31:16 | OETRIG | OSCNT<2:0> | | | — | — | — | — | — | — | POLACE | — | PSSACE<1:0> | | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 0530 | CCP5STAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | PRLWIP | TMRHWIP | TMRLWIP | RBWIP | RAWIP | 0000 |
| 15:0 | — | — | — | — | — | ICGARM | — | — | CCPTRIG | TRSET | TRCLR | ASEVT | SCEVT | ICDIS | ICOV | ICBNE | 0000 |
| 0540 | CCP5TMR | 31:16 | TMRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | TMRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0550 | CCP5PR | 31:16 | PRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | PRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0560 | CCP5RA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPA<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0570 | CCP5RB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0580 | CCP5BUF | 31:16 | BUFH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | BUFL<15:0> | | | | | | | | | | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 146

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 0600 | CCP6CON1 | 31:16 | OPSSRC | RTRGEN | — | — | OPS<3:0> | | | | TRIGEN | ONESHOT | ALTSYNC | SYNC<4:0> | | | | | 0000 |
| 15:0 | ON | — | SIDL | CCPSLP | TMRSYNC | CLKSEL<2:0> | | | TMRPS<1:0> | | T32 | CCSEL | MOD<3:0> | | | | 0000 |
| 0610 | CCP6CON2 | 31:16 | OENSYNC | — | OCFEN | OCEEN | OCDEN | OCCEN | OCBEN | OCAEN | ICGSM<1:0> | | — | AUXOUT<1:0> | | ICS<2:0> | | | 0100 |
| 15:0 | PWMRSEN | ASDGM | — | SSDG | — | — | — | — | ASDG<7:0> | | | | | | | | 0000 |
| 0620 | CCP6CON3 | 31:16 | OETRIG | OSCNT<2:0> | | | — | — | — | — | — | — | POLACE | — | PSSACE<1:0> | | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 0630 | CCP6STAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | PRLWIP | TMRHWIP | TMRLWIP | RBWIP | RAWIP | 0000 |
| 15:0 | — | — | — | — | — | ICGARM | — | — | CCPTRIG | TRSET | TRCLR | ASEVT | SCEVT | ICDIS | ICOV | ICBNE | 0000 |
| 0640 | CCP6TMR | 31:16 | TMRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | TMRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0650 | CCP6PR | 31:16 | PRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | PRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0660 | CCP6RA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPA<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0670 | CCP6RB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0680 | CCP6BUF | 31:16 | BUFH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | BUFL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0700 | CCP7CON1 | 31:16 | OPSSRC | RTRGEN | — | — | OPS<3:0> | | | | TRIGEN | ONESHOT | ALTSYNC | SYNC<4:0> | | | | | 0000 |
| 15:0 | ON | — | SIDL | CCPSLP | TMRSYNC | CLKSEL<2:0> | | | TMRPS<1:0> | | T32 | CCSEL | MOD<3:0> | | | | 0000 |
| 0710 | CCP7CON2 | 31:16 | OENSYNC | — | OCFEN | OCEEN | OCDEN | OCCEN | OCBEN | OCAEN | ICGSM<1:0> | | — | AUXOUT<1:0> | | ICS<2:0> | | | 0100 |
| 15:0 | PWMRSEN | ASDGM | — | SSDG | — | — | — | — | ASDG<7:0> | | | | | | | | 0000 |
| 0720 | CCP7CON3 | 31:16 | OETRIG | OSCNT<2:0> | | | — | — | — | — | — | — | POLACE | — | PSSACE<1:0> | | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 0730 | CCP7STAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | PRLWIP | TMRHWIP | TMRLWIP | RBWIP | RAWIP | 0000 |
| 15:0 | — | — | — | — | — | ICGARM | — | — | CCPTRIG | TRSET | TRCLR | ASEVT | SCEVT | ICDIS | ICOV | ICBNE | 0000 |
| 0740 | CCP7TMR | 31:16 | TMRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | TMRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0750 | CCP7PR | 31:16 | PRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | PRL<15:0> | | | | | | | | | | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 147

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 0760 | CCP7RA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPA<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0770 | CCP7RB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0780 | CCP7BUF | 31:16 | BUFH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | BUFL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0800 | CCP8CON1 | 31:16 | OPSSRC | RTRGEN | — | — | OPS<3:0> | | | | TRIGEN | ONESHOT | ALTSYNC | SYNC<4:0> | | | | | 0000 |
| 15:0 | ON | — | SIDL | CCPSLP | TMRSYNC | CLKSEL<2:0> | | | TMRPS<1:0> | | T32 | CCSEL | MOD<3:0> | | | | 0000 |
| 0810 | CCP8CON2 | 31:16 | OENSYNC | — | OCFEN | OCEEN | OCDEN | OCCEN | OCBEN | OCAEN | ICGSM<1:0> | | — | AUXOUT<1:0> | | ICS<2:0> | | | 0100 |
| 15:0 | PWMRSEN | ASDGM | — | SSDG | — | — | — | — | ASDG<7:0> | | | | | | | | 0000 |
| 0820 | CCP8CON3 | 31:16 | OETRIG | OSCNT<2:0> | | | — | — | — | — | — | — | POLACE | — | PSSACE<1:0> | | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 0830 | CCP8STAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | PRLWIP | TMRHWIP | TMRLWIP | RBWIP | RAWIP | 0000 |
| 15:0 | — | — | — | — | — | ICGARM | — | — | CCPTRIG | TRSET | TRCLR | ASEVT | SCEVT | ICDIS | ICOV | ICBNE | 0000 |
| 0840 | CCP8TMR | 31:16 | TMRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | TMRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0850 | CCP8PR | 31:16 | PRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | PRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0860 | CCP8RA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPA<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0870 | CCP8RB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0880 | CCP8BUF | 31:16 | BUFH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | BUFL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0900 | CCP9CON1 | 31:16 | OPSSRC | RTRGEN | — | — | OPS<3:0> | | | | TRIGEN | ONESHOT | ALTSYNC | SYNC<4:0> | | | | | 0000 |
| 15:0 | ON | — | SIDL | CCPSLP | TMRSYNC | CLKSEL<2:0> | | | TMRPS<1:0> | | T32 | CCSEL | MOD<3:0> | | | | 0000 |
| 0910 | CCP9CON2 | 31:16 | OENSYNC | — | OCFEN | OCEEN | OCDEN | OCCEN | OCBEN | OCAEN | ICGSM<1:0> | | — | AUXOUT<1:0> | | ICS<2:0> | | | 0100 |
| 15:0 | PWMRSEN | ASDGM | — | SSDG | — | — | — | — | ASDG<7:0> | | | | | | | | 0000 |
| 0920 | CCP9CON3 | 31:16 | OETRIG | OSCNT<2:0> | | | — | — | — | — | — | — | POLACE | — | PSSACE<1:0> | | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 148

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 0930 | CCP9STAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | PRLWIP | TMRHWIP | TMRLWIP | RBWIP | RAWIP | 0000 |
| 15:0 | — | — | — | — | — | ICGARM | — | — | CCPTRIG | TRSET | TRCLR | ASEVT | SCEVT | ICDIS | ICOV | ICBNE | 0000 |
| 0940 | CCP9TMR | 31:16 | TMRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | TMRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0950 | CCP9PR | 31:16 | PRH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | PRL<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0960 | CCP9RA | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPA<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0970 | CCP9RB | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | CMPB<15:0> | | | | | | | | | | | | | | | | 0000 |
| 0980 | CCP9BUF | 31:16 | BUFH<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | BUFL<15:0> | | | | | | | | | | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

REGISTER 14-1: CCPxCON1: CAPTURE/COMPARE/PWMx CONTROL 1 REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| OPSSRC**(**[**1**](#_bookmark343)**)** | RTRGEN**(**[**2**](#_bookmark344)**)** | — | — | OPS<3:0>**(**[**3**](#_bookmark345)**)** | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| TRIGEN | ONESHOT | ALTSYNC | SYNC<4:0> | | | | |
| 15:8 | R/W-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| ON**(**[**1**](#_bookmark343)**)** | — | SIDL | CCPSLP | TMRSYNC | CLKSEL<2:0> | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| TMRPS<1:0> | | T32 | CCSEL | MOD<3:0> | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **OPSSRC:** Output Postscaler Source Select bit**(**[**1**](#_bookmark343)**)**

1 = Output postscaler scales the Special Event Trigger output events

0 = Output postscaler scales the timer interrupt events bit 30 **RTRGEN:** Retrigger Enable bit**(**[**2**](#_bookmark344)**)**

1 = Time base can be retriggered when CCPTRIG = 1

0 = Time base may not be retriggered when CCPTRIG = 1

bit 29-28 **Unimplemented:** Read as ‘0’

bit 27-24 **OPS<3:0>:** CCPx Interrupt Output Postscale Select bits**(**[**3**](#_bookmark345)**)**

1111 = Interrupt every 16th time base period match

1110 = Interrupt every 15th time base period match

**. . .**

0100 = Interrupt every 5th time base period match

0011 = Interrupt every 4th time base period match or 4th input capture event 0010 = Interrupt every 3rd time base period match or 3rd input capture event 0001 = Interrupt every 2nd time base period match or 2nd input capture event 0000 = Interrupt after each time base period match or input capture event

bit 23 **TRIGEN:** CCPx Triggered Enable bit

1 = Triggered operation of the timer is enabled

0 = Triggered operation of the timer is disabled bit 22 **ONESHOT:** One-Shot Mode Enable bit

1 = One-Shot Triggered mode is enabled; trigger duration is set by OSCNT<2:0>

0 = One-Shot Triggered mode is disabled bit 21 **ALTSYNC:** CCPx Clock Select bit

1 = An alternate signal is used as the module synchronization output signal

0 = The module synchronization output signal is the Time Base Reset/rollover event

**Note 1:** This control bit has no function in Input Capture modes.

**2:** This control bit has no function when TRIGEN = 0.

**3:** Values greater than ‘0011’ will cause a FIFO buffer overflow in Input Capture mode.

REGISTER 14-1: CCPxCON1: CAPTURE/COMPARE/PWMx CONTROL 1 REGISTER (CONTINUED)

bit 20-16 **SYNC<4:0>:** CCPx Synchronization Source Select bits

11111 = Off

11110 = Reserved

**. . .**

11100 = Reserved

11011 = Time base is synchronized to the start of ADC conversion

11010 = Time base is synchronized to Comparator 3 11001 = Time base is synchronized to Comparator 2 11000 = Time base is synchronized to Comparator 1 10111 = Reserved

**. . .**

10010 = Reserved

10011 = Time base is synchronized to CLC4 10010 = Time base is synchronized to CLC3 10001 = Time base is synchronized to CLC2 10001 = Time base is synchronized to CLC1 01111 = Time base is synchronized to SCCP9 01110 = Time base is synchronized to SCCP8

01101 = Time base is synchronized to the INT4 Pin (Remappable)

01100 = Time base is synchronized to the INT3 Pin 01011 = Time base is synchronized to the INT2 Pin 01010 = Time base is synchronized to the INT1 Pin 01001 = Time base is synchronized to the INT0 Pin 01000 = Reserved

**. . .**

00101 = Reserved

00100 = Time base is synchronized to SCCP3 00011 = Time base is synchronized to SCCP2 00010 = Time base is synchronized to MCCP1

00001 = Time base is synchronized to this MCCP/SCCP

00000 = No external synchronization; timer rolls over at FFFFh or matches with the Timer Period register bit 15 **ON:** CCPx Module Enable bit**(**[**1**](#_bookmark343)**)**

1 = Module is enabled with the operating mode specified by the MOD<3:0> bits

0 = Module is disabled

bit 14 **Unimplemented:** Read as ‘0’

bit 13 **SIDL:** CCPx Stop in Idle Mode bit

1 = Discontinues module operation when device enters Idle mode

0 = Continues module operation in Idle mode bit 12 **CCPSLP:** CCPx Sleep Mode Enable bit

1 = Module continues to operate in Sleep modes

0 = Module does not operate in Sleep modes

bit 11 **TMRSYNC:** Time Base Clock Synchronization bit

1 = Module time base clock is synchronized to internal system clocks; timing restrictions apply

0 = Module time base clock is not synchronized to internal system clocks

**Note 1:** This control bit has no function in Input Capture modes.

**2:** This control bit has no function when TRIGEN = 0.

**3:** Values greater than ‘0011’ will cause a FIFO buffer overflow in Input Capture mode.

REGISTER 14-1: CCPxCON1: CAPTURE/COMPARE/PWMx CONTROL 1 REGISTER (CONTINUED)

bit 10-8 **CLKSEL<2:0>:** CCPx Time Base Clock Select bits

111 = TCKIA pin (remappable) 110 = TCKIB pin (remappable) 101 = Reserved

100 = Reserved

011 = CLC1 output for MCCP1 CLC2 output for MCCP2 CLC3 output for MCCP3 CLC1 output for SCCP4 CLC2 output for SCCP5 CLC3 output for SCCP6 CLC4 output for SCCP7 CLC1 output for SCCP8 CLC1 output for SCCP9

010 = Secondary Oscillator (SOSC) clock

001 = REFO1 output clock

000 = System clock (TCY)

bit 7-6 **TMRPS<1:0>:** CCPx Time Base Prescale Select bits

11 = 1:64 prescaler

10 = 1:16 prescaler

01 = 1:4 prescaler

00 = 1:1 prescaler

bit 5 **T32:** 32-Bit Time Base Select bit

1 = 32-bit time base for timer, single edge output compare or input capture function

0 = 16-bit time base for timer, single edge output compare or input capture function bit 4 **CCSEL:** Capture/Compare Mode Select bit

1 = Input Capture mode

0 = Output Compare/PWM or Timer mode (exact function is selected by the MOD<3:0> bits) bit 3-0 **MOD<3:0>:** CCPx Mode Select bits

CCSEL = 1 (Input Capture modes):

1xxx = Reserved

011x = Reserved

0101 = Capture every 16th rising edge

0100 = Capture every 4th rising edge

0011 = Capture every rising and falling edge

0010 = Capture every falling edge

0001 = Capture every rising edge

0000 = Capture every rising and falling edge (Edge Detect mode) CCSEL = 0 (Output Compare modes):

1111 = External Input mode: Pulse generator is disabled, source is selected by ICS<2:0>

1110 = Reserved 110x = Reserved 10xx = Reserved

0111 = Variable Frequency Pulse mode

0110 = Center-Aligned Pulse Compare mode, buffered

0101 = Dual Edge Compare mode, buffered

0100 = Dual Edge Compare mode

0011 = 16-Bit/32-Bit Single Edge mode: Toggles output on compare match 0010 = 16-Bit/32-Bit Single Edge mode: Drives output low on compare match 0001 = 16-Bit/32-Bit Single Edge mode: Drives output high on compare match 0000 = 16-Bit/32-Bit Timer mode: Output functions are disabled

**Note 1:** This control bit has no function in Input Capture modes.

**2:** This control bit has no function when TRIGEN = 0.

**3:** Values greater than ‘0011’ will cause a FIFO buffer overflow in Input Capture mode.

REGISTER 14-2: CCPxCON2: CAPTURE/COMPARE/PWMx CONTROL 2 REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-1 |
| OENSYNC | — | OCFEN**(**[**1**](#_bookmark348)**)** | OCEEN**(**[**1**](#_bookmark348)**)** | OCDEN**(**[**1**](#_bookmark348)**)** | OCCEN**(**[**1**](#_bookmark348)**)** | OCBEN**(**[**1**](#_bookmark348)**)** | OCAEN |
| 23:16 | R/W-0 | R/W-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| ICGSM<1:0> | | — | AUXOUT<1:0> | | ICS<2:0> | | |
| 15:8 | R/W-0 | R/W-0 | U-0 | R/W-0 | U-0 | U-0 | U-0 | U-0 |
| PWMRSEN | ASDGM | — | SSDG | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| ASDG<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **OENSYNC:** Output Enable Synchronization bit

1 = Update by output enable bits occurs on the next Time Base Reset or rollover

0 = Update by output enable bits occurs immediately bit 30 **Unimplemented:** Read as ‘0’

bit 29-24 **OC<F:A>EN:** Output Enable/Steering Control bits**(**[**1**](#_bookmark348)**)**

1 = OCx pin is controlled by the CCPx module and produces an output compare or PWM signal

0 = OCx pin is not controlled by the CCPx module; the pin is available to the port logic or another peripheral multiplexed on the pin

bit 23-22 **ICGSM<1:0>:** Input Capture Gating Source Mode Control bits

11 = Reserved

10 = One-Shot mode: Falling edge from gating source disables future capture events (ICDIS = 1) 01 = One-Shot mode: Rising edge from gating source enables future capture events (ICDIS = 0)

00 = Level-Sensitive mode: A high level from gating source will enable future capture events; a low level will disable future capture events

bit 21 **Unimplemented:** Read as ‘0’

bit 20-19 **AUXOUT<1:0>:** Auxiliary Output Signal on Event Selection bits

11 = Input capture or output compare event; no signal in Timer mode

10 = Signal output depends on module operating mode

01 = Time base rollover event (all modes)

00 = Disabled

bit 18-16 **ICS<2:0>:** Input Capture Source Select bits

111 = CLC4 output 110 = CLC3 output 101 = CLC2 output 100 = CLC1 output

011 = Comparator 3 output

010 = Comparator 2 output

001 = Comparator 1 output

000 = ICMx pin**(**[**2**](#_bookmark349)**)**

bit 15 **PWMRSEN:** CCPx PWM Restart Enable bit

1 = ASEVT bit clears automatically at the beginning of the next PWM period, after the shutdown input has ended

0 = ASEVT must be cleared in software to resume PWM activity on output pins

**Note 1:** OCFEN through OCBEN (bits<29:25>) are implemented in MCCP modules only.

**2:** This pin is remappable from SCCP modules.

REGISTER 14-2: CCPxCON2: CAPTURE/COMPARE/PWMx CONTROL 2 REGISTER (CONTINUED)

bit 14 **ASDGM:** CCPx Auto-Shutdown Gate Mode Enable bit

1 = Waits until the next Time Base Reset or rollover for shutdown to occur

0 = Shutdown event occurs immediately bit 13 **Unimplemented:** Read as ‘0’

bit 12 **SSDG:** CCPx Software Shutdown/Gate Control bit

1 = Manually forces auto-shutdown, timer clock gate or input capture signal gate event (setting the ASDGM bit still applies)

0 = Normal module operation bit 11-8 **Unimplemented:** Read as ‘0’

bit 7-0 **ASDG<7:0>:** CCPx Auto-Shutdown/Gating Source Enable bits

1xxx xxxx = Auto-shutdown is controlled by the OCFB pin (remappable) x1xx xxxx = Auto-shutdown is controlled by the OCFA pin (remappable) xx1x xxxx = Auto-shutdown is controlled by CLC1 for MCCP1

Auto-shutdown is controlled by CLC2 for MCCP2 Auto-shutdown is controlled by CLC3 for MCCP3 Auto-shutdown is controlled by CLC1 for SCCP4 Auto-shutdown is controlled by CLC2 for SCCP5 Auto-shutdown is controlled by CLC3 for SCCP6 Auto-shutdown is controlled by CLC4 for SCCP7 Auto-shutdown is controlled by CLC1 for SCCP8 Auto-shutdown is controlled by CLC2 for SCCP9

xxx1 xxxx = Auto-shutdown is controlled by the SCCP4 output for MCCP1/MCCP2/MCCP3

Auto-shutdown is controlled by the MCCP1 output for SCCP4/SCCP5/SCCP6/SCCP7/ SCCP8/SCCP9

xxxx 1xxx = Auto-shutdown is controlled by the SCCP5 output for MCCP1/MCCP2/MCCP3

Auto-shutdown is controlled by the MCCP2 output for SCCP4/SCCP5/SCCP6/SCCP7/ SCCP8/SCCP9

xxxx x1xx = Auto-shutdown is controlled by Comparator 3 xxxx xx1x = Auto-shutdown is controlled by Comparator 2 xxxx xxx1 = Auto-shutdown is controlled by Comparator 1

**Note 1:** OCFEN through OCBEN (bits<29:25>) are implemented in MCCP modules only.

**2:** This pin is remappable from SCCP modules.

REGISTER 14-3: CCPxCON3: CAPTURE/COMPARE/PWMx CONTROL 3 REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | R/W-0 | R/W-0 | R/W-0 |
| OETRIG | OSCNT<2:0> | | | — | OUTM<2:0>**(**[**1**](#_bookmark352)**)** | | |
| 23:16 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | POLACE | POLBDF**(**[**1**](#_bookmark352)**)** | PSSACE<1:0> | | PSSBDF<1:0>**(**[**1**](#_bookmark352)**)** | |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | DT<5:0>**(**[**1**](#_bookmark352)**)** | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **OETRIG:** PWM Dead-Time Select bit

1 = For Triggered mode (TRIGEN = 1), the module does not drive enabled output pins until triggered

0 = Normal output pin operation

bit 30-28 **OSCNT<2:0>:** One-Shot Event Count bits

Extends the duration of a one-shot trigger event by an additional n clock cycles (n + 1 total cycles).

111 = 7 timer count periods (8 cycles total)

110 = 6 timer count periods (7 cycles total)

101 = 5 timer count periods (6 cycles total)

100 = 4 timer count periods (5 cycles total)

011 = 3 timer count periods (4 cycles total)

010 = 2 timer count periods (3 cycles total)

001 = 1 timer count period (2 cycles total)

000 = Does not extend the one-shot trigger event (the event takes 1 timer count period) bit 27 **Unimplemented:** Read as ‘0’

bit 26-24 **OUTM<2:0>:** PWMx Output Mode Control bits**(**[**1**](#_bookmark352)**)**

111 = Reserved

110 = Output Scan mode

101 = Brush DC Output mode, forward 100 = Brush DC Output mode, reverse 011 = Reserved

010 = Half-Bridge Output mode

001 = Push-Pull Output mode

000 = Steerable Single Output mode bit 23-22 **Unimplemented:** Read as ‘0’

bit 21 **POLACE:** CCPx Output Pins, OCxA, OCxC and OCxE, Polarity Control bit

1 = Output pin polarity is active-low

0 = Output pin polarity is active-high

bit 20 **POLBDF:** CCPx Output Pins, OCxB, OCxD and OCxF, Polarity Control bit**(**[**1**](#_bookmark352)**)**

1 = Output pin polarity is active-low

0 = Output pin polarity is active-high

**Note 1:** These bits are implemented in MCCP modules only.

REGISTER 14-3: CCPxCON3: CAPTURE/COMPARE/PWMx CONTROL 3 REGISTER (CONTINUED)

bit 19-18 **PSSACE<1:0>:** PWMx Output Pins, OCxA, OCxC and OCxE, Shutdown State Control bits

11 = Pins are driven active when a shutdown event occurs

10 = Pins are driven inactive when a shutdown event occurs

0x = Pins are in a high-impedance state when a shutdown event occurs

bit 17-16 **PSSBDF<1:0>:** PWMx Output Pins, OCxB, OCxD and OCxF, Shutdown State Control bits**(**[**1**](#_bookmark352)**)**

11 = Pins are driven active when a shutdown event occurs

10 = Pins are driven inactive when a shutdown event occurs

0x = Pins are in a high-impedance state when a shutdown event occurs bit 15-6 **Unimplemented:** Read as ‘0’

bit 5-0 **DT<5:0>:** PWM Dead-Time Select bits**(**[**1**](#_bookmark352)**)**

111111 = Insert 63 dead-time delay periods between complementary output signals

111110 = Insert 62 dead-time delay periods between complementary output signals

**. . .**

000010 = Insert 2 dead-time delay periods between complementary output signals 000001 = Insert 1 dead-time delay period between complementary output signals 000000 = Dead-time logic is disabled

**Note 1:** These bits are implemented in MCCP modules only.

REGISTER 14-4: CCPxSTAT: CAPTURE/COMPARE/PWMx STATUS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| — | — | — | PRLWIP | TMRHWIP | TMRLWIP | RBWIP | RAWIP |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | R/C-0 | U-0 | U-0 |
| — | — | — | — | — | ICGARM**(**[**1**](#_bookmark355)**)** | — | — |
| 7:0 | R-0 | W1-0 | W1-0 | R/C-0 | R/C-0 | R/C-0 | R/C-0 | R/C-0 |
| CCPTRIG | TRSET | TRCLR | ASEVT | SCEVT | ICDIS | ICOV | ICBNE |

|  |  |  |
| --- | --- | --- |
| **Legend:** | C = Clearable bit |  |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-21 **Unimplemented:** Read as ‘0’

bit 20 **PRLWIP:** CCPxPRL Write in Progress Status bit

1 = An update to the CCPxPRL register with the buffered contents is in progress

0 = An update to the CCPxPRL register is not in progress bit 19 **TMRHWIP:** CCPxTMRH Write in Progress Status bit

1 = An update to the CCPxTMRH register with the buffered contents is in progress

0 = An update to the CCPxTMRH register is not in progress bit 18 **TMRLWIP:** CCPxTMRL Write in Progress Status bit

1 = An update to the CCPxTMRL register with the buffered contents is in progress

0 = An update to the CCPxTMRL register is not in progress bit 17 **RBWIP:** CCPxRB Write in Progress Status bit

1 = An update to the CCPxRB register with the buffered contents is in progress

0 = An update to the CCPxRB register is not in progress bit 16 **RAWIP:** CCPxRA Write in Progress Status bit

1 = An update to the CCPxRA register with the buffered contents is in progress

0 = An update to the CCPxRA register is not in progress bit 15-11 **Unimplemented:** Read as ‘0’

bit 10 **ICGARM:** Input Capture Gate Arm bit**(**[**1**](#_bookmark355)**)**

A write of ‘1’ to this location will arm the input capture gating logic for a one-shot gate event when ICGSM<1:0> = 01 or 10. The bit location reads as ‘0’.

bit 9-8 **Unimplemented:** Read as ‘0’

bit 7 **CCPTRIG:** CCPx Trigger Status bit

1 = Timer has been triggered and is running (set by hardware or writing to TRSET)

0 = Timer has not been triggered and is held in Reset (cleared by writing to TRCLR) bit 6 **TRSET:** CCPx Trigger Set Request bit

Write ‘1’ to this location to trigger the timer when TRIGEN = 1 (location always reads ‘0’). bit 5 **TRCLR:** CCPx Trigger Clear Request bit

Write ‘1’ to this location to cancel the timer trigger when TRIGEN = 1 (location always reads ‘0’). bit 4 **ASEVT:** CCPx Auto-Shutdown Event Status/Control bit

1 = A shutdown event is in progress; CCPx outputs are in the shutdown state

0 = CCPx outputs operate normally

**Note 1:** This is not a physical bit location and will always read as ‘0’. A write of ‘1’ will initiate the hardware event.

REGISTER 14-4: CCPxSTAT: CAPTURE/COMPARE/PWMx STATUS REGISTER (CONTINUED)

bit 3 **SCEVT:** Single Edge Compare Event Status bit

1 = A single edge compare event has occurred

0 = A single edge compare event has not occurred bit 2 **ICDIS:** Input Capture Disable bit

1 = Event on input capture pin does not generate a capture event

0 = Event on input capture pin will generate a capture event bit 1 **ICOV:** Input Capture Buffer Overflow Status bit

1 = The input capture FIFO buffer has overflowed

0 = The input capture FIFO buffer has not overflowed bit 0 **ICBNE:** Input Capture Buffer Status bit

1 = The input capture buffer has data available

0 = The input capture buffer is empty

**Note 1:** This is not a physical bit location and will always read as ‘0’. A write of ‘1’ will initiate the hardware event.

NOTES:

# SERIAL PERIPHERAL INTERFACE (SPI) AND INTER-IC SOUND (I2S)

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To com- plement the information in this data sheet, refer to **Section 23. “Serial Peripheral Interface (SPI)”** (DS61106) in the *“PIC32 Family Reference Manual”*[, which is](http://www.microchip.com/PIC32) [available from the Microchip web site](http://www.microchip.com/PIC32) [(](http://www.microchip.com/PIC32)[www.microchip.com/PIC32).](http://www.microchip.com/PIC32)) The informa- tion in this data sheet supersedes the information in the FRM.

The SPI/I2S module is a synchronous serial interface that is useful for communicating with external peripherals and other microcontroller devices, as well

as digital audio devices. These peripheral devices may be serial EEPROMs, shift registers, display drivers, Analog-to-Digital Converters (ADC), etc.

The SPI/I2S module is compatible with Motorola® SPI and SIOP interfaces.

Some of the key features of the SPI module are:

* Master and Slave modes Support
* Four Different Clock Formats
* Enhanced Framed SPI Protocol Support
* User-Configurable 8-Bit, 16-Bit and 32-Bit Data Width
* Separate SPI FIFO Buffers for Receive and Transmit:
  + FIFO buffers act as 4/8/16-level deep FIFOs based on 32/16/8-bit data width
* Programmable Interrupt Event on every 8-Bit, 16-Bit and 32-Bit Data Transfer
* Operation during Sleep and Idle modes
* Audio Codec Support:
  + I2S protocol



FIGURE 15-1: SPI/I2S MODULE BLOCK DIAGRAM

Internal Data Bus

SPIxBUF

Read

Write

FIFOs Share Address SPIxBUF

SPIxRXB FIFO SPIxTXB FIFO

Transmit

Receive

SPIxSR

SDIx

bit 0

SDOx

Shift Control

Clock Control

MCLKSEL

SSx/FSYNC1

Slave Select and Frame Sync Control

Edge Select

REFOCLK

Baud Rate Generator

SCKx

PBCLK

MSTEN

**Note:** Access the SPIxTXB and SPIxRXB FIFOs via the SPIxBUF register.



### SPI Control Registers

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 160

TABLE 15-1: SPI1, SPI2 AND SPI3 REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 8100 | SPI1CON | 31:16 | FRMEN | FRMSYNC | FRMPOL | MSSEN | FRMSYPW | FRMCNT<2:0> | | | MCLKSEL | — | — | — | — | — | SPIFE | ENHBUF | 0000 |
| 15:0 | ON | — | SIDL | DISSDO | MODE32 | MODE16 | SMP | CKE | SSEN | CKP | MSTEN | DISSDI | STXISEL<1:0> | | SRXISEL<1:0> | | 0000 |
| 8110 | SPI1STAT | 31:16 | — | — | — | RXBUFELM<4:0> | | | | | — | — | — | TXBUFELM<4:0> | | | | | 0000 |
| 15:0 | — | — | — | FRMERR | SPIBUSY | — | — | SPITUR | SRMT | SPIROV | SPIRBE | — | SPITBE | — | SPITBF | SPIRBF | 0008 |
| 8120 | SPI1BUF | 31:16 | DATA<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 8130 | SPI1BRG | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | BRG<12:0> | | | | | | | | | | | | | 0000 |
| 8140 | SPI1CON2 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | SPISGNEXT | — | — | FRMERREN | SPIROVEN | SPITUREN | IGNROV | IGNTUR | AUDEN | — | — | — | AUDMONO | — | AUDMOD<1:0> | | 0000 |
| 8200 | SPI2CON | 31:16 | FRMEN | FRMSYNC | FRMPOL | MSSEN | FRMSYPW | FRMCNT<2:0> | | | MCLKSEL | — | — | — | — | — | SPIFE | ENHBUF | 0000 |
| 15:0 | ON | — | SIDL | DISSDO | MODE32 | MODE16 | SMP | CKE | SSEN | CKP | MSTEN | DISSDI | STXISEL<1:0> | | SRXISEL<1:0> | | 0000 |
| 8210 | SPI2STAT | 31:16 | — | — | — | RXBUFELM<4:0> | | | | | — | — | — | TXBUFELM<4:0> | | | | | 0000 |
| 15:0 | — | — | — | FRMERR | SPIBUSY | — | — | SPITUR | SRMT | SPIROV | SPIRBE | — | SPITBE | — | SPITBF | SPIRBF | 0008 |
| 8220 | SPI2BUF | 31:16 | DATA<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 8230 | SPI2BRG | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | BRG<12:0> | | | | | | | | | | | | | 0000 |
| 8240 | SPI2CON2 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | SPISGNEXT | — | — | FRMERREN | SPIROVEN | SPITUREN | IGNROV | IGNTUR | AUDEN | — | — | — | AUDMONO | — | AUDMOD<1:0> | | 0000 |
| 8300 | SPI3CON | 31:16 | FRMEN | FRMSYNC | FRMPOL | MSSEN | FRMSYPW | FRMCNT<2:0> | | | MCLKSEL | — | — | — | — | — | SPIFE | ENHBUF | 0000 |
| 15:0 | ON | — | SIDL | DISSDO | MODE32 | MODE16 | SMP | CKE | SSEN | CKP | MSTEN | DISSDI | STXISEL<1:0> | | SRXISEL<1:0> | | 0000 |
| 8310 | SPI3STAT | 31:16 | — | — | — | RXBUFELM<4:0> | | | | | — | — | — | TXBUFELM<4:0> | | | | | 0000 |
| 15:0 | — | — | — | FRMERR | SPIBUSY | — | — | SPITUR | SRMT | SPIROV | SPIRBE | — | SPITBE | — | SPITBF | SPIRBF | 0008 |
| 8330 | SPI3BUF | 31:16 | DATA<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 8320 | SPI3BRG | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | BRG<12:0> | | | | | | | | | | | | | 0000 |
| 8340 | SPI3CON2 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | SPISGNEXT | — | — | FRMERREN | SPIROVEN | SPITUREN | IGNROV | IGNTUR | AUDEN | — | — | — | AUDMONO | — | AUDMOD<1:0> | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table, except SPIxBUF, have corresponding CLR, SET and INV registers at their virtual addresses, plus offsets of 0x4, 0x8 and 0xC, respectively.

REGISTER 15-1: SPIxCON: SPIx CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| FRMEN | FRMSYNC | FRMPOL | MSSEN | FRMSYPW | FRMCNT<2:0> | | |
| 23:16 | R/W-0 | U-0 | U-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 |
| MCLKSEL**(**[**1**](#_bookmark364)**)** | — | — | — | — | — | SPIFE | ENHBUF**(**[**1**](#_bookmark364)**)** |
| 15:8 | R/W-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| ON | — | SIDL | DISSDO**(**[**4**](#_bookmark367)**)** | MODE32 | MODE16 | SMP | CKE**(**[**2**](#_bookmark365)**)** |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| SSEN | CKP**(**[**3**](#_bookmark366)**)** | MSTEN | DISSDI**(**[**4**](#_bookmark367)**)** | STXISEL<1:0> | | SRXISEL<1:0> | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **FRMEN:** Framed SPI Support bit

1 = Framed SPI support is enabled (SSx pin is used as the FSYNC1 input/output)

0 = Framed SPI support is disabled

bit 30 **FRMSYNC:** Frame Sync Pulse Direction Control on SSx Pin bit (Framed SPI mode only)

1 = Frame sync pulse input (Slave mode)

0 = Frame sync pulse output (Master mode)

bit 29 **FRMPOL:** Frame Sync Polarity bit (Framed SPI mode only)

1 = Frame pulse is active-high

0 = Frame pulse is active-low

bit 28 **MSSEN:** Master Mode Slave Select Enable bit

1 = Slave select SPI support is enabled; the SSx pin is automatically driven during transmission in Master mode, polarity is determined by the FRMPOL bit

0 = Slave select SPI support is disabled bit 27 **FRMSYPW:** Frame Sync Pulse-Width bit

1 = Frame sync pulse is one character wide

0 = Frame sync pulse is one clock wide

bit 26-24 **FRMCNT<2:0>:** Frame Sync Pulse Counter bits

Controls the number of data characters transmitted per pulse. This bit is only valid in Framed mode.

111 = Reserved

110 = Reserved

101 = Generates a frame sync pulse on every 32 data characters 100 = Generates a frame sync pulse on every 16 data characters 011 = Generates a frame sync pulse on every 8 data characters 010 = Generates a frame sync pulse on every 4 data characters 001 = Generates a frame sync pulse on every 2 data characters 000 = Generates a frame sync pulse on every data character

**Note 1:** These bits can only be written when the ON bit = 0. Refer to [**Section 29.0 “Electrical Characteristics”**](#_bookmark636) for maximum clock frequency requirements.

**2:** This bit is not used in the Framed SPI mode. The user should program this bit to ‘0’ for the Framed SPI mode (FRMEN = 1).

**3:** When AUDEN = 1, the SPI/I2S module functions as if the CKP bit is equal to ‘1’, regardless of the actual value of the CKP bit.

**4:** These bits are present for legacy compatibility and are superseded by PPS functionality on these devices (see [**Section 10.9 “Peripheral Pin Select (PPS)”**](#_bookmark262) for more information).

REGISTER 15-1: SPIxCON: SPIx CONTROL REGISTER (CONTINUED)

bit 23 **MCLKSEL:** Master Clock Enable bit**(**[**1**](#_bookmark364)**)**

1 = REFO1 is used by the Baud Rate Generator

0 = PBCLK is used by the Baud Rate Generator bit 22-18 **Unimplemented:** Read as ‘0’

bit 17 **SPIFE:** Frame Sync Pulse Edge Select bit (Framed SPI mode only)

1 = Frame synchronization pulse coincides with the first bit clock

0 = Frame synchronization pulse precedes the first bit clock bit 16 **ENHBUF:** Enhanced Buffer Enable bit**(**[**1**](#_bookmark364)**)**

1 = Enhanced Buffer mode is enabled

0 = Enhanced Buffer mode is disabled bit 15 **ON:** SPIx Module On bit

1 = SPIx module is enabled

0 = SPIx module is disabled bit 14 **Unimplemented:** Read as ‘0’

bit 13 **SIDL:** SPIx Stop in Idle Mode bit

1 = Discontinues operation when CPU enters Idle mode

0 = Continues operation in Idle mode bit 12 **DISSDO:** Disable SDOx Pin bit**(**[**4**](#_bookmark367)**)**

1 = SDOx pin is not used by the module; the pin is controlled by the associated PORTx register

0 = SDOx pin is controlled by the module

bit 11-10 **MODE<32,16>:** 32/16/8-Bit Communication Select bits

|  |  |  |
| --- | --- | --- |
| When AUDEN = 1: | | |
| MODE32 | MODE16 | Communication |
| 1 | 1 | 24-bit data, 32-bit FIFO, 32-bit channel/64-bit frame |
| 1 | 0 | 32-bit data, 32-bit FIFO, 32-bit channel/64-bit frame |
| 0 | 1 | 16-bit data, 16-bit FIFO, 32-bit channel/64-bit frame |
| 0 | 0 | 16-bit data, 16-bit FIFO, 16-bit channel/32-bit frame |
| When AUDEN = 0: | | |
| MODE32 | MODE16 | Communication |
| 1 | x | 32-bit |
| 0 | 1 | 16-bit |
| 0 | 0 | 8-bit |

bit 9 **SMP:** SPIx Data Input Sample Phase bit Master mode (MSTEN = 1):

1 = Input data is sampled at end of data output time

0 = Input data is sampled at middle of data output time Slave mode (MSTEN = 0):

SMP value is ignored when SPIx is used in Slave mode. The module always uses SMP = 0.

bit 8 **CKE:** SPIx Clock Edge Select bit**(**[**2**](#_bookmark365)**)**

1 = Serial output data changes on transition from active clock state to Idle clock state (see the CKP bit)

0 = Serial output data changes on transition from Idle clock state to active clock state (see the CKP bit)

**Note 1:** These bits can only be written when the ON bit = 0. Refer to **Section 29.0 “Electrical Characteristics”** for maximum clock frequency requirements.

**2:** This bit is not used in the Framed SPI mode. The user should program this bit to ‘0’ for the Framed SPI mode (FRMEN = 1).

**3:** When AUDEN = 1, the SPI/I2S module functions as if the CKP bit is equal to ‘1’, regardless of the actual value of the CKP bit.

**4:** These bits are present for legacy compatibility and are superseded by PPS functionality on these devices (see **Section 10.9 “Peripheral Pin Select (PPS)”** for more information).

REGISTER 15-1: SPIxCON: SPIx CONTROL REGISTER (CONTINUED)

bit 7 **SSEN:** Slave Select Enable (Slave mode) bit

1 = SSx pin is used for Slave mode

0 = SSx pin is not used for Slave mode, pin is controlled by port function bit 6 **CKP:** Clock Polarity Select bit**(**[**3**](#_bookmark366)**)**

1 = Idle state for clock is a high level; active state is a low level

0 = Idle state for clock is a low level; active state is a high level bit 5 **MSTEN:** Master Mode Enable bit

1 = Master mode

0 = Slave mode

bit 4 **DISSDI:** Disable SDIx bit**(**[**4**](#_bookmark367)**)**

1 = SDIx pin is not used by the SPIx module (pin is controlled by port function)

0 = SDIx pin is controlled by the SPIx module

bit 3-2 **STXISEL<1:0>:** SPIx Transmit Buffer Empty Interrupt Mode bits

11 = Interrupt is generated when the buffer is not full (has one or more empty elements)

10 = Interrupt is generated when the buffer is empty by one-half or more

01 = Interrupt is generated when the buffer is completely empty

00 = Interrupt is generated when the last transfer is shifted out of SPIxSR and transmit operations are complete bit 1-0 **SRXISEL<1:0>:** SPIx Receive Buffer Full Interrupt Mode bits

11 = Interrupt is generated when the buffer is full

10 = Interrupt is generated when the buffer is full by one-half or more

01 = Interrupt is generated when the buffer is not empty

00 = Interrupt is generated when the last word in the receive buffer is read (i.e., buffer is empty)

**Note 1:** These bits can only be written when the ON bit = 0. Refer to **Section 29.0 “Electrical Characteristics”** for maximum clock frequency requirements.

**2:** This bit is not used in the Framed SPI mode. The user should program this bit to ‘0’ for the Framed SPI mode (FRMEN = 1).

**3:** When AUDEN = 1, the SPI/I2S module functions as if the CKP bit is equal to ‘1’, regardless of the actual value of the CKP bit.

**4:** These bits are present for legacy compatibility and are superseded by PPS functionality on these devices (see **Section 10.9 “Peripheral Pin Select (PPS)”** for more information).

REGISTER 15-2: SPIxCON2: SPIx CONTROL REGISTER 2

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| SPISGNEXT | — | — | FRMERREN | SPIROVEN | SPITUREN | IGNROV | IGNTUR |
| 7:0 | R/W-0 | U-0 | U-0 | U-0 | R/W-0 | U-0 | R/W-0 | R/W-0 |
| AUDEN**(**[**1**](#_bookmark369)**)** | — | — | — | AUDMONO**(**[**1**](#_bookmark369)**,**[**2**](#_bookmark370)**)** | — | AUDMOD<1:0>**(**[**1**](#_bookmark369)**,**[**2**](#_bookmark370)**)** | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’

bit 15 **SPISGNEXT:** SPIx Sign-Extend Read Data from the RX FIFO bit

1 = Data from RX FIFO is sign-extended

0 = Data from RX FIFO is not sign-extended bit 14-13 **Unimplemented:** Read as ‘0’

bit 12 **FRMERREN:** Enable Interrupt Events via FRMERR bit

1 = Frame error overflow generates error events

0 = Frame error does not generate error events

bit 11 **SPIROVEN:** Enable Interrupt Events via SPIROV bit

1 = Receive Overflow (ROV) generates error events

0 = Receive Overflow does not generate error events bit 10 **SPITUREN:** Enable Interrupt Events via SPITUR bit

1 = Transmit Underrun (TUR) generates error events

0 = Transmit Underrun does not generate error events

bit 9 **IGNROV:** Ignore Receive Overflow (ROV) bit (for audio data transmissions)

1 = A ROV is not a critical error; during ROV, data in the FIFO is not overwritten by receive data

0 = A ROV is a critical error which stops SPIx operation

bit 8 **IGNTUR:** Ignore Transmit Underrun (TUR) bit (for audio data transmissions)

1 = A TUR is not a critical error and zeros are transmitted until the SPIxTXB is not empty

0 = A TUR is a critical error which stops SPIx operation bit 7 **AUDEN:** Enable Audio Codec Support bit**(**[**1**](#_bookmark369)**)**

1 = Audio protocol is enabled

0 = Audio protocol is disabled bit 6-4 **Unimplemented:** Read as ‘0’

bit 3 **AUDMONO:** Transmit Audio Data Format bit**(**[**1**](#_bookmark369)**,**[**2**](#_bookmark370)**)**

1 = Audio data is mono (each data word is transmitted on both left and right channels)

0 = Audio data is stereo

bit 2 **Unimplemented:** Read as ‘0’

bit 1-0 **AUDMOD<1:0>:** Audio Protocol Mode bits**(**[**1**](#_bookmark369)**,**[**2**](#_bookmark370)**)**

11 = PCM/DSP mode

10 = Right Justified mode 01 = Left Justified mode 00 = I2S mode

**Note 1:** These bits can only be written when the ON bit = 0.

**2:** These bits are only valid for AUDEN = 1.

REGISTER 15-3: SPIxSTAT: SPIx STATUS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| — | — | — | RXBUFELM<4:0> | | | | |
| 23:16 | U-0 | U-0 | U-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| — | — | — | TXBUFELM<4:0> | | | | |
| 15:8 | U-0 | U-0 | U-0 | R/C-0, HS | R-0 | U-0 | U-0 | R-0 |
| — | — | — | FRMERR | SPIBUSY | — | — | SPITUR |
| 7:0 | R-0 | R/W-0 | R-0 | U-0 | R-1 | U-0 | R-0 | R-0 |
| SRMT | SPIROV | SPIRBE | — | SPITBE | — | SPITBF | SPIRBF |

|  |  |  |
| --- | --- | --- |
| **Legend:** | C = Clearable bit | HS = Hardware Settable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-29 **Unimplemented:** Read as ‘0’

bit 28-24 **RXBUFELM<4:0>:** Receive Buffer Element Count bits (valid only when ENHBUF = 1) bit 23-21 **Unimplemented:** Read as ‘0’

bit 20-16 **TXBUFELM<4:0>:** Transmit Buffer Element Count bits (valid only when ENHBUF = 1) bit 15-13 **Unimplemented:** Read as ‘0’

bit 12 **FRMERR:** SPIx Frame Error status bit

1 = Frame error detected

0 = No frame error detected

This bit is only valid when FRMEN = 1. bit 11 **SPIBUSY:** SPIx Activity Status bit

1 = SPIx peripheral is currently busy with some transactions

0 = SPIx peripheral is currently Idle bit 10-9 **Unimplemented:** Read as ‘0’

bit 8 **SPITUR:** Transmit Underrun (TUR) bit

1 = Transmit buffer has encountered an underrun condition

0 = Transmit buffer has no underrun condition

This bit is only valid in Framed Sync mode; the underrun condition must be cleared by disabling/re-enabling the module.

bit 7 **SRMT:** Shift Register Empty bit (valid only when ENHBUF = 1) 1 = When the SPIx Shift register is empty

0 = When the SPIx Shift register is not empty

bit 6 **SPIROV:** Receive Overflow (ROV) Flag bit

1 = A new data is completely received and discarded; the user software has not read the previous data in the SPIxBUF register

0 = No overflow has occurred

This bit is set in hardware; it can only be cleared (= 0) in software. bit 5 **SPIRBE:** RX FIFO Empty bit (valid only when ENHBUF = 1)

1 = RX FIFO is empty (CPU Read Pointer (CRPTR) = SPI Write Pointer (SWPTR))

0 = RX FIFO is not empty (CRPTR  SWPTR) bit 4 **Unimplemented:** Read as ‘0’

REGISTER 15-3: SPIxSTAT: SPIx STATUS REGISTER (CONTINUED)

bit 3 **SPITBE:** SPIx Transmit Buffer Empty Status bit

1 = Transmit buffer, SPIxTXB, is empty

0 = Transmit buffer, SPIxTXB, is not empty

Automatically set in hardware when SPIx transfers data from SPIxTXB to SPIxSR. Automatically cleared in hardware when SPIxBUF is written to, loading SPIxTXB.

bit 2 **Unimplemented:** Read as ‘0’

bit 1 **SPITBF:** SPIx Transmit Buffer Full Status bit

1 = Transmit has not yet started, SPIxTXB is full

0 = Transmit buffer is not full Standard Buffer mode:

Automatically set in hardware when the core writes to the SPIxBUF location, loading SPIxTXB. Automatically

cleared in hardware when the SPIx module transfers data from SPIxTXB to SPIxSR. Enhanced Buffer mode:

Set when CPU Write Pointer (CWPTR) + 1 = SPI Read Pointer (SRPTR); cleared otherwise.

bit 0 **SPIRBF:** SPIx Receive Buffer Full Status bit

1 = Receive buffer, SPIxRXB, is full

0 = Receive buffer, SPIxRXB, is not full Standard Buffer mode:

Automatically set in hardware when the SPIx module transfers data from SPIxSR to SPIxRXB. Automatically

cleared in hardware when SPIxBUF is read from, reading SPIxRXB. Enhanced Buffer mode:

Set when SWPTR + 1 = CRPTR; cleared otherwise.

# INTER-INTEGRATED CIRCUIT (I2C)

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To complement the information in this data

sheet, refer to **Section 24. “Inter- Integrated Circuit™ (I2C™)”** (DS61116)

in the *“PIC32 Family Reference Manual”*, which is available from the Microchip web site ([www.microchip.com/PIC32](http://www.microchip.com/PIC32)). The information in this data sheet supersedes the information in the FRM.

The I2C module provides complete hardware support for both Slave and Multi-Master modes of the I2C serial communication standard.

Each I2C module has a 2-pin interface:

* SCLx pin is clock
* SDAx pin is data

Each I2C module offers the following key features:

* I2C Interface Supporting Both Master and Slave Operation
* I2C Slave mode Supports 7-Bit and 10-Bit Addressing
* I2C Master mode Supports 7-Bit and 10-Bit Addressing
* I2C Port allows Bidirectional Transfers between Master and Slaves
* Serial Clock Synchronization for the I2C Port can be used as a Handshake Mechanism to Suspend and Resume Serial Transfer (SCLREL control)
* I2C Supports Multi-Master Operation; Detects Bus Collision and Arbitrates Accordingly
* Provides Support for Address Bit Masking
* SMBus Support

[Figure 16-1](#_bookmark375) illustrates the I2C module block diagram.

FIGURE 16-1: I2Cx BLOCK DIAGRAM



Internal Data Bus

Read

SCLx

Shift Clock

LSB

SDAx

Address Match

Write

Write

Read

Read

Write

Read

Write

Read

Write

LSB

Shift Clock

Read

Write

Read

PBCLK

BRG Down Counter

**I2CxBRG**

**I2CxMSK**

Match Detect

**I2CxRSR**

**I2CxTRN**

Clock Stretching

Acknowledge Generation

Collision Detect

Start and Stop Bit Generation

Start and Stop Bit Detect

Reload Control

**I2CxADD**

**I2CxRCV**

**I2CxCON**

**I2CxSTAT**

Control Logic

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 169

### I2C Control Registers

TABLE 16-1: I2C1, I2C2 AND I2C3 REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 1500 | I2C1CON | 31:16 | — | — | — | — | — | — | — | — | — | PCIE | SCIE | BOEN | SDAHT | SBCDE | r | r | 0000 |
| 15:0 | ON | — | SIDL | SCLREL | STRICT | A10M | DISSLW | SMEN | GCEN | STREN | ACKDT | ACKEN | RCEN | PEN | RSEN | SEN | 1000 |
| 1510 | I2C1STAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ACKSTAT | TRSTAT | ACKTIM | — | — | BCL | GCSTAT | ADD10 | IWCOL | I2COV | D/A | P | S | R/W | RBF | TBF | 0000 |
| 1520 | I2C1ADD | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | I2C1 Address Register | | | | | | | | | | 0000 |
| 1530 | I2C1MSK | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | I2C1 Address Mask Register | | | | | | | | | | 0000 |
| 1540 | I2C1BRG | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | Baud Rate Generator Register | | | | | | | | | | | | | | | | 0000 |
| 1550 | I2C1TRN | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | I2C1 Transmit Register | | | | | | | | 0000 |
| 1560 | I2C1RCV | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | I2C1 Receive Register | | | | | | | | 0000 |
| 1600 | I2C2CON | 31:16 | — | — | — | — | — | — | — | — | — | PCIE | SCIE | BOEN | SDAHT | SBCDE | r | r | 0000 |
| 15:0 | ON | — | SIDL | SCLREL | STRICT | A10M | DISSLW | SMEN | GCEN | STREN | ACKDT | ACKEN | RCEN | PEN | RSEN | SEN | 1000 |
| 1610 | I2C2STAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ACKSTAT | TRSTAT | ACKTIM | — | — | BCL | GCSTAT | ADD10 | IWCOL | I2COV | D/A | P | S | R/W | RBF | TBF | 0000 |
| 1620 | I2C2ADD | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | I2C2 Address Register | | | | | | | | | | 0000 |
| 1630 | I2C2MSK | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | I2C2 Address Mask Register | | | | | | | | | | 0000 |
| 1640 | I2C2BRG | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | Baud Rate Generator Register | | | | | | | | | | | | | | | | 0000 |
| 1650 | I2C2TRN | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | I2C2 Transmit Register | | | | | | | | 0000 |
| 1660 | I2C2RCV | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | I2C2 Receive Register | | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’; r = reserved bit. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table, except I2CxRCV, have corresponding CLR, SET and INV registers at their virtual addresses, plus offsets of 0x4, 0x8 and 0xC, respectively.

TABLE 16-1: I2C1, I2C2 AND I2C3 REGISTER MAP (CONTINUED)

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 170

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 1700 | I2C3CON | 31:16 | — | — | — | — | — | — | — | — | — | PCIE | SCIE | BOEN | SDAHT | SBCDE | r | r | 0000 |
| 15:0 | ON | — | SIDL | SCLREL | STRICT | A10M | DISSLW | SMEN | GCEN | STREN | ACKDT | ACKEN | RCEN | PEN | RSEN | SEN | 1000 |
| 1710 | I2C3STAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ACKSTAT | TRSTAT | ACKTIM | — | — | BCL | GCSTAT | ADD10 | IWCOL | I2COV | D/A | P | S | R/W | RBF | TBF | 0000 |
| 1720 | I2C3ADD | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | I2C2 Address Register | | | | | | | | | | 0000 |
| 1730 | I2C3MSK | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | I2C2 Address Mask Register | | | | | | | | | | 0000 |
| 1740 | I2C3BRG | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | Baud Rate Generator Register | | | | | | | | | | | | | | | | 0000 |
| 1750 | I2C3TRN | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | I2C2 Transmit Register | | | | | | | | 0000 |
| 1760 | I2C3RCV | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | I2C2 Receive Register | | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’; r = reserved bit. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table, except I2CxRCV, have corresponding CLR, SET and INV registers at their virtual addresses, plus offsets of 0x4, 0x8 and 0xC, respectively.

REGISTER 16-1: I2CxCON: I2Cx CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | r-0 | r-0 |
| — | PCIE | SCIE | BOEN | SDAHT | SBCDE | — | — |
| 15:8 | R/W-0 | U-0 | R/W-0 | R/W-1, HC | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| ON | — | SIDL | SCLREL | STRICT | A10M | DISSLW | SMEN |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0, HC | R/W-0, HC | R/W-0, HC | R/W-0, HC | R/W-0, HC |
| GCEN | STREN | ACKDT | ACKEN | RCEN | PEN | RSEN | SEN |

|  |  |  |
| --- | --- | --- |
| **Legend:** | r = Reserved bit | HC = Hardware Clearable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-23 **Unimplemented:** Read as ‘0’

bit 22 **PCIE:** Stop Condition Interrupt Enable bit (I2C Slave mode only)

1 = Enables interrupt on detection of Stop condition

0 = Stop detection interrupts are disabled

bit 21 **SCIE:** Start Condition Interrupt Enable bit (I2C Slave mode only)

1 = Enables interrupt on detection of Start or Restart conditions

0 = Start detection interrupts are disabled

bit 20 **BOEN:** Buffer Overwrite Enable bit (I2C Slave mode only)

1 = I2CxRCV is updated and an ACK is generated for a received address/data byte, ignoring the state of the I2COV bit (I2CxSTAT<6>) only if the RBF bit (I2CxSTAT<1>) = 0

0 = I2CxRCV is only updated when the I2COV bit (I2CxSTAT<6>) is clear bit 19 **SDAHT:** SDAx Hold Time Selection bit

1 = Minimum of 300 ns hold time on SDAx after the falling edge of SCLx

0 = Minimum of 100 ns hold time on SDAx after the falling edge of SCLx

bit 18 **SBCDE:** Slave Mode Bus Collision Detect Enable bit (I2C Slave mode only)

1 = Enables slave bus collision interrupts

0 = Slave bus collision interrupts are disabled bit 17-16 **Reserved:** Maintain as ‘0’

bit 15 **ON:** I2Cx Enable bit

1 = Enables the I2Cx module and configures the SDAx and SCLx pins as serial port pins

0 = Disables the I2Cx module; all I2C pins are controlled by port functions

bit 14 **Unimplemented:** Read as ‘0’ bit 13 **SIDL:** I2Cx Stop in Idle Mode bit

1 = Discontinues module operation when device enters Idle mode

0 = Continues module operation in Idle mode

bit 12 **SCLREL:** SCLx Release Control bit (when operating as I2C slave)

1 = Releases SCLx clock

0 = Holds SCLx clock low (clock stretch) If STREN = 1:

Bit is R/W (i.e., software can write ‘0’ to initiate stretch and write ‘1’ to release clock). Hardware is clear at

the beginning of slave transmission. Hardware is clear at the end of slave reception. If STREN = 0:

Bit is R/S (i.e., software can only write ‘1’ to release clock). Hardware is clear at the beginning of slave

transmission.

REGISTER 16-1: I2CxCON: I2Cx CONTROL REGISTER (CONTINUED)

bit 11 **STRICT:** Strict I2C Reserved Address Rule Enable bit

1 = Strict reserved addressing is enforced; device does not respond to reserved address space or generates addresses in reserved address space

0 = Strict I2C reserved address rule is not enabled

bit 10 **A10M:** 10-Bit Slave Address bit

1 = I2CxADD is a 10-bit slave address

0 = I2CxADD is a 7-bit slave address bit 9 **DISSLW:** Disable Slew Rate Control bit

1 = Slew rate control is disabled

0 = Slew rate control is enabled bit 8 **SMEN:** SMBus Input Levels bit

1 = Enables I/O pin thresholds compliant with the SMBus specification

0 = Disables SMBus input thresholds

bit 7 **GCEN:** General Call Enable bit (when operating as I2C slave)

1 = Enables interrupt when a general call address is received in the I2CxRSR (module is enabled for reception)

0 = General call address is disabled

bit 6 **STREN:** SCLx Clock Stretch Enable bit (when operating as I2C slave) Used in conjunction with the SCLREL bit.

1 = Enables software or receives clock stretching

0 = Disables software or receives clock stretching

bit 5 **ACKDT:** Acknowledge Data bit (when operating as I2C master, applicable during master receive) Value that is transmitted when the software initiates an Acknowledge sequence.

1 = Sends NACK during Acknowledge

0 = Sends ACK during Acknowledge

bit 4 **ACKEN:** Acknowledge Sequence Enable bit

(when operating as I2C master, applicable during master receive)

1 = Initiates Acknowledge sequence on the SDAx and SCLx pins and transmits the ACKDT data bit; hardware is clear at the end of the master Acknowledge sequence

0 = Acknowledge sequence is not in progress

bit 3 **RCEN:** Receive Enable bit (when operating as I2C master)

1 = Enables Receive mode for I2C; hardware is clear at the end of the eighth bit of the master receive data byte

0 = Receive sequence is not in progress

bit 2 **PEN:** Stop Condition Enable bit (when operating as I2C master)

1 = Initiates Stop condition on SDAx and SCLx pins; hardware is clear at the end of the master Stop sequence

0 = Stop condition is not in progress

bit 1 **RSEN:** Repeated Start Condition Enable bit (when operating as I2C master)

1 = Initiates Repeated Start condition on SDAx and SCLx pins; hardware is clear at the end of the master Repeated Start sequence

0 = Repeated Start condition is not in progress

bit 0 **SEN:** Start Condition Enable bit (when operating as I2C master)

1 = Initiates Start condition on SDAx and SCLx pins; hardware is clear at the end of the master Start sequence

0 = Start condition is not in progress

REGISTER 16-2: I2CxSTAT: I2Cx STATUS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R-0, HSC | R-0, HSC | R/C-0, HSC | U-0 | U-0 | R/C-0, HS | R-0, HSC | R-0, HSC |
| ACKSTAT | TRSTAT | ACKTIM | — | — | BCL | GCSTAT | ADD10 |
| 7:0 | R/C-0, HS | R/C-0, HS | R-0, HSC | R/C-0, HSC | R/C-0, HSC | R-0, HSC | R-0, HSC | R-0, HSC |
| IWCOL | I2COV | D/A | P | S | R/W | RBF | TBF |

|  |  |  |
| --- | --- | --- |
| **Legend:** | HS = Hardware Settable bit | HSC = Hardware Settable/Clearable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared C = Clearable bit |

bit 31-16 **Unimplemented:** Read as ‘0’

bit 15 **ACKSTAT:** Acknowledge Status bit (when operating as I2C master, applicable to master transmit operation)

1 = NACK received from slave

0 = ACK received from slave

Hardware is set or clear at the end of slave Acknowledge.

bit 14 **TRSTAT:** Transmit Status bit (when operating as I2C master, applicable to master transmit operation)

1 = Master transmit is in progress (8 bits + ACK)

0 = Master transmit is not in progress

Hardware is set at the beginning of master transmission. Hardware is clear at the end of slave Acknowledge. bit 13 **ACKTIM:** Acknowledge Time Status bit (valid in I2C Slave mode only)

1 = I2C bus is in an Acknowledge sequence, set on 8th falling edge of SCLx clock

0 = Not an Acknowledge sequence, cleared on 9th rising edge of SCLx clock bit 12-11 **Unimplemented:** Read as ‘0’

bit 10 **BCL:** Master Bus Collision Detect bit

1 = A bus collision has been detected during a master operation

0 = No collision

Hardware is set at detection of a bus collision. bit 9 **GCSTAT:** General Call Status bit

1 = General call address was received

0 = General call address was not received

Hardware is set when the address matches the general call address. Hardware is clear at Stop detection. bit 8 **ADD10:** 10-Bit Address Status bit

1 = 10-bit address was matched

0 = 10-bit address was not matched

Hardware is set at match of the 2nd byte of matched 10-bit address. Hardware is clear at Stop detection. bit 7 **IWCOL:** I2Cx Write Collision Detect bit

1 = An attempt to write to the I2CxTRN register failed because the I2C module is busy

0 = No collision

Hardware is set at occurrence of a write to I2CxTRN while busy (cleared by software). bit 6 **I2COV:** I2Cx Receive Overflow Flag bit

1 = A byte was received while the I2CxRCV register is still holding the previous byte

0 = No overflow

Hardware is set at attempt to transfer I2CxRSR to I2CxRCV (cleared by software).

REGISTER 16-2: I2CxSTAT: I2Cx STATUS REGISTER (CONTINUED)

bit 5 **D/A:** Data/Address bit (when operating as I2C slave)

1 = Indicates that the last byte received was data

0 = Indicates that the last byte received was a device address

Hardware is clear at a device address match. Hardware is set by reception of a slave byte. bit 4 **P:** Stop bit

1 = Indicates that a Stop bit has been detected last

0 = Stop bit was not detected last

Hardware is set or clear when Start, Repeated Start or Stop is detected. bit 3 **S:** Start bit

1 = Indicates that a Start (or Repeated Start) bit has been detected last

0 = Start bit was not detected last

Hardware is set or clear when Start, Repeated Start or Stop is detected. bit 2 **R/W:** Read/Write Information bit (when operating as I2C slave)

1 = Read – Indicates data transfer is output from slave

0 = Write – Indicates data transfer is input to slave

Hardware is set or clear after reception of an I2C device address byte.

bit 1 **RBF:** Receive Buffer Full Status bit

1 = Receive is complete, I2CxRCV is full

0 = Receive is not complete, I2CxRCV is empty

Hardware is set when I2CxRCV is written with the received byte. Hardware is clear when software reads I2CxRCV.

bit 0 **TBF:** Transmit Buffer Full Status bit

1 = Transmit is in progress, I2CxTRN is full

0 = Transmit is complete, I2CxTRN is empty

Hardware is set when software writes to I2CxTRN. Hardware is clear at completion of the data transmission.

# UNIVERSAL ASYNCHRONOUS RECEIVER TRANSMITTER (UART)

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To complement the information in this data sheet, refer to **Section 21. “UART”** (DS61107) in the *“PIC32 Family Reference Manual”*, which is available from the Microchip web site ([www.microchip.com/](http://www.microchip.com/PIC32) [PIC32](http://www.microchip.com/PIC32)). The information in this data sheet supersedes the information in the FRM.

The UART module is one of the serial I/O modules available in the PIC32MM0256GPM064 family devices. The UART is a full-duplex, asynchronous communication channel that communicates with peripheral devices and personal computers through protocols, such as RS-232, RS-485, LIN/J2602 and IrDA®. The module also supports the hardware flow control option with the UxCTS and UxRTS pins, and

also includes an IrDA® encoder and decoder.

The primary features of the UART module are:

* Full-Duplex, 8-Bit or 9-Bit Data Transmission
* Even, Odd or No Parity Options (for 8-bit data)
* One or Two Stop Bits
* Hardware Auto-Baud Feature
* Hardware Flow Control Option
* Fully Integrated Baud Rate Generator (BRG) with 16-Bit Prescaler
* Baud rates ranging from 47.4 bps to 6.25 Mbps at 25 MHz
* 8-Level Deep First-In-First-Out (FIFO) Transmit Data Buffer
* 8-Level Deep FIFO Receive Data Buffer
* Parity, Framing and Buffer Overrun Error Detection
* Support for Interrupt Only on Address Detect (9th bit = 1)
* Separate Transmit and Receive Interrupts
* Loopback mode for Diagnostic Support
* LIN/J2602 Protocol Support
* IrDA Encoder and Decoder with 16x Baud Clock Output for External IrDA Encoder/Decoder Support
* Supports Separate UART Baud Clock Input
* Ability to Continue to Run when a Receive Overflow Condition Exists
* Ability to Run and rEceive Data during Sleep mode

[Figure 17-1](#_bookmark384) illustrates a simplified block diagram of the UART module.

FIGURE 17-1: UARTx SIMPLIFIED BLOCK DIAGRAM

PBCLK

Baud Rate Generator

IrDA®

Hardware Flow Control

UxRTS/BCLKx

UxCTS

UxRX

UARTx Transmitter

UxTX



UARTx Receiver

### UART Control Registers

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 176

TABLE 17-1: UART1, UART2 AND UART3 REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 1800 | U1MODE**(**[**1**](#_bookmark387)**)** | 31:16 | — | — | — | — | — | — | — | — | SLPEN | ACTIVE | — | — | — | CLKSEL<1:0> | | OVFDIS | 0000 |
| 15:0 | ON | — | SIDL | IREN | RTSMD | — | UEN<1:0> | | WAKE | LPBACK | ABAUD | RXINV | BRGH | PDSEL<1:0> | | STSEL | 0000 |
| 1810 | U1STA**(**[**1**](#_bookmark387)**)** | 31:16 | UART1 MASK<7:0> | | | | | | | | UART1 ADDR<7:0> | | | | | | | | 0000 |
| 15:0 | UTXISEL<1:0> | | UTXINV | URXEN | UTXBRK | UTXEN | UTXBF | TRMT | URXISEL<1:0> | | ADDEN | RIDLE | PERR | FERR | OERR | URXDA | 0110 |
| 1820 | U1TXREG | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | TX8 | UART1 Transmit Register | | | | | | | | 0000 |
| 1830 | U1RXREG | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | RX8 | UART1 Receive Register | | | | | | | | 0000 |
| 1840 | U1BRG**(**[**1**](#_bookmark387)**)** | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | Baud Rate Generator Prescaler | | | | | | | | | | | | | | | | 0000 |
| 1900 | U2MODE**(**[**1**](#_bookmark387)**)** | 31:16  15:0 | — | — | — | — | — | — | — | — | SLPEN | ACTIVE | — | — | — | CLKSEL<1:0> | | OVFDIS | 0000 |
| ON | — | SIDL | IREN | RTSMD | — | UEN<1:0> | | WAKE | LPBACK | ABAUD | RXINV | BRGH | PDSEL<1:0> | | STSEL | 0000 |
| 1910 | U2STA**(**[**1**](#_bookmark387)**)** | 31:16 | UART2 MASK<7:0> | | | | | | | | UART2 ADDR<7:0> | | | | | | | | 0000 |
| 15:0 | UTXISEL<1:0> | | UTXINV | URXEN | UTXBRK | UTXEN | UTXBF | TRMT | URXISEL<1:0> | | ADDEN | RIDLE | PERR | FERR | OERR | URXDA | 0110 |
| 1920 | U2TXREG | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | TX8 | UART2 Transmit Register | | | | | | | | 0000 |
| 1930 | U2RXREG | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | RX8 | UART2 Receive Register | | | | | | | | 0000 |
| 1940 | U2BRG**(**[**1**](#_bookmark387)**)** | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | Baud Rate Generator Prescaler | | | | | | | | | | | | | | | | 0000 |
| 2000 | U3MODE**(**[**1**](#_bookmark387)**)** | 31:16 | — | — | — | — | — | — | — | — | SLPEN | ACTIVE | — | — | — | CLKSEL<1:0> | | OVFDIS | 0000 |
| 15:0 | ON | — | SIDL | IREN | RTSMD | — | UEN<1:0> | | WAKE | LPBACK | ABAUD | RXINV | BRGH | PDSEL<1:0> | | STSEL | 0000 |
| 2010 | U3STA**(**[**1**](#_bookmark387)**)** | 31:16 | UART2 MASK<7:0> | | | | | | | | UART2 ADDR<7:0> | | | | | | | | 0000 |
| 15:0 | UTXISEL<1:0> | | UTXINV | URXEN | UTXBRK | UTXEN | UTXBF | TRMT | URXISEL<1:0> | | ADDEN | RIDLE | PERR | FERR | OERR | URXDA | 0110 |
| 2020 | U3TXREG | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | TX8 | UART2 Transmit Register | | | | | | | | 0000 |
| 2030 | U3RXREG | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | RX8 | UART2 Receive Register | | | | | | | | 0000 |
| 2040 | U3BRG**(**[**1**](#_bookmark387)**)** | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | Baud Rate Generator Prescaler | | | | | | | | | | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** These registers have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

REGISTER 17-1: UxMODE: UARTx MODE REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | R/W-0 | R/W-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 |
| SLPEN | ACTIVE | — | — | — | CLKSEL<1:0> | | OVFDIS |
| 15:8 | R/W-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | R/W-0 | R/W-0 |
| ON | — | SIDL | IREN | RTSMD | — | UEN<1:0>**(**[**1**](#_bookmark389)**)** | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| WAKE | LPBACK | ABAUD | RXINV | BRGH | PDSEL<1:0> | | STSEL |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-24 **Unimplemented:** Read as ‘0’

bit 23 **SLPEN:** UARTx Run During Sleep Enable bit

1 = UARTx clock runs during Sleep

0 = UARTx clock is turned off during Sleep bit 22 **ACTIVE:** UARTx Running Status bit

1 = UARTx is active (UxMODE register shouldn’t be updated)

0 = UARTx is not active (UxMODE register can be updated) bit 21-19 **Unimplemented:** Read as ‘0’

bit 18-17 **CLKSEL:** UARTx Clock Selection bits

11 = The UARTx clock is the Reference Output (REFO1) clock

10 = The UARTx clock is the FRC oscillator clock

01 = The UARTx clock is the SYSCLK

00 = The UARTx clock is the PBCLK

bit 16 **OVFDIS:** Run During Overflow Condition Mode bit

1 = When an Overflow Error (OERR) condition is detected, the shift register continues to run to remain synchronized

0 = When an Overflow Error (OERR) condition is detected, the shift register stops accepting new data (Legacy mode)

bit 15 **ON:** UARTx Enable bit

1 = UARTx is enabled; UARTx pins are controlled by UARTx, as defined by the UEN<1:0> and UTXEN control bits

0 = UARTx is disabled; all UARTx pins are controlled by the corresponding bits in the PORTx, TRISx and LATx registers, UARTx power consumption is minimal

bit 14 **Unimplemented:** Read as ‘0’

bit 13 **SIDL:** UARTx Stop in Idle Mode bit

1 = Discontinues operation when device enters Idle mode

0 = Continues operation in Idle mode

bit 12 **IREN:** IrDA® Encoder and Decoder Enable bit

1 = IrDA is enabled

0 = IrDA is disabled

**Note 1:** These bits are present for legacy compatibility and are superseded by PPS functionality on these devices (see [**Section 10.9 “Peripheral Pin Select (PPS)”**](#_bookmark262) for more information).

REGISTER 17-1: UxMODE: UARTx MODE REGISTER (CONTINUED)

bit 11 **RTSMD:** Mode Selection for UxRTS Pin bit

1 = UxRTS pin is in Simplex mode

0 = UxRTS pin is in Flow Control mode bit 10 **Unimplemented:** Read as ‘0’

bit 9-8 **UEN<1:0>:** UARTx Enable bits**(**[**1**](#_bookmark389)**)**

11 = UxTX, UxRX and UxBCLK pins are enabled and used; UxCTS pin is controlled by corresponding bits in the PORTx register

10 = UxTX, UxRX, UxCTS and UxRTS pins are enabled and used

01 = UxTX, UxRX and UxRTS pins are enabled and used; UxCTS pin is controlled by corresponding bits in the PORTx register

00 = UxTX and UxRX pins are enabled and used; UxCTS and UxRTS/UxBCLK pins are controlled by corresponding bits in the PORTx register

bit 7 **WAKE:** Enable Wake-up on Start bit Detect During Sleep Mode bit

1 = Wake-up is enabled

0 = Wake-up is disabled

bit 6 **LPBACK:** UARTx Loopback Mode Select bit

1 = Loopback mode is enabled

0 = Loopback mode is disabled bit 5 **ABAUD:** Auto-Baud Enable bit

1 = Enables baud rate measurement on the next character – requires reception of a Sync character (0x55); cleared by hardware upon completion

0 = Baud rate measurement is disabled or has completed bit 4 **RXINV:** Receive Polarity Inversion bit

1 = UxRX Idle state is ‘0’

0 = UxRX Idle state is ‘1’

bit 3 **BRGH:** High Baud Rate Enable bit

1 = High-Speed mode – 4x baud clock is enabled

0 = Standard Speed mode – 16x baud clock is enabled bit 2-1 **PDSEL<1:0>:** Parity and Data Selection bits

11 = 9-bit data, no parity 10 = 8-bit data, odd parity 01 = 8-bit data, even parity 00 = 8-bit data, no parity

bit 0 **STSEL:** Stop Selection bit

1 = 2 Stop bits

0 = 1 Stop bit

**Note 1:** These bits are present for legacy compatibility and are superseded by PPS functionality on these devices (see **Section 10.9 “Peripheral Pin Select (PPS)”** for more information).

REGISTER 17-2: UxSTA: UARTx STATUS AND CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| MASK<7:0> | | | | | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| ADDR<7:0> | | | | | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R-0 | R-1 |
| UTXISEL<1:0> | | UTXINV | URXEN | UTXBRK | UTXEN | UTXBF | TRMT |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R-1 | R-0 | R-0 | R/W-0 | R-0 |
| URXISEL<1:0> | | ADDEN | RIDLE | PERR | FERR | OERR | URXDA |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-24 **MASK<7:0>:** UARTx Address Match Mask bits Used to mask the ADDR<7:0> bits.

For MASK<x>:

1 = ADDR<x> is used to detect the address match

0 = ADDR<x> is not used to detect the address match bit 23-16 **ADDR<7:0>:** UARTx Automatic Address Mask bits

When the ADDEN bit is ‘1’, this value defines the address character to use for automatic address detection. bit 15-14 **UTXISEL<1:0>:** UARTx TX Interrupt Mode Selection bits

11 = Reserved, do not use

10 = Interrupt is generated and asserted while the transmit buffer is empty

01 = Interrupt is generated and asserted when all characters have been transmitted

00 = Interrupt is generated and asserted while the transmit buffer contains at least one empty space bit 13 **UTXINV:** UARTx Transmit Polarity Inversion bit

If IrDA mode is Disabled (i.e., IREN (UxMODE<12>) is ‘0’):

1 = UxTX Idle state is ‘0’

0 = UxTX Idle state is ‘1’

If IrDA mode is Enabled (i.e., IREN (UxMODE<12>) is ‘1’):

1 = IrDA® encoded UxTX Idle state is ‘1’

0 = IrDA encoded UxTX Idle state is ‘0’ bit 12 **URXEN:** UARTx Receiver Enable bit

1 = UARTx receiver is enabled, UxRX pin is controlled by UARTx (if ON = 1) 0 = UARTx receiver is disabled, UxRX pin is ignored by the UARTx module

bit 11 **UTXBRK:** UARTx Transmit Break bit

1 = Sends Break on next transmission; Start bit, followed by twelve ‘0’ bits, followed by Stop bit, cleared by hardware upon completion

0 = Break transmission is disabled or has completed bit 10 **UTXEN:** UARTx Transmit Enable bit

1 = UARTx transmitter is enabled, UxTX pin is controlled by UARTx (if ON = 1)

0 = UARTx transmitter is disabled, any pending transmission is aborted and the buffer is reset bit 9 **UTXBF:** UARTx Transmit Buffer Full Status bit (read-only)

1 = Transmit buffer is full

0 = Transmit buffer is not full, at least one more character can be written bit 8 **TRMT:** Transmit Shift Register (TSR) is Empty bit (read-only)

1 = Transmit Shift Register is empty and transmit buffer is empty (the last transmission has completed)

0 = Transmit Shift Register is not empty, a transmission is in progress or queued in the transmit buffer

REGISTER 17-2: UxSTA: UARTx STATUS AND CONTROL REGISTER (CONTINUED)

bit 7-6 **URXISEL<1:0>:** UARTx Receive Interrupt Mode Selection bits

11 = Reserved

10 = Interrupt flag bit is asserted while receive buffer is 3/4 or more full

01 = Interrupt flag bit is asserted while receive buffer is 1/2 or more full

00 = Interrupt flag bit is asserted while receive buffer is not empty (i.e., has at least 1 data character) bit 5 **ADDEN:** Address Character Detect bit (bit 8 of received data = 1)

1 = Address Detect mode is enabled; if 9-bit mode is not selected, this control bit has no effect

0 = Address Detect mode is disabled bit 4 **RIDLE:** Receiver Idle bit (read-only)

1 = Receiver is Idle

0 = Data is being received

bit 3 **PERR:** Parity Error Status bit (read-only)

1 = Parity error has been detected for the current character

0 = Parity error has not been detected

bit 2 **FERR:** Framing Error Status bit (read-only)

1 = Framing error has been detected for the current character

0 = Framing error has not been detected

bit 1 **OERR:** Receive Buffer Overrun Error Status bit

This bit is set in hardware and can only be cleared (= 0) in software. Clearing a previously set OERR bit resets the receiver buffer and RSR to the empty state.

1 = Receive buffer has overflowed

0 = Receive buffer has not overflowed

bit 0 **URXDA:** UARTx Receive Buffer Data Available bit (read-only)

1 = Receive buffer has data, at least one more character can be read

0 = Receive buffer is empty

# USB ON-THE-GO (OTG)

**Note 1:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To complement the information in this data sheet, refer to **Section 27. “USB On- The-Go (OTG)”** (DS61126) in the *“PIC32*

*Family Reference Manual”*, which is available from the Microchip web site ([www.microchip.com/PIC32](http://www.microchip.com/PIC32)).

**2:** Some registers and associated bits described in this section may not be available on all devices. Refer to **Section 4.0 “Memory Organization”** in this data sheet for device-specific register and bit information.

The Universal Serial Bus (USB) module contains analog and digital components to provide a USB 2.0 full-speed and low-speed embedded Host, full-speed Device or OTG implementation, with a minimum of external components. This module in Host mode is intended for use as an embedded host, and therefore, does not implement a UHCI or OHCI controller.

The USB module consists of the clock generator, the USB voltage comparators, the transceiver, the Serial Interface Engine (SIE), a dedicated USB DMA Control- ler, pull-up and pull-down resistors, and the register interface. A block diagram of the PIC32 USB OTG module is presented in [Figure 18-1](#_bookmark401).

### Reclaiming USB Pins When the USB Module is Operating

Select USB pins that are not used on all USB operating modes (USBID and VBUSON) can be reclaimed when the module is operating in a mode that does not require them. These pins can be reclaimed by clearing the appropriate device Configuration bit (refer to [Register 26-1](#_bookmark589)).

For example:

* USBID and VBUSON can be reclaimed in Device mode
* VBUSON can be reclaimed in Host mode if it is not used for the power VBUS control

### Reclaiming USB Pins When the USB Module is Disabled

All USB signaling pins, D+, D-, VBUS, VBUSON and USBID, can be reclaimed and used for GPIO or other peripherals if available on the pin when the USB module is disabled. For proper operation of the RB10 and RB11 pins, the USB module must be disabled, but powered. Refer to [**Section 18.1 “Reclaiming USB**](#_bookmark393)[**Pins When the USB Module is Operating”**](#_bookmark393) for more information.

### Introduction

The clock generator provides the 48 MHz clock required for USB full-speed and low-speed communi- cation. The voltage comparators monitor the voltage on the VBUS pin to determine the state of the bus. The transceiver provides the analog translation between the USB bus and the digital logic. The SIE is a state machine that transfers data to and from the endpoint buffers, and generates the hardware protocol for data transfers. The dedicated USB DMA Controller transfers data between the data buffers in RAM and the SIE. The integrated pull-up and pull-down resistors eliminate the need for external signaling components. The register interface allows the CPU to configure and communicate with the module.

The USB module includes the following features:

* USB Full-Speed Support for Host and Device
* Low-Speed Support for Host and Device
* USB OTG Support
* Integrated Signaling Resistors
* Integrated Analog Comparators for VBUS Monitoring
* Integrated USB Transceiver
* Transaction Handshaking performed by Hardware
* Endpoint Buffering anywhere in System RAM
* Integrated DMA to access System RAM and Flash

**Note:** The implementation and use of the USB specifications, as well as other third party specifications or technologies, may require licensing; including, but not limited to, USB Implementers Forum, Inc. (also referred to as USB-IF). The user is fully responsible for investigating and satisfying any applicable licensing obligations.

**Note:** Adding any circuitry to the USB D+/D- pins, other than the connection to a USB connector, may degrade the USB signal quality and violate USB specifications.

**PIC32MM0256GPM064 FAMILY**

### Powering the USB Transceiver

The VUSB3V3 pin is used to power the USB transceiver. During USB operation, this provides the power for USB transceiver drivers. When the USB module is disabled, this pin can be used to bias the transceiver circuit to prevent additional current draw when using RB10 and/or RB11 as GPIOs.

Available options for VUSB power:

1. For USB operation, an external power source is required. For voltage compliant USB operation, the voltage applied to VUSB3V3 must be in the range specified by Parameter [USB313](#_bookmark776) in [Table 29-38](#_bookmark774) regardless of the device operating voltage. If the device VDD voltage meets these requirements, it can be used to power VUSB3V3.
2. For non-USB operation with RB11 and/or RB10 as GPIOs, the USB module must be disabled and power applied to VUSB3V3 via VDD.
3. For non-USB operation without using RB11 and/or RB10, the VUSB3V3 pin should be connected to ground. This configuration has the lowest operating current.
   * 1. OPERATION OF PORT PINS SHARED WITH THE USB TRANSCEIVER

The USB transceiver shares pins with GPIO port pins. The D+ pin is shared with RB11 and the D- pin is shared with RB10. When the USB module is enabled, the pins are controlled by the module as D+ and D-, and are not usable as GPIOs. When the module is disabled, the pins can be used as RB11 and RB10 GPIOs if the VUSB3V3 pin is powered internally or externally. Refer to [**Section 18.4 “Powering the USB Transceiver”**](#_bookmark398)for more information.

**Note:** To prevent additional current draw, VUSB3V3 must either be powered or grounded.

FIGURE 18-1: PIC32MM0256GPM064 FAMILY USB INTERFACE DIAGRAM



OSC1



USBEN

USB Suspend

CPU Clock not POSC

Sleep

Primary Osc (POSC)

PLL = 96 MHz

Div 2

USB Suspend

To Clock Generator for Core and Peripherals Sleep or Idle

**USB Module**

SRP Charge

SRP Discharge

USB

Voltage Comparators

48 MHz USB Clock**(1)**

Full-Speed Pull-up

Host Pull-Down

Registers and Control Interface

SIE

Transceiver

Low-Speed Pull-up

DMA

System Memory

Host Pull-down

ID Pull-up

Transceiver Power 3.3V

|  |  |  |
| --- | --- | --- |
|  | |  |
| illator | FOUT  UFIN  PLL(5)  PLLMULT<6:0> | |

OSC2

VBUS/RB6**(2)**

D+/RB11**(3)**

D-/RB10**(3)**

USBID/RB5**(4)** VBUSON/RB14**(4)**

VUSB3V3

**Note 1:** A 48 MHz clock is required for proper USB operation.

**2:** This pin can be used as a GPIO when the USB module is disabled.

**3:** This pin can be used as a GPIO if the USB module is disabled and powered by an external source.

**4:** This pin is controlled by the USB module when the module is enabled in Host or OTG mode. If the module is dis- abled or enabled in a mode that does not require it, this pin can be reclaimed via a device Configuration bit (refer to [Register 26-1](#_bookmark589)).

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 184

**Name(1)**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF88\_#)** | **Register** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 8440 | U1OTGIR**(**[**2**](#_bookmark405)**)** | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | IDIF | T1MSECIF | LSTATEIF | ACTVIF | SESVDIF | SESENDIF | — | VBUSVDIF | 0000 |
| 8450 | U1OTGIE | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | IDIE | T1MSECIE | LSTATEIE | ACTVIE | SESVDIE | SESENDIE | — | VBUSVDIE | 0000 |
| 8460 | U1OTGSTAT**(**[**3**](#_bookmark406)**)** | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | ID | — | LSTATE | — | SESVD | SESEND | — | VBUSVD | 0000 |
| 8470 | U1OTGCON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | DPPULUP | DMPULUP | DPPULDWN | DMPULDWN | VBUSON | OTGEN | VBUSCHG | VBUSDIS | 0000 |
| 8480 | U1PWRC | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | UACTPND**(**[**4**](#_bookmark407)**)** | — | — | USLPGRD | USBBUSY | — | USUSPEND | USBPWR | 0000 |
| 8600 | U1IR**(**[**2**](#_bookmark405)**)** | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | STALLIF | ATTACHIF | RESUMEIF | IDLEIF | TRNIF | SOFIF | UERRIF | URSTIF | 0000 |
| DETACHIF | 0000 |
| 8610 | U1IE | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | STALLIE | ATTACHIE | RESUMEIE | IDLEIE | TRNIE | SOFIE | UERRIE | URSTIE | 0000 |
| DETACHIE | 0000 |
| 8620 | U1EIR**(**[**2**](#_bookmark405)**)** | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | BTSEF | BMXEF | DMAEF | BTOEF | DFN8EF | CRC16EF | CRC5EF | PIDEF | 0000 |
| EOFEF | 0000 |
| 8630 | U1EIE | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | BTSEE | BMXEE | DMAEE | BTOEE | DFN8EE | CRC16EE | CRC5EE | PIDEE | 0000 |
| EOFEE | 0000 |
| 8640 | U1STAT**(**[**3**](#_bookmark406)**)** | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | ENDPT<3:0>**(**[**4**](#_bookmark407)**)** | | | | DIR | PPBI | — | — | 0000 |
| 8650 | U1CON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | JSTATE**(**[**4**](#_bookmark407)**)** | SE0**(**[**4**](#_bookmark407)**)** | PKTDIS | USBRST | HOSTEN | RESUME | PPBRST | USBEN | 0000 |
| TOKBUSY | SOFEN | 0000 |
| 8660 | U1ADDR | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | LSPDEN | DEVADDR<6:0> | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table (except as noted) have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC respectively. See [**Section 10.1 “CLR, SET and INV Registers”**](#_bookmark250) for more information.

**2:** This register does not have associated SET and INV registers.

**3:** This register does not have associated CLR, SET and INV registers.

**4:** Reset value for these bits is undefined.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 185

TABLE 18-1: USB OTG REGISTER MAP (CONTINUED)

**Name(1)**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF88\_#)** | **Register** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 8670 | U1BDTP1 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | BDTPTRL<7:1> | | | | | | | — | 0000 |
| 8680 | U1FRML**(**[**3**](#_bookmark406)**)** | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | FRML<7:0> | | | | | | | | 0000 |
| 8690 | U1FRMH**(**[**3**](#_bookmark406)**)** | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | FRMH<2:0> | | | 0000 |
| 86A0 | U1TOK | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | PID<3:0> | | | | EP<3:0> | | | | 0000 |
| 86B0 | U1SOF | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | CNT<7:0> | | | | | | | | 0000 |
| 86C0 | U1BDTP2 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | BDTPTRH<7:0> | | | | | | | | 0000 |
| 86D0 | U1BDTP3 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | BDTPTRU<7:0> | | | | | | | | 0000 |
| 86E0 | U1CNFG1 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | UTEYE | UOEMON | — | USBSIDL | LSDEV | — | — | UASUSPND | 0001 |
| 8700 | U1EP0 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | LSPD | RETRYDIS | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 8710 | U1EP1 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 8720 | U1EP2 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 8730 | U1EP3 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 8740 | U1EP4 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 8750 | U1EP5 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 8760 | U1EP6 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table (except as noted) have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC respectively. See **Section 10.1 “CLR, SET and INV Registers”** for more information.

**2:** This register does not have associated SET and INV registers.

**3:** This register does not have associated CLR, SET and INV registers.

**4:** Reset value for these bits is undefined.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 186

**Name(1)**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF88\_#)** | **Register** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 8770 | U1EP7 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 8780 | U1EP8 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 8790 | U1EP9 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 87A0 | U1EP10 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 87B0 | U1EP11 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 87C0 | U1EP12 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 87D0 | U1EP13 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 87E0 | U1EP14 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |
| 87F0 | U1EP15 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table (except as noted) have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC respectively. See **Section 10.1 “CLR, SET and INV Registers”** for more information.

**2:** This register does not have associated SET and INV registers.

**3:** This register does not have associated CLR, SET and INV registers.

**4:** Reset value for these bits is undefined.

### Control Registers

REGISTER 18-1: U1OTGIR: USB OTG INTERRUPT STATUS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS | U-0 | R/WC-0, HS |
| IDIF | T1MSECIF | LSTATEIF | ACTVIF | SESVDIF | SESENDIF | — | VBUSVDIF |

|  |  |  |
| --- | --- | --- |
| **Legend:** | WC = Write ‘1’ to Clear bit | HS = Hardware Settable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7 **IDIF:** ID State Change Indicator bit

1 = Change in ID state is detected

0 = No change in ID state is detected bit 6 **T1MSECIF:** 1 Millisecond Timer bit

1 = 1 millisecond timer has expired

0 = 1 millisecond timer has not expired bit 5 **LSTATEIF:** Line State Stable Indicator bit

1 = USB line state has been stable for 1 ms, but different from last time

0 = USB line state has not been stable for 1 ms bit 4 **ACTVIF:** Bus Activity Indicator bit

1 = Activity on the D+, D-, ID or VBUS pins has caused the device to wake-up

0 = Activity has not been detected

bit 3 **SESVDIF:** Session Valid Change Indicator bit

1 = VBUS voltage has dropped below the session end level

0 = VBUS voltage has not dropped below the session end level bit 2 **SESENDIF:** B-Device VBUS Change Indicator bit

1 = Change on the session end input was detected

0 = No change on the session end input was detected bit 1 **Unimplemented:** Read as ‘0’

bit 0 **VBUSVDIF:** A-Device VBUS Change Indicator bit

1 = Change on the session valid input was detected

0 = No change on the session valid input was detected

REGISTER 18-2: U1OTGIE: USB OTG INTERRUPT ENABLE REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | R/W-0 |
| IDIE | T1MSECIE | LSTATEIE | ACTVIE | SESVDIE | SESENDIE | — | VBUSVDIE |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’ bit 7 **IDIE:** ID Interrupt Enable bit

1 = ID interrupt is enabled

0 = ID interrupt is disabled

bit 6 **T1MSECIE:** 1 Millisecond Timer Interrupt Enable bit

1 = 1 millisecond timer interrupt is enabled

0 = 1 millisecond timer interrupt is disabled bit 5 **LSTATEIE:** Line State Interrupt Enable bit

1 = Line state interrupt is enabled

0 = Line state interrupt is disabled

bit 4 **ACTVIE:** Bus Activity Interrupt Enable bit

1 = Activity interrupt is enabled

0 = Activity interrupt is disabled

bit 3 **SESVDIE:** Session Valid Interrupt Enable bit

1 = Session valid interrupt is enabled

0 = Session valid interrupt is disabled

bit 2 **SESENDIE:** B-Session End Interrupt Enable bit

1 = B-session end interrupt is enabled

0 = B-session end interrupt is disabled bit 1 **Unimplemented:** Read as ‘0’

bit 0 **VBUSVDIE:** A-VBUS Valid Interrupt Enable bit

1 = A-VBUS valid interrupt is enabled

0 = A-VBUS valid interrupt is disabled

REGISTER 18-3: U1OTGSTAT: USB OTG STATUS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R-0 | U-0 | R-0 | U-0 | R-0 | R-0 | U-0 | R-0 |
| ID | — | LSTATE | — | SESVD | SESEND | — | VBUSVD |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’ bit 7 **ID:** ID Pin State Indicator bit

1 = No cable is attached or a “Type B” cable has been inserted into the USB receptacle

0 = A “Type A” OTG cable has been inserted into the USB receptacle bit 6 **Unimplemented:** Read as ‘0’

bit 5 **LSTATE:** Line State Stable Indicator bit

1 = USB line state (SE0 (U1CON<6> and JSTATE (U1CON<7>) has been stable for the previous 1 ms

0 = USB line state (SE0 (U1CON<6> and JSTATE (U1CON<7>) has not been stable for the previous 1 ms bit 4 **Unimplemented:** Read as ‘0’

bit 3 **SESVD:** Session Valid Indicator bit

1 = The VBUS voltage is above VA\_SESS\_VLD (as defined in the USB OTG Specification) on the A or B-device

0 = The VBUS voltage is below VA\_SESS\_VLD on the A or B-device bit 2 **SESEND:** B-Device Session End Indicator bit

1 = The VBUS voltage is above VB\_SESS\_END (as defined in the USB OTG Specification) on the B-device

0 = The VBUS voltage is below VB\_SESS\_END on the B-device bit 1 **Unimplemented:** Read as ‘0’

bit 0 **VBUSVD:** A-Device VBUS Valid Indicator bit

1 = The VBUS voltage is above VA\_VBUS\_VLD (as defined in the USB OTG Specification) on the A-device

0 = The VBUS voltage is below VA\_VBUS\_VLD on the A-device

REGISTER 18-4: U1OTGCON: USB OTG CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| DPPULUP | DMPULUP | DPPULDWN | DMPULDWN | VBUSON | OTGEN | VBUSCHG | VBUSDIS |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7 **DPPULUP:** D+ Pull-Up Enable bit

1 = D+ data line pull-up resistor is enabled

0 = D+ data line pull-up resistor is disabled bit 6 **DMPULUP:** D- Pull-Up Enable bit

1 = D- data line pull-up resistor is enabled

0 = D- data line pull-up resistor is disabled bit 5 **DPPULDWN:** D+ Pull-Down Enable bit

1 = D+ data line pull-down resistor is enabled

0 = D+ data line pull-down resistor is disabled bit 4 **DMPULDWN:** D- Pull-Down Enable bit

1 = D- data line pull-down resistor is enabled

0 = D- data line pull-down resistor is disabled bit 3 **VBUSON:** VBUS Power-on bit

1 = VBUS line is powered

0 = VBUS line is not powered

bit 2 **OTGEN:** OTG Functionality Enable bit

1 = DPPULUP, DMPULUP, DPPULDWN and DMPULDWN bits are under software control

0 = DPPULUP, DMPULUP, DPPULDWN and DMPULDWN bits are under USB hardware control bit 1 **VBUSCHG:** VBUS Charge Enable bit

1 = VBUS line is charged through a pull-up resistor

0 = VBUS line is not charged through a resistor bit 0 **VBUSDIS:** VBUS Discharge Enable bit

1 = VBUS line is discharged through a pull-down resistor

0 = VBUS line is not discharged through a resistor

REGISTER 18-5: U1PWRC: USB POWER CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R-0 | U-0 | U-0 | R/W-0 | R/W-0 | U-0 | R/W-0 | R/W-0 |
| UACTPND | — | — | USLPGRD | USBBUSY**(**[**1**](#_bookmark414)**)** | — | USUSPEND | USBPWR**(**[**1**](#_bookmark414)**)** |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7 **UACTPND:** USB Activity Pending bit

1 = USB bus activity has been detected, but an interrupt is pending; it has not been generated yet

0 = An interrupt is not pending bit 6-5 **Unimplemented:** Read as ‘0’

bit 4 **USLPGRD:** USB Sleep Entry Guard bit

1 = Sleep entry is blocked if USB bus activity is detected or if a notification is pending

0 = USB module does not block Sleep entry bit 3 **USBBUSY:** USB Module Busy bit**(**[**1**](#_bookmark414)**)**

1 = USB module is active or disabled, but not ready to be enabled

0 = USB module is not active and is ready to be enabled bit 2 **Unimplemented:** Read as ‘0’

bit 1 **USUSPEND:** USB Suspend Mode bit

1 = USB module is placed in Suspend mode

(The 48 MHz USB clock will be gated off. The transceiver is placed in a low-power state.)

0 = USB module operates normally

bit 0 **USBPWR:** USB Operation Enable bit**(**[**1**](#_bookmark414)**)**

1 = USB module is turned on

0 = USB module is disabled

(Outputs held inactive, device pins not used by USB, analog features are shut down to reduce power consumption.)

**Note 1:** When USBPWR = 0 and USBBUSY = 1, status from all other registers is invalid and writes to all USB module registers produce undefined results.

REGISTER 18-6: U1IR: USB INTERRUPT REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS | R-0 | R/WC-0, HS |
| STALLIF | ATTACHIF**(**[**1**](#_bookmark416)**)** | RESUMEIF**(**[**2**](#_bookmark417)**)** | IDLEIF | TRNIF**(**[**3**](#_bookmark418)**)** | SOFIF | UERRIF**(**[**4**](#_bookmark419)**)** | URSTIF**(**[**5**](#_bookmark420)**)** |
| DETACHIF**(**[**6**](#_bookmark421)**)** |

|  |  |  |
| --- | --- | --- |
| **Legend:** | WC = Write ‘1’ to Clear bit | HS = Hardware Settable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7 **STALLIF:** Stall Handshake Interrupt bit

1 = In Host mode, a Stall handshake was received during the handshake phase of the transaction; in Device mode, a Stall handshake was transmitted during the handshake phase of the transaction

0 = Stall handshake has not been sent

bit 6 **ATTACHIF:** Peripheral Attach Interrupt bit**(**[**1**](#_bookmark416)**)**

1 = Peripheral attachment was detected by the USB module

0 = Peripheral attachment was not detected bit 5 **RESUMEIF:** Resume Interrupt bit**(**[**2**](#_bookmark417)**)**

1 = K-State is observed on the D+ or D- pin for 2.5 µs

0 = K-State is not observed

bit 4 **IDLEIF:** Idle Detect Interrupt bit

1 = Idle condition detected (constant Idle state of 3 ms or more)

0 = No Idle condition detected

bit 3 **TRNIF:** Token Processing Complete Interrupt bit**(**[**3**](#_bookmark418)**)**

1 = Processing of current token is complete; a read of the U1STAT register will provide endpoint information

0 = Processing of current token not complete bit 2 **SOFIF:** SOF Token Interrupt bit

1 = SOF token received by the peripheral or the SOF threshold reached by the host

0 = SOF token was not received nor threshold reached bit 1 **UERRIF**: USB Error Condition Interrupt bit**(**[**4**](#_bookmark419)**)**

1 = Unmasked error condition has occurred

0 = Unmasked error condition has not occurred

**Note 1:** This bit is only valid if the HOSTEN bit is set (see [Register 18-11](#_bookmark437)), there is no activity on the USB for 2.5 µs and the current bus state is not SE0.

**2:** When not in Suspend mode, this interrupt should be disabled.

**3:** Clearing this bit will cause the STAT FIFO to advance.

**4:** Only error conditions enabled through the U1EIE register will set this bit.

**5:** Device mode.

**6:** Host mode.

REGISTER 18-6: U1IR: USB INTERRUPT REGISTER (CONTINUED)

bit 0 **URSTIF:** USB Reset Interrupt bit (Device mode)**(**[**5**](#_bookmark420)**)**

1 = Valid USB Reset has occurred

0 = No USB Reset has occurred

**DETACHIF:** USB Detach Interrupt bit (Host mode)**(**[**6**](#_bookmark421)**)**

1 = Peripheral detachment was detected by the USB module

0 = Peripheral detachment was not detected

**Note 1:** This bit is only valid if the HOSTEN bit is set (see Register 18-11), there is no activity on the USB for 2.5 µs and the current bus state is not SE0.

**2:** When not in Suspend mode, this interrupt should be disabled.

**3:** Clearing this bit will cause the STAT FIFO to advance.

**4:** Only error conditions enabled through the U1EIE register will set this bit.

**5:** Device mode.

**6:** Host mode.

REGISTER 18-7: U1IE: USB INTERRUPT ENABLE REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| STALLIE | ATTACHIE | RESUMEIE | IDLEIE | TRNIE | SOFIE | UERRIE**(**[**1**](#_bookmark423)**)** | URSTIE**(**[**2**](#_bookmark424)**)** |
| DETACHIE**(**[**3**](#_bookmark425)**)** |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7 **STALLIE:** Stall Handshake Interrupt Enable bit

1 = Stall interrupt is enabled

0 = Stall interrupt is disabled

bit 6 **ATTACHIE:** Attach Interrupt Enable bit

1 = Attach interrupt is enabled

0 = Attach interrupt is disabled

bit 5 **RESUMEIE:** Resume Interrupt Enable bit

1 = Resume interrupt is enabled

0 = Resume interrupt is disabled

bit 4 **IDLEIE:** Idle Detect Interrupt Enable bit

1 = Idle interrupt is enabled

0 = Idle interrupt is disabled

bit 3 **TRNIE:** Token Processing Complete Interrupt Enable bit

1 = TRNIF interrupt is enabled

0 = TRNIF interrupt is disabled

bit 2 **SOFIE:** SOF Token Interrupt Enable bit

1 = SOFIF interrupt is enabled

0 = SOFIF interrupt is disabled

bit 1 **UERRIE:** USB Error Interrupt Enable bit**(**[**1**](#_bookmark423)**)**

1 = USB error interrupt is enabled

0 = USB error interrupt is disabled

bit 0 **URSTIE:** USB Reset Interrupt Enable bit**(**[**2**](#_bookmark424)**)**

1 = URSTIF interrupt is enabled

0 = URSTIF interrupt is disabled

**DETACHIE:** USB Detach Interrupt Enable bit**(**[**3**](#_bookmark425)**)**

1 = DATTCHIF interrupt is enabled

0 = DATTCHIF interrupt is disabled

**Note 1:** For an interrupt to propagate USBIF, the UERRIE bit (U1IE<1>) must be set.

**2:** Device mode.

**3:** Host mode.

REGISTER 18-8: U1EIR: USB ERROR INTERRUPT STATUS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS | R/WC-0, HS |
| BTSEF | BMXEF | DMAEF**(**[**1**](#_bookmark427)**)** | BTOEF**(**[**2**](#_bookmark428)**)** | DFN8EF | CRC16EF | CRC5EF**(**[**4**](#_bookmark430)**)** | PIDEF |
| EOFEF**(**[**3**](#_bookmark429)**,**[**5**](#_bookmark431)**)** |

|  |  |  |
| --- | --- | --- |
| **Legend:** | WC = Write ‘1’ to Clear bit | HS = Hardware Settable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’ bit 7 **BTSEF:** Bit Stuff Error Flag bit

1 = Packet rejected due to bit stuff error

0 = Packet accepted

bit 6 **BMXEF:** Bus Matrix Error Flag bit

1 = Invalid base address of the BDT or the address of an individual buffer pointed to by a BDT entry

0 = No address error

bit 5 **DMAEF:** DMA Error Flag bit**(**[**1**](#_bookmark427)**)**

1 = USB DMA error condition detected

0 = No DMA error

bit 4 **BTOEF:** Bus Turnaround Time-out Error Flag bit**(**[**2**](#_bookmark428)**)**

1 = Bus turnaround time-out has occurred

0 = No bus turnaround time-out has occurred bit 3 **DFN8EF:** Data Field Size Error Flag bit

1 = Data field received is not an integral number of bytes

0 = Data field received is an integral number of bytes bit 2 **CRC16EF:** CRC16 Failure Flag bit

1 = Data packet rejected due to CRC16 error

0 = Data packet accepted

**Note 1:** This type of error occurs when the module’s request for the DMA bus is not granted in time to service the module’s demand for memory, resulting in an overflow or underflow condition, and/or the allocated buffer size is not sufficient to store the received data packet causing it to be truncated.

**2:** This type of error occurs when more than 16-bit times of Idle from the previous End-of-Packet (EOP) has elapsed.

**3:** This type of error occurs when the module is transmitting or receiving data and the SOF counter has reached zero.

**4:** Device mode.

**5:** Host mode.

REGISTER 18-8: U1EIR: USB ERROR INTERRUPT STATUS REGISTER (CONTINUED)

bit 1 **CRC5EF:** CRC5 Host Error Flag bit**(**[**4**](#_bookmark430)**)**

1 = Token packet rejected due to CRC5 error

0 = Token packet accepted

**EOFEF:** EOF Error Flag bit**(**[**3**](#_bookmark429)**,**[**5**](#_bookmark431)**)**

1 = EOF error condition detected

0 = No EOF error condition

bit 0 **PIDEF:** PID Check Failure Flag bit

1 = PID check failed

0 = PID check passed

**Note 1:** This type of error occurs when the module’s request for the DMA bus is not granted in time to service the module’s demand for memory, resulting in an overflow or underflow condition, and/or the allocated buffer size is not sufficient to store the received data packet causing it to be truncated.

**2:** This type of error occurs when more than 16-bit times of Idle from the previous End-of-Packet (EOP) has elapsed.

**3:** This type of error occurs when the module is transmitting or receiving data and the SOF counter has reached zero.

**4:** Device mode.

**5:** Host mode.

REGISTER 18-9: U1EIE: USB ERROR INTERRUPT ENABLE REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| BTSEE | BMXEE | DMAEE | BTOEE | DFN8EE | CRC16EE | CRC5EE**(**[**1**](#_bookmark433)**)** | PIDEE |
| EOFEE**(**[**2**](#_bookmark434)**)** |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7 **BTSEE:** Bit Stuff Error Interrupt Enable bit

1 = BTSEF interrupt is enabled

0 = BTSEF interrupt is disabled

bit 6 **BMXEE:** Bus Matrix Error Interrupt Enable bit

1 = BMXEF interrupt is enabled

0 = BMXEF interrupt is disabled

bit 5 **DMAEE:** DMA Error Interrupt Enable bit

1 = DMAEF interrupt is enabled

0 = DMAEF interrupt is disabled

bit 4 **BTOEE:** Bus Turnaround Time-out Error Interrupt Enable bit

1 = BTOEF interrupt is enabled

0 = BTOEF interrupt is disabled

bit 3 **DFN8EE:** Data Field Size Error Interrupt Enable bit

1 = DFN8EF interrupt is enabled

0 = DFN8EF interrupt is disabled

bit 2 **CRC16EE:** CRC16 Failure Interrupt Enable bit

1 = CRC16EF interrupt is enabled

0 = CRC16EF interrupt is disabled

bit 1 **CRC5EE:** CRC5 Host Error Interrupt Enable bit**(**[**1**](#_bookmark433)**)**

1 = CRC5EF interrupt is enabled

0 = CRC5EF interrupt is disabled **EOFEE:** EOF Error Interrupt Enable bit**(**[**2**](#_bookmark434)**)** 1 = EOF interrupt is enabled

0 = EOF interrupt is disabled

bit 0 **PIDEE:** PID Check Failure Interrupt Enable bit

1 = PIDEF interrupt is enabled

0 = PIDEF interrupt is disabled

**Note 1:** Device mode.

**2:** Host mode.

REGISTER 18-10: U1STAT: USB STATUS REGISTER([1](#_bookmark436))

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R-x | R-x | R-x | R-x | R-x | R-x | U-0 | U-0 |
| ENDPT<3:0> | | | | DIR | PPBI | — | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7-4 **ENDPT<3:0>:** Encoded Number of Last Endpoint Activity bits (Represents the number of the BDT, updated by the last USB transfer.) 1111 = Endpoint 15

1110 = Endpoint 14

•

•

•

0001 = Endpoint 1

0000 = Endpoint 0

bit 3 **DIR:** Last Buffer Descriptor Direction Indicator bit

1 = Last transaction was a transmit transfer (TX)

0 = Last transaction was a receive transfer (RX)

bit 2 **PPBI:** Ping-Pong Buffer Descriptor Pointer Indicator bit

1 = Last transaction was to the Odd buffer descriptor bank

0 = Last transaction was to the Even buffer descriptor bank bit 1-0 **Unimplemented:** Read as ‘0’

**Note 1:** The U1STAT register is a window into a 4-byte FIFO maintained by the USB module. The U1STAT value is only valid when TRNIF (U1IR<3>)> is active. Clearing the TRNIF bit advances the FIFO. The data in the register is invalid when TRNIF = 0.

REGISTER 18-11: U1CON: USB CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R-x | R-x | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| JSTATE | SE0 | PKTDIS**(**[**4**](#_bookmark442)**)** | USBRST | HOSTEN**(**[**2**](#_bookmark440)**)** | RESUME**(**[**3**](#_bookmark441)**)** | PPBRST | USBEN**(**[**4**](#_bookmark442)**)** |
| TOKBUSY**(**[**1**](#_bookmark439)**,**[**5**](#_bookmark443)**)** | SOFEN**(**[**5**](#_bookmark443)**)** |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7 **JSTATE:** Live Differential Receiver JSTATE Flag bit

1 = JSTATE was detected on the USB

0 = JSTATE was not detected

bit 6 **SE0:** Live Single-Ended Zero Flag bit

1 = Single-ended zero was detected on the USB

0 = Single-ended zero was not detected bit 5 **PKTDIS:** Packet Transfer Disable bit**(**[**4**](#_bookmark442)**)**

1 = Token and packet processing are disabled (set upon SETUP token received)

0 = Token and packet processing are enabled

**TOKBUSY:** Token Busy Indicator bit**(**[**1**](#_bookmark439)**,**[**5**](#_bookmark443)**)**

1 = Token is being executed by the USB module

0 = No token is being executed bit 4 **USBRST:** Module Reset bit

1 = USB Reset is generated

0 = USB Reset is terminated

bit 3 **HOSTEN:** Host Mode Enable bit**(**[**2**](#_bookmark440)**)**

1 = USB host capability is enabled

0 = USB host capability is disabled

bit 2 **RESUME:** Resume Signaling Enable bit**(**[**3**](#_bookmark441)**)**

1 = Resume signaling is activated

0 = Resume signaling is disabled

**Note 1:** Software is required to check this bit before issuing another token command to the U1TOK register (see [Register 18-15](#_bookmark447)).

**2:** All host control logic is reset any time that the value of this bit is toggled.

**3:** Software must set RESUME for 10 ms in Device mode, or for 25 ms in Host mode, and then clear it to enable remote wake-up. In Host mode, the USB module will append a low-speed EOP to the Resume signaling when this bit is cleared.

**4:** Device mode.

**5:** Host mode.

REGISTER 18-11: U1CON: USB CONTROL REGISTER (CONTINUED)

bit 1 **PPBRST:** Ping-Pong Buffers Reset bit

1 = Resets all Even/Odd Buffer Pointers to the Even buffer descriptor banks

0 = Even/Odd Buffer Pointers are not reset bit 0 **USBEN:** USB Module Enable bit**(**[**4**](#_bookmark442)**)**

1 = USB module and supporting circuitry are enabled

0 = USB module and supporting circuitry are disabled

**SOFEN:** SOF Enable bit**(**[**5**](#_bookmark443)**)**

1 = SOF token is sent every 1 ms

0 = SOF token is disabled

**Note 1:** Software is required to check this bit before issuing another token command to the U1TOK register (see Register 18-15).

**2:** All host control logic is reset any time that the value of this bit is toggled.

**3:** Software must set RESUME for 10 ms in Device mode, or for 25 ms in Host mode, and then clear it to enable remote wake-up. In Host mode, the USB module will append a low-speed EOP to the Resume signaling when this bit is cleared.

**4:** Device mode.

**5:** Host mode.

REGISTER 18-12: U1ADDR: USB ADDRESS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| LSPDEN | DEVADDR<6:0> | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7 **LSPDEN:** Low-Speed Enable Indicator bit

1 = Next token command to be executed at low speed

0 = Next token command to be executed at full speed bit 6-0 **DEVADDR<6:0>:** 7-Bit USB Device Address bits

REGISTER 18-13: U1FRML: USB FRAME NUMBER LOW REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 | R-0 |
| FRML<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7-0 **FRML<7:0>:** 11-Bit Frame Number Lower bits

These register bits are updated with the current frame number whenever a SOF token is received.

REGISTER 18-14: U1FRMH: USB FRAME NUMBER HIGH REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | U-0 | U-0 | U-0 | U-0 | U-0 | R-0 | R-0 | R-0 |
| — | — | — | — | — | FRMH<2:0> | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-3 **Unimplemented:** Read as ‘0’

bit 2-0 **FRMH<2:0>:** Upper 3 Bits of the Frame Numbers bits

These register bits are updated with the current frame number whenever a SOF token is received.

REGISTER 18-15: U1TOK: USB TOKEN REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| PID<3:0>**(**[**1**](#_bookmark449)**)** | | | | EP<3:0> | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7-4 **PID<3:0>:** Token Type Indicator bits**(**[**1**](#_bookmark449)**)**

1101 = SETUP (TX) token type transaction 1001 = IN (RX) token type transaction 0001 = OUT (TX) token type transaction

bit 3-0 **EP<3:0>:** Token Command Endpoint Address bits The 4-bit value must specify a valid endpoint.

**Note 1:** All other values not listed are reserved and must not be used.

REGISTER 18-16: U1SOF: USB SOF THRESHOLD REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CNT<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7-0 **CNT<7:0>:** SOF Threshold Value bits Typical Values of the Threshold are:

01001010 = 64-byte packet

00101010 = 32-byte packet 00011010 = 16-byte packet 00010010 = 8-byte packet

REGISTER 18-17: U1BDTP1: USB BUFFER DESCRIPTOR TABLE PAGE 1 REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | U-0 |
| BDTPTRL<7:1> | | | | | | | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7-1 **BDTPTRL<7:1>:** BDT Base Address bits

This 7-bit value provides Address bits 7 through 1 of the BDT base address, which defines the starting location of the BDT in system memory.

The 32-bit BDT base address is 512-byte aligned. bit 0 **Unimplemented:** Read as ‘0’

REGISTER 18-18: U1BDTP2: USB BUFFER DESCRIPTOR TABLE PAGE 2 REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| BDTPTRH<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7-0 **BDTPTRH<7:0>:** BDT Base Address bits

This 8-bit value provides Address bits 7 through 0 of the BDT base address, which defines the starting location of the BDT in system memory.

The 32-bit BDT base address is 512-byte aligned.

REGISTER 18-19: U1BDTP3: USB BUFFER DESCRIPTOR TABLE PAGE 3 REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| BDTPTRU<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7-0 **BDTPTRU<7:0>:** BDT Base Address bits

This 8-bit value provides Address bits 7 through 0 of the BDT base address, defines the starting location of the BDT in system memory.

The 32-bit BDT base address is 512-byte aligned.

REGISTER 18-20: U1CNFG1: USB CONFIGURATION 1 REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | U-0 | R/W-0 | R/W-0 | U-0 | U-0 | R/W-0 |
| UTEYE | UOEMON | — | USBSIDL | LSDEV | — | — | UASUSPND |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7 **UTEYE:** USB Eye Pattern Test Enable bit

1 = Eye pattern test is enabled

0 = Eye pattern test is disabled

bit 6 **UOEMON:** USB OE Monitor Enable bit

1 = OE signal is active; it indicates intervals during which the D+/D- lines are driving

0 = OE signal is inactive

bit 5 **Unimplemented:** Read as ‘0’

bit 4 **USBSIDL:** USB Stop in Idle Mode bit

1 = Discontinues module operation when device enters Idle mode

0 = Continues module operation in Idle mode bit 3 **LSDEV:** USB Low-Speed Device Enable bit

1 = USB macro operates in Low-Speed Device Only mode

0 = USB macro operates in OTG, Host or Fast Speed Device mode bit 2-1 **Unimplemented:** Read as ‘0’

bit 0 **UASUSPND:** Automatic Suspend Enable bit

1 = USB module automatically suspends upon entry to Sleep mode; see the USUSPEND bit (U1PWRC<1>) in [Register 18-5](#_bookmark412)

0 = USB module does not automatically suspend upon entry to Sleep mode; software must use the USUSPEND bit (U1PWRC<1>) to suspend the module, including the USB 48 MHz clock

REGISTER 18-21: U1EP0-U1EP15: USB ENDPOINT CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| LSPD | RETRYDIS | — | EPCONDIS | EPRXEN | EPTXEN | EPSTALL | EPHSHK |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7 **LSPD:** Low-Speed Direct Connection Enable bit (Host mode and U1EP0 only)

1 = Direct connection to a low-speed device is enabled

0 = Direct connection to a low-speed device is disabled; hub required with PRE\_PID bit 6 **RETRYDIS:** Retry Disable bit (Host mode and U1EP0 only)

1 = Retry NACK’d transactions are disabled

0 = Retry NACK’d transactions are enabled; retry done in hardware bit 5 **Unimplemented:** Read as ‘0’

bit 4 **EPCONDIS:** Bidirectional Endpoint Control bit If EPTXEN = 1 and EPRXEN = 1:

1 = Disables Endpoint n from control transfers; only TX and RX transfers are allowed

0 = Enables Endpoint n for control (SETUP) transfers; TX and RX transfers are also allowed Otherwise, this bit is ignored.

bit 3 **EPRXEN:** Endpoint Receive Enable bit

1 = Endpoint n receive is enabled

0 = Endpoint n receive is disabled

bit 2 **EPTXEN:** Endpoint Transmit Enable bit

1 = Endpoint n transmit is enabled

0 = Endpoint n transmit is disabled bit 1 **EPSTALL:** Endpoint Stall Status bit

1 = Endpoint n was stalled

0 = Endpoint n was not stalled

bit 0 **EPHSHK:** Endpoint Handshake Enable bit

1 = Endpoint handshake is enabled

0 = Endpoint handshake is disabled (typically used for isochronous endpoints)

NOTES:

# REAL-TIME CLOCK AND CALENDAR (RTCC)

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To complement the information in this data sheet, refer to **Section 28. “RTCC with Timestamp”** (DS60001362) in the *“PIC32 Family Reference Manual”*[,](http://www.microchip.com/PIC32) [which is available from the Microchip](http://www.microchip.com/PIC32) [web site (](http://www.microchip.com/PIC32)[www.microchip.com/PIC32).](http://www.microchip.com/PIC32)) The information in this data sheet supersedes the information in the FRM.

The RTCC module is intended for applications in which accurate time must be maintained for extended periods of time with minimal or no CPU intervention. Low- power optimization provides extended battery lifetime while keeping track of time.

FIGURE 19-1: RTCC BLOCK DIAGRAM



CLKSEL<1:0>

PWRLCLK Input Pin

Peripheral Clock (PBCLK) 32.768 kHz Input from

Secondary Oscillator (SOSC)

32 kHz Input from Internal Oscillator (LPRC)

TRTC

0.5 seconds

Alarm Event

RTCC Interrupt Logic

RTCC Interrupt Alarm Pulse

Seconds Pulse

RTCC Pin**(**[**1**](#_bookmark460)**)**

TRTC

RTCOE

OUTSEL<2:0>

**Note 1:** In Retention mode, the maximum peripheral output frequency to an I/O pin must be limited to 33 kHz or less.

RTCC Prescalers

Repeat Counter

ALRMVAL

RTCVAL

Key features of the RTCC module are:

* + - * Time: Hours, Minutes and Seconds
      * 24-Hour Format (military time)
      * Visibility of One-Half Second Period
      * Provides Calendar: Weekday, Date, Month and Year
      * Alarm Intervals are Configurable for Half of a Second, 1 Second, 10 Seconds, 1 Minute, 10 Minutes, 1 Hour, 1 Day, 1 Week, 1 Month and 1 Year
      * Alarm Repeat with Decrementing Counter
      * Alarm with Indefinite Repeat: Chime
      * Year Range: 2000 to 2099
      * Leap Year Correction
      * BCD Format for Smaller Firmware Overhead
      * Optimized for Long-Term Battery Operation
      * Fractional Second Synchronization
      * User Calibration of the Clock Crystal Frequency with Auto-Adjust
      * Uses External 32.768 kHz Crystal, 32 kHz Internal Oscillator, PWRLCLK Input Pin or Peripheral Clock
      * Alarm Pulse, Seconds Clock or Internal Clock Output on RTCC Pin



Comparator

Compare Registers with Masks



RTCC Timer

|  |  |
| --- | --- |
|  | YEAR, MTH, DAY |
|  | WKDAY |
|  | HR, MIN, SEC |

|  |  |
| --- | --- |
|  | MTH, DAY |
|  | WKDAY |
|  | HR, MIN, SEC |

### RTCC Control Registers

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 210

TABLE 19-1: RTCC REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 0000 | RTCCON1 | 31:16 | ALRMEN | CHIME | — | — | AMASK<3:0> | | | | ALMRPT<7:0> | | | | | | | | 0000 |
| 15:0 | ON | — | — | — | WRLOCK | — | — | — | RTCOE | OUTSEL<2:0> | | | — | — | — | — | 0000 |
| 0010 | RTCCON2 | 31:16 | DIV<15:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | FDIV<4:0> | | | | | — | — | — | — | — | PS<1:0> | | — | — | CLKSEL<1:0> | | 0000 |
| 0030 | RTCSTAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | ALMEVT | — | — | SYNC | ALMSYNC | HALFSEC | 0000 |
| 0040 | RTCTIME | 31:16 | — | HRTEN<2:0> | | | HRONE<3:0> | | | | — | MINTEN<2:0> | | | MINONE<3:0> | | | | xxxx |
| 15:0 | SECTEN<3:0> | | | | SECONE<3:0> | | | | — | — | — | — | — | — | — | — | xx00 |
| 0050 | RTCDATE | 31:16 | YRTEN<3:0> | | | | YRONE<3:0> | | | | — | — | — | MTHTEN | MTHONE<3:0> | | | | 0000 |
| 15:0 | — | — | DAYTEN<1:0> | | DAYONE<3:0> | | | | — | — | — | — | — | WDAY<2:0> | | | 0000 |
| 0060 | ALMTIME | 31:16 | — | HRTEN<2:0> | | | HRONE<3:0> | | | | — | MINTEN<2:0> | | | MINONE<3:0> | | | | xxxx |
| 15:0 | SECTEN<3:0> | | | | SECONE<3:0> | | | | — | — | — | — | — | — | — | — | xx00 |
| 0070 | ALMDATE | 31:16 | — | — | — | — | — | — | — | — | — | — | — | MTHTEN | MTHONE<3:0> | | | | 0000 |
| 15:0 | — | — | DAYTEN<1:0> | | DAYONE<3:0> | | | | — | — | — | — | — | WDAY<2:0> | | | 0000 |

**Legend:** x = unknown value on Reset; — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

REGISTER 19-1: RTCCON1: RTCC CONTROL 1 REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| ALRMEN | CHIME | — | — | AMASK<3:0> | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| ALMRPT<7:0>**(**[**1**](#_bookmark465)**)** | | | | | | | |
| 15:8 | R/W-0 | U-0 | U-0 | U-0 | R/W-0 | U-0 | U-0 | U-0 |
| ON | — | — | — | WRLOCK | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | U-0 | U-0 | U-0 |
| RTCOE | OUTSEL<2:0> | | | — | — | — | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **ALRMEN:** Alarm Enable bit

1 = Alarm is enabled

0 = Alarm is disabled

bit 30 **CHIME:** Chime Enable bit

1 = Chime is enabled; ALMRPT<7:0> bits are allowed to underflow from ‘00’ to ‘FF’

0 = Chime is disabled; ALMRPT<7:0> bits stop once they reach ‘00’ bit 29-28 **Unimplemented:** Read as ‘0’

bit 27-24 **AMASK<3:0>:** Alarm Mask Configuration bits

11xx = Reserved, do not use

101x = Reserved, do not use

1001 = Once a year (or once every 4 years when configured for February 29th)

1000 = Once a month 0111 = Once a week 0110 = Once a day 0101 = Every hour

0100 = Every 10 minutes 0011 = Every minute 0010 = Every 10 seconds 0001 = Every second 0000 = Every half-second

bit 23-16 **ALMRPT<7:0>:** Alarm Repeat Counter Value bits**(**[**1**](#_bookmark465)**)**

11111111 = Alarm will repeat 255 more times

11111110 = Alarm will repeat 254 more times

• • •

00000010 = Alarm will repeat 2 more times 00000001 = Alarm will repeat 1 more time 00000000 = Alarm will not repeat

bit 15 **ON:** RTCC Enable bit

1 = RTCC is enabled and counts from selected clock source

0 = RTCC is disabled

bit 14-12 **Unimplemented:** Read as ‘0’

**Note 1:** The counter decrements on any alarm event. The counter is prevented from rolling over from ‘00’ to ‘FF’ unless CHIME = 1.

REGISTER 19-1: RTCCON1: RTCC CONTROL 1 REGISTER (CONTINUED)

bit 11 **WRLOCK:** RTCC Registers Write Lock bit

1 = Registers associated with accurate timekeeping are locked

0 = Registers associated with accurate timekeeping may be written to by user bit 10-8 **Unimplemented:** Read as ‘0’

bit 7 **RTCOE:** RTCC Output Enable bit

1 = RTCC clock output is enabled; signal selected by OUTSEL<2:0> is presented on the RTCC pin

0 = RTCC clock output is disabled

bit 6-4 **OUTSEL<2:0>:** RTCC Signal Output Selection bits

111 = Reserved

• • •

011 = Reserved

010 = RTCC input clock source (user-defined divided output based on the combination of the RTCCON2 bits, DIV<15:0> and PS<1:0>)

001 = Seconds clock

000 = Alarm event

bit 3-0 **Unimplemented:** Read as ‘0’

**Note 1:** The counter decrements on any alarm event. The counter is prevented from rolling over from ‘00’ to ‘FF’ unless CHIME = 1.

REGISTER 19-2: RTCCON2: RTCC CONTROL 2 REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| DIV<15:8> | | | | | | | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| DIV<7:0> | | | | | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | U-0 | U-0 |
| FDIV<4:0> | | | | | — | — | — |
| 7:0 | U-0 | U-0 | R/W-0 | R/W-0 | U-0 | U-0 | R/W-0 | R/W-0 |
| — | — | PS<1:0> | | — | — | CLKSEL<1:0> | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **DIV<15:0>:** Clock Divide bits

Sets the period of the clock divider counter for the seconds output. bit 15-11 **FDIV<4:0>:** Fractional Clock Divide bits

11111 = Clock period increases by 31 RTCC input clock cycles every 16 seconds

11101 = Clock period increases by 30 RTCC input clock cycles every 16 seconds

• • •

00010 = Clock period increases by 2 RTCC input clock cycles every 16 seconds 00001 = Clock period increases by 1 RTCC input clock cycle every 16 seconds 00000 = No fractional clock division

bit 10-6 **Unimplemented:** Read as ‘0’ bit 5-4 **PS<1:0>:** Prescale Select bits

Sets the prescaler for the seconds output.

11 = 1:256

10 = 1:64

01 = 1:16

00 = 1:1

bit 3-2 **Unimplemented:** Read as ‘0’

bit 1-0 **CLKSEL<1:0>:** Clock Select bits

11 = Peripheral clock (FCY) 10 = PWRLCLK input pin 01 = LPRC

00 = SOSC

REGISTER 19-3: RTCSTAT: RTCC STATUS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | U-0 | U-0 | R-0, HS, HC | U-0 | U-0 | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC |
| — | — | ALMEVT | — | — | SYNC | ALMSYNC | HALFSEC |

|  |  |  |
| --- | --- | --- |
| **Legend:** | HC = Hardware Clearable bit | HS = Hardware Settable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-6 **Unimplemented:** Read as ‘0’ bit 5 **ALMEVT:** Alarm Event bit

1 = An alarm event has occurred

0 = An alarm event has not occurred bit 4-3 **Unimplemented:** Read as ‘0’

bit 2 **SYNC:** Synchronization Status bit

1 = Time registers may change during software read

0 = Time registers may be read safely

bit 1 **ALMSYNC:** Alarm Synchronization Status bit

1 = Alarm registers (ALMTIME and ALMDATE) and RTCCON1 should not be modified; the ALRMEN and ALMRPT<7:0> bits may change during software read

0 = Alarm registers and Alarm Control registers may be modified safely bit 0 **HALFSEC:** Half-Second Status bit

1 = Second half of 1-second period

0 = First half of 1-second period

REGISTER 19-4: RTCTIME/ALMTIME: RTCC TIME/ALARM REGISTERS

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | HRTEN<2:0> | | | HRONE<3:0> | | | |
| 23:16 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | MINTEN<2:0> | | | MINONE<3:0> | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| SECTEN<3:0> | | | | SECONE<3:0> | | | |
| 7:0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **Unimplemented:** Read as ‘0’

bit 30-28 **HRTEN<2:0>:** Binary Coded Decimal Value of Hours 10-Digit bits Contains a value from 0 to 2.

bit 27-24 **HRONE<3:0>:** Binary Coded Decimal Value of Hours 1-Digit bits Contains a value from 0 to 9.

bit 23 **Unimplemented:** Read as ‘0’

bit 22-20 **MINTEN<2:0>:** Binary Coded Decimal Value of Minutes 10-Digit bits Contains a value from 0 to 5.

bit 19-16 **MINONE<3:0>:** Binary Coded Decimal Value of Minutes 1-Digit bits Contains a value from 0 to 9.

bit 15-12 **SECTEN<2:0>:** Binary Coded Decimal Value of Seconds 10-Digit bits Contains a value from 0 to 5.

bit 11-8 **SECONE<3:0>:** Binary Coded Decimal Value of Seconds 1-Digit bits Contains a value from 0 to 9.

bit 7-0 **Unimplemented:** Read as ‘0’

REGISTER 19-5: RTCDATE/ALMDATE: RTCC DATE/ALARM REGISTERS

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | MTHTEN | MTHONE<3:0> | | | |
| 15:8 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | DAYTEN<1:0> | | DAYONE<3:0> | | | |
| 7:0 | U-0 | U-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | — | — | WDAY<2:0> | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-21 **Unimplemented:** Read as ‘0’

bit 20 **MTHTEN:** Binary Coded Decimal Value of Months 10-Digit bit Contains a value from 0 to 1.

bit 19-16 **MTHONE<3:0>:** Binary Coded Decimal Value of Months 1-Digit bits Contains a value from 0 to 9.

bit 15-14 **Unimplemented:** Read as ‘0’

bit 13-12 **DAYTEN<1:0>:** Binary Coded Decimal Value of Days 10-Digit bits Contains a value from 0 to 3.

bit 11-8 **DAYONE<3:0>:** Binary Coded Decimal Value of Days 1-Digit bits Contains a value from 0 to 9.

bit 7-3 **Unimplemented:** Read as ‘0’

bit 2-0 **WDAY<2:0>:** Binary Coded Decimal Value of Weekdays Digit bits Contains a value from 0 to 6.

# 12-BIT ADC CONVERTER WITH THRESHOLD DETECT

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a compre- hensive reference source. To complement the information in this data sheet, refer to **Section 25. “12-Bit Analog-to-Digital Converter (ADC) with Threshold Detect”** (DS60001359) in the *“PIC32 Family Refer- ence Manual”*[, which is available from the](http://www.microchip.com/PIC32) [Microchip web site (](http://www.microchip.com/PIC32)[www.microchip.com/](http://www.microchip.com/) PIC32). The information in this data sheet supersedes the information in the FRM.

### Introduction

The 12-bit ADC Converter with Threshold Detect includes the following features:

* + - * Successive Approximation Register (SAR) Conversion
      * Conversion Speeds of up to 300 ksps
      * User-Selectable Resolution of 10 or 12 bits
      * Up to 24 Analog Inputs (internal and external)
      * External Voltage Reference Input Pins
      * Unipolar Differential Sample-and-Hold Amplifier (SHA)
      * Automated Threshold Scan and Compare Operation to Pre-Evaluate Conversion Results
      * Selectable Conversion Trigger Source
      * Fixed-Length Configurable Conversion Result Buffer
      * Eight Options for Result Alignment and Encoding
      * Configurable Interrupt Generation
      * Operation during CPU Sleep and Idle modes

[Figure 20-1](#_bookmark474) illustrates a block diagram of the 12-bit ADC. The 12-bit ADC has external analog inputs, AN0 through AN19, and 4 internal analog inputs connected to VDD, VSS, VCORE and band gap. In addition, there are two analog input pins for external voltage reference connections.

The analog inputs are connected through a multiplexer to the SHA. Unipolar differential conversions are possible on all inputs (see [Figure 20-1](#_bookmark474)).

The Automatic Input Scan mode sequentially converts multiple analog inputs. A special control register speci- fies which inputs will be included in the scanning sequence. The 12-bit ADC is connected to a 22-word result buffer. The 12-bit result is converted to one of eight output formats in either 32-bit or 16-bit word widths.

FIGURE 20-1: ADC BLOCK DIAGRAM



AVDD AVSS VCORE

Band Gap

AN19

VCFG<2:0>

AN0

VREFH

VREFL

SHA

+

SAR ADC

CH0SA<4:0>

–

CSCNA

AVss

Channel Scan

VREF+ AVDD VREF- AVSS

|  |
| --- |
| ADC1BUF0 |
| ADC1BUF1 |
| ADC1BUF2 |
|  |
| ADC1BUF20 |
| ADC1BUF21 |

### Control Registers

The ADC module has the following Special Function Registers (SFRs):

* [**AD1CON1: ADC Control Register 1**](#_bookmark481)
* [**AD1CON2: ADC Control Register 2**](#_bookmark485)
* [**AD1CON3: ADC Control Register 3**](#_bookmark487)
* [**AD1CON5: ADC Control Register 5**](#_bookmark489)

The AD1CON1, AD1CON2, AD1CON3 and

AD1CON5 registers control the operation of the ADC module.

* [**AD1CHS: ADC Input Select Register**](#_bookmark492)

The AD1CHS register selects the input pins to be connected to the SHA.

* [**AD1CSS: ADC Input Scan Select Register**](#_bookmark497)

The AD1CSS register selects inputs to be sequentially scanned.

* [**AD1CHIT: ADC Compare Hit Register**](#_bookmark502)

The AD1CHIT register indicates the channels meeting specified comparison requirements.

[Table 20-1](#_bookmark477) provides a summary of all ADC related registers, including their addresses and formats. Corresponding registers appear after the summary, followed by a detailed description of each register. All unimplemented registers and/or bits within a register read as zero.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 219

TABLE 20-1: ADC REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(2)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2100 | ADC1BUF0 | 31:16 | ADC1BUF0<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2110 | ADC1BUF1 | 31:16 | ADC1BUF1<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2120 | ADC1BUF2 | 31:16 | ADC1BUF2<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2130 | ADC1BUF3 | 31:16 | ADC1BUF3<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2140 | ADC1BUF4 | 31:16 | ADC1BUF4<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2150 | ADC1BUF5 | 31:16 | ADC1BUF5<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2160 | ADC1BUF6 | 31:16 | ADC1BUF6<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2170 | ADC1BUF7 | 31:16 | ADC1BUF7<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2180 | ADC1BUF8 | 31:16 | ADC1BUF8<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2190 | ADC1BUF9 | 31:16 | ADC1BUF9<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 21A0 | ADC1BUF10 | 31:16 | ADC1BUF10<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 21B0 | ADC1BUF11 | 31:16 | ADC1BUF11<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 21C0 | ADC1BUF12 | 31:16 | ADC1BUF12<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 21D0 | ADC1BUF13 | 31:16 | ADC1BUF13<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 21E0 | ADC1BUF14 | 31:16 | ADC1BUF14<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** The CSS<19:12> bits are not implemented in 28-pin devices. The CSS<19:15> bits are not implemented in 36-pin and 40-pin devices. The CSS<17:14> bits are not implemented in 48-pin devices.

**2:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

TABLE 20-1: ADC REGISTER MAP (CONTINUED)

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 220

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(2)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 21F0 | ADC1BUF15 | 31:16 | ADC1BUF15<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2200 | ADC1BUF16 | 31:16 | ADC1BUF16<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2210 | ADC1BUF17 | 31:16 | ADC1BUF17<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2220 | ADC1BUF18 | 31:16 | ADC1BUF18<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2230 | ADC1BUF19 | 31:16 | ADC1BUF19<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2240 | ADC1BUF20 | 31:16 | ADC1BUF20<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2250 | ADC1BUF21 | 31:16 | ADC1BUF21<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |
| 2260 | AD1CON1 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON |  | SIDL | — | — | FORM<2:0> | | | SSRC<3:0> | | | | MODE12 | ASAM | SAMP | DONE | 0000 |
| 2270 | AD1CON2 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | VCFG<2:0> | | | OFFCAL | BUFREGEN | CSCNA | — | — | BUFS | — | SMPI<3:0> | | | | BUFM | — | 0000 |
| 2280 | AD1CON3 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ADRC | EXTSAM | — | SAMC<4:0> | | | | | ADCS<7:0> | | | | | | | | 0000 |
| 2290 | AD1CHS | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | CHONA<2:0> | | | CHOSA<4:0> | | | | | 0000 |
| 22A0 | AD1CSS | 31:16 | — | CSS<30:27> | | | | — | — | — | — | — | — | — | CSS<19:16> | | | | 0000 |
| 15:0 | CSS<15:0>**(**[**1**](#_bookmark479)**)** | | | | | | | | | | | | | | | | 0000 |
| 22C0 | AD1CON5 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ASEN | LPEN | — | BGREQ | — | — | ASINT<1:0> | | — | — | — | — | WM<1:0> | | CM<1:0> | | 0000 |
| 22D0 | AD1CHIT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | CHH<19:16> | | | | 0000 |
| 15:0 | CHH<15:0> | | | | | | | | | | | | | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** The CSS<19:12> bits are not implemented in 28-pin devices. The CSS<19:15> bits are not implemented in 36-pin and 40-pin devices. The CSS<17:14> bits are not implemented in 48-pin devices.

**2:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

REGISTER 20-1: AD1CON1: ADC CONTROL REGISTER 1

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | U-0 | R/W-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 |
| ON | — | SIDL | — | — | FORM<2:0> | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0, HSC | R/W-0, HSC |
| SSRC<3:0> | | | | MODE12 | ASAM | SAMP**(**[**2**](#_bookmark484)**)** | DONE**(**[**1**](#_bookmark483)**)** |

**Legend:**

R = Readable bit

-n = Value at POR

HSC = Hardware Settable/Clearable bit

W = Writable bit

‘1’ = Bit is set

U = Unimplemented bit, read as ‘0’

‘0’ = Bit is cleared

x = Bit is unknown

|  |  |  |
| --- | --- | --- |
| bit 31-16  bit 15 | **Unimplemented:** Read as ‘0’  **ON:** ADC Operating Mode bit  1 = ADC module is operating |  |
|  | 0 = ADC is off |
| bit 14 | **Unimplemented:** Read as ‘0’ |
| bit 13 | **SIDL:** ADC Stop in Idle Mode bit |
|  | 1 = Discontinues module operation when device enters Idle mode  0 = Continues module operation in Idle mode |
| bit 12-11 | **Unimplemented:** Read as ‘0’ |
| bit 10-8 | **FORM<2:0>:** Data Output Format bits |
|  | For 12-Bit Operation (MODE12 bit = 1):  111 = Signed fractional 32-bit (DOUT = sddd dddd dddd 0000 0000 | 0000 0000) |
|  | 110 = Fractional 32-bit (DOUT = dddd dddd dddd 0000 0000 0000 | 0000 0000) |

101 = Signed integer 32-bit (DOUT = ssss ssss ssss ssss ssss sddd dddd dddd) 100 = Integer 32-bit (DOUT = 0000 0000 0000 0000 0000 dddd dddd dddd)

011 = Signed fractional 16-bit (DOUT = 0000 0000 0000 0000 sddd dddd dddd 0000)

010 = Fractional 16-bit (DOUT = 0000 0000 0000 0000 dddd dddd dddd 0000)

001 = Signed integer 16-bit (DOUT = 0000 0000 0000 0000 ssss sddd dddd dddd)

000 = Integer 16-bit (DOUT = 0000 0000 0000 0000 0000 dddd dddd dddd) For 10-Bit Operation (MODE12 bit = 0):

111 = Signed fractional 32-bit (DOUT = sddd dddd dd00 0000 0000 0000 0000)

110 = Fractional 32-bit (DOUT = dddd dddd dd00 0000 0000 0000 0000 0000) 101 = Signed integer 32-bit (DOUT = ssss ssss ssss ssss ssss sssd dddd dddd) 100 = Integer 32-bit (DOUT = 0000 0000 0000 0000 0000 00dd dddd dddd)

011 = Signed fractional 16-bit (DOUT = 0000 0000 0000 0000 sddd dddd dd00 0000)

010 = Fractional 16-bit (DOUT = 0000 0000 0000 0000 dddd dddd dd00 0000)

001 = Signed integer 16-bit (DOUT = 0000 0000 0000 0000 ssss sssd dddd dddd)

000 = Integer 16-bit (DOUT = 0000 0000 0000 0000 0000 00dd dddd dddd)

**Note 1:** The DONE bit is not persistent in Automatic modes; it is cleared by hardware at the beginning of the next sample.

**2:** The SAMP bit is cleared and cannot be written if the ADC is disabled (ON bit = 0).

REGISTER 20-1: AD1CON1: ADC CONTROL REGISTER 1 (CONTINUED)

bit 7-4 **SSRC<3:0>:** Conversion Trigger Source Select bits

1111 = CLC2 module event ends sampling and starts conversion 1110 = CLC1 module event ends sampling and starts conversion 1101 = SCCP6 module event ends sampling and starts conversion 1100 = SCCP5 module event ends sampling and starts conversion 1011 = SCCP4 module event ends sampling and starts conversion 1010 = MCCP3 module event ends sampling and starts conversion 1001 = MCCP2 module event ends sampling and starts conversion 1000 = MCCP1 module event ends sampling and starts conversion

0111 = Internal counter ends sampling and starts conversion (auto-convert)

0110 = Timer1 period match ends sampling and starts conversion (can trigger during Sleep mode) 0101 = Timer1 period match ends sampling and starts conversion (will not trigger during Sleep mode) 0100-0011 = Reserved

0010 = Timer3 period match ends sampling and starts conversion

0001 = Active transition on INT0 pin ends sampling and starts conversion

0000 = Clearing the SAMP bit ends sampling and starts conversion bit 3 **MODE12:** 12-Bit Operation Mode bit

1 = 12-bit ADC operation

0 = 10-bit ADC operation

bit 2 **ASAM:** ADC Sample Auto-Start bit

1 = Sampling begins immediately after last conversion completes; SAMP bit is automatically set

0 = Sampling begins when SAMP bit is set bit 1 **SAMP:** ADC Sample Enable bit**(**[**2**](#_bookmark484)**)**

1 = The ADC Sample-and-Hold Amplifier (SHA) is sampling

0 = The ADC SHA is holding

When ASAM = 0, writing ‘1’ to this bit starts sampling. When SSRC<3:0 = 0000, writing ‘0’ to this bit will end sampling and start conversion.

bit 0 **DONE:** ADC Conversion Status bit**(**[**1**](#_bookmark483)**)**

1 = Analog-to-Digital conversion is done

0 = Analog-to-Digital conversion is not done or has not started Clearing this bit will not affect any operation in progress.

**Note 1:** The DONE bit is not persistent in Automatic modes; it is cleared by hardware at the beginning of the next sample.

**2:** The SAMP bit is cleared and cannot be written if the ADC is disabled (ON bit = 0).

REGISTER 20-2: AD1CON2: ADC CONTROL REGISTER 2

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | U-0 |
| VCFG<2:0> | | | OFFCAL | BUFREGEN | CSCNA | — | — |
| 7:0 | R/W-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | U-0 |
| BUFS | — | SMPI<3:0> | | | | BUFM | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’

bit 15-13 **VCFG<2:0>:** Voltage Reference Configuration bits

|  |  |  |
| --- | --- | --- |
|  | **ADC VR+** | **ADC VR-** |
| 000 | AVDD | AVSS |
| 001 | AVDD | External VREF- Pin |
| 010 | External VREF+ Pin | AVSS |
| 011 | External VREF+ Pin | External VREF- Pin |
| 1xx | Unimplemented; do not use | |

bit 12 **OFFCAL:** Input Offset Calibration Mode Select bit

1 = Enables Offset Calibration mode: The inputs of the SHA are connected to the negative reference

0 = Disables Offset Calibration mode: The inputs to the SHA are controlled by AD1CHS or AD1CSS bit 11 **BUFREGEN:** ADC Buffer Register Enable bit

1 = Conversion result is loaded into the buffer location determined by the converted channel

0 = ADC result buffer is treated as a FIFO

bit 10 **CSCNA:** Scan Input Selections for CH0+ SHA Input for Input Multiplexer Setting bit

1 = Scans inputs

0 = Does not scan inputs

bit 9-8 **Unimplemented:** Read as ‘0’ bit 7 **BUFS:** Buffer Fill Status bit

Only valid when BUFM = 1 (ADC buffers split into 2 x 11-word buffers).

1 = ADC is currently filling Buffers 11-21, user should access data in 0-10

0 = ADC is currently filling Buffers 0-10, user should access data in 11-21 bit 6 **Unimplemented:** Read as ‘0’

bit 5-2 **SMPI<3:0>:** Sample/Convert Sequences Per Interrupt Selection bits

1111 = Interrupts at the completion of conversion for each 16th sample/convert sequence

1110 = Interrupts at the completion of conversion for each 15th sample/convert sequence

•

•

•

0001 = Interrupts at the completion of conversion for each 2nd sample/convert sequence

0000 = Interrupts at the completion of conversion for each sample/convert sequence bit 1 **BUFM:** ADC Result Buffer Mode Select bit

1 = Buffer configured as two 11-word buffers, ADC1BUF(0...10), ADC1BUF(11...21)

0 = Buffer configured as one 22-word buffer, ADC1BUF(0...21) bit 0 **Unimplemented:** Read as ‘0’

REGISTER 20-3: AD1CON3: ADC CONTROL REGISTER 3

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | R/W-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| ADRC | EXTSAM | — | SAMC<4:0> | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| ADCS<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’

bit 15 **ADRC:** ADC Conversion Clock Source (TSRC) bit

1 = Clock derived from the Fast RC (FRC) oscillator

0 = Clock derived from the Peripheral Bus Clock (PBCLK, 1:1 with SYSCLK) bit 14 **EXTSAM:** Extended Sampling Time bit

1 = ADC is still sampling after SAMP bit = 0 0 = ADC stops sampling when SAMP bit = 0

bit 13 **Unimplemented:** Read as ‘0’

bit 12-8 **SAMC<4:0>:** Auto-Sample Time bits

11111 = 31 TAD

•

•

•

00001 = 1 TAD

00000 = 0 TAD (Not allowed)

bit 7-0 **ADCS<7:0>:** ADC Conversion Clock Select bits

11111111 = 2 • TSRC • ADCS<7:0> = 510 • TSRC = TAD

•

•

•

00000001 = 2 • TSRC • ADCS<7:0> = 2 • TSRC = TAD

00000000 = 1 • TSRC = TAD

Where TSRC is a period of clock selected by the ADRC bit (AD1CON3<15>).

REGISTER 20-4: AD1CON5: ADC CONTROL REGISTER 5

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | R/W-0 | U-0 | R/W-0 | U-0 | U-0 | R/W-0 | R/W-0 |
| ASEN | LPEN | — | BGREQ | — | — | ASINT<1:0>**(**[**1**](#_bookmark491)**)** | |
| 7:0 | U-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | — | WM<1:0> | | CM<1:0> | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’ bit 15 **ASEN:** Auto-Scan Enable bit

1 = Auto-scan is enabled

0 = Auto-scan is disabled

bit 14 **LPEN:** Low-Power Enable bit

1 = Low power is enabled after scan

0 = Full power is enabled after scan bit 13 **Unimplemented:** Read as ‘0’

bit 12 **BGREQ:** Band Gap Request bit

1 = Band gap is enabled when the ADC is enabled and active

0 = Band gap is not enabled by the ADC bit 11-10 **Unimplemented:** Read as ‘0’

bit 9-8 **ASINT<1:0>:** Auto-Scan (Threshold Detect) Interrupt Mode bits**(**[**1**](#_bookmark491)**)**

11 = Interrupt after Threshold Detect sequence has completed and a valid compare has occurred

10 = Interrupt after valid compare has occurred

01 = Interrupt after Threshold Detect sequence has completed

00 = No interrupt

bit 7-4 **Unimplemented:** Read as ‘0’ bit 3-2 **WM<1:0>:** Write Mode bits

11 = Reserved

10 = Auto-compare only (conversion results are not saved, but interrupts are generated when a valid match occurs, as defined by the CM<1:0> and ASINT<1:0> bits)

01 = Convert and save (conversion results saved to locations as determined by register bits when a match occurs, as defined by the CM<1:0> bits)

00 = Legacy operation (conversion data saved to location determined by buffer register bits) bit 1-0 **CM<1:0>:** Compare Mode bits

11 = Outside Window mode (valid match occurs if the conversion result is outside of the window defined by the corresponding buffer pair)

10 = Inside Window mode (valid match occurs if the conversion result is inside the window defined by the corresponding buffer pair)

01 = Greater Than mode (valid match occurs if the result is greater than value in the corresponding buffer register)

00 = Less Than mode (valid match occurs if the result is less than value in the corresponding buffer register)

**Note 1:** The ASINT<1:0> bits setting only takes effect when ASEN (AD1CON5<15>) = 1. Interrupt generation is governed by the SMPI<3:0> bits field.

REGISTER 20-5: AD1CHS: ADC INPUT SELECT REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CH0NA<2:0> | | | CH0SA<4:0> | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-8 **Unimplemented:** Read as ‘0’

bit 7-5 **CH0NA<2:0>:** Negative Input Select bits

111-001 = Reserved

000 = Negative input is AVSS

bit 4-0 **CH0SA<4:0>:** Positive Input Select bits

11111 = Reserved

11110 = Positive input is AVDD

11101 = Positive input is AVSS

11100 = Positive input is Band Gap Reference (VBG)

11011 = VDD core

10100-10110 = Reserved 10011 = Positive input is AN19**(**[**1**](#_bookmark494)**)** 10010 = Positive input is AN18**(**[**1**](#_bookmark494)**)** 10001 = Positive input is AN17**(**[**1**](#_bookmark494)**)** 10000 = Positive input is AN16**(**[**1**](#_bookmark494)**)** 01111 = Positive input is AN15**(**[**2**](#_bookmark495)**)** 01110 = Positive input is AN14**(**[**3**](#_bookmark496)**)** 01101 = Positive input is AN13**(**[**3**](#_bookmark496)**)** 01100 = Positive input is AN12**(**[**3**](#_bookmark496)**)**

01011 = Positive input is AN11

01010 = Positive input is AN10 01001 = Positive input is AN9 01000 = Positive input is AN8 00111 = Positive input is AN7 00110 = Positive input is AN6 00101 = Positive input is AN5 00100 = Positive input is AN4 00011 = Positive input is AN3 00010 = Positive input is AN2 00001 = Positive input is AN1 00000 = Positive input is AN0

**Note 1:** This option is not available in 28, 36, 40 or 48-pin packages.

**2:** This option is not available in 28, 36 or 40-pin packages.

**3:** This option is not available in 28-pin packages.

)

REGISTER 20-6: AD1CSS: ADC INPUT SCAN SELECT REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | U-0 | U-0 |
| — | CSS<30:27> | | | | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | — | CSS<19:16>**(**[**1**](#_bookmark499)**,**[**2**](#_bookmark500)**,**[**3**](#_bookmark501)**)** | | | |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CSS<15:8> | | | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CSS<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **Unimplemented:** Read as ‘0’

bit 30-27 **CSS<30:27>:** ADC Input Pin Scan Selection bits

1 = Selects ANx for the input scan

0 = Skips ANx for the input scan bit 26-20 **Unimplemented:** Read as ‘0’

bit 19-0 **CSS<19:0>:** ADC Input Pin Scan Selection bits**(**[**1**](#_bookmark499)**,**[**2**](#_bookmark500)**,**[**3**](#_bookmark501)**)**

1 = Selects ANx for the input scan

0 = Skips ANx for the input scan

**Note 1:** The CSS<19:12> bits are not implemented in 28-pin devices

**2:** The CSS<19:15> bits are not implemented in 36-pin and 40-pin devices

**3:** The CSS<17:14> bits are not implemented in 48-pin devices

REGISTER 20-7: AD1CHIT: ADC COMPARE HIT REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | — | CHH<19:16>**(**[**1**](#_bookmark504)**,**[**2**](#_bookmark505)**,**[**3**](#_bookmark506)**)** | | | |
| 15:8 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | CHH<13:8> | | | | | |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| CHH<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-20 **Unimplemented:** Read as ‘0’

bit 19-0 **CHH<21:16>:** ADC Compare Hit bits**(**[**1**](#_bookmark504)**,**[**2**](#_bookmark505)**,**[**3**](#_bookmark506)**)** If CM<1:0> = 11:

1 = ADC Result Buffer n has been written with data or a match has occurred

0 = ADC Result Buffer n has not been written with data For All Other Values of CM<1:0>:

1 = A match has occurred on ADC Result Channel n

0 = No match has occurred on ADC Result Channel n

**Note 1:** The CHH<19:12> bits are not implemented in 28-pin devices

**2:** The CHH<19:15> bits are not implemented in 36-pin and 40-pin devices

**3:** The CHH<17:14> bits are not implemented in 48-pin devices

# CONFIGURABLE LOGIC CELL (CLC)

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a compre- hensive reference source. To complement the information in this data sheet, refer to **Section 36. “Configurable Logic Cell”** (DS60001363) in the *“PIC32 Family Refer- ence Manual”*, which is available from the Microchip web site ([www.microchip.com/](http://www.microchip.com/) PIC32). The information in this data sheet supersedes the information in the FRM.

The Configurable Logic Cell (CLC) module allows the user to specify combinations of signals as inputs to a logic function and to use the logic output to control other peripherals or I/O pins. This provides greater flex- ibility and potential in embedded designs since the CLC module can operate outside the limitations of software execution, and supports a vast amount of output designs.

There are four input gates to the selected logic func- tion. These four input gates select from a pool of up to 32 signals that are selected using four data source selection multiplexers. [Figure 21-1](#_bookmark510) shows an overview of the module. [Figure 21-3](#_bookmark514) shows the details of the data source multiplexers and logic input gate connections.

Input Data Selection Gates

FIGURE 21-1: CLCx MODULE



CLCIN[0] CLCIN[1] CLCIN[2] CLCIN[3] CLCIN[4] CLCIN[5] CLCIN[6] CLCIN[7] CLCIN[8] CLCIN[9] CLCIN[10] CLCIN[11] CLCIN[12] CLCIN[13] CLCIN[14] CLCIN[15] CLCIN[16] CLCIN[17] CLCIN[18] CLCIN[19] CLCIN[20] CLCIN[21] CLCIN[22] CLCIN[23] CLCIN[24] CLCIN[25] CLCIN[26] CLCIN[27] CLCIN[28] CLCIN[29] CLCIN[30] CLCIN[31]

See [Figure 21-2](#_bookmark512)

LCOE

Gate 1

Gate 2

Gate 3

Gate 4

ON

Logic

Function Logic

Output

CLCx

Output

TRISx Control

CLCx

LCPOL

MODE<2:0>

Interrupt

det

INTP

INTN

Sets CLCxIF

Flag

Interrupt

det

See [Figure 21-3](#_bookmark514)

**Note:** All register bits shown in this figure can be found in the CLCxCON register.

FIGURE 21-2: CLCx LOGIC FUNCTION COMBINATORIAL OPTIONS



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **AND – OR** |  |  | **OR – XOR** |
| Gate 1 |  |  | Gate 1 |  |
| Gate 2  Gate 3 |  | Logic Output | Gate 2  Gate 3 | Logic Output |
| Gate 4 |  |  | Gate 4 |  |
|  | MODE<2:0> = 000 |  |  | MODE<2:0> = 001 |
|  | **4-Input AND** | |  | **S-R Latch** |
| Gate 1  Gate 2  Gate 3  Gate 4 | Logic Output | | Gate 1  Gate 2  Gate 3  Gate 4 | S Q Logic Output    R |
|  | MODE<2:0> = 010 | |  | MODE<2:0> = 011 |
| **1-Input D Flip-Flop with S and R**  Gate 4  S  Gate 2 D Q Logic Output  Gate 1 R  Gate 3  MODE<2:0> = 100 | | | Gate 4  Gate 2 | **2-Input D Flip-Flop with R**  D Q Logic Output    Gate 1  R  Gate 3  MODE<2:0> = 101 |
| Gate 2  Gate 1  Gate 4  Gate 3 | **J-K Flip-Flop with R**   1. Q Logic Output 2. R   MODE<2:0> = 110 | | **1-Input Transparent Latch with S and R**  Gate 4  S  Gate 2 D Q Logic Output  Gate 1 LE R  Gate 3  MODE<2:0> = 111 | |

FIGURE 21-3: CLCx INPUT SOURCE SELECTION DIAGRAM

**Data Selection**

CLCIN[0] ~~0~~00 CLCIN[1] CLCIN[2] CLCIN[3] CLCIN[4] CLCIN[5] CLCIN[6]

CLCIN[7] ~~1~~11

Data Gate 1

Data 1 Non-Inverted

G1D1T

Data 1 Inverted

G1D1N

G1D2T

DS1x (CLCxSEL<2:0>)

G1D2N

Gate 1

CLCIN[8] ~~0~~00 CLCIN[9] CLCIN[10] CLCIN[11] CLCIN[12] CLCIN[13] CLCIN[14]

CLCIN[15] ~~1~~11

G1D3T

Data 2 Non-Inverted

Data 2 Inverted

G1POL

(CLCxCON<0>)

G1D3N

G1D4T

DS2x (CLCxSEL<6:4>) G1D4N

CLCIN[16] ~~0~~00 CLCIN[17] CLCIN[18] CLCIN[19] CLCIN[20] CLCIN[21] CLCIN[22]

CLCIN[23] ~~1~~11

Gate 2

Data 3 Non-Inverted

Data 3 Inverted

Gate 3

DS3x (CLCxSEL<10:8>)

CLCIN[24] ~~0~~00 CLCIN[25] CLCIN[26] CLCIN[27] CLCIN[28] CLCIN[29] CLCIN[30]




CLCIN[31] ~~1~~11

Gate 4

Data 4 Non-Inverted

Data 4 Inverted

DS4x (CLCxSEL<14:12>)



Data Gate 4

(Same as Data Gate 1)

Data Gate 3

(Same as Data Gate 1)

Data Gate 2

(Same as Data Gate 1)

### Control Registers

The CLCx module is controlled by the following registers:

* CLCxCON
* CLCxSEL
* CLCxGLS

The CLCx Control register (CLCxCON) is used to enable the module and interrupts, control the output enable bit, select output polarity and select the logic function. The CLCx Control registers also allow the user to control the logic polarity of not only the cell output, but also some intermediate variables.

The CLCx Source Select register (CLCxSEL) allows the user to select up to 4 data input sources using the 4 data input selection multiplexers. Each multiplexer has a list of 8 data sources available.

The CLCx Gate Logic Select register (CLCxGLS) allows the user to select which outputs from each of the selection MUXes are used as inputs to the input gates of the logic cell. Each data source MUX outputs both a true and a negated version of its output. All of these 8 signals are enabled, ORed together by the logic cell input gates.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 233

TABLE 21-1: CLC1, CLC2 AND CLC3 REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2480 | CLC1CON | 32:16 | — | — | — | — | — | — | — | — | — | — | — | — | G4POL | G3POL | G2POL | G1POL | 0000 |
| 15:0 | ON | — | SIDL | — | INTP | INTN | — | — | LCOE | LCOUT | LCPOL | — | — | MODE<2:0> | | | 0000 |
| 2490 | CLC1SEL | 32:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | DS4<2:0> | | | — | DS3<2:0> | | | — | DS2<2:0> | | | — | DS1<2:0> | | | 0000 |
| 24A0 | CLC1GLS | 32:16 | G4D4T | G4D4N | G4D3T | G4D3N | G4D2T | G4D2N | G4D1T | G4D1N | G3D4T | G3D4N | G3D3T | G3D3N | G3D2T | G3D2N | G3D1T | G3D1N | 0000 |
| 15:0 | G2D4T | G2D4N | G2D3T | G2D3N | G2D2T | G2D2N | G2D1T | G2D1N | G1D4T | G1D4N | G1D3T | G1D3N | G1D2T | G1D2N | G1D1T | G1D1N | 0000 |
| 2500 | CLC2CON | 32:16 | — | — | — | — | — | — | — | — | — | — | — | — | G4POL | G3POL | G2POL | G1POL | 0000 |
| 15:0 | ON | — | SIDL | — | INTP | INTN | — | — | LCOE | LCOUT | LCPOL | — | — | MODE<2:0> | | | 0000 |
| 2510 | CLC2SEL | 32:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | DS4<2:0> | | | — | DS3<2:0> | | | — | DS2<2:0> | | | — | DS1<2:0> | | | 0000 |
| 2520 | CLC2GLS | 32:16 | G4D4T | G4D4N | G4D3T | G4D3N | G4D2T | G4D2N | G4D1T | G4D1N | G3D4T | G3D4N | G3D3T | G3D3N | G3D2T | G3D2N | G3D1T | G3D1N | 0000 |
| 15:0 | G2D4T | G2D4N | G2D3T | G2D3N | G2D2T | G2D2N | G2D1T | G2D1N | G1D4T | G1D4N | G1D3T | G1D3N | G1D2T | G1D2N | G1D1T | G1D1N | 0000 |
| 2580 | CLC3CON | 32:16 | — | — | — | — | — | — | — | — | — | — | — | — | G4POL | G3POL | G2POL | G1POL | 0000 |
| 15:0 | ON | — | SIDL | — | INTP | INTN | — | — | LCOE | LCOUT | LCPOL | — | — | MODE<2:0> | | | 0000 |
| 2590 | CLC3SEL | 32:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | DS4<2:0> | | | — | DS3<2:0> | | | — | DS2<2:0> | | | — | DS1<2:0> | | | 0000 |
| 25A0 | CLC3GLS | 32:16 | G4D4T | G4D4N | G4D3T | G4D3N | G4D2T | G4D2N | G4D1T | G4D1N | G3D4T | G3D4N | G3D3T | G3D3N | G3D2T | G3D2N | G3D1T | G3D1N | 0000 |
| 15:0 | G2D4T | G2D4N | G2D3T | G2D3N | G2D2T | G2D2N | G2D1T | G2D1N | G1D4T | G1D4N | G1D3T | G1D3N | G1D2T | G1D2N | G1D1T | G1D1N | 0000 |
| 2600 | CLC4CON | 32:16 | — | — | — | — | — | — | — | — | — | — | — | — | G4POL | G3POL | G2POL | G1POL | 0000 |
| 15:0 | ON | — | SIDL | — | INTP | INTN | — | — | LCOE | LCOUT | LCPOL | — | — | MODE<2:0> | | | 0000 |
| 2610 | CLC4SEL | 32:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | DS4<2:0> | | | — | DS3<2:0> | | | — | DS2<2:0> | | | — | DS1<2:0> | | | 0000 |
| 2620 | CLC4GLS | 32:16 | G4D4T | G4D4N | G4D3T | G4D3N | G4D2T | G4D2N | G4D1T | G4D1N | G3D4T | G3D4N | G3D3T | G3D3N | G3D2T | G3D2N | G3D1T | G3D1N | 0000 |
| 15:0 | G2D4T | G2D4N | G2D3T | G2D3N | G2D2T | G2D2N | G2D1T | G2D1N | G1D4T | G1D4N | G1D3T | G1D3N | G1D2T | G1D2N | G1D1T | G1D1N | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

REGISTER 21-1: CLCxCON: CLCx CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | — | G4POL | G3POL | G2POL | G1POL |
| 15:8 | R/W-0 | U-0 | R/W-0 | U-0 | R/W-0 | R/W-0 | U-0 | U-0 |
| ON | — | SIDL | — | INTP**(**[**1**](#_bookmark520)**)** | INTN**(**[**1**](#_bookmark520)**)** | — | — |
| 7:0 | R/W-0 | R-0, HS, HC | R/W-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 |
| LCOE | LCOUT | LCPOL | — | — | MODE<2:0> | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** | HC = Hardware Clearable bit | HS = Hardware Settable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-20 **Unimplemented:** Read as ‘0’

bit 19 **G4POL:** Gate 4 Polarity Control bit

1 = The output of Channel 4 logic is inverted when applied to the logic cell

0 = The output of Channel 4 logic is not inverted bit 18 **G3POL:** Gate 3 Polarity Control bit

1 = The output of Channel 3 logic is inverted when applied to the logic cell

0 = The output of Channel 3 logic is not inverted bit 17 **G2POL:** Gate 2 Polarity Control bit

1 = The output of Channel 2 logic is inverted when applied to the logic cell

0 = The output of Channel 2 logic is not inverted bit 16 **G1POL:** Gate 1 Polarity Control bit

1 = The output of Channel 1 logic is inverted when applied to the logic cell

0 = The output of Channel 1 logic is not inverted bit 15 **ON:** CLCx Enable bit

1 = CLCx is enabled and mixing input signals

0 = CLCx is disabled and has logic zero outputs bit 14 **Unimplemented:** Read as ‘0’

bit 13 **SIDL:** CLCx Stop in Idle Mode bit

1 = Discontinues module operation when device enters Idle mode

0 = Continues module operation in Idle mode bit 12 **Unimplemented:** Read as ‘0’

bit 11 **INTP:** CLCx Positive Edge Interrupt Enable bit**(**[**1**](#_bookmark520)**)**

1 = Interrupt will be generated when a rising edge occurs on LCOUT

0 = Interrupt will not be generated

bit 10 **INTN:** CLCx Negative Edge Interrupt Enable bit**(**[**1**](#_bookmark520)**)**

1 = Interrupt will be generated when a falling edge occurs on LCOUT

0 = Interrupt will not be generated bit 9-8 **Unimplemented:** Read as ‘0’

bit 7 **LCOE:** CLCx Port Enable bit

1 = CLCx port pin output is enabled

0 = CLCx port pin output is disabled

**Note 1:** The INTP and INTN bits should not be set at the same time for proper interrupt functionality.

REGISTER 21-1: CLCxCON: CLCx CONTROL REGISTER (CONTINUED)

bit 6 **LCOUT:** CLCx Data Output Status bit

1 = CLCx output high

0 = CLCx output low

bit 5 **LCPOL:** CLCx Output Polarity Control bit

1 = The output of the module is inverted

0 = The output of the module is not inverted bit 4-3 **Unimplemented:** Read as ‘0’

bit 2-0 **MODE<2:0>:** CLCx Mode bits

111 = Cell is a 1-input transparent latch with S and R

110 = Cell is a JK flip-flop with R

101 = Cell is a 2-input D flip-flop with R

100 = Cell is a 1-input D flip-flop with S and R

011 = Cell is an SR latch 010 = Cell is a 4-input AND 001 = Cell is an OR-XOR 000 = Cell is a AND-OR

**Note 1:** The INTP and INTN bits should not be set at the same time for proper interrupt functionality.

REGISTER 21-2: CLCxSEL: CLCx INPUT MUX SELECT REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | R/W-0 | R/W-0 | R/W-0 |
| — | DS4<2:0> | | | — | DS3<2:0> | | |
| 7:0 | U-0 | R/W-0 | R/W-0 | R/W-0 | U-0 | R/W-0 | R/W-0 | R/W-0 |
| — | DS2<2:0> | | | — | DS1<2:0> | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-15 **Unimplemented:** Read as ‘0’

bit 14-12 **DS4<2:0>:** Data Selection MUX 4 Signal Selection bits For CLC1:

111 = SCCP5 OCMP compare match event

110 = MCCP1 OCMP compare match event

101 = RTCC event

100 = CMP3 out

011 = SPI1 SDI1 in

010 = SCCP5 OCM5 output

001 = CLC2 out

000 = CLCINB I/O pin For CLC2:

111 = SCCP5 OCMP compare match event

110 = MCCP1 OCMP compare match event

101 = RTCC event

100 = CMP3 out

011 = SPI2 SDI2 in

010 = SCCP5 OCM6 output

001 = CLC1 out

000 = CLCINB I/O pin For CLC3:

111 = SCCP7 OCMP compare match event

110 = MCCP2 OCMP compare match event

101 = RTCC event

100 = CMP3 out

011 = SPI3 SDI3 in

010 = SCCP7 OCM7A output

001 = CLC4 out

000 = CLCINB I/O pin For CLC4:

111 = SCCP7 OCMP compare match event

110 = MCCP3 OCMP compare match event

101 = RTCC event

100 = CMP3 out

011 = Reserved

010 = SCCP7 OCM3A output

001 = CLC3 out

000 = CLCINB I/O pin

REGISTER 21-2: CLCxSEL: CLCx INPUT MUX SELECT REGISTER (CONTINUED)

bit 11 **Unimplemented:** Read as ‘0’

bit 10-8 **DS3<2:0>:** Data Selection MUX 3 Signal Selection bits For CLC1:

111 = Unused

110 = MCCP1 OCMP compare match event

101 = DMA Channel 0 interrupt 100 = ADC end of conversion 011 = UART1 TX out

010 = CMP1 out

001 = CLC2 out

000 = CLCINB I/O pin For CLC2:

111 = Unused

110 = MCCP1 OCMP compare match event

101 = DMA Channel 1 interrupt 100 = ADC end of conversion 011 = UART2 TX out

010 = CMP1 out

001 = CLC1 out

000 = CLCINB I/O pin For CLC3:

111 = Reserved

110 = MCCP2 OCMP compare match event

101 = DMA Channel 0 interrupt 100 = ADC end of conversion 011 = UART3 TX out

010 = CMP1 out

001 = CLC4 out

000 = CLCINB I/O pin For CLC4:

111 = Reserved

110 = MCCP3 OCMP compare match event

101 = DMA Channel 1 interrupt 100 = ADC end of conversion 011 = Reserved

010 = CMP1 out

001 = CLC3 out

000 = CLCINB I/O pin

bit 7 **Unimplemented:** Read as ‘0’

REGISTER 21-2: CLCxSEL: CLCx INPUT MUX SELECT REGISTER (CONTINUED)

bit 6-4 **DS2<2:0>:** Data Selection MUX 2 Signal Selection bits For CLC1:

111 = SCCP5 OCMP compare match event

110 = SCCP4 OCMP compare match event

101 = SCCP4 OCM4 output

100 = UART1 RX in

011 = SPI1 SDO1 out

010 = CMP2 out

001 = CLC1 out

000 = CLCINA I/O pin For CLC2:

111 = SCCP5 OCMP compare match event

110 = SCCP4 OCMP compare match event

101 = SCCP4 OCM4 output

100 = UART2 RX in

011 = SPI2 SDO2 out

010 = CMP2 out

001 = CLC2 out

000 = CLCINA I/O pin For CLC3:

111 = SCCP7 OCMP compare match event

110 = SCCP6 OCMP compare match event

101 = SCCP6 OCM6A output

100 = UART3 RX in

011 = SPI3 SDO3 out

010 = CMP2 out

001 = CLC3 out

000 = CLCINA I/O pin For CLC4:

111 = SCCP7 OCMP compare match event

110 = SCCP6 OCMP compare match event

101 = SCCP6 OCM2A output

100 = Reserved

011 = Reserved

010 = CMP2 out

001 = CLC4 out

000 = CLCINA I/O pin

bit 3 **Unimplemented:** Read as ‘0’

REGISTER 21-2: CLCxSEL: CLCx INPUT MUX SELECT REGISTER (CONTINUED)

bit 2-0 **DS1<2:0>:** Data Selection MUX 1 Signal Selection bits For CLC1:

111 = SCCP5 OCMP compare match event

110 = MCCP1 OCMP compare match event

101 = RTCC event

100 = CMP3 out

011 = SPI1 SDI1 in

010 = SCCP5 OCM5 output

001 = CLC2 out

000 = CLCINB I/O pin For CLC2:

111 = SCCP5 OCMP compare match event

110 = MCCP1 OCMP compare match event

101 = RTCC event

100 = CMP3 out

011 = SPI2 SDI2 in

010 = SCCP5 OCM6 output

001 = CLC1 out

000 = CLCINB I/O pin For CLC3:

111 = SCCP7 OCMP compare match event

110 = MCCP2 OCMP compare match event

101 = RTCC event

100 = CMP3 out

011 = SPI3 SDI3 in

010 = SCCP7 OCM7A output

001 = CLC4 out

000 = CLCINB I/O pin For CLC4:

111 = SCCP7 OCMP compare match event

110 = MCCP3 OCMP compare match event

101 = RTCC event

100 = CMP3 out

011 = Reserved

010 = SCCP7 OCM3A output

001 = CLC3 out

000 = CLCINB I/O pin

REGISTER 21-3: CLCxGLS: CLCx GATE LOGIC INPUT SELECT REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| G4D4T | G4D4N | G4D3T | G4D3N | G4D2T | G4D2N | G4D1T | G4D1N |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| G3D4T | G3D4N | G3D3T | G3D3N | G3D2T | G3D2N | G3D1T | G3D1N |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| G2D4T | G2D4N | G2D3T | G2D3N | G2D2T | G2D2N | G2D1T | G2D1N |
| 7:0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| G1D4T | G1D4N | G1D3T | G1D3N | G1D2T | G1D2N | G1D1T | G1D1N |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **G4D4T:** Gate 4 Data Source 4 True Enable bit

1 = The Data Source 4 signal is enabled for Gate 4

0 = The Data Source 4 signal is disabled for Gate 4 bit 30 **G4D4N:** Gate 4 Data Source 4 Negated Enable bit

1 = The Data Source 4 inverted signal is enabled for Gate 4

0 = The Data Source 4 inverted signal is disabled for Gate 4 bit 29 **G4D3T:** Gate 4 Data Source 3 True Enable bit

1 = The Data Source 3 signal is enabled for Gate 4

0 = The Data Source 3 signal is disabled for Gate 4 bit 28 **G4D3N:** Gate 4 Data Source 3 Negated Enable bit

1 = The Data Source 3 inverted signal is enabled for Gate 4

0 = The Data Source 3 inverted signal is disabled for Gate 4 bit 27 **G4D2T:** Gate 4 Data Source 2 True Enable bit

1 = The Data Source 2 signal is enabled for Gate 4

0 = The Data Source 2 signal is disabled for Gate 4 bit 26 **G4D2N:** Gate 4 Data Source 2 Negated Enable bit

1 = The Data Source 2 inverted signal is enabled for Gate 4

0 = The Data Source 2 inverted signal is disabled for Gate 4 bit 25 **G4D1T:** Gate 4 Data Source 1 True Enable bit

1 = The Data Source 1 signal is enabled for Gate 4

0 = The Data Source 1 signal is disabled for Gate 4 bit 24 **G4D1N:** Gate 4 Data Source 1 Negated Enable bit

1 = The Data Source 1 inverted signal is enabled for Gate 4

0 = The Data Source 1 inverted signal is disabled for Gate 4 bit 23 **G3D4T:** Gate 3 Data Source 4 True Enable bit

1 = The Data Source 4 signal is enabled for Gate 3

0 = The Data Source 4 signal is disabled for Gate 3 bit 22 **G3D4N:** Gate 3 Data Source 4 Negated Enable bit

1 = The Data Source 4 inverted signal is enabled for Gate 3

0 = The Data Source 4 inverted signal is disabled for Gate 3 bit 21 **G3D3T:** Gate 3 Data Source 3 True Enable bit

1 = The Data Source 3 signal is enabled for Gate 3

0 = The Data Source 3 signal is disabled for Gate 3

REGISTER 21-3: CLCxGLS: CLCx GATE LOGIC INPUT SELECT REGISTER (CONTINUED)

bit 20 **G3D3N:** Gate 3 Data Source 3 Negated Enable bit

1 = The Data Source 3 inverted signal is enabled for Gate 3

0 = The Data Source 3 inverted signal is disabled for Gate 3 bit 19 **G3D2T:** Gate 3 Data Source 2 True Enable bit

1 = The Data Source 2 signal is enabled for Gate 3

0 = The Data Source 2 signal is disabled for Gate 3 bit 18 **G3D2N:** Gate 3 Data Source 2 Negated Enable bit

1 = The Data Source 2 inverted signal is enabled for Gate 3

0 = The Data Source 2 inverted signal is disabled for Gate 3 bit 17 **G3D1T:** Gate 3 Data Source 1 True Enable bit

1 = The Data Source 1 signal is enabled for Gate 3

0 = The Data Source 1 signal is disabled for Gate 3 bit 16 **G3D1N:** Gate 3 Data Source 1 Negated Enable bit

1 = The Data Source 1 inverted signal is enabled for Gate 3

0 = The Data Source 1 inverted signal is disabled for Gate 3 bit 15 **G2D4T:** Gate 2 Data Source 4 True Enable bit

1 = The Data Source 4 signal is enabled for Gate 2

0 = The Data Source 4 signal is disabled for Gate 2 bit 14 **G2D4N:** Gate 2 Data Source 4 Negated Enable bit

1 = The Data Source 4 inverted signal is enabled for Gate 2

0 = The Data Source 4 inverted signal is disabled for Gate 2 bit 13 **G2D3T:** Gate 2 Data Source 3 True Enable bit

1 = The Data Source 3 signal is enabled for Gate 2

0 = The Data Source 3 signal is disabled for Gate 2 bit 12 **G2D3N:** Gate 2 Data Source 3 Negated Enable bit

1 = The Data Source 3 inverted signal is enabled for Gate 2

0 = The Data Source 3 inverted signal is disabled for Gate 2 bit 11 **G2D2T:** Gate 2 Data Source 2 True Enable bit

1 = The Data Source 2 signal is enabled for Gate 2

0 = The Data Source 2 signal is disabled for Gate 2 bit 10 **G2D2N:** Gate 2 Data Source 2 Negated Enable bit

1 = The Data Source 2 inverted signal is enabled for Gate 2

0 = The Data Source 2 inverted signal is disabled for Gate 2 bit 9 **G2D1T:** Gate 2 Data Source 1 True Enable bit

1 = The Data Source 1 signal is enabled for Gate 2

0 = The Data Source 1 signal is disabled for Gate 2 bit 8 **G2D1N:** Gate 2 Data Source 1 Negated Enable bit

1 = The Data Source 1 inverted signal is enabled for Gate 2

0 = The Data Source 1 inverted signal is disabled for Gate 2 bit 7 **G1D4T:** Gate 1 Data Source 4 True Enable bit

1 = The Data Source 4 signal is enabled for Gate 1

0 = The Data Source 4 signal is disabled for Gate 1 bit 6 **G1D4N:** Gate 1 Data Source 4 Negated Enable bit

1 = The Data Source 4 inverted signal is enabled for Gate 1

0 = The Data Source 4 inverted signal is disabled for Gate 1 bit 5 **G1D3T:** Gate 1 Data Source 3 True Enable bit

1 = The Data Source 3 signal is enabled for Gate 1

0 = The Data Source 3 signal is disabled for Gate 1

REGISTER 21-3: CLCxGLS: CLCx GATE LOGIC INPUT SELECT REGISTER (CONTINUED)

bit 4 **G1D3N:** Gate 1 Data Source 3 Negated Enable bit

1 = The Data Source 3 inverted signal is enabled for Gate 1

0 = The Data Source 3 inverted signal is disabled for Gate 1 bit 3 **G1D2T:** Gate 1 Data Source 2 True Enable bit

1 = The Data Source 2 signal is enabled for Gate 1

0 = The Data Source 2 signal is disabled for Gate 1 bit 2 **G1D2N:** Gate 1 Data Source 2 Negated Enable bit

1 = The Data Source 2 inverted signal is enabled for Gate 1

0 = The Data Source 2 inverted signal is disabled for Gate 1 bit 1 **G1D1T:** Gate 1 Data Source 1 True Enable bit

1 = The Data Source 1 signal is enabled for Gate 1

0 = The Data Source 1 signal is disabled for Gate 1 bit 0 **G1D1N:** Gate 1 Data Source 1 Negated Enable bit

1 = The Data Source 1 inverted signal is enabled for Gate 1

0 = The Data Source 1 inverted signal is disabled for Gate 1



* 1. **COMPARATOR** The comparator module provides three dual input comparators. The inputs to the comparator can be con-

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To com- plement the information in this data sheet, refer to **Section 19. “Comparator”** (DS60001110) in the *“PIC32 Family Refer- ence Manual”*, which is available from the Microchip web site ([www.microchip.com/](http://www.microchip.com/) PIC32). The information in this data sheet supersedes the information in the FRM.

figured to use any one of five external analog inputs (CxINA, CxINB, CxINC, CxIND and CVREF+). The

comparator outputs may be directly connected to the CxOUT pins. When the respective COE bit equals ‘1’, the I/O pad logic makes the unsynchronized output of the comparator available on the pin.

A simplified block diagram of the module in shown in [Figure 22-1](#_bookmark525). Each comparator has its own control register, CMxCON ([Register 22-2](#_bookmark532)), for enabling and configuring its operation. The output and event status of two comparators is provided in the CMSTAT register ([Register 22-1](#_bookmark530)).

FIGURE 22-1: THREE DUAL COMPARATOR MODULES BLOCK DIAGRAM

CCH<1:0>

EVPOL<1:0>

Input Select Logic

CPOL

Trigger/Interrupt Logic

CEVT

COE

CxINB

00

VIN-

VIN+

C1

C1OUT

Pin

CxINC

01

COUT

–

CxIND

10

Band Gap 11

EVPOL<1:0>

CPOL

Trigger/Interrupt Logic

CEVT

COE

VIN-

VIN+

C2

COUT

C2OUT

Pin

CxINA

0

+

EVPOL<1:0>

Comparator Voltage 0

Reference

CVREF+ 1

CVREFSEL

1

CPOL

Trigger/Interrupt Logic

CEVT

COE

VIN-

VIN+ C3

COUT

C3OUT

Pin

CREF



### Comparator Control Registers

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 244

TABLE 22-1: COMPARATORS 1, 2 AND 3 REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2300 | CMSTAT | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | C3EVT | C2EVT | C1EVT | 0000 |
| 15:0 | — | — | SIDL | — | — | — | — | CVREFSEL | — | — | — | — | — | C3OUT | C2OUT | C1OUT | 0000 |
| 2310 | CM1CON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON | COE | CPOL | — | — | — | CEVT | COUT | EVPOL<1:0> | | — | CREF | — | — | CCH<1:0> | | 0000 |
| 2330 | CM2CON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON | COE | CPOL | — | — | — | CEVT | COUT | EVPOL<1:0> | | — | CREF | — | — | CCH<1:0> | | 0000 |
| 2350 | CM3CON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON | COE | CPOL | — | — | — | CEVT | COUT | EVPOL<1:0> | | — | CREF | — | — | CCH<1:0> | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

REGISTER 22-1: CMSTAT: COMPARATOR MODULE STATUS REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC |
| — | — | — | — | — | C3EVT | C2EVT | C1EVT |
| 15:8 | U-0 | U-0 | R/W-0 | U-0 | U-0 | U-0 | U-0 | R/W-0 |
| — | — | SIDL | — | — | — | — | CVREFSEL |
| 7:0 | U-0 | U-0 | U-0 | U-0 | U-0 | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC |
| — | — | — | — | — | C3OUT | C2OUT | C1OUT |

|  |  |  |
| --- | --- | --- |
| **Legend:** | HC = Hardware Clearable bit | HS = Hardware Settable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-19 **Unimplemented:** Read as ‘0’

bit 18 **C3EVT:** Comparator 3 Event Status bit (read-only)

Shows the current event status of Comparator 3 (CM3CON<9>). bit 17 **C2EVT:** Comparator 2 Event Status bit (read-only)

Shows the current event status of Comparator 2 (CM2CON<9>).

bit 16 **C1EVT:** Comparator 1 Event Status bit (read-only)

Shows the current event status of Comparator 1 (CM1CON<9>). bit 15-14 **Unimplemented:** Read as ‘0’

bit 13 **SIDL:** Comparator Stop in Idle Mode bit

1 = Discontinues operation of all comparators when device enters Idle mode

0 = Continues operation of all enabled comparators in Idle mode bit 12-9 **Unimplemented:** Read as ‘0’

bit 8 **CVREFSEL:** Comparator Reference Voltage Select Enable bit

1 = External voltage reference from the CVREF+ pin is selected

0 = Internal band gap voltage reference is selected bit 7-3 **Unimplemented:** Read as ‘0’

bit 2 **C3OUT:** Comparator 3 Output Status bit (read-only) Shows the current output of Comparator 3 (CM3CON<8>).

bit 1 **C2OUT:** Comparator 2 Output Status bit (read-only) Shows the current output of Comparator 2 (CM2CON<8>).

bit 0 **C1OUT:** Comparator 1 Output Status bit (read-only) Shows the current output of Comparator 1 (CM1CON<8>).

REGISTER 22-2: CMxCON: COMPARATOR x CONTROL REGISTERS (COMPARATORS 1, 2 AND 3)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/W-0 | R/W-0 | R/W-0 | U-0 | U-0 | U-0 | R-0, HS, HC | R-0, HS, HC |
| ON | COE | CPOL | — | — | — | CEVT | COUT |
| 7:0 | R/W-0 | R/W-0 | U-0 | R/W-0 | U-0 | U-0 | R/W-0 | R/W-0 |
| EVPOL<1:0> | | — | CREF | — | — | CCH<1:0> | |

|  |  |  |
| --- | --- | --- |
| **Legend:** | HC = Hardware Clearable bit | HS = Hardware Settable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’ bit 15 **ON:** Comparator Enable bit

1 = Comparator is enabled

0 = Comparator is disabled

bit 14 **COE:** Comparator Output Enable bit

1 = Comparator output is present on the CxOUT pin

0 = Comparator output is internal only

bit 13 **CPOL:** Comparator Output Polarity Select bit

1 = Comparator output is inverted

0 = Comparator output is not inverted bit 12-10 **Unimplemented:** Read as ‘0’

bit 9 **CEVT:** Comparator Event bit

1 = Comparator event that is defined by EVPOL<1:0> has occurred; subsequent triggers and interrupts are disabled until the bit is cleared

0 = Comparator event has not occurred bit 8 **COUT:** Comparator Output bit

When CPOL = 0:

1 = VIN+ > VIN-

0 = VIN+ < VIN- When CPOL = 1: 1 = VIN+ < VIN-

0 = VIN+ > VIN-

REGISTER 22-2: CMxCON: COMPARATOR x CONTROL REGISTERS (COMPARATORS 1, 2 AND 3) (CONTINUED)

bit 7-6 **EVPOL<1:0>:** Trigger/Event/Interrupt Polarity Select bits

11 = Trigger/event/interrupt is generated on any change of the comparator output (while CEVT = 0) 10 = Trigger/event/interrupt is generated on transition of the comparator output:

If CPOL = 0 (non-inverted polarity):

High-to-low transition only.

If CPOL = 1 (inverted polarity):

Low-to-high transition only.

01 = Trigger/event/interrupt is generated on transition of the comparator output: If CPOL = 0 (non-inverted polarity):

Low-to-high transition only.

If CPOL = 1 (inverted polarity):

High-to-low transition only.

00 = Trigger/event/interrupt generation is disabled bit 5 **Unimplemented:** Read as ‘0’

bit 4 **CREF:** Comparator Reference Select bit (non-inverting input)

1 = Non-inverting input connects to the internal reference defined by the CVREFSEL bit in CMSTAT register

0 = Non-inverting input connects to the CxINA pin bit 3-2 **Unimplemented:** Read as ‘0’

bit 1-0 **CCH<1:0>:** Comparator Channel Select bits

11 = Inverting input of the comparator connects to the band gap reference voltage

10 = Inverting input of the comparator connects to the CxIND pin 01 = Inverting input of the comparator connects to the CxINC pin 00 = Inverting input of the comparator connects to the CxINB pin

NOTES:

* 1. **VOLTAGE** **REFERENCE (CVREF)** The CVREF module is a 32-TAP DAC that provides a

32-to-1 MUX

selectable reference voltage. Although its primary

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a comprehensive reference source. To complement the information in this data sheet, refer to **Section 20. “Comparator Voltage Reference”** (DS61109) in the *“PIC32 Family Reference Manual”*, which is available from the Microchip web site ([www.microchip.com/PIC32)](http://www.microchip.com/PIC32). The informa- tion in this data sheet supersedes the information in the FRM.

purpose is to provide a reference for the analog comparators, it may also be used independently from them.

The module’s supply reference can be provided from either the device VDD/VSS or an external voltage refer- ence pin. The CVREF output is available for the comparators and for pin output.

The voltage reference has the following features:

* + - 32 Output Levels are Available
    - Internally Connected to Comparators to Conserve Device Pins
    - Output can be Connected to a Pin

A block diagram of the CVREF module is illustrated in [Figure 23-1](#_bookmark536).

FIGURE 23-1: VOLTAGE REFERENCE BLOCK DIAGRAM



REFSEL<1:0>

CVREF+

AVDD

DACDAT<4:0>

R

R

Output to

Comparators

R

R

32 Steps

CVREF

R

R R

DACOE

AVSS

### Voltage Reference Control Registers

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 250

TABLE 23-1: VOLTAGE REFERENCE REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2380 | DAC1CON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | DACDAT<4:0> | | | | | 0000 |
| 15:0 | ON | — | — | — | — | — | — | DACOE | — | — | — | — | — | — | REFSEL<1:0> | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** The register in this table has corresponding CLR, SET and INV registers at its virtual address, plus offsets of 0x4, 0x8 and 0xC, respectively.

REGISTER 23-1: DAC1CON: VOLTAGE REFERENCE CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | DACDAT<4:0> | | | | |
| 15:8 | R/W-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | R/W-0 |
| ON | — | — | — | — | — | — | DACOE |
| 7:0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 |
| — | — | — | — | — | — | REFSEL<1:0> | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-21 **Unimplemented:** Read as ‘0’

bit 20-16 **DACDAT<4:0>:** Voltage Reference Selection bits

11111 = (DACDAT<4:0> \* CVREF+/32) or (DACDAT<4:0> \* AVDD/32) volts depending on the REFSEL<1:0> bits

•

•

•

00000 = 0.0 volts

bit 15 **ON:** Voltage Reference Enable bit

1 = Voltage reference is enabled

0 = Voltage reference is disabled bit 14-9 **Unimplemented:** Read as ‘0’

bit 8 **DACOE:** Voltage Reference Output Enable bit

1 = Voltage level is output on the CVREF pin

0 = Voltage level is disconnected from the CVREF pin bit 7-2 **Unimplemented:** Read as ‘0’

bit 1-0 **REFSEL<1:0>:** Voltage Reference Source Select bits

11 = Reference voltage is AVDD

10 = No reference is selected – output is AVSS

01 = Reference voltage is the CVREF+ input pin voltage

00 = No reference is selected – output is AVSS

**PIC32MM0256GPM064 FAMILY**

NOTES:

DS60001387C-page 252  2016-2017 Microchip Technology Inc.

# HIGH/LOW-VOLTAGE DETECT (HLVD)

The High/Low-Voltage Detect (HLVD) module is a programmable circuit that allows the user to specify both the device voltage trip point and the direction of change.

An interrupt flag is set if the device experiences an excursion past the trip point in the direction of change. If the interrupt is enabled, the program execution will branch to the interrupt vector address and the software can then respond to the interrupt.

The HLVD Control register (see [Register 24-1](#_bookmark547)) completely controls the operation of the HLVD module. This allows the circuitry to be “turned off” by the user under software control, which minimizes the current consumption for the device.

16-to-1 MUX

FIGURE 24-1: HIGH/LOW-VOLTAGE DETECT (HLVD) MODULE BLOCK DIAGRAM



VDD

Externally Generated Trip Point

LVDIN

VDD

HLVDL<3:0>

ON VDIR

–

+

Set HLVDIF

**Band Gap 1.2V Typical**

ON

### High/Low-Voltage Detect Registers

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 254

TABLE 24-1: HIGH/LOW-VOLTAGE DETECT REGISTER MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2920 | HLVDCON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | ON | — | SIDL | — | VDIR | BGVST | IRVST | HLEVT | — | — | — | — | HLVDL<3:0> | | | | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** The register in this table has corresponding CLR, SET and INV registers at its virtual address, plus offsets of 0x4, 0x8 and 0xC, respectively.

REGISTER 24-1: HLVDCON: HIGH/LOW-VOLTAGE DETECT CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — |  |
| 15:8 | R/W-0 | U-0 | R/W-0 | U-0 | R/W-0 | R-0, HS, HC | R-0, HS, HC | R-0, HS, HC |
| ON | — | SIDL | — | VDIR | BGVST | IRVST | HLEVT |
| 7:0 | U-0 | U-0 | U-0 | U-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| — | — | — | — | HLVDL<3:0> | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** | HC = Hardware Clearable bit | HS = Hardware Settable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Unimplemented:** Read as ‘0’ bit 15 **ON:** HLVD Power Enable bit

1 = HLVD is enabled

0 = HLVD is disabled

bit 14 **Unimplemented:** Read as ‘0’

bit 13 **SIDL:** HLVD Stop in Idle Mode bit

1 = Discontinues module operation when device enters Idle mode

0 = Continues module operation in Idle mode bit 12 **Unimplemented:** Read as ‘0’

bit 11 **VDIR:** Voltage Change Direction Select bit

1 = Event occurs when voltage equals or exceeds trip point (HLVDL<3:0>)

0 = Event occurs when voltage equals or falls below trip point (HLVDL<3:0>) bit 10 **BGVST:** Band Gap Voltage Stable Flag bit

1 = Indicates that the band gap voltage is stable

0 = Indicates that the band gap voltage is unstable bit 9 **IRVST:** Internal Reference Voltage Stable Flag bit

1 = Internal reference voltage is stable; the High-Voltage Detect logic generates the interrupt flag at the specified voltage range

0 = Internal reference voltage is unstable; the High-Voltage Detect logic will not generate the interrupt flag at the specified voltage range and the HLVD interrupt should not be enabled

bit 8 **HLEVT:** High/Low-Voltage Detection Event Status bit

1 = Indicates HLVD event is active

0 = Indicates HLVD event is not active bit 7-4 **Unimplemented:** Read as ‘0’

REGISTER 24-1: HLVDCON: HIGH/LOW-VOLTAGE DETECT CONTROL REGISTER (CONTINUED)

bit 3-0 **HLVDL<3:0>:** High/Low-Voltage Detection Limit bits

1111 = External analog input is used (input comes from the LVDIN pin and compared with 1.2V band gap)

1110 = VDD trip point is between 2.00V and 2.22V 1101 = VDD trip point is between 2.08V and 2.33V 1100 = VDD trip point is between 2.15V and 2.44V 1011 = VDD trip point is between 2.25V and 2.55V 1010 = VDD trip point is between 2.35V and 2.69V 1001 = VDD trip point is between 2.45V and 2.80V 1000 = VDD trip point is between 2.65V and 2.98V 0111 = VDD trip point is between 2.75V and 3.09V 0110 = VDD trip point is between 2.95V and 3.30V 0101 = VDD trip point is between 3.25V and 3.63V 0100-0000 = Reserved; do not use.

# POWER-SAVING FEATURES

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. It is not intended to be a compre- hensive reference source. To complement the information in this data sheet, refer to **Section 10. “Power-Saving Modes”** (DS60001130) in the *“PIC32 Family “Refer- ence Manual”*, which is available from the Microchip web site ([www.microchip.com/](http://www.microchip.com/PIC32) [PIC32](http://www.microchip.com/PIC32)). The information in this data sheet supersedes the information in the FRM.

This section describes the power-saving features for the PIC32MM0256GPM064 family devices. These devices offer various methods and modes that allow the application to balance power consumption with device performance. In all of the methods and modes described in this section, power saving is controlled by software. The peripherals and CPU can be halted or disabled to reduce power consumption.

### Sleep Mode

In Sleep mode, the CPU and most peripherals are halted and the associated clocks are disabled. Some peripherals can continue to operate in Sleep mode and can be used to wake the device from Sleep. See the individual peripheral module sections for descriptions of behavior in Sleep. The device enters Sleep mode when the SLPEN bit (OSCCON<4>) is set and a WAIT instruction is executed.

Sleep mode includes the following characteristics:

* + There can be a Wake-up Delay based on the Oscillator Selection
  + The Fail-Safe Clock Monitor (FSCM) does not Operate During Sleep mode
  + The BOR Circuit remains Operative during Sleep mode
  + The WDT, if Enabled, is not automatically Cleared prior to Entering Sleep mode
  + Some Peripherals can Continue to Operate at Limited Functionality in Sleep mode; these Periph- erals include I/O Pins that Detect a Change in the Input Signal, WDT, ADC, UART and Peripherals that use an External Clock Input or the Internal LPRC Oscillator (e.g., RTCC and Timer1)
  + I/O Pins Continue to Sink or Source Current in the Same Manner as they do when the Device is not in Sleep

The processor will exit, or “wake-up”, from Sleep on one of the following events:

* + On any interrupt from an enabled source that is operating in Sleep. The interrupt priority must be greater than the current CPU priority.
  + On any form of device Reset.
  + On a WDT time-out.

If the interrupt priority is lower than or equal to the current priority, the CPU will remain halted, but the Peripheral Bus Clock (PBCLK) will start running and the device will enter into Idle mode. To set or clear the SLPEN bit, an unlock sequence must be executed. Refer to [**Section 26.4**](#_bookmark570)[**“System Registers Write Protection”**](#_bookmark570) for details.

### Standby Sleep Mode

Standby Sleep mode places the voltage regulator in Standby mode. This mode draws less power than Sleep mode but has a longer wake-up time. Standby Sleep mode is entered by setting the VREGS bit (PWRCON<0>) prior to entering Sleep by executing a WAIT instruction. All peripherals that can operate in Sleep mode can operate in Standby Sleep mode.

### Retention Sleep Mode

Retention Sleep uses a separate voltage regulator to provide the lowest power Sleep mode. This mode has a longer wake-up time than Sleep or Standby Sleep. This mode is entered by clearing the RETVR Configu- ration bit (FPOR<2>) and setting the RETEN bit (PWRCON<1>), prior to entering Sleep mode, and executing a WAIT instruction.

Only select peripherals, such as Timer1, WDT, RTCC and REFO, can operate in Retention Sleep mode.

**Note:** In Retention mode, the maximum peripheral output frequency to an I/O pin must be less than 33 kHz.

**Note:** When MCLR is used to wake the device from Retention Sleep, a POR Reset will occur.

### Idle Mode

In Idle mode, the CPU is halted; however, all clocks are still enabled. This allows peripherals to continue to operate. Peripherals can be individually configured to halt when entering Idle by setting their respective SIDL bit. Latency, when exiting Idle mode, is very low due to the CPU oscillator source remaining active.

The device enters Idle mode when the SLPEN bit (OSCCON<4>) is clear and a WAIT instruction is executed.

The processor will wake or exit from Idle mode on the following events:

* + On any interrupt event for which the interrupt source is enabled. The priority of the interrupt event must be greater than the current priority of the CPU. If the priority of the interrupt event is lower than or equal to the current priority of the CPU, the CPU will remain halted and the device will remain in Idle mode.
  + On any form of device Reset.
  + On a WDT time-out interrupt.

To set or clear the SLPEN bit, an unlock sequence must be executed. Refer to [**Section 26.4 “System**](#_bookmark570)[**Registers Write Protection”**](#_bookmark570) for details.

### Peripheral Module Disable

The Peripheral Module Disable (PMD) registers pro- vide a method to disable a peripheral module by stopping all clock sources supplied to that module. When a peripheral is disabled using the appropriate PMD control bit, the peripheral is in a minimum power consumption state. The control and status registers associated with the peripheral are also disabled, so writes to those registers do not take effect and read values are invalid.

To disable a peripheral, the associated PMDx bit must be set to ‘1’. To enable a peripheral, the associated PMDx bit must be cleared (default).

To prevent accidental configuration changes under nor- mal operation, writes to the PMDx registers are not allowed. Attempted writes appear to execute normally, but the contents of the registers remain unchanged. To change these registers, they must be unlocked in hardware. The register lock is controlled by the PMDLOCK bit in the PMDCON register (PMDCON<11>). Setting PMDLOCK prevents writes to the control registers; clearing PMDLOCK allows writes. To set or clear PMDLOCK, an unlock sequence must be executed. Refer to [**Section 26.4 “System Registers**](#_bookmark570)[**Write Protection”**](#_bookmark570) for details.

[Table 25-1](#_bookmark558) lists the module disable bits locations for all modules.

TABLE 25-1: PERIPHERAL MODULE DISABLE BITS AND LOCATIONS

|  |  |  |
| --- | --- | --- |
| **Peripheral** | **PMDx Bit Name** | **Register Name and Bit Location** |
| Analog-to-Digital Converter (ADC) | ADCMD | PMD1<0> |
| Voltage Reference (VR) | VREFMD | PMD1<12> |
| High/Low-Voltage Detect (HLVD) | HLVDMD | PMD1<20> |
| Comparator 1 (CMP1) | CMP1MD | PMD2<0> |
| Comparator 2 (CMP2) | CMP2MD | PMD2<1> |
| Comparator 3 (CMP3) | CMP3MD | PMD2<2> |
| Configurable Logic Cell 1 (CLC1) | CLC1MD | PMD2<24> |
| Configurable Logic Cell 2 (CLC2) | CLC2MD | PMD2<25> |
| Configurable Logic Cell 3 (CLC3) | CLC3MD | PMD2<26> |
| Configurable Logic Cell 4 (CLC4) | CLC4MD | PMD2<27> |
| Multiple Outputs Capture/Compare/PWM/ Timer1 (MCCP1) | CCP1MD | PMD3<8> |
| Multiple Outputs Capture/Compare/PWM/ Timer2 (MCCP2) | CCP2MD | PMD3<9> |
| Multiple Outputs Capture/Compare/PWM/ Timer3 (MCCP3) | CCP3MD | PMD3<10> |
| Single Output Capture/Compare/PWM/ Timer4 (SCCP4) | CCP4MD | PMD3<11> |
| Single Output Capture/Compare/PWM/ Timer5 (SCCP5) | CCP5MD | PMD3<12> |
| Single Output Capture/Compare/PWM/ Timer6 (SCCP6) | CCP6MD | PMD3<13> |
| Single Output Capture/Compare/PWM/ Timer7 (SCCP7) | CCP7MD | PMD3<14> |
| Single Output Capture/Compare/PWM/ Timer8 (SCCP8) | CCP8MD | PMD3<15> |
| Single Output Capture/Compare/PWM/ Timer9 (SCCP9) | CCP9MD | PMD3<16> |
| Timer1 (TMR1) | T1MD | PMD4<0> |
| Timer2 (TMR2) | T2MD | PMD4<1> |
| Timer3 (TMR3) | T3MD | PMD4<2> |
| Universal Asynchronous Receiver Transmitter 1 (UART1) | U1MD | PMD5<0> |

TABLE 25-1: PERIPHERAL MODULE DISABLE BITS AND LOCATIONS (CONTINUED)

|  |  |  |
| --- | --- | --- |
| **Peripheral** | **PMDx Bit Name** | **Register Name and Bit Location** |
| Universal Asynchronous Receiver Transmitter 2 (UART2) | U2MD | PMD5<1> |
| Universal Asynchronous Receiver Transmitter 3 (UART3) | U3MD | PMD5<2> |
| Serial Peripheral Interface 1 (SPI1) | SPI1MD | PMD5<8> |
| Serial Peripheral Interface 2 (SPI2) | SPI2MD | PMD5<9> |
| Serial Peripheral Interface 3 (SPI3) | SPI3MD | PMD5<10> |
| Inter-Integrated Circuit Interface 1 (I2C1) | I2C1MD | PMD5<16> |
| Inter-Integrated Circuit Interface 2 (I2C2) | I2C2MD | PMD5<17> |
| Inter-Integrated Circuit Interface 3 (I2C3) | I2C3MD | PMD5<18> |
| Universal Serial Bus (USB) | USBMD | PMD5<24> |
| Real-Time Clock and Calendar (RTCC) | RTCCMD | PMD6<0> |
| Reference Clock Output (REFO1) | REFOMD | PMD6<8> |
| Direct Memory Access (DMA) | DMAMD | PMD7<4> |

TABLE 25-2: PERIPHERAL MODULE DISABLE REGISTERS MAP

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 260

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name(1)** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 35B0 | PMDCON | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | FFFF |
| 15:0 | — | — | — | — | PMDLOCK | — | — | — | — | — | — | — | — | — | — | — | F7FF |
| 35C0 | PMD1 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | HLVDMD | — | — | — | — | FFEF |
| 15:0 | — | — | — | VREFMD | — | — | — | — | — | — | — | — | — | — | — | ADCMD | EFFE |
| 35D0 | PMD2 | 31:16 | — | — | — | — | CLC4MD | CLC3MD | CLC2MD | CLC1MD | — | — | — | — | — | — | — | — | F0FF |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | CMP3MD | CMP2MD | CMP1MD | FFF8 |
| 35E0 | PMD3 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | CCP9MD | FFFE |
| 15:0 | CCP8MD | CCP7MD | CCP6MD | CCP5MD | CCP4MD | CCP3MD | CCP2MD | CCP1MD | — | — | — | — | — | — | — | — | 00FF |
| 35F0 | PMD4 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | FFFF |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | T3MD | T2MD | T1MD | FFF8 |
| 3600 | PMD5 | 31:16 | — | — | — | — | — | — | — | USBMD | — | — | — | — | — | I2C3MD | I2C2MD | I2C1MD | FEF8 |
| 15:0 | — | — | — | — | — | SPI3MD | SPI2MD | SPI1MD | — | — | — | — | — | U3MD | U2MD | U1MD | F8F8 |
| 3610 | PMD6 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | FEFF |
| 15:0 | — | — | — | — | — | — | — | REFOMD | — | — | — | — | — | — | — | RTCCMD | FEFE |
| 3620 | PMD7 | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | FFFF |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | DMAMD | — | — | — | — | FFEF |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** All registers in this table have corresponding CLR, SET and INV registers at their virtual addresses, plus offsets of 0x4, 0x8 and 0xC, respectively.

### On-Chip Voltage Regulator Low-Power Modes

The main on-chip regulator always consumes a small incremental amount of current over IDD/IPD, including when the device is in Sleep mode, even though the core digital logic does not require power. To provide additional savings in applications where power resources are critical, the regulator can be made to enter Standby mode on its own whenever the device goes into Sleep mode. This feature is controlled by the VREGS bit (PWRCON<0>). Clearing the VREGS bit enables Standby mode.

**Note 1:** The SYSKEY register is used to unlock the PWRCON register.

When in Sleep mode, PIC32MM0256GPM064 family devices may use a separate low-power, low-voltage/ retention regulator to power critical circuits. This regula- tor, which operates at 1.2V nominal, maintains power to data RAM, WDT, Timer1 and the RTCC, while all other core digital logic is powered down. The low-voltage/ retention regulator is only available when Sleep mode is invoked. It is controlled by the RETVR Configuration bit (FPOR<2>) and in firmware by the RETEN bit (PWRCON<1>). RETVR must be programmed to zero (= 0) and the RETEN bit must be set (= 1) for the regulator to be enabled. When the retention regulator is enabled, the main regulator is off and does not consume power.

The main voltage regulator takes approximately 10 μS to generate output. During this time, designated as TVREG, code execution is disabled. TVREG is applied every time the device resumes operation after standby (VREGS bit = 0) or retention (RETEN bit = 1, RETVR bit = 0) modes. The TVREG specification is listed in [Table 29-12](#_bookmark681).

### Low-Power Brown-out Reset

The PIC32MM0256GPM064 family devices have a second low-power Brown-out Reset circuit with a reduced trip point precision. This low-power BOR circuit can be activated when the main BOR is dis- abled. It can be done by programming the LPBOREN Configuration bit (FPOR<3>) to one.

**Note 1:** When using the low-voltage/retention regulator, VREGS (PWRCON<0>) must be set to ‘1’.

NOTES:

# SPECIAL FEATURES

**Note:** This data sheet summarizes the features of the PIC32MM0256GPM064 family of devices. However, it is not intended to be a comprehensive reference source. To complement the information in this data sheet, refer to **Section 33. “Programming and Diagnostics”** (DS61129) in the *“PIC32 Family Reference Manual”*[, which is](http://www.microchip.com/PIC32) [available from the Microchip web site](http://www.microchip.com/PIC32) [(](http://www.microchip.com/PIC32)[www.microchip.com/PIC32).](http://www.microchip.com/PIC32)) The informa- tion in this data sheet supersedes the information in the FRM.

### Configuration Bits

PIC32MM0256GPM064 family devices contain a Boot Flash Memory (BFM) with an associated config- uration space. All Configuration Words are listed in [Table 26-3](#_bookmark583) and [Table 26-4](#_bookmark586), and [Register 26-1](#_bookmark590) through [Register 26-6](#_bookmark595) describe the configuration options.

### Code Execution from RAM

PIC32MM0256GPM064 family devices allow executing the code from RAM. The starting boundary of this special RAM space can be adjusted using the EXECADDR<7:0> bits in the CFGCON register with a 1-Kbyte step. Writing a non-zero value to these bits will move the boundary, effectively reducing the total amount of program memory space in RAM. Refer to [Table 26-5](#_bookmark597) and Register 26-7 for more information.

### Device ID

The Device ID identifies the device used. The ID can be read from the DEVID register. The Device IDs for the PIC32MM0256GPM064 family devices are listed in [Table 26-1](#_bookmark569). Also refer to [Table 26-5](#_bookmark597) and [Register 26-8](#_bookmark602) for more information.

TABLE 26-1: DEVICE IDs FOR

PIC32MM0256GPM064 FAMILY DEVICES

|  |  |
| --- | --- |
| **Device** | **DEVID** |
| PIC32MM0064GPM028 | 0x07708053 |
| PIC32MM0128GPM028 | 0x07710053 |
| PIC32MM0256GPM028 | 0x07718053 |
| PIC32MM0064GPM036 | 0x0770A053 |
| PIC32MM0128GPM036 | 0x07712053 |
| PIC32MM0256GPM036 | 0x0771A053 |
| PIC32MM0064GPM048 | 0x0772C053 |
| PIC32MM0128GPM048 | 0x07734053 |
| PIC32MM0256GPM048 | 0x0773C053 |
| PIC32MM0064GPM064 | 0x0770E053 |
| PIC32MM0128GPM064 | 0x07716053 |
| PIC32MM0256GPM064 | 0x0771E053 |

### System Registers Write Protection

The critical registers in the PIC32MM0256GPM064 family devices are protected (locked) to prevent an accidental write. If the registers are locked, a special two-step unlock sequence is required to modify the content of these registers (refer to [Example 26-1](#_bookmark572)). Once an unlock sequence is performed, the registers remain unlocked until they are relocked by writing an invalid key value.

A system unlock sequence is invalidated by writes to addresses other than SYSKEY. To prevent this, DMA transfers and interrupts should be disabled or the unlock sequence can be performed until a read of SYSKEY indicates a successful unlock (refer to [Example 26-2](#_bookmark574)).

To unlock the registers, the following steps should be done:

1. Disable interrupts and DMA transfers prior to the system unlock sequence.
2. Write a non-key value (such as 0x00000000) to the SYSKEY register to perform a lock.
3. Execute the system unlock sequence by writing the key values of 0xAA996655 and 0x556699AA to the SYSKEY register, in two back-to-back assembly or ‘C’ instructions.
4. Write the new value to the required register.
5. Write a non-key value (such as 0x00000000) to the SYSKEY register to perform a lock.
6. Re-enable interrupts and DMA transfers.

EXAMPLE 26-1: SYSTEM UNLOCK

SYSKEY = 0;

SYSKEY = AA996655; SYSKEY = 556699AA;

// force lock

// unlock sequence

// lock sequence

// user code to modify register contents SYSKEY = 0; // relock

EXAMPLE 26-2: SYSTEM UNLOCK WITH

DMA AND INTERRUPTS ENABLED

While (SYSKEY == 0) // repeat unlock sequence

until unlock succeeds

{

SYSKEY = 0; // force lock SYSKEY = AA996655; // unlock sequence SYSKEY = 556699AA; // lock sequence

}

// user code to modify register contents SYSKEY = 0; // relock

The registers that require this unlocking sequence are listed in the [Table 26-2](#_bookmark576).

TABLE 26-2: SYSTEM LOCKED REGISTERS

|  |  |  |
| --- | --- | --- |
| **Register Name** | **Register Description** | **Peripheral** |
| OSCCON | Oscillator Control | Oscillator |
| SPLLCON | System PLL Control | Oscillator |
| OSCTUN | FRC Tuning | Oscillator |
| PMDCON | Peripheral Module Disable Control | PMD |
| RSWRST | Software Reset | Reset |
| RPCON | Peripheral Pin Select Configuration | I/O Ports |
| PWRCON | Sleep Power Control | System |
| RTCCON1 | RTCC Control | RTCC |

The SYSKEY register read value indicates the status. A value of ‘0’ indicates that the system registers are locked. A value of ‘1’ indicates that the system registers are unlocked. For more information about the SYSKEY register refer to [Table 26-5](#_bookmark597) and [Register 26-9](#_bookmark606).

### Band Gap Voltage Reference

PIC32MM0256GPM064 family devices have a precision voltage reference band gap circuit used by many modules. The analog buffers are implemented between the band gap circuit and these modules. The buffers are automatically enabled by the hardware if some part of the device needs the band gap reference. The stabilization time is required when the buffer is switched on. The soft- ware can enable these buffers in advance to allow the band gap voltage to stabilize before the module uses it. The ANGFG register contains bits to enable the band gap buffers for the comparators (VBGCMP bit) and ADC (VBGADC bit). Refer to [Table 26-6](#_bookmark607) and [Register 26-10](#_bookmark611) for more information.

### Programming and Diagnostics

PIC32MM0256GPM064 family devices provide a complete range of programming and diagnostic features:

* Simplified field programmability using two-wire

In-Circuit Serial Programming™ (ICSP™) interfaces

* Debugging using ICSP
* Programming and debugging capabilities using the EJTAG extension of JTAG
* JTAG boundary scan testing for device and board diagnostics

### Unique Device Identifier (UDID)

PIC32MM0256GPM064 family devices are individually encoded during final manufacturing with a Unique Device Identifier or UDID. The UDID cannot be erased by a bulk erase command or any other user accessible means. This feature allows for manufacturing trace- ability of Microchip Technology devices in applications where this is a requirement. It may also be used by the application manufacturer for any number of things that may require unique identification, such as:

* Tracking the device
* Unique serial number
* Unique security key

The UDID comprises five 32-bit program words. When taken together, these fields form a unique 160-bit identifier.

The UDID is stored in five read-only locations, located from 0xBFC41840 to 0xBFC41850 in the device configuration space. [Table 26-7](#_bookmark613) lists the addresses of the Identifier Words.

### Reserved Registers

PIC32MM0256GPM064 family devices have 3 reserved registers, located at 0xBF800400, 0xBF800480 and 0xBF802280. The application code must not modify these reserved locations. [Table 26-8](#_bookmark615) lists the addresses of these reserved registers.

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 265

### Configuration Word Registers

TABLE 26-3: CONFIGURATION WORDS SUMMARY

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BFC0\_#)** | **Register Name** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | |
| **31\15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 17C0 | RESERVED | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 17C4 | FDEVOPT | 31:16 | USERID<15:0> | | | | | | | | | | | | | | | |
| 15:0 | FVBUSIO | FUSBIDIO | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | ALTI2C | SOSCHP | r-1 | r-1 | r-1 |
| 17C8 | FICD | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | ICS<1:0> | | JTAGEN | r-1 | r-1 |
| 17CC | FPOR | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | LPBOREN | RETVR | BOREN<1:0> | |
| 17D0 | FWDT | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | FWDTEN | RCLKSEL<1:0> | | RWDTPS<4:0> | | | | | WINDIS | FWDTWINSZ<1:0> | | SWDTPS<4:0> | | | | |
| 17D4 | FOSCSEL | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | FCKSM<1:0> | | r-1 | SOSCSEL | r-1 | OSCIOFNC | POSCMOD<1:0> | | IESO | SOSCEN | r-1 | PLLSRC | r-1 | FNOSC<2:0> | | |
| 17D8 | FSEC | 31:16 | CP | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 17DC | RESERVED | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 17E0 | RESERVED | 31:16 | r-0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 17E4 | RESERVED | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |

**Legend:** r-0 = Reserved bit, must be programmed as ‘0’; r-1 = Reserved bit, must be programmed as ‘1’.

TABLE 26-4: ALTERNATE CONFIGURATION WORDS SUMMARY

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 266

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BFC0\_#)** | **Register Name** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | |
| **31\15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 1740 | RESERVED | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 1744 | AFDEVOPT | 31:16 | USERID<15:0> | | | | | | | | | | | | | | | |
| 15:0 | FVBUSIO | FUSBIDIO | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | ALTI2C | SOSCHP | r-1 | r-1 | r-1 |
| 1748 | AFICD | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | ICS<1:0> | | JTAGEN | r-1 | r-1 |
| 174C | AFPOR | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | LPBOREN | RETVR | BOREN<1:0> | |
| 1750 | AFWDT | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | FWDTEN | RCLKSEL<1:0> | | RWDTPS<4:0> | | | | | WINDIS | FWDTWINSZ<1:0> | | SWDTPS<4:0> | | | | |
| 1754 | AFOSCSEL | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | FCKSM<1:0> | | r-1 | SOSCSEL | r-1 | OSCIOFNC | POSCMOD<1:0> | | IESO | SOSCEN | r-1 | PLLSRC | r-1 | FNOSC<2:0> | | |
| 1758 | AFSEC | 31:16 | CP | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 175C | RESERVED | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 1760 | RESERVED | 31:16 | r-0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 1764 | RESERVED | 31:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| 15:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |

**Legend:** r-0 = Reserved bit, must be programmed as ‘0’; r-1 = Reserved bit, must be programmed as ‘1’.

REGISTER 26-1: FDEVOPT/AFDEVOPT: DEVICE OPTIONS CONFIGURATION REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/P | R/P | R/P | R/P | R/P | R/P | R/P | R/P |
| USERID<15:8> | | | | | | | |
| 23:16 | R/P | R/P | R/P | R/P | R/P | R/P | R/P | R/P |
| USERID<7:0> | | | | | | | |
| 15:8 | R/P | R/P | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| FVBUSIO | FUSBIDIO | — | — | — | — | — | — |
| 7:0 | r-1 | r-1 | r-1 | R/P | R/P | r-1 | r-1 | r-1 |
| — | — | — | ALTI2C | SOSCHP | — | — | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** | r = Reserved bit | P = Programmable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **USERID<15:0>:** User ID bits (2 bytes which can programmed to any value) bit 15 **FVBUSIO:** USB VBUS\_ON Selection bit

1 = VBUSON pin is controlled by the USB module

0 = VBUSON pin is controlled by the port function bit 14 **FUSBIDIO:** USB USBID Selection bit

1 = USBID pin is controlled by the USB module

0 = USBID pin is controlled by the port function bit 13-5 **Reserved:** Program as ‘1’

bit 4 **ALTI2C:** Alternate I2C1 Location Select bit

1 = SDA1 and SCL1 are on pins, RB8 and RB9

0 = SDA1 and SCL1 are moved to alternate I2C locations, RB5 and RC9

bit 3 **SOSCHP:** Secondary Oscillator (SOSC) High-Power Enable bit

1 = SOSC operates in normal power mode

0 = SOSC operates in High-Power mode bit 2-0 **Reserved:** Program as ‘1’

REGISTER 26-2: FICD/AFICD: ICD/DEBUG CONFIGURATION REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| — | — | — | — | — | — | — | — |
| 23:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| — | — | — | — | — | — | — | — |
| 15:8 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| — | — | — | — | — | — | — | — |
| 7:0 | r-1 | r-1 | r-1 | R/P | R/P | R/P | r-1 | r-1 |
| — | — | — | ICS<1:0> | | JTAGEN | — | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** | r = Reserved bit | P = Programmable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-5 **Reserved:** Program as ‘1’

bit 4-3 **ICS<1:0>:** ICE/ICD Communication Channel Selection bits

11 = Communicates on PGEC1/PGED1 10 = Communicates on PGEC2/PGED2 01 = Communicates on PGEC3/PGED3 00 = Not connected

bit 2 **JTAGEN:** JTAG Enable bit

1 = JTAG is enabled

0 = JTAG is disabled

bit 1-0 **Reserved:** Program as ‘1’

REGISTER 26-3: FPOR/AFPOR: POWER-UP SETTINGS CONFIGURATION REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| — | — | — | — | — | — | — | — |
| 23:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| — | — | — | — | — | — | — | — |
| 15:8 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| — | — | — | — | — | — | — | — |
| 7:0 | r-1 | r-1 | r-1 | r-1 | R/P | R/P | R/P | R/P |
| — | — | — | — | LPBOREN | RETVR | BOREN<1:0> | |

|  |  |  |
| --- | --- | --- |
| **Legend:** | r = Reserved bit | P = Programmable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-4 **Reserved:** Program as ‘1’

bit 3 **LPBOREN:** Low-Power BOR Enable bit

1 = Low-Power BOR is enabled when main BOR is disabled

0 = Low-Power BOR is disabled

bit 2 **RETVR:** Retention Voltage Regulator Enable bit

1 = Retention regulator is disabled

0 = Retention regulator is enabled and controlled by the RETEN bit during Sleep bit 1-0 **BOREN<1:0>:** Brown-out Reset Enable bits

11 = Brown-out Reset is enabled in hardware; SBOREN bit is disabled

10 = Brown-out Reset is enabled only while device is active and disabled in Sleep; SBOREN bit is disabled

01 = Brown-out Reset is controlled with the SBOREN bit setting

00 = Brown-out Reset is disabled in hardware; SBOREN bit is disabled

REGISTER 26-4: FWDT/AFWDT: WATCHDOG TIMER CONFIGURATION REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| — | — | — | — | — | — | — | — |
| 23:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/P | R/P | R/P | R/P | R/P | R/P | R/P | R/P |
| FWDTEN | RCLKSEL<1:0> | | RWDTPS<4:0> | | | | |
| 7:0 | R/P | R/P | R/P | R/P | R/P | R/P | R/P | R/P |
| WINDIS | FWDTWINSZ<1:0> | | SWDTPS<4:0> | | | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Legend:**  R = Readable bit  -n = Value at POR | | r = Reserved bit W = Writable bit  ‘1’ = Bit is set | P = Programmable bit  U = Unimplemented bit, read as ‘0’  ‘0’ = Bit is cleared x = Bit is unknown |
| bit 31-16 | **Reserved:** Program as ‘1’ | | |
| bit 15 | **FWDTEN:** Watchdog Timer Enable bit | | |
|  | 1 = WDT is enabled  0 = WDT is disabled | | |
| bit 14-13 | **RCLKSEL<1:0>:** Run Mode Watchdog Timer Clock Source Selection bits | | |
|  | 11 = Clock source is the LPRC oscillator (same as for Sleep mode)  10 = Clock source is the FRC oscillator  01 = Reserved  00 = Clock source is the system clock | | |
| bit 12-8 | **RWDTPS<4:0>:** Run Mode Watchdog Timer Postscale Select bits | | |
|  | From 10100 to 11111 = 1:1048576.  10011 = 1:524288  10010 = 1:262144  10001 = 1:131072  10000 = 1:65536  01111 = 1:32768  01110 = 1:16384  01101 = 1:8192  01100 = 1:4096  01011 = 1:2048  01010 = 1:1024  01001 = 1:512  01000 = 1:256  00111 = 1:128  00110 = 1:64  00101 = 1:32  00100 = 1:16  00011 = 1:8  00010 = 1:4  00001 = 1:2  00000 = 1:1 | | |
| bit 7 | **WINDIS:** Windowed Watchdog Timer Disable bit | | |
|  | 1 = Windowed mode is disabled  0 = Windowed mode is enabled | | |

REGISTER 26-4: FWDT/AFWDT: WATCHDOG TIMER CONFIGURATION REGISTER (CONTINUED)

bit 6-5 **FWDTWINSZ<1:0>:** Watchdog Timer Window Size bits

11 = Watchdog Timer window size is 25% 10 = Watchdog Timer window size is 37.5% 01 = Watchdog Timer window size is 50% 00 = Watchdog Timer window size is 75%

bit 4-0 **SWDTPS<4:0>:** Sleep Mode Watchdog Timer Postscale Select bits From 10100 to 11111 = 1:1048576.

10011 = 1:524288

10010 = 1:262144

10001 = 1:131072

10000 = 1:65536

01111 = 1:32768

01110 = 1:16384

01101 = 1:8192

01100 = 1:4096

01011 = 1:2048

01010 = 1:1024

01001 = 1:512

01000 = 1:256

00111 = 1:128

00110 = 1:64

00101 = 1:32

00100 = 1:16

00011 = 1:8

00010 = 1:4

00001 = 1:2

00000 = 1:1

REGISTER 26-5: FOSCSEL/AFOSCSEL: OSCILLATOR SELECTION CONFIGURATION REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| — | — | — | — | — | — | — | — |
| 23:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| — | — | — | — | — | — | — | — |
| 15:8 | R/P | R/P | r-1 | R/P | r-1 | R/P | R/P | R/P |
| FCKSM<1:0> | | — | SOSCSEL | — | OSCIOFNC | POSCMOD<1:0> | |
| 7:0 | R/P | R/P | r-1 | R/P | r-1 | R/P | R/P | R/P |
| IESO | SOSCEN | — | PLLSRC | — | FNOSC<2:0> | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** | r = Reserved bit | P = Programmable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-16 **Reserved:** Program as ‘1’

bit 15-14 **FCKSM<1:0>:** Clock Switching and Fail-Safe Clock Monitor Enable bits

11 = Clock switching is enabled; Fail-Safe Clock Monitor is enabled 10 = Clock switching is disabled; Fail-Safe Clock Monitor is enabled 01 = Clock switching is enabled; Fail-Safe Clock Monitor is disabled 00 = Clock switching is disabled; Fail-Safe Clock Monitor is disabled

bit 13 **Reserved:** Program as ‘1’

bit 12 **SOSCSEL:** Secondary Oscillator (SOSC) External Clock Enable bit

1 = Crystal is used (RA4 and RB4 pins are controlled by the SOSC)

0 = External clock connected to the SOSCO pin is used (RA4 and RB4 pins are controlled by I/O PORTx registers)

bit 11 **Reserved:** Program as ‘1’

bit 10 **OSCIOFNC:** System Clock on CLKO Pin Enable bit

1 = CLKO/OSC2 pin operates as normal I/O

0 = System clock is connected to the CLKO/OSC2 pin

bit 9-8 **POSCMOD<1:0>:** Primary Oscillator (POSC) Mode Selection bits

11 = Primary Oscillator is disabled 10 = HS Oscillator mode is selected 01 = XT Oscillator mode is selected

00 = External Clock (EC) mode is selected bit 7 **IESO:** Two-Speed Start-up Enable bit

1 = Two-Speed Start-up is enabled

0 = Two-Speed Start-up is disabled

bit 6 **SOSCEN:** Secondary Oscillator (SOSC) Enable bit

1 = Secondary Oscillator enable

0 = Secondary Oscillator disable bit 5 **Reserved:** Program as ‘1’

bit 4 **PLLSRC:** System PLL Input Clock Selection bit

1 = FRC oscillator is selected as the PLL reference input on a device Reset

0 = Primary Oscillator (POSC) is selected as the PLL reference input on a device Reset bit 3 **Reserved:** Program as ‘1’

REGISTER 26-5: FOSCSEL/AFOSCSEL: OSCILLATOR SELECTION CONFIGURATION REGISTER (CONTINUED)

bit 2-0 **FNOSC<2:0>:** Oscillator Selection bits

110 and 111 = Reserved (selects Fast RC (FRC) Oscillator with Divide-by-N)

101 = Low-Power RC Oscillator (LPRC) 100 = Secondary Oscillator (SOSC) 011 = Reserved

010 = Primary Oscillator (XT, HS, EC)

001 = Primary or FRC Oscillator with PLL

000 = Fast RC Oscillator (FRC) with Divide-by-N

REGISTER 26-6: FSEC/AFSEC: CODE-PROTECT CONFIGURATION REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R/P | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| CP | — | — | — | — | — | — | — |
| 23:16 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| — | — | — | — | — | — | — | — |
| 15:8 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| — | — | — | — | — | — | — | — |
| 7:0 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 | r-1 |
| — | — | — | — | — | — | — | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** | r = Reserved bit | P = Programmable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31 **CP:** Code Protection Enable bit

1 = Code protection is disabled

0 = Code protection is enabled bit 30-0 **Reserved:** Program as ‘1’

TABLE 26-5: RAM CONFIGURATION, DEVICE ID AND SYSTEM LOCK REGISTERS MAP

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 274

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets(1)** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 3640 | CFGCON | 31:16 | — | — | — | — | BMXERRDIS | — | BMXARB<1:0> | | EXECADDR<7:0> | | | | | | | | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | JTAGEN | — | r | r | 0003 |
| 3660 | DEVID | 31:16 | VER<3:0> | | | | DEVID<27:16> | | | | | | | | | | | | xxxx |
| 15:0 | DEVID<15:0> | | | | | | | | | | | | | | | | xxxx |
| 3670 | SYSKEY | 31:16 | SYSKEY<31:16> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | SYSKEY<15:0> | | | | | | | | | | | | | | | | 0001 |

**Legend:** x = unknown value on Reset; r = reserved bit; — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** Reset values are dependent on the device variant.

REGISTER 26-7: CFGCON: CONFIGURATION CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | R/W-0 | U-0 | R/W-0 | R/W-0 |
| — | — | — | — | BMXERRDIS | — | BMXARB<1:0> | |
| 23:16 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 | R/W-0 |
| EXECADDR<7:0> | | | | | | | |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | U-0 | U-0 | U-0 | U-0 | R/W-P | U-0 | r-1 | r-1 |
| — | — | — | — | JTAGEN | — | — | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** | r = Reserved bit |  |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-28 **Unimplemented:** Read as ‘0’

bit 27 **BMXERRDIS:** Bus Matrix (BMX) Exception Error Disable bit

1 = Disables BMX error exception generation**(**[**1**](#_bookmark601)**)**

0 = Enables BMX error exception generation bit 26 **Unimplemented:** Read as ‘0’

bit 25-24 **BMXARB<1:0>:** Bus Matrix Arbitration Mode Select bits

11 = Reserved

10 = Mode 2 – Round Robin

01 = Mode 1 – Fixed with CPU as the lowest priority

00 = Mode 0 – Fixed with CPU as the highest priority

bit 23-16 **EXECADDR<7:0>:** RAM Program Space Start Address bits

11111111 = RAM program space starts at the 255-Kbyte boundary (from 0xA003FC00)

•

•

•

00000010 = RAM program space starts at 2-Kbyte boundary (from 0xA0000800) 00000001 = RAM program space starts at 1-Kbyte boundary (from 0xA0000400) 00000000 = All data RAM is allocated to program space (from 0xA0000000)

bit 15-4 **Unimplemented:** Read as ‘0’ bit 3 **JTAGEN:** JTAG Enable bit

1 = Enables 4-wire JTAG

0 = Disables 4-wire JTAG

bit 2 **Unimplemented:** Read as ‘0’

bit 1-0 **Reserved:** Maintain as ‘1’

**Note 1:** An exception is not generated when an unimplemented address is accessed. The returned value on a read operation of unimplemented memory is 0x00000000.

REGISTER 26-8: DEVID: DEVICE ID REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | R-x | R-x | R-x | R-x | R-x | R-x | R-x | R-x |
| VER<3:0>**(**[**1**](#_bookmark604)**)** | | | | ID<27:24>**(**[**1**](#_bookmark604)**)** | | | |
| 23:16 | R-x | R-x | R-x | R-x | R-x | R-x | R-x | R-x |
| ID<23:16>**(**[**1**](#_bookmark604)**)** | | | | | | | |
| 15:8 | R-x | R-x | R-x | R-x | R-x | R-x | R-x | R-x |
| ID<15:8>**(**[**1**](#_bookmark604)**)** | | | | | | | |
| 7:0 | R-x | R-x | R-x | R-x | R-x | R-x | R-x | R-x |
| ID<7:0>**(**[**1**](#_bookmark604)**)** | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-28 **VER<3:0>:** Revision Identifier bits**(**[**1**](#_bookmark604)**)** bit 27-0 **DEVID<27:0>:** Device ID bits**(**[**1**](#_bookmark604)**)**

**Note 1:** Reset values are dependent on the device variant.

REGISTER 26-9: SYSKEY: SYSTEM UNLOCK REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 |
| SYSKEY<31:24> | | | | | | | |
| 23:16 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 |
| SYSKEY<23:16> | | | | | | | |
| 15:8 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 |
| SYSKEY<15:8> | | | | | | | |
| 7:0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | W-0 | R/W-1 |
| SYSKEY<7:0> | | | | | | | |

|  |  |  |
| --- | --- | --- |
| **Legend:** |  | |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-0 **SYSKEY<31:0>:** Unlock and Lock Key bits

A write of 0xAA996655, followed by a write of 0x556699AA to SYSKEY, is required to unlock select system registers. Refer to [Example 26-1](#_bookmark572).

Bit 0 Indicates System Lock Status:

1 = The system is unlocked

0 = The system is locked

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 277

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2300 | ANCFG**(**[**1**](#_bookmark610)**)** | 31:16 | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | — | 0000 |
| 15:0 | — | — | — | — | — | — | — | — | — | — | — | — | — | VBGADC | VBGCMP | — | 0000 |

**Legend:** — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

**Note 1:** This register has corresponding CLR, SET and INV registers at its virtual address, plus an offset of 0x4, 0x8 and 0xC, respectively.

REGISTER 26-10: ANCFG: BAND GAP CONTROL REGISTER

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Bit Range** | **Bit 31/23/15/7** | **Bit 30/22/14/6** | **Bit 29/21/13/5** | **Bit 28/20/12/4** | **Bit 27/19/11/3** | **Bit 26/18/10/2** | **Bit 25/17/9/1** | **Bit 24/16/8/0** |
| 31:24 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 23:16 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 15:8 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 | U-0 |
| — | — | — | — | — | — | — | — |
| 7:0 | U-0 | U-0 | U-0 | U-0 | U-0 | R/W-0, HS, HC | R/W-0, HS, HC | U-0 |
| — | — | — | — | — | VBGADC | VBGCMP | — |

|  |  |  |
| --- | --- | --- |
| **Legend:** | HC = Hardware Clearable bit | HS = Hardware Settable bit |
| R = Readable bit | W = Writable bit | U = Unimplemented bit, read as ‘0’ |
| -n = Value at POR | ‘1’ = Bit is set | ‘0’ = Bit is cleared x = Bit is unknown |

bit 31-3 **Unimplemented:** Read as ‘0’

bit 2 **VBGADC:** ADC Band Gap Enable bit

1 = ADC band gap is enabled

0 = ADC band gap is disabled

bit 1 **VBGCMP:** Comparator Band Gap Enable bit

1 = Comparator band gap is enabled

0 = Comparator band gap is disabled bit 0 **Unimplemented:** Read as ‘0’

**PIC32MM0256GPM064 FAMILY**

 2016-2017 Microchip Technology Inc.

DS60001387C-page 279

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF84\_#)** | **Register Name** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 1840 | UDID1 | 31:16 | UDID Word 1<31:0> | | | | | | | | | | | | | | | | xxxx |
| 15:0 | xxxx |
| 1844 | UDID2 | 31:16 | UDID Word 2<31:0> | | | | | | | | | | | | | | | | xxxx |
| 15:0 | xxxx |
| 1848 | UDID3 | 31:16 | UDID Word 3<31:0> | | | | | | | | | | | | | | | | xxxx |
| 15:0 | xxxx |
| 184C | UDID4 | 31:16 | UDID Word 4<31:0> | | | | | | | | | | | | | | | | xxxx |
| 15:0 | xxxx |
| 1850 | UDID5 | 31:16 | UDID Word 5<31:0> | | | | | | | | | | | | | | | | xxxx |
| 15:0 | xxxx |

**Legend:** x = unknown value on Reset; — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

TABLE 26-8: RESERVED REGISTERS MAP

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Virtual Address (BF80\_#)** | **Register Name** | **Bit Range** | **Bits** | | | | | | | | | | | | | | | | **All Resets** |
| **31/15** | **30/14** | **29/13** | **28/12** | **27/11** | **26/10** | **25/9** | **24/8** | **23/7** | **22/6** | **21/5** | **20/4** | **19/3** | **18/2** | **17/1** | **16/0** |
| 2900 | RESERVED1 | 31:16 | Reserved Register 1<31:0> | | | | | | | | | | | | | | | | 0000 |
| 15:0 | 0000 |

**Legend:** x = unknown value on Reset; — = unimplemented, read as ‘0’. Reset values are shown in hexadecimal.

NOTES:

# 27.0 INSTRUCTION SET

The PIC32MM0256GPM064 family instruction set complies with the MIPS® Release 3 instruction set architecture. Only microMIPS32™ instructions are

supported. The PIC32MM0256GPM064 family does not have the following features:

* + - Core extend instructions
    - Coprocessor 1 instructions
    - Coprocessor 2 instructions

**Note:** Refer to the *“MIPS® Architecture for Programmers Volume II-B: The microMIPS32™ Instruction Set”* at [www.imgtec.com](http://www.imgtec.com/) for more information.

NOTES:

# DEVELOPMENT SUPPORT

The PIC® microcontrollers (MCU) and dsPIC® digital signal controllers (DSC) are supported with a full range of software and hardware development tools:

* + - Integrated Development Environment
      * MPLAB® X IDE Software
    - Compilers/Assemblers/Linkers
      * MPLAB XC Compiler
      * MPASMTM Assembler
      * MPLINKTM Object Linker/ MPLIBTM Object Librarian
      * MPLAB Assembler/Linker/Librarian for Various Device Families
    - Simulators
      * MPLAB X SIM Software Simulator
    - Emulators
      * MPLAB REAL ICE™ In-Circuit Emulator
    - In-Circuit Debuggers/Programmers
      * MPLAB ICD 3
      * PICkit™ 3
    - Device Programmers
      * MPLAB PM3 Device Programmer
    - Low-Cost Demonstration/Development Boards, Evaluation Kits and Starter Kits
    - Third-party development tools

### MPLAB X Integrated Development Environment Software

The MPLAB X IDE is a single, unified graphical user interface for Microchip and third-party software, and hardware development tool that runs on Windows®, Linux and Mac OS® X. Based on the NetBeans IDE, MPLAB X IDE is an entirely new IDE with a host of free software components and plug-ins for high-

performance application development and debugging. Moving between tools and upgrading from software simulators to hardware debugging and programming tools is simple with the seamless user interface.

With complete project management, visual call graphs, a configurable watch window and a feature-rich editor that includes code completion and context menus, MPLAB X IDE is flexible and friendly enough for new users. With the ability to support multiple tools on multiple projects with simultaneous debugging, MPLAB X IDE is also suitable for the needs of experienced users.

Feature-Rich Editor:

* Color syntax highlighting
* Smart code completion makes suggestions and provides hints as you type
* Automatic code formatting based on user-defined rules
* Live parsing

User-Friendly, Customizable Interface:

* Fully customizable interface: toolbars, toolbar buttons, windows, window placement, etc.
* Call graph window Project-Based Workspaces:
* Multiple projects
* Multiple tools
* Multiple configurations
* Simultaneous debugging sessions File History and Bug Tracking:
* Local file history feature
* Built-in support for Bugzilla issue tracker

### MPLAB XC Compilers

The MPLAB XC Compilers are complete ANSI C compilers for all of Microchip’s 8, 16 and 32-bit MCU and DSC devices. These compilers provide powerful integration capabilities, superior code optimization and ease of use. MPLAB XC Compilers run on Windows, Linux or MAC OS X.

For easy source level debugging, the compilers provide debug information that is optimized to the MPLAB X IDE.

The free MPLAB XC Compiler editions support all devices and commands, with no time or memory restrictions, and offer sufficient code optimization for most applications.

MPLAB XC Compilers include an assembler, linker and utilities. The assembler generates relocatable object files that can then be archived or linked with other relocatable object files and archives to create an exe- cutable file. MPLAB XC Compiler uses the assembler to produce its object file. Notable features of the assembler include:

* Support for the entire device instruction set
* Support for fixed-point and floating-point data
* Command-line interface
* Rich directive set
* Flexible macro language
* MPLAB X IDE compatibility

### MPASM Assembler

The MPASM Assembler is a full-featured, universal macro assembler for PIC10/12/16/18 MCUs.

The MPASM Assembler generates relocatable object files for the MPLINK Object Linker, Intel® standard HEX files, MAP files to detail memory usage and symbol reference, absolute LST files that contain source lines and generated machine code, and COFF files for debugging.

The MPASM Assembler features include:

* Integration into MPLAB X IDE projects
* User-defined macros to streamline assembly code
* Conditional assembly for multipurpose source files
* Directives that allow complete control over the assembly process

### MPLINK Object Linker/ MPLIB Object Librarian

The MPLINK Object Linker combines relocatable objects created by the MPASM Assembler. It can link relocatable objects from precompiled libraries, using directives from a linker script.

The MPLIB Object Librarian manages the creation and modification of library files of precompiled code. When a routine from a library is called from a source file, only the modules that contain that routine will be linked in with the application. This allows large libraries to be used efficiently in many different applications.

The object linker/library features include:

* Efficient linking of single libraries instead of many smaller files
* Enhanced code maintainability by grouping related modules together
* Flexible creation of libraries with easy module listing, replacement, deletion and extraction

### MPLAB Assembler, Linker and Librarian for Various Device Families

MPLAB Assembler produces relocatable machine code from symbolic assembly language for PIC24, PIC32 and dsPIC DSC devices. MPLAB XC Compiler uses the assembler to produce its object file. The assembler generates relocatable object files that can then be archived or linked with other relocatable object files and archives to create an executable file. Notable features of the assembler include:

* Support for the entire device instruction set
* Support for fixed-point and floating-point data
* Command-line interface
* Rich directive set
* Flexible macro language
* MPLAB X IDE compatibility

### MPLAB X SIM Software Simulator

The MPLAB X SIM Software Simulator allows code development in a PC-hosted environment by simulat- ing the PIC MCUs and dsPIC DSCs on an instruction level. On any given instruction, the data areas can be examined or modified and stimuli can be applied from a comprehensive stimulus controller. Registers can be logged to files for further run-time analysis. The trace buffer and logic analyzer display extend the power of the simulator to record and track program execution, actions on I/O, most peripherals and internal registers.

The MPLAB X SIM Software Simulator fully supports symbolic debugging using the MPLAB XC Compilers, and the MPASM and MPLAB Assemblers. The soft- ware simulator offers the flexibility to develop and debug code outside of the hardware laboratory envi- ronment, making it an excellent, economical software development tool.

### MPLAB REAL ICE In-Circuit Emulator System

The MPLAB REAL ICE In-Circuit Emulator System is Microchip’s next generation high-speed emulator for Microchip Flash DSC and MCU devices. It debugs and programs all 8, 16 and 32-bit MCU, and DSC devices with the easy-to-use, powerful graphical user interface of the MPLAB X IDE.

The emulator is connected to the design engineer’s PC using a high-speed USB 2.0 interface and is connected to the target with either a connector compatible with in-circuit debugger systems (RJ-11) or with the new high-speed, noise tolerant, Low- Voltage Differential Signal (LVDS) interconnection (CAT5).

The emulator is field upgradable through future firmware downloads in MPLAB X IDE. MPLAB REAL ICE offers significant advantages over competitive emulators including full-speed emulation, run-time variable watches, trace analysis, complex breakpoints, logic probes, a ruggedized probe interface and long (up to three meters) interconnection cables.

### MPLAB ICD 3 In-Circuit Debugger System

The MPLAB ICD 3 In-Circuit Debugger System is Microchip’s most cost-effective, high-speed hardware debugger/programmer for Microchip Flash DSC and MCU devices. It debugs and programs PIC Flash microcontrollers and dsPIC DSCs with the powerful, yet easy-to-use graphical user interface of the MPLAB IDE.

The MPLAB ICD 3 In-Circuit Debugger probe is connected to the design engineer’s PC using a high- speed USB 2.0 interface and is connected to the target with a connector compatible with the MPLAB ICD 2 or MPLAB REAL ICE systems (RJ-11). MPLAB ICD 3

supports all MPLAB ICD 2 headers.

### PICkit 3 In-Circuit Debugger/ Programmer

The MPLAB PICkit 3 allows debugging and program- ming of PIC and dsPIC Flash microcontrollers at a most affordable price point using the powerful graphical user interface of the MPLAB IDE. The MPLAB PICkit 3 is connected to the design engineer’s PC using a full- speed USB interface and can be connected to the target via a Microchip debug (RJ-11) connector (com- patible with MPLAB ICD 3 and MPLAB REAL ICE). The connector uses two device I/O pins and the Reset line to implement in-circuit debugging and In-Circuit Serial Programming™ (ICSP™).

### MPLAB PM3 Device Programmer

The MPLAB PM3 Device Programmer is a universal, CE compliant device programmer with programmable voltage verification at VDDMIN and VDDMAX for maximum reliability. It features a large LCD display (128 x 64) for menus and error messages, and a mod- ular, detachable socket assembly to support various package types. The ICSP cable assembly is included as a standard item. In Stand-Alone mode, the MPLAB PM3 Device Programmer can read, verify and program PIC devices without a PC connection. It can also set code protection in this mode. The MPLAB PM3 connects to the host PC via an RS-232 or USB cable. The MPLAB PM3 has high-speed communications and optimized algorithms for quick programming of large memory devices, and incorporates an MMC card for file storage and data applications.

### Demonstration/Development Boards, Evaluation Kits and Starter Kits

A wide variety of demonstration, development and evaluation boards for various PIC MCUs and dsPIC DSCs allows quick application development on fully functional systems. Most boards include prototyping areas for adding custom circuitry and provide applica- tion firmware and source code for examination and modification.

The boards support a variety of features, including LEDs, temperature sensors, switches, speakers, RS-232 interfaces, LCD displays, potentiometers and additional EEPROM memory.

The demonstration and development boards can be used in teaching environments, for prototyping custom circuits and for learning about various microcontroller applications.

In addition to the PICDEM™ and dsPICDEM™ demonstration/development board series of circuits, Microchip has a line of evaluation kits and demonstra- tion software for analog filter design, KEELOQ® security ICs, CAN, IrDA®, PowerSmart battery management, SEEVAL® evaluation system, Sigma-Delta ADC, flow rate sensing, plus many more.

Also available are starter kits that contain everything needed to experience the specified device. This usually includes a single application and debug capability, all on one board.

[Check the Microchip web page (](http://www.microchip.com/)www.microchip.com) for the complete list of demonstration, development and evaluation kits.

### Third-Party Development Tools

Microchip also offers a great collection of tools from third-party vendors. These tools are carefully selected to offer good value and unique functionality.

* Device Programmers and Gang Programmers from companies, such as SoftLog and CCS
* Software Tools from companies, such as Gimpel and Trace Systems
* Protocol Analyzers from companies, such as Saleae and Total Phase
* Demonstration Boards from companies, such as MikroElektronika, Digilent® and Olimex
* Embedded Ethernet Solutions from companies, such as EZ Web Lynx, WIZnet and IPLogika®

# ELECTRICAL CHARACTERISTICS

This section provides an overview of the PIC32MM0256GPM064 family electrical characteristics. Additional information will be provided in future revisions of this document as it becomes available.

Absolute maximum ratings for the PIC32MM0256GPM064 family are listed below. Exposure to these maximum rating conditions for extended periods may affect device reliability. Functional operation of the device at these, or any other conditions above the parameters indicated in the operation listings of this specification, is not implied.

### Absolute Maximum Ratings([†](#_bookmark639))

Ambient temperature under bias ..-40°C to +105°C

Storage temperature .. -65°C to +150°C

Voltage on VDD with respect to VSS V to +4.0V

Voltage on any general purpose digital or analog pin (not 5.5V tolerant) with respect to VSS 0.3V to (VDD + 0.3V)

Voltage on any general purpose digital or analog pin (5.5V tolerant) with respect to VSS:

When VDD = 0V: V to +4.0V

When VDD  2.0V: V to +6.0V

Voltage on AVDD with respect to VDD (VDD – 0.3V) to (lesser of: 4.0V or (VDD + 0.3V))

Voltage on AVSS with respect to VSS V to +0.3V

Maximum current out of VSS pin 100 mA

Maximum current into VDD pin**(**[**1**](#_bookmark638)**)** 300 mA

Maximum output current sunk by I/O pin 11 mA

Maximum output current sourced by I/O pin 16 mA

Maximum output current sunk by I/O pin with increased current drive strength

(RA3, RA8, RA10, RB8, RB9, RB13, RB15, RC9, RC13 and RD0) 17 mA

Maximum output current sourced by I/O pin with increased current drive strength

(RA3, RA8, RA10, RB8, RB9, RB13, RB15, RC9, RC13 and RD0) 24 mA

Maximum current sunk by all ports 300 mA

Maximum current sourced by all ports**(**[**1**](#_bookmark638)**)** 300 mA

**Note 1:** Maximum allowable current is a function of device maximum power dissipation (see [Table 29-1](#_bookmark643)).

† **NOTICE:** Stresses above those listed under “Absolute Maximum Ratings” may cause permanent damage to the device. This is a stress rating only and functional operation of the device at those or any other conditions above those indicated in the operation listings of this specification is not implied. Exposure to maximum rating conditions for extended periods may affect device reliability.

### DC Characteristics

FIGURE 29-1: PIC32MM0256GPM064 FAMILY VOLTAGE-FREQUENCY GRAPH

3.6V

3.6V

2.0V

2.0V

0V

25 MHz

**Frequency**

**Voltage (VDD)**

**PIC32MM0XXXGPM0XX**

TABLE 29-1: THERMAL OPERATING CONDITIONS

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Rating** | **Symbol** | **Min** | **Typ** | **Max** | **Unit** |
| PIC32MM0XXXGPM0XX:  Operating Junction Temperature Range Operating Ambient Temperature Range | TJ TA | -40  -40 | —  — | +125  +85 | °C  °C |
| Power Dissipation:  Internal Chip Power Dissipation:  PINT = VDD x (IDD –  IOH)  I/O Pin Power Dissipation:  PI/O =  ({VDD – VOH} x IOH) +  (VOL x IOL) | PD | PINT + PI/O | | | W |
| Maximum Allowed Power Dissipation | PDMAX | (TJ – TA)/JA | | | W |

TABLE 29-2: PACKAGE THERMAL RESISTANCE([1](#_bookmark647))

|  |  |  |  |
| --- | --- | --- | --- |
| **Package** | **Symbol** | **Typ** | **Unit** |
| 28-Pin SSOP | JA | 71.0 | °C/W |
| 28-Pin QFN | JA | 69.7 | °C/W |
| 28-Pin UQFN | JA | 26 | °C/W |
| 36-Pin VQFN | JA | 30.0 | °C/W |
| 40-Pin UQFN | JA | 41 | °C/W |
| 48-Pin UQFN | JA | 24.5 | °C/W |
| 48-Pin TQFP | JA | 51 | °C/W |
| 64-Pin QFN | JA | 29.4 | °C/W |
| 64-Pin TQFP | JA | 44.5 | °C/W |

**Note 1:** Junction to ambient thermal resistance; Theta-JA (JA) numbers are achieved by package simulations.

TABLE 29-3: OPERATING VOLTAGE SPECIFICATIONS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **DC CHARACTERISTICS** | | | **Operating Conditions: 2.0V < VDD < 3.6V, -40°C < TA < +85°C (unless otherwise stated)** | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ** | **Max** | **Units** | **Conditions** |
| DC10 | VDD | **Supply Voltage** | 2.0 | — | 3.6 | V |  |
| DC16 | VPOR**(**[**1**](#_bookmark649)**)** | **VDD Start Voltage**  to Ensure Internal Power-on Reset Signal | VSS | — | 100 | mV |  |
| DC17A | SVDD**(**[**1**](#_bookmark649)**)** | **Recommended VDD Rise Rate**  to Ensure Internal Power-on Reset Signal | 0.05 | — | — | V/ms | 0-3.3V in 66 ms, 0-2.0V in 40 ms |
| DC17B | VBOR | **Brown-out Reset Voltage** on VDD Transition, High-to-Low | 2.0 | — | 2.083 | V |  |

**Note 1:** If the VPOR or SVDD parameters are not met, or the application experiences slow power-down VDD ramp rates, it is recommended to enable and use BOR.

TABLE 29-4: OPERATING CURRENT (IDD)([2](#_bookmark652))

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **DC CHARACTERISTICS** | | | | | | |
| **Parameter No.** | **Typical(**[**1**](#_bookmark651)**)** | **Max** | **Units** | **Operating Temperature** | **VDD** | **Conditions** |
| DC19 | .72 | .96 | mA | -40°C to +85°C | 2.0V | FSYS = 1 MHz |
| — | .96 | mA | -40°C to +85°C | 3.3V |
| DC23 | 2.5 | 3.7 | mA | -40°C to +85°C | 2.0V | FSYS = 8 MHz |
| 2.5 | 3.7 | mA | -40°C to +85°C | 3.3V |
| DC24 | 7.9 | 10.2 | mA | -40°C to +85°C | 2.0V | FSYS = 25 MHz |
| 7.9 | 10.2 | mA | -40°C to +85°C | 3.3V |
| DC25 | .4 | .8 | A | -40°C to +85°C | 2.0V | LPRC,  FSYS = 32 kHz |
| .4 | .8 | A | -40°C to +85°C | 3.3V |

**Note 1:** Typical parameters are for design guidance only and are not tested.

**2:** IDD is primarily a function of the operating voltage and frequency. Other factors, such as I/O pin loading and switching rate, oscillator type, internal code execution pattern and temperature, also have an impact on the current consumption. The test conditions for all IDD measurements are as follows:

* + - Oscillator is configured in EC mode with PLL, OSC1 is driven with external square wave from rail-to-rail (EC Clock Overshoot/Undershoot < 250 mV required)
    - CLKO is configured as an I/O input pin in the Configuration Word
    - All I/O pins are configured as outputs and driving low
    - MCLR = VDD; WDT and FSCM are disabled
    - CPU, SRAM, program memory and data memory are operational
    - No peripheral modules are operating or being clocked (defined PMDx bits are all ones)
    - CPU executing:

while(1)

{ NOP();

}

**3:** JTAG is disabled

TABLE 29-5: IDLE CURRENT (IIDLE)([2](#_bookmark656))

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **DC CHARACTERISTICS** | | | | | | |
| **Parameter No.** | **Typical(**[**1**](#_bookmark655)**)** | **Max** | **Units** | **Operating Temperature** | **VDD** | **Conditions** |
| DC40 | .69 | .8 | A | -40°C to +85°C | 2.0V | FSYS = 1 MHz |
| .69 | .8 | A | -40°C to +85°C | 3.3V |
| DC41 | .98 | 1.7 | mA | -40°C to +85°C | 2.0V | FSYS = 8 MHz |
| .98 | 1.7 | mA | -40°C to +85°C | 3.3V |
| DC42 | 2.9 | 3.7 | mA | -40°C to +85°C | 2.0V | FSYS = 25 MHz |
| 2.9 | 3.7 | mA | -40°C to +85°C | 3.3V |
| DC44 | .36 | .7 | A | -40°C to +85°C | 2.0V | FSYS = 32 kHz |
| .36 | .7 | A | -40°C to +85°C | 3.3V |

**Note 1:** Parameters are for design guidance only and are not tested.

**2:** Base IIDLE current is measured with the core in Idle, the clock on and all modules turned off. OSC1 driven with external square wave from rail-to-rail (EC Clock Overshoot/Undershoot < 250 mV required).

Peripheral Module Disable SFR registers are zeroed. All I/O pins are configured as inputs and pulled to VSS.

TABLE 29-6: POWER-DOWN CURRENT (IPD)([2](#_bookmark660))

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **DC CHARACTERISTICS** | | | | | | |
| **Parameter No.** | **Typical(**[**1**](#_bookmark659)**)** | **Max** | **Units** | **Operating Temperature** | **VDD** | **Conditions** |
| DC60 | 130 | 255 | A | -40°C | 2.0V | Sleep with active main Voltage Regulator (VREGS (PWRCON<0>) bit = 1,  RETEN (PWRCON<1>) bit = 0) |
| 130 | 255 | A | +25°C |
| 145 | 265 | A | +85°C |
| 130 | 255 | A | -40°C | 3.3V |
| 130 | 265 | A | +25°C |
| 145 | 275 | A | +85°C |
| DC61 | 3.5 | 12 | A | -40°C |  | Sleep with main Voltage Regulator in Standby mode  (VREGS (PWRCON<0>) bit = 0, RETEN (PWRCON<1>) bit = 0) |
|  | 4.5 | 22 | A | +25°C | 2.0V |
|  | 15 | 35 | A | +85°C |  |
| 4 | 17 | A | -40°C |  |
|  | 5 | 30 | A | +25°C | 3.3V |
|  | 18 | 38 | A | +85°C |  |
| DC62 | 4.3 | — | A | -40°C |  | Sleep with enabled Retention Voltage Regulator  (RETEN (PWRCON<1>) bit = 1, RETVR (FPOR<2>) bit = 0) |
|  | 5 | — | A | +25°C | 2.0V |
|  | 10 | — | A | +85°C |  |
| 5 | — | A | -40°C |  |
|  | 5.6 | — | A | +25°C | 3.3V |
|  | 12 | — | A | +85°C |  |
| DC63 | .3 | — | µA | -40°C |  | Sleep with enabled Retention Voltage Regulator  (VREGS (PWRCON<0>) bit = 0, RETEN (PWRCON<1>) bit = 1, RETVR (FPOR<2>) bit = 0) |
|  | .4 | — | µA | +25°C | 2.0V |
|  | 3.5 | — | µA | +85°C |  |
| 0.35 | — | µA | -40°C |  |
|  | 0.45 | — | µA | +25°C | 3.3V |
|  | 4.5 | — | µA | +85°C |  |

**Note 1:** Parameters are for design guidance only and are not tested.

**2:** Base IPD is measured with:

* + - Oscillator is configured in FRC mode without PLL (FNOSC<2:0> (FOSCSEL<2:0>) = 000)
    - OSC1 pin is driven with external square wave from rail-to-rail (EC Clock Overshoot/Undershoot < 250 mV required)
    - OSC2 is configured as an I/O in Configuration Words (OSCIOFNC (FOSCSEL<10>) = 1)
    - FSCM is disabled (FCKSM<1:0> (FOSCSEL<15:14>) = 00)
    - Secondary Oscillator circuits are disabled (SOSCEN (FOSCSEL<6>) = 0 and SOSCSEL (FOSCSEL<12>) = 0)
    - Main and low-power BOR circuits are disabled (BOREN<1:0> (FPOR<1:0>) = 00 and LPBOREN (FPOR<3>) = 0)
    - Watchdog Timer is disabled (FWDTEN (FWDT<15>) = 0)
    - All I/O pins (excepting OSC1) are configured as outputs and driven low
    - No peripheral modules are operating or being clocked (defined PMDx bits are all ones)

TABLE 29-7:  CURRENT([2](#_bookmark664))

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **DC CHARACTERISTICS** | | | | | | |
| **Parameter No.** | **Typical(**[**1**](#_bookmark663)**)** | **Max** | **Units** | **Operating Temperature** | **VDD** | **Conditions** |
| **Incremental Current Brown-out Reset (BOR)** | | | | | | |
| DC71 | 3 | — | A | -40°C to +85°C | 2.0V | BOR |
| 4 | — | A | -40°C to +85°C | 3.3V |
| **Incremental Current Watchdog Timer (WDT)** | | | | | | |
| DC72 | 0.22 | — | A | -40°C to +85°C | 2.0V | WDT (with LPRC) |
| 0.3 | — | A | -40°C to +85°C | 3.3V |
| **Incremental Current High/Low-Voltage Detect (HLVD)** | | | | | | |
| DC73 | 2.1 | — | A | -40°C to +85°C | 2.0V | HLVD |
| 2.4 | — | A | -40°C to +85°C | 3.3V |
| **Incremental Current Real-Time Clock and Calendar (RTCC)** | | | | | | |
| DC74 | 1.1 | — | A | -40°C to +85°C | 2.0V | RTCC (with SOSC) |
| 1.2 | — | A | -40°C to +85°C | 3.3V |
| DC75 | 0.35 | — | A | -40°C to +85°C | 2.0V | RTCC (with LPRC) |
| 0.45 | — | A | -40°C to +85°C | 3.3V |
| **Incremental Current ADC (ADC** | | | | | | |
| DC76 | 450 | — | A | -40°C to +85°C | 2.0V | ΔADC (with Timer1 and  ADC internal oscillator enabled) |
| 475 | — | A | -40°C to +85°C | 3.3V |
| **Incremental Current Fast RC Oscillator (FRC)** | | | | | | |
| DC78 | — | — | A | -40°C to +85°C | 2.0V | ΔFRC |
| — | — | A | -40°C to +85°C | 3.3V |
| **Incremental Current PLL (PLL)** | | | | | | |
| DC79 | 1200 | — | A | -40°C to +85°C | 2.0V | ΔPLL (24 MHz) |
| 1340 | — | A | -40°C to +85°C | 3.3V |
| DC79a | 1460 | — | A | -40°C to +85°C | 2.0V | ΔPLL (48 MHz) |
| 1600 | — | A | -40°C to +85°C | 3.3V |
| **Incremental Current Voltage Reference CVREF (VREF)** | | | | | | |
| DC80 | 30 | — | A | -40°C to +85°C | 2.0V | ΔVREF |
| 35 | — | A | -40°C to +85°C | 3.3V |

**Note 1:** Data in the “Typical” column is for design guidance only and is not tested.

**2:** The  current is the additional current consumed when the module is enabled. This current should be added to the base IPD current.

TABLE 29-8: DC CHARACTERISTICS: I/O PIN INPUT SPECIFICATIONS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **DC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ(**[**1**](#_bookmark667)**)** | **Max** | **Units** | **Conditions** |
|  | VIL | **Input Low Voltage(**[**3**](#_bookmark669)**)** |  |  |  |  |  |
| DI10 |  | I/O Pins with ST Buffer | VSS | — | 0.2 VDD | V |
| DI15 |  | MCLR | VSS | — | 0.2 VDD | V |  |
| DI16 |  | OSC1 (XT mode) | VSS | — | 0.2 VDD | V |
| DI17 |  | OSC1 (HS mode) | VSS | — | 0.2 VDD | V |
|  | VIH | **Input High Voltage(**[**3**](#_bookmark669)**)**  I/O Pins with ST Buffer: Without 5V Tolerance With 5V Tolerance |  |  |  |  |  |
| DI20 |  |  |  |  |  |
|  |  | 0.8 VDD | — | VDD | V |
|  |  | 0.8 VDD | — | 5.5 | V |
| DI25 |  | MCLR | 0.8 VDD | — | VDD | V |  |
| DI26 |  | OSCI (XT mode) | 0.7 VDD | — | VDD | V |
| DI27 |  | OSCI (HS mode) | 0.7 VDD | — | VDD | V |
| DI30 | ICNPU | **CNPUx Pull-up Current** | 150 | 350 | 450 | A | VDD = 3.3V, VPIN = VSS |
| DI30A | ICNPD | **CNPDx Pull-Down Current** | 230 | 300 | 500 | A | VDD = 3.3V, VPIN = VDD |
|  | IIL | **Input Leakage Current(**[**2**](#_bookmark668)**)** |  |  |  |  |  |
| DI50 |  | I/O Pins – 5V Tolerant | — | — | 1 | A | VSS  VPIN  VDD,  pin at high-impedance |
| DI51 |  | I/O Pins – Not 5V Tolerant | — | — | 1 | A | VSS  VPIN  VDD,  pin at high-impedance |
| DI55 |  | MCLR | — | — | 1 | A | VSS  VPIN  VDD |
| DI56 |  | OSC1/CLKI | — | — | 1 | A | VSS  VPIN  VDD,  XT and HS modes |

**Note 1:** Data in the “Typ” column is at 3.3V, +25°C unless otherwise stated. Parameters are for design guidance only and are not tested.

**2:** Negative current is defined as current sourced by the pin.

**3:** Refer to [Table 1-1](#_bookmark27) for I/O pin buffer types.

TABLE 29-9: DC CHARACTERISTICS: I/O PIN INPUT INJECTION CURRENT SPECIFICATIONS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **DC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C | | | | |
| **Param No.** | **Symbol** | **Characteristics** | **Min.** | **Typical(**[**1**](#_bookmark671)**)** | **Max.** | **Units** | **Conditions** |
| DI60a | IICL | **Input Low Injection Current** | 0 | — | -5**(**[**2**](#_bookmark672)**,**[**5**](#_bookmark675)**)** | mA | This parameter applies to all pins. Maximum IICH current for this exception is 0 mA. |
| DI60b | IICH | **Input High Injection Current** | 0 | — | +5**(**[**3**](#_bookmark673)**,**[**4**](#_bookmark674)**,**[**5**](#_bookmark675)**)** | mA | This parameter applies to all pins, with the exception of all 5V tolerant pins and SOSCI. Maximum IICH current for these exceptions is 0 mA. |
| DI60c | IICT | **Total Input Injection Current (sum of all I/O and control pins)** | -20**(**[**6**](#_bookmark676)**)** | — | +20**(**[**6**](#_bookmark676)**)** | mA | Absolute instantaneous sum of all ± input injection currents from all I/O pins:  ( | IICL + | IICH | )  IICT |

**Note 1:** Data in the “Typical” column is at 3.3V, +25°C unless otherwise stated. Parameters are for design guidance only and are not tested.

**2:** VIL Source < (VSS – 0.3). Characterized but not tested.

**3:** VIH Source > (VDD + 0.3) for non-5V tolerant pins only.

**4:** Digital 5V tolerant pins do not have an internal high side diode to VDD, and therefore, cannot tolerate any “positive” input injection current.

**5:** Injection currents > | 0 | can affect the ADC results by approximately 4 to 6 counts (i.e., VIH Source > (VDD + 0.3) or VIL Source < (VSS – 0.3)).

**6:** Any number and/or combination of I/O pins, not excluded under IICL or IICH conditions, are permitted provided the “absolute instantaneous” sum of the input injection currents from all pins do not

exceed the specified limit. If [**Note 2**](#_bookmark672), IICL = (((VSS – 0.3) – VIL Source)/RS). If [**Note 3**](#_bookmark673),

IICH = (((IICH Source – (VDD + 0.3))/RS). RS = Resistance between input source voltage and device pin. If (VSS – 0.3)  VSOURCE  (VDD + 0.3), Injection Current = 0.

TABLE 29-10: DC CHARACTERISTICS: I/O PIN OUTPUT SPECIFICATIONS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **DC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ(**[**1**](#_bookmark678)**)** | **Max** | **Units** | **Conditions** |
|  | VOL | **Output Low Voltage** |  |  |  |  |  |
| DO10 |  | I/O Ports | — | — | .4 | V | IOL = 6.6 mA, VDD = 3.6V |
|  |  |  | — | — | .21 | V | IOL = 5.0 mA, VDD = 2V |
| DO16 |  | OSC2/CLKO | — | — | .16 | V | IOL = 6.6 mA, VDD = 3.6V |
|  |  |  | — | — | .12 | V | IOL = 5.0 mA, VDD = 2V |
|  | VOH | **Output High Voltage** |  |  |  |  |  |
| DO20 |  | I/O Ports | 3.25 | — | — | V | IOH = -6.0 mA, VDD = 3.6V |
|  |  |  | 1.4 | — | — | V | IOH = -3.0 mA, VDD = 2V |
| DO26 |  | OSC2/CLKO | 3.3 | — | — | V | IOH = -6.0 mA, VDD = 3.6V |
|  |  |  | 1.55 | — | — | V | IOH = -1.0 mA, VDD = 2V |

**Note 1:** Data in the “Typ” column is at 3.3V, +25°C unless otherwise stated. Parameters are for design guidance only and are not tested.

TABLE 29-11: DC CHARACTERISTICS: PROGRAM MEMORY

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **DC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ(**[**1**](#_bookmark680)**)** | **Max** | **Units** | **Conditions** |
|  |  | **Program Flash Memory** |  |  |  |  |  |
| D130 | EP | Cell Endurance | 10000 | 20000 | — | E/W |  |
| D131 | VPR | VDD for Read | 2.0 | — | 3.6 | V |  |
| D132B |  | VDD for Self-Timed Write | 2.0 | — | 3.6 | V |  |
| D133A | TIW | Self-Timed Double-Word Write Cycle Time | 61.4 | 62.5 | 63.6 | s | 8 bytes, data is not all ‘1’s |
|  |  | Self-Timed Row Write Cycle Time | 1.41 | 1.44 | 1.47 | ms | 512 bytes, data is not all ‘1’s; SYSCLK > 2 MHz |
| D133B | TIE | Self-Timed Page Erase Time | 4.18 | 4.26 | 4.33 | ms | 2048 bytes |
| D134 | TRETD | Characteristic Retention | 20 | — | — | Year | If no other specifications are violated |
| D136 | TCE | Self-Timed Chip Erase Time | 16.6 | 16.9 | 17.3 | ms |  |

**Note 1:** Data in the “Typ” column is at 3.3V, +25°C unless otherwise stated.

TABLE 29-12: INTERNAL VOLTAGE REGULATOR SPECIFICATIONS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Operating Conditions:** -40°C < TA < +85°C (unless otherwise stated) | | | | | | | |
| **Param No.** | **Symbol** | **Characteristics** | **Min** | **Typ** | **Max** | **Units** | **Comments** |
| DVR10 | VBG | Internal Band Gap Reference | — | 1.2 | — | V |  |
| DVR20 | VRGOUT | Regulator Output Voltage | — | 1.8 | — | V | VDD > 1.9V |
| DVR21 | CEFC | External Filter Capacitor Value | 4.7 | 10 | — | F | Series Resistance < 3 recommended; < 5  required |
| DVR30 | VLVR | Low-Voltage Regulator Output Voltage | 0.9 | — | 1.2 | V | RETEN = 1,  RETVR (FPOR<2>) = 0 |

TABLE 29-13: HIGH/LOW-VOLTAGE DETECT CHARACTERISTICS

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Operating Conditions:** -40°C < TA < +85°C (unless otherwise stated) | | | | | | | | |
| **Param No.** | **Symbol** | **Characteristic** | | **Min** | **Typ** | **Max** | **Units** | **Conditions** |
| DC18 | VHLVD | HLVD Voltage on VDD Transition | HLVDL<3:0> = 0101 | 3.25 | — | 3.63 | V |  |
| HLVDL<3:0> = 0110 | 2.95 | — | 3.30 | V |
| HLVDL<3:0> = 0111 | 2.75 | — | 3.09 | V |
| HLVDL<3:0> = 1000 | 2.65 | — | 2.98 | V |
| HLVDL<3:0> = 1001 | 2.45 | — | 2.80 | V |
| HLVDL<3:0> = 1010 | 2.35 | — | 2.69 | V |
| HLVDL<3:0> = 1011 | 2.25 | — | 2.55 | V |
| HLVDL<3:0> = 1100 | 2.15 | — | 2.44 | V |
| HLVDL<3:0> = 1101 | 2.08 | — | 2.33 | V |
| HLVDL<3:0> = 1110 | 2.00 | — | 2.22 | V |
| DC101 | VTHL | HLVD Voltage on LVDIN Pin Transition | HLVDL<3:0> = 1111 | — | 1.2 | — | V |  |

TABLE 29-14: COMPARATOR DC SPECIFICATIONS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Operating Conditions:** 2.0V < VDD < 3.6V, -40°C < TA < +85°C (unless otherwise stated) | | | | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ** | **Max** | **Units** | **Comments** |
| D300 | VIOFF | Input Offset Voltage | -20 | — | +20 | mV | **(**[**Note 1**](#_bookmark686)**)** |
| D301 | VICM | Input Common-Mode Voltage | VSS – 0.3V | — | VDD + 0.3V | V | **(**[**Note 1**](#_bookmark686)**)** |
| D307 | TRESP | Response Time | — | 150 | — | ns | **(**[**Note 2**](#_bookmark687)**)** |

**Note 1:** Parameters are characterized but not tested.

**2:** Measured with one input at VDD/2 and the other transitioning from VSS to VDD, 40 mV step, 15 mV overdrive.

TABLE 29-15: VOLTAGE REFERENCE DC SPECIFICATIONS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Operating Conditions:** 2.0V < VDD < 3.6V, -40°C < TA < +85°C (unless otherwise stated) | | | | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ** | **Max** | **Units** | **Comments** |
| VRD310 | TSET | Settling Time | — | — | 10 | µs | **(**[**Note 1**](#_bookmark689)**)** |
| VRD311 | VRAA | Absolute Accuracy | -1 | — | 1 | LSb |  |
| VRD312 | VRUR | Unit Resistor Value (R) | — | 4.5 | — | k |  |

**Note 1:** Measures the interval while DACDAT<4:0> transitions from ‘11111’ to ‘00000’.

### AC Characteristics and Timing Parameters

The information contained in this section defines the PIC32MM0256GPM064 family AC characteristics and timing parameters.

TABLE 29-16: TEMPERATURE AND VOLTAGE SPECIFICATIONS – AC

**Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**

Operating temperature -40°C  TA  +85°C

Operating voltage VDD range as described in [**Section 29.1 “DC Characteristics”**](#_bookmark640).

**AC CHARACTERISTICS**

FIGURE 29-2: LOAD CONDITIONS FOR DEVICE TIMING SPECIFICATIONS

Load Condition 1 – for all pins except OSC2/CLKO

Load Condition 2 – for OSC2/CLKO

VDD/2

RL

Pin

CL

VSS

Pin

CL

RL = 464

VSS CL = 50 pF for all pins except OSC2/CLKO 15 pF for OSC2/CLKO output



TABLE 29-17: CAPACITIVE LOADING CONDITIONS ON OUTPUT PINS



|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ(**[**1**](#_bookmark695)**)** | **Max** | **Units** | **Conditions** |
| DO50 | COSCO | OSC2/CLKO Pin | — | — | TBD | pF | In XT and HS modes when external clock is used to drive OSC1/CLKI |
| DO56 | CIO | All I/O Pins and OSC2 | — | — | TBD | pF | EC mode |
| DO58 | CB | SCLx, SDAx | — | — | TBD | pF | In I2C mode |

**Legend:** TBD = To Be Determined

**Note 1:** Data in the “Typ” column is at 3.3V, +25°C unless otherwise stated. Parameters are for design guidance only and are not tested.

FIGURE 29-3: EXTERNAL CLOCK TIMING

Q4

Q1 Q2 Q3 Q4 Q1 Q2 Q3 Q4

Q1 Q2 Q3

OSCI

OS20

OS25

OS30 OS30

OS31 OS31

CLKO

OS40

OS41



TABLE 29-18: EXTERNAL CLOCK TIMING REQUIREMENTS



|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C for Industrial | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ(**[**1**](#_bookmark698)**)** | **Max** | **Units** | **Conditions** |
| OS10 | FOSC | External CLKI Frequency | DC 2 | —  — | 32  48 | MHz MHz | EC ECPLL**(**[**2**](#_bookmark699)**)** |
| Oscillator Frequency | 3.5  3.5  10  10  31 | —  —  —  —  — | 10  10  32  24  50 | MHz MHz MHz MHz kHz | XT XTPLL HS HSPLL SOSC |
| OS20 | TOSC | TOSC = 1/FOSC | — | — | — | — | See Parameter OS10 for FOSC value |
| OS25 | TCY | Instruction Cycle Time | 40 | — | DC | ns |  |
| OS30 | TosL, TosH | External Clock in (OSC1) High or Low Time | 0.45 x TOSC | — | — | ns | EC |
| OS31 | TosR, TosF | External Clock in (OSC1) Rise or Fall Time | — | — | TBD | ns | EC |
| OS40 | TckR | CLKO Rise Time**(**[**3**](#_bookmark700)**)** | — | 15 | 30 | ns |  |
| OS41 | TckF | CLKO Fall Time**(**[**3**](#_bookmark700)**)** | — | 15 | 30 | ns |  |

**Legend:** TBD = To Be Determined

**Note 1:** Data in the “Typ” column is at 3.3V, +25°C unless otherwise stated. Parameters are for design guidance only and are not tested.

**2:** Represents input to the system clock prescaler. PLL dividers and postscalers must still be configured so that the system clock frequency does not exceed the maximum frequency, as shown in [Figure 29-1](#_bookmark641).

**3:** Measurements are taken in EC mode. The CLKO signal is measured on the OSC2 pin.

TABLE 29-19: PLL CLOCK TIMING SPECIFICATIONS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C for Industrial | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ** | **Max** | **Units** | **Conditions** |
| OS50 | FPLLI | PLL Input Frequency Range**(**[**1**](#_bookmark702)**)** | 2 | — | 24 | MHz |  |
| OS54 | FPLLO | PLL Output Frequency Range**(**[**1**](#_bookmark702)**)** | 16 | — | 96 | MHz |  |
| OS52 | TLOCK | PLL Start-up Time (Lock Time) | — | — | 24 | s |  |
| OS53 | DCLK | CLKO Stability (Jitter) | -0.12 | — | 0.12 | % |  |

**Note 1:** These parameters are characterized but not tested in manufacturing.

TABLE 29-20: INTERNAL RC ACCURACY

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C for Industrial | | | | |
| **Param No.** | **Characteristic** | **Min** | **Typ** | **Max** | **Units** | **Conditions** |
| F20 | FRC Accuracy @ 8 MHz | -1.5 | — | 1.5 | % | 2.0V  VDD  3.6V, -40°C  TA  +85°C**(**[**1**](#_bookmark705)**)** |
| F21 | LPRC @ 32 kHz | -20 | — | 20 | % | VCAP Output Voltage = 1.8V |
| F22 | FRC Tune Step-Size (in OSCTUN register) | — | .05 | — | %/bit |  |

**Note 1:** To achieve this accuracy, physical stress applied to the microcontroller package (ex., by flexing the PCB) must be kept to a minimum.

TABLE 29-21: RC OSCILLATOR START-UP TIME

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C for Industrial | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ** | **Max** | **Units** | **Conditions** |
| FR0 | TFRC | FRC Oscillator Start-up Time | — | — | 2 | s |  |
| FR1 | TLPRC | Low-Power RC Oscillator Start-up Time | — | — | 70 | s |  |

FIGURE 29-4: CLKO AND I/O TIMING CHARACTERISTICS

I/O Pin (Input)

DI35 DI40

I/O Pin (Output)

Old Value

New Value

DO31 DO32

**Note:** Refer to [Figure 29-2](#_bookmark691) for load conditions.



TABLE 29-22: CLKO AND I/O TIMING REQUIREMENTS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C for Industrial | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ(**[**1**](#_bookmark711)**)** | **Max** | **Units** | **Conditions** |
| DO31 | TIOR | Port Output Rise Time | — | 10 | 25 | ns |  |
| DO32 | TIOF | Port Output Fall Time | — | 10 | 25 | ns |  |
| DI35 | TINP | INTx Pin High or Low Time (input) | 1 | — | — | TCY |  |
| DI40 | TRBP | CNx High or Low Time (input) | 1 | — | — | TCY |  |

**Note 1:** Data in the “Typ” column is at 3.3V, +25°C unless otherwise stated.

TABLE 29-23: RESET AND BROWN-OUT RESET REQUIREMENTS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C for Industrial | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ(**[**1**](#_bookmark713)**)** | **Max** | **Units** | **Conditions** |
| SY10 | TMCL | MCLR Pulse Width (Low) | 2 | — | — | s |  |
| SY13 | TIOZ | I/O High-Impedance from MCLR Low or Watchdog Timer Reset | — | 1 | — | s | Device running or in Idle |
| SY25 | TBOR | Brown-out Reset Pulse Width | 1 | — | — | s | VDD  VBOR |
| SY45 | TRST | Internal State Reset Time | — | 25 | — | s |  |
| SY71 | TPM | Program Memory Wake-up Time | — | 22 | — | s | Sleep wake-up with VREGS = 0 |
| — | 3.8 | — | s | Sleep wake-up with VREGS = 1 |
| SY72 | TLVR | Low-Voltage Regulator Wake-up Time | — | 163 | — | s | Sleep wake-up with VREGS = 0 |
| — | 23 | — | s | Sleep wake-up with VREGS = 1 |

**Note 1:** Parameters are for design guidance and are not tested.

FIGURE 29-5: TIMER1 EXTERNAL CLOCK TIMING CHARACTERISTICS

T1CK

TA10

TA11

TA15

TA20

TMR1

**Note:** Refer to [Figure 29-2](#_bookmark691) for load conditions.

TABLE 29-24: TIMER1 EXTERNAL CLOCK TIMING REQUIREMENTS

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C **** TA **** +85°C | | | | |
| **Param No.** | **Symbol** | **Characteristics(**[**1**](#_bookmark716)**)** | | **Min.** | **Typ.** | **Max.** | **Units** | **Conditions** |
| TA10 | TTXH | T1CK  High Time | Synchronous, with Prescaler | [(12.5 ns or 1 TPBCLK)/N] + 20 ns | — | — | ns | Must also meet Parameter TA15**(**[**2**](#_bookmark717)**)** |
| Asynchronous, with Prescaler | 10 | — | — | ns |  |
| TA11 | TTXL | T1CK  Low Time | Synchronous, with Prescaler | [(12.5 ns or 1 TPBCLK)/N] + 20 ns | — | — | ns | Must also meet Parameter TA15**(**[**2**](#_bookmark717)**)** |
| Asynchronous, with Prescaler | 10 | — | — | ns |  |
| TA15 | TTXP | T1CK  Input Period | Synchronous, with Prescaler | [(Greater of 20 ns or 2 TPBCLK)/N] + 30 ns | — | — | ns | VDD > 2.0V**(**[**2**](#_bookmark717)**)** |
| [(Greater of 20 ns or 2 TPBCLK)/N] + 50 ns | — | — | ns | VDD < 2.0V**(**[**2**](#_bookmark717)**)** |
| Asynchronous, with Prescaler | 20 | — | — | ns | VDD > 2.0V |
| 50 | — | — | ns | VDD < 2.0V |
| TA20 | TCKEXTMRL | Delay from External T1CK Clock Edge to Timer Increment | | — |  | 1 | TPBCLK |  |

**Note 1:** This parameter is characterized but not tested in manufacturing.

**2:** N = Prescale Value (1, 8, 64, 256).

FIGURE 29-6: MCCP AND SCCP INPUT CAPTURE MODE TIMING CHARACTERISTICS

ICMx

IC10

IC11

IC15

**Note:** Refer to [Figure 29-2](#_bookmark691) for load conditions.

TABLE 29-25: MCCP AND SCCP INPUT CAPTURE MODE TIMING REQUIREMENTS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise st****ated)**  Operating temperature -40°C **** TA **** +85°C | | | |
| **Param No.** | **Symbol** | **Characteristics(**[**1**](#_bookmark720)**)** | **Min.** | **Max.** | **Units** | **Conditions** |
| IC10 | TCCL | ICMx Input Low Time | [(12.5 ns or 1 TPBCLK)/N] + 25 ns | — | ns | Must also meet Parameter IC15 |
| IC11 | TCCH | ICMx Input High Time | [(12.5 ns or 1 TPBCLK)/N] + 25 ns | — | ns | Must also meet Parameter IC15 |
| IC15 | TCCP | ICMx Input Period | [(25 ns or 2 TPBCLK)/N] + 50 ns | — | ns |  |

**Note 1:** These parameters are characterized but not tested in manufacturing.

FIGURE 29-7: MCCP AND SCCP OUTPUT COMPARE MODE TIMING CHARACTERISTICS

OCMx

OC11

OC10

**Note:** Refer to [Figure 29-2](#_bookmark691) for load conditions.

TABLE 29-26: MCCP AND SCCP OUTPUT COMPARE MODE TIMING REQUIREMENTS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless other****wise stated)**  Operating temperature -40°C  TA  +85°C | | | | |
| **Param No.** | **Symbol** | **Characteristics(**[**1**](#_bookmark723)**)** | **Min.** | **Typical** | **Max.** | **Units** | **Conditions** |
| OC10 | TCCF | OCMx Output Fall Time | — | — | — | ns | See Parameter [DO32](#_bookmark710) |
| OC11 | TCCR | OCMx Output Rise Time | — | — | — | ns | See Parameter [DO31](#_bookmark709) |

**Note 1:** These parameters are characterized but not tested in manufacturing.

FIGURE 29-8: MCCP AND SCCP PWM MODE TIMING CHARACTERISTICS

OC20

OCFA/OCFB

OC15

OCx

**Note:** Refer to [Figure 29-2](#_bookmark691) for load conditions.

OCMx is Tri-Stated



TABLE 29-27: MCCP AND SCCP PWM MODE TIMING REQUIREMENTS



|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V** **(unless otherwise stated)**  Operating temperature -40°C  TA  +85°C | | | | |
| **Param No.** | **Symbol** | **Characteristics(**[**1**](#_bookmark726)**)** | **Min** | **Typical** | **Max** | **Units** | **Conditions** |
| OC15 | TFD | Fault Input to PWM I/O Change | — | — | 50 | ns |  |
| OC20 | TFLT | Fault Input Pulse Width | 10 | — | — | ns |  |

**Note 1:** These parameters are characterized but not tested in manufacturing.



FIGURE 29-9: SPIx MODULE MASTER MODE (CKE = 0) TIMING CHARACTERISTICS



SCKx (CKP = 0)

SP11

SP10

SP21

SP20

SCKx (CKP = 1)

SP35

SP20

SP21

SDOx

MSb

Bit 14 1

LSb

SP31

SP30

SDIx

MSb In

Bit 14 1

LSb In

SP40 SP41

**Note:** Refer to [Figure 29-2](#_bookmark691) for load conditions.

TABLE 29-28: SPIx MASTER MODE (CKE = 0) TIMING REQUIREMENTS



|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V(unless othe****rwise stated)**  Operating temperature -40°C  TA  +85°C | | | | |
| **Param No.** | **Symbol** | **Characteristics(**[**1**](#_bookmark729)**)** | **Min.** | **Typical(**[**2**](#_bookmark730)**)** | **Max.** | **Units** | **Conditions** |
| SP10 | TSCL | SCKx Output Low Time**(**[**3**](#_bookmark731)**)** | TSCK/2 | — | — | ns |  |
| SP11 | TSCH | SCKx Output High Time**(**[**3**](#_bookmark731)**)** | TSCK/2 | — | — | ns |  |
| SP20 | TSCF | SCKx Output Fall Time**(**[**4**](#_bookmark732)**)** | — | — | — | ns | See Parameter [DO32](#_bookmark710) |
| SP21 | TSCR | SCKx Output Rise Time**(**[**4**](#_bookmark732)**)** | — | — | — | ns | See Parameter [DO31](#_bookmark709) |
| SP30 | TDOF | SDOx Data Output Fall Time**(**[**4**](#_bookmark732)**)** | — | — | — | ns | See Parameter [DO32](#_bookmark710) |
| SP31 | TDOR | SDOx Data Output Rise Time**(**[**4**](#_bookmark732)**)** | — | — | — | ns | See Parameter [DO31](#_bookmark709) |
| SP35 | TSCH2DOV, TSCL2DOV | SDOx Data Output Valid after SCKx Edge | — | — | 7 | ns | VDD > 2.0V |
| — | — | 10 | ns | VDD < 2.0V |
| SP40 | TDIV2SCH, TDIV2SCL | Setup Time of SDIx Data Input to SCKx Edge | 5 | — | — | ns |  |
| SP41 | TSCH2DIL, TSCL2DIL | Hold Time of SDIx Data Input to SCKx Edge | 5 | — | — | ns |  |

**Note 1:** These parameters are characterized but not tested in manufacturing.

**2:** Data in the “Typical” column is at 3.3V, +25°C unless otherwise stated. Parameters are for design guidance only and are not tested.

**3:** The minimum clock period for SCKx is 40 ns. Therefore, the clock generated in Master mode must not violate this specification.

**4:** Assumes 10 pF load on all SPIx pins.

FIGURE 29-10: SPIx MODULE MASTER MODE (CKE = 1) TIMING CHARACTERISTICS



SP36

SCKx (CKP = 0)

SP11

SP10

SP21

SP20

SCKx (CKP = 1)

SP35

SP20

SP21

SDOx

MSb

Bit 14 1

LSb

SP30, SP31

SDIx

MSb In

SP41

Bit 14 1

LSb In

SP40

**Note:** Refer to [Figure 29-2](#_bookmark691) for load conditions.

TABLE 29-29: SPIx MODULE MASTER MODE (CKE = 1) TIMING REQUIREMENTS



|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless other****wise stated)**  Operating temperature -40°C  TA  +85°C | | | | |
| **Param No.** | **Symbol** | **Characteristics(**[**1**](#_bookmark735)**)** | **Min.** | **Typ.(**[**2**](#_bookmark736)**)** | **Max.** | **Units** | **Conditions** |
| SP10 | TSCL | SCKx Output Low Time**(**[**3**](#_bookmark737)**)** | TSCK/2 | — | — | ns |  |
| SP11 | TSCH | SCKx Output High Time**(**[**3**](#_bookmark737)**)** | TSCK/2 | — | — | ns |  |
| SP20 | TSCF | SCKx Output Fall Time**(**[**4**](#_bookmark738)**)** | — | — | — | ns | See Parameter [DO32](#_bookmark710) |
| SP21 | TSCR | SCKx Output Rise Time**(**[**4**](#_bookmark738)**)** | — | — | — | ns | See Parameter [DO31](#_bookmark709) |
| SP30 | TDOF | SDOx Data Output Fall Time**(**[**4**](#_bookmark738)**)** | — | — | — | ns | See Parameter [DO32](#_bookmark710) |
| SP31 | TDOR | SDOx Data Output Rise Time**(**[**4**](#_bookmark738)**)** | — | — | — | ns | See Parameter [DO31](#_bookmark709) |
| SP35 | TSCH2DOV, TSCL2DOV | SDOx Data Output Valid after SCKx Edge | — | — | 7 | ns | VDD > 2.0V |
| — | — | 10 | ns | VDD < 2.0V |
| SP36 | TDOV2SC, TDOV2SCL | SDOx Data Output Setup to First SCKx Edge | 7 | — | — | ns |  |
| SP40 | TDIV2SCH, TDIV2SCL | Setup Time of SDIx Data Input to SCKx Edge | 7 | — | — | ns | VDD > 2.0V |
| 10 | — | — | ns | VDD < 2.0V |
| SP41 | TSCH2DIL, TSCL2DIL | Hold Time of SDIx Data Input to SCKx Edge | 7 | — | — | ns | VDD > 2.0V |
| 10 | — | — | ns | VDD < 2.0V |

**Note 1:** These parameters are characterized but not tested in manufacturing.

**2:** Data in the “Typ.” column is at 3.3V, +25°C unless otherwise stated. Parameters are for design guidance only and are not tested.

**3:** The minimum clock period for SCKx is 40 ns. Therefore, the clock generated in Master mode must not violate this specification.

**4:** Assumes 10 pF load on all SPIx pins.

FIGURE 29-11: SPIx MODULE SLAVE MODE (CKE = 0) TIMING CHARACTERISTICS



SSx

SP50

SP52

SCKx (CKP = 0)

SP71 SP70

SP73 SP72

SCKx (CKP = 1)

SP35

SP72 SP73

SDOx

MSb

Bit 14 1

LSb

SP30, SP31

SP51

SDIx

SP40

MSb In

SP41

Bit 14 1

LSb In

**Note:** Refer to [Figure 29-2](#_bookmark691) for load conditions.

TABLE 29-30: SPIx MODULE SLAVE MODE (CKE = 0) TIMING REQUIREMENTS



|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless ot****herwise stated)**  Operating temperature -40°C  TA  +85°C | | | | |
| **Param No.** | **Symbol** | **Characteristics(**[**1**](#_bookmark741)**)** | **Min.** | **Typ.(**[**2**](#_bookmark742)**)** | **Max.** | **Units** | **Conditions** |
| SP70 | TSCL | SCKx Input Low Time**(**[**3**](#_bookmark743)**)** | TSCK/2 | — | — | ns |  |
| SP71 | TSCH | SCKx Input High Time**(**[**3**](#_bookmark743)**)** | TSCK/2 | — | — | ns |  |
| SP72 | TSCF | SCKx Input Fall Time | — | — | — | ns | See Parameter [DO32](#_bookmark710) |
| SP73 | TSCR | SCKx Input Rise Time | — | — | — | ns | See Parameter [DO31](#_bookmark709) |
| SP30 | TDOF | SDOx Data Output Fall Time**(**[**4**](#_bookmark744)**)** | — | — | — | ns | See Parameter [DO32](#_bookmark710) |
| SP31 | TDOR | SDOx Data Output Rise Time**(**[**4**](#_bookmark744)**)** | — | — | — | ns | See Parameter [DO31](#_bookmark709) |
| SP35 | TSCH2DOV, TSCL2DOV | SDOx Data Output Valid after SCKx Edge | — | — | 7 | ns | VDD > 2.0V |
| — | — | 10 | ns | VDD < 2.0V |
| SP40 | TDIV2SCH, TDIV2SCL | Setup Time of SDIx Data Input to SCKx Edge | 5 | — | — | ns |  |
| SP41 | TSCH2DIL, TSCL2DIL | Hold Time of SDIx Data Input to SCKx Edge | 5 | — | — | ns |  |
| SP50 | TSSL2SCH, TSSL2SCL | SSx  to SCKx  or SCKx Input | 88 | — | — | ns |  |
| SP51 | TSSH2DOZ | SSx  to SDOx Output High-Impedance**(**[**4**](#_bookmark744)**)** | 2.5 | — | 12 | ns |  |
| SP52 | TSCH2SSH TSCL2SSH | SSx after SCKx Edge | 10 | — | — | ns |  |

**Note 1:** These parameters are characterized but not tested in manufacturing.

**2:** Data in “Typ.” column is at 3.3V, +25°C unless otherwise stated. Parameters are for design guidance only and are not tested.

**3:** The minimum clock period for SCKx is 40 ns.

**4:** Assumes 10 pF load on all SPIx pins.



FIGURE 29-12: SPIx MODULE SLAVE MODE (CKE = 1) TIMING CHARACTERISTICS



SP60

SSx

SP50

SP52

SCKx (CKP = 0)

SP71

SP70

SP73

SP72

SCKx (CKP = 1)

SP35

SP72

SP73

SDOx

MSb

Bit 14 1

LSb

SP30, SP31

SP51

SDIx

MSb In

SP41

Bit 14 1

LSb In

SP40

**Note:** Refer to [Figure 29-2](#_bookmark691) for load conditions.

TABLE 29-31: SPIx MODULE SLAVE MODE (CKE = 1) TIMING REQUIREMENTS

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | | **Standard Operating Conditions: 2.0V to 3.6V (****unless otherwise stated)**  Operating temperature -40°C  TA  +85°C | | | | |
| **Param No.** | **Symbol** | **Characteristics(**[**1**](#_bookmark747)**)** | | **Min.** | **Typical(**[**2**](#_bookmark748)**)** | **Max.** | **Units** | **Conditions** |
| SP70 | TSCL | SCKx Input Low Time**(**[**3**](#_bookmark749)**)** | | TSCK/2 | — | — | ns |  |
| SP71 | TSCH | SCKx Input High Time**(**[**3**](#_bookmark749)**)** | | TSCK/2 | — | — | ns |  |
| SP72 | TSCF | SCKx Input Fall Time | | — | — | 10 | ns |  |
| SP73 | TSCR | SCKx Input Rise Time | | — | — | 10 | ns |  |
| SP30 | TDOF | SDOx Data Output Fall Time**(**[**4**](#_bookmark750)**)** | | — | — | — | ns | See Parameter [DO32](#_bookmark710) |
| SP31 | TDOR | SDOx Data Output Rise Time**(**[**4**](#_bookmark750)**)** | | — | — | — | ns | See Parameter [DO31](#_bookmark709) |
| SP35 | TSCH2DOV, TSCL2DOV | SDOx Data Output Valid after SCKx Edge | | — | — | 10 | ns | VDD > 2.0V |
| — | — | 15 | ns | VDD < 2.0V |
| SP40 | TDIV2SCH, TDIV2SCL | Setup Time of SDIx Data Input to SCKx Edge | | 0 | — | — | ns |  |
| SP41 | TSCH2DIL, TSCL2DIL | Hold Time of SDIx Data Input to SCKx Edge | | 7 | — | — | ns |  |
| SP50 | TSSL2SCH, TSSL2SCL | SSx  to SCKx  or SCKx  Input | | 88 | — | — | ns |  |
| SP51 | TSSH2DOZ | SSx  to SDOx Output High-Impedance**(**[**4**](#_bookmark750)**)** | | 2.5 | — | 12 | ns |  |
| SP52 | TSCH2SSH TSCL2SSH | SSx  after SCKx Edge | | 10 | — | — | ns |  |
| SP60 | TSSL2DOV | SDOx Data Output Valid after | | — | — | 12.5 | ns |  |
| SSx | Edge |

**Note 1:** These parameters are characterized but not tested in manufacturing.

**2:** Data in the “Typical” column is at 3.3V, +25°C unless otherwise stated. Parameters are for design guidance only and are not tested.

**3:** The minimum clock period for SCKx is 40 ns.

**4:** Assumes 10 pF load on all SPIx pins.

FIGURE 29-13: I2Cx BUS START/STOP BITS TIMING CHARACTERISTICS (MASTER MODE)

SCLx

IM31

IM34

IM30 IM33

SDAx

Start Condition

Stop Condition

**Note:** Refer to [Figure 29-2](#_bookmark691) for load conditions.



FIGURE 29-14: I2Cx BUS DATA TIMING CHARACTERISTICS (MASTER MODE)

IM20

IM11

IM21

IM10

SCLx

IM11

IM26

IM10

IM25

IM33

SDAx

In

IM40

IM40

IM45

SDAx

Out

**Note:** Refer to [Figure 29-2](#_bookmark691) for load conditions.



TABLE 29-32: I2Cx BUS DATA TIMING REQUIREMENTS (MASTER MODE)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise** **stated)**  Operating temperature -40°C  TA  +85°C | | | |
| **Param No.** | **Sym** | **Characteristics** | | **Min.(**[**1**](#_bookmark754)**)** | **Max.** | **Units** | **Conditions** |
| IM10 | TLO:SCL | Clock Low Time | 100 kHz mode | TSYSCLK \* (BRG + 2) | — | s |  |
| 400 kHz mode | TSYSCLK \* (BRG + 2) | — | s |  |
| 1 MHz mode**(**[**2**](#_bookmark755)**)** | TSYSCLK \* (BRG + 2) | — | s |  |
| IM11 | THI:SCL | Clock High Time | 100 kHz mode | TSYSCLK \* (BRG + 2) | — | s |  |
| 400 kHz mode | TSYSCLK \* (BRG + 2) | — | s |  |
| 1 MHz mode**(**[**2**](#_bookmark755)**)** | TSYSCLK \* (BRG + 2) | — | s |  |
| IM20 | TF:SCL | SDAx and SCLx Fall Time | 100 kHz mode | — | 300 | ns | CB is specified to be from 10 to 400 pF |
| 400 kHz mode | 20 + 0.1 CB | 300 | ns |
| 1 MHz mode**(**[**2**](#_bookmark755)**)** | — | 100 | ns |
| IM21 | TR:SCL | SDAx and SCLx Rise Time | 100 kHz mode | — | 1000 | ns | CB is specified to be from 10 to 400 pF |
| 400 kHz mode | 20 + 0.1 CB | 300 | ns |
| 1 MHz mode**(**[**2**](#_bookmark755)**)** | — | 300 | ns |

**Note 1:** BRG is the value of the I2C Baud Rate Generator.

**2:** Maximum Pin Capacitance = 10 pF for all I2Cx pins (for 1 MHz mode only).

**3:** The typical value for this parameter is 104 ns.

TABLE 29-32: I2Cx BUS DATA TIMING REQUIREMENTS (MASTER MODE) (CONTINUED)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C | | | |
| **Param No.** | **Sym** | **Characteristics** | | **Min.(1)** | **Max.** | **Units** | **Conditions** |
| IM25 | TSU:DAT | Data Input Setup Time | 100 kHz mode | 250 | — | ns |  |
| 400 kHz mode | 100 | — | ns |
| 1 MHz mode**(**[**2**](#_bookmark755)**)** | 100 | — | ns |
| IM26 | THD:DAT | Data Input Hold Time | 100 kHz mode | 0 | — | s |  |
| 400 kHz mode | 0 | 0.9 | s |
| 1 MHz mode**(**[**2**](#_bookmark755)**)** | 0 | 0.3 | s |
| IM30 | TSU:STA | Start Condition Setup Time | 100 kHz mode | TPBCLK \* (BRG + 2) | — | s | Only relevant for Repeated Start condition |
| 400 kHz mode | TPBCLK \* (BRG + 2) | — | s |
| 1 MHz mode**(**[**2**](#_bookmark755)**)** | TPBCLK \* (BRG + 2) | — | s |
| IM31 | THD:STA | Start Condition Hold Time | 100 kHz mode | TPBCLK \* (BRG + 2) | — | s | After this period, the first clock pulse is generated |
| 400 kHz mode | TPBCLK \* (BRG + 2) | — | s |
| 1 MHz mode**(**[**2**](#_bookmark755)**)** | TPBCLK \* (BRG + 2) | — | s |
| IM33 | TSU:STO | Stop Condition Setup Time | 100 kHz mode | TPBCLK \* (BRG + 2) | — | s |  |
| 400 kHz mode | TPBCLK \* (BRG + 2) | — | s |
| 1 MHz mode**(**[**2**](#_bookmark755)**)** | TPBCLK \* (BRG + 2) | — | s |
| IM34 | THD:STO | Stop Condition Hold Time  Output Valid from Clock | 100 kHz mode | TPBCLK \* (BRG + 2) | — | ns |  |
| 400 kHz mode | TPBCLK \* (BRG + 2) | — | ns |
| 1 MHz mode**(**[**2**](#_bookmark755)**)** | TPBCLK \* (BRG + 2) | — | ns |
| IM40 | TAA:SCL | 100 kHz mode | — | 3500 | ns |  |
| 400 kHz mode | — | 1000 | ns |  |
| 1 MHz mode**(**[**2**](#_bookmark755)**)** | — | 350 | ns |  |
| IM45 | TBF:SDA | Bus Free Time | 100 kHz mode | 4.7 | — | s | The amount of time the bus must be free before a new transmission can start |
| 400 kHz mode | 1.3 | — | s |
| 1 MHz mode**(**[**2**](#_bookmark755)**)** | 0.5 | — | s |
| IM50 | CB | Bus Capacitive Loading | | — | — | pF | See Parameter [DO58](#_bookmark694) |
| IM51 | TPGD | Pulse Gobbler Delay | | 52 | 312 | ns | **(**[**Note 3**](#_bookmark756)**)** |

**Note 1:** BRG is the value of the I2C Baud Rate Generator.

**2:** Maximum Pin Capacitance = 10 pF for all I2Cx pins (for 1 MHz mode only).

**3:** The typical value for this parameter is 104 ns.

FIGURE 29-15: I2Cx BUS START/STOP BITS TIMING CHARACTERISTICS (SLAVE MODE)

SCLx

IS31

IS34

IS30 IS33

SDAx

Start Condition

Stop Condition

**Note:** Refer to [Figure 29-2](#_bookmark691) for load conditions.



FIGURE 29-16: I2Cx BUS DATA TIMING CHARACTERISTICS (SLAVE MODE)

IS20

IS11

IS21

IS10

SCLx

IS30

IS31

IS26

IS25

IS33

SDAx

In

IS40

IS40

IS45

SDAx

Out

**Note:** Refer to [Figure 29-2](#_bookmark691) for load conditions.



TABLE 29-33: I2Cx BUS DATA TIMING REQUIREMENTS (SLAVE MODE)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C | | | |
| **Param No.** | **Sym** | **Characteristics** | | **Min.** | **Max.** | **Units** | **Conditions** |
| IS10 | TLO:SCL | Clock Low Time | 100 kHz mode | 4.7 | — | s | PBCLK must operate at a minimum of 800 kHz |
| 400 kHz mode | 1.3 | — | s | PBCLK must operate at a minimum of 3.2 MHz |
| 1 MHz mode**(**[**1**](#_bookmark760)**)** | 0.5 | — | s |  |
| IS11 | THI:SCL | Clock High Time | 100 kHz mode | 4.0 | — | s | PBCLK must operate at a minimum of 800 kHz |
| 400 kHz mode | 0.6 | — | s | PBCLK must operate at a minimum of 3.2 MHz |
| 1 MHz mode**(**[**1**](#_bookmark760)**)** | 0.5 | — | s |  |
| IS20 | TF:SCL | SDAx and SCLx Fall Time | 100 kHz mode | — | 300 | ns | CB is specified to be from 10 to 400 pF |
| 400 kHz mode | 20 + 0.1 CB | 300 | ns |
| 1 MHz mode**(**[**1**](#_bookmark760)**)** | — | 100 | ns |

**Note 1:** Maximum Pin Capacitance = 10 pF for all I2Cx pins (for 1 MHz mode only).

TABLE 29-33: I2Cx BUS DATA TIMING REQUIREMENTS (SLAVE MODE) (CONTINUED)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C | | | |
| **Param No.** | **Sym** | **Characteristics** | | **Min.** | **Max.** | **Units** | **Conditions** |
| IS21 | TR:SCL | SDAx and SCLx Rise Time | 100 kHz mode | — | 1000 | ns | CB is specified to be from 10 to 400 pF |
| 400 kHz mode | 20 + 0.1 CB | 300 | ns |
| 1 MHz mode**(**[**1**](#_bookmark760)**)** | — | 300 | ns |
| IS25 | TSU:DAT | Data Input Setup Time | 100 kHz mode | 250 | — | ns |  |
| 400 kHz mode | 100 | — | ns |
| 1 MHz mode**(**[**1**](#_bookmark760)**)** | 100 | — | ns |
| IS26 | THD:DAT | Data Input Hold Time | 100 kHz mode | 0 | — | ns |  |
| 400 kHz mode | 0 | 0.9 | s |
| 1 MHz mode**(**[**1**](#_bookmark760)**)** | 0 | 0.3 | s |
| IS30 | TSU:STA | Start Condition Setup Time | 100 kHz mode | 4700 | — | ns | Only relevant for Repeated Start condition |
| 400 kHz mode | 600 | — | ns |
| 1 MHz mode**(**[**1**](#_bookmark760)**)** | 250 | — | ns |
| IS31 | THD:STA | Start Condition Hold Time | 100 kHz mode | 4000 | — | ns | After this period, the first clock pulse is generated |
| 400 kHz mode | 600 | — | ns |
| 1 MHz mode**(**[**1**](#_bookmark760)**)** | 250 | — | ns |
| IS33 | TSU:STO | Stop Condition Setup Time | 100 kHz mode | 4000 | — | ns |  |
| 400 kHz mode | 600 | — | ns |
| 1 MHz mode**(**[**1**](#_bookmark760)**)** | 600 | — | ns |
| IS34 | THD:STO | Stop Condition Hold Time | 100 kHz mode | 4000 | — | ns |  |
| 400 kHz mode | 600 | — | ns |
| 1 MHz mode**(**[**1**](#_bookmark760)**)** | 250 | — | ns |
| IS40 | TAA:SCL | Output Valid from Clock | 100 kHz mode | 0 | 3500 | ns |  |
| 400 kHz mode | 0 | 1000 | ns |
| 1 MHz mode**(**[**1**](#_bookmark760)**)** | 0 | 350 | ns |
| IS45 | TBF:SDA | Bus Free Time | 100 kHz mode | 4.7 | — | s | The amount of time the bus must be free before a new transmission can start |
| 400 kHz mode | 1.3 | — | s |
| 1 MHz mode**(**[**1**](#_bookmark760)**)** | 0.5 | — | s |
| IS50 | CB | Bus Capacitive Loading | | — | — | pF | See Parameter [DO58](#_bookmark694) |

**Note 1:** Maximum Pin Capacitance = 10 pF for all I2Cx pins (for 1 MHz mode only).

TABLE 29-34: ADC MODULE INPUTS SPECIFICATIONS

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Operating Conditions:** 2.0V  VDD  3.6V, -40°C  TA  +85°C (unless otherwise stated) | | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Max** | **Units** |
| **Reference Inputs** | | | | | |
| AD05 | VREFH | Reference Voltage High | AVSS + 1.7 | AVDD | V |
| AD06 | VREFL | Reference Voltage Low | AVSS | AVDD – 1.7 | V |
| AD07 | VREF | Absolute Reference Voltage | AVSS – 0.3 | AVDD + 0.3 | V |
| **Analog Inputs** | | | | | |
| AD10 | VINH-VINL | Full-Scale Input Span | VREFL | VREFH | V |
| AD11 | VIN | Absolute Input Voltage | AVSS – 0.3 | AVDD + 0.3 | V |
| AD12 | VINL | Absolute VINL Input Voltage | AVSS – 0.3 | AVDD + 0.3 | V |
| AD17 | RIN | Recommended Impedance of Analog Voltage Source | — | 2.5K |  |

TABLE 29-35: ADC ACCURACY AND CONVERSION TIMING REQUIREMENTS FOR 12-BIT MODE([1](#_bookmark765))

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Operating Conditions:** VDD = 3.3V, AVSS = VREFL = 0V, AVDD = VREFH = 3.3V, -40°C  TA  +85°C | | | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ(**[**2**](#_bookmark766)**)** | **Max** | **Units** |
| **ADC Accuracy** | | | | | | |
| AD20B | Nr | Resolution | — | 12 | — | bits |
| AD21B | INL | Integral Nonlinearity | — | ±2.5 | ±3.5 | LSb |
| AD22B | DNL | Differential Nonlinearity | — | ±0.75 | +1.75/-0.95 | LSb |
| AD23B | GERR | Gain Error | – | +2 | +3 | LSb |
| AD24B | EOFF | Offset Error | — | +1 | +2 | LSb |
| **Clock Parameters** | | | | | | |
| AD50B | TAD | ADC Clock Period | 280 | — | — | ns |
| AD61B | tPSS | Sample Start Delay from Setting Sample bit (SAMP) | 2 | — | 3 | TAD |
| **Conversion Rate** | | | | | | |
| AD55B | tCONV | Conversion Time | — | 14 | — | TAD |
| AD56B | FCNV | Throughput Rate | — | — | 200 | ksps |

**Note 1:** Measurements are taken with the external VREF+ and VREF- used as the ADC voltage reference.

**2:** Data in the “Typ” column is at 3.3V, +25°C unless otherwise stated. Parameters are for design guidance only and are not tested.

TABLE 29-36: ADC ACCURACY AND CONVERSION TIMING REQUIREMENTS FOR 10-BIT MODE([1](#_bookmark769))

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Operating Conditions:** VDD = 3.3V, AVSS = VREFL = 0V, AVDD = VREFH = 3.3V, -40°C  TA  +85°C | | | | | | |
| **Param No.** | **Symbol** | **Characteristic** | **Min** | **Typ(**[**2**](#_bookmark770)**)** | **Max** | **Units** |
| **ADC Accuracy** | | | | | | |
| AD20A | Nr | Resolution | — | 10 | — | bits |
| AD21A | INL | Integral Nonlinearity | — | ±0.5 | — | LSb |
| AD22A | DNL | Differential Nonlinearity | — | ±0.5 | — | LSb |
| AD23A | GERR | Gain Error | — | +0.75 | — | LSb |
| AD24A | EOFF | Offset Error | — | +0.25 | — | LSb |
| **Clock Parameters** | | | | | | |
| AD50A | TAD | ADC Clock Period | 200 | — | — | ns |
| AD61A | tPSS | Sample Start Delay from Setting Sample bit (SAMP) | 2 | — | 3 | TAD |
| **Conversion Rate** | | | | | | |
| AD55A | tCONV | Conversion Time | — | 12 | — | TAD |
| AD56A | FCNV | Throughput Rate | — | — | 300 | ksps |

**Note 1:** Measurements are taken with the external VREF+ and VREF- used as the ADC voltage reference.

**2:** Data in the “Typ” column is at 3.3V, +25°C unless otherwise stated. Parameters are for design guidance only and are not tested.

FIGURE 29-17: EJTAG TIMING CHARACTERISTICS

TTCKcyc

TTCKhigh

TTCKlow

Trf

TCK

Trf

TMS

TDI

TTsetup TThold

Trf

Trf

TDO

TRST\*

TTRST\*low

T

TDOout

T

TDOzstate

Defined

Undefined

Trf



TABLE 29-37: EJTAG TIMING REQUIREMENTS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.0V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C | | | |
| **Param No.** | **Symbol** | **Description(**[**1**](#_bookmark773)**)** | **Min.** | **Max.** | **Units** | **Conditions** |
| EJ1 | TTCKCYC | TCK Cycle Time | 25 | — | ns |  |
| EJ2 | TTCKHIGH | TCK High Time | 10 | — | ns |  |
| EJ3 | TTCKLOW | TCK Low Time | 10 | — | ns |  |
| EJ4 | TTSETUP | TAP Signals Setup Time before Rising TCK | 5 | — | ns |  |
| EJ5 | TTHOLD | TAP Signals Hold Time after Rising TCK | 3 | — | ns |  |
| EJ6 | TTDOOUT | TDO Output Delay Time from Falling TCK | — | 5 | ns |  |
| EJ7 | TTDOZSTATE | TDO 3-State Delay Time from Falling TCK | — | 5 | ns |  |
| EJ8 | TTRSTLOW | TRST Low Time | 25 | — | ns |  |
| EJ9 | TRF | TAP Signals Rise/Fall Time, All Input and Output | — | — | ns |  |

**Note 1:** These parameters are characterized but not tested in manufacturing.

TABLE 29-38: USB OTG ELECTRICAL SPECIFICATIONS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AC CHARACTERISTICS** | | | **Standard Operating Conditions: 2.3V to 3.6V (unless otherwise stated)**  Operating temperature -40°C  TA  +85°C for Industrial | | | | |
| **Param. No.** | **Symbol** | **Characteristics(**[**1**](#_bookmark777)**)** | **Min.** | **Typical** | **Max.** | **Units** | **Conditions** |
| USB313 | VUSB3V3 | USB Voltage | 3.0 | — | 3.6 | V | Voltage on VUSB3V3 must be in this range for proper USB operation |
| USB315 | VILUSB | Input Low Voltage for USB Buffer | — | — | 0.8 | V |  |
| USB316 | VIHUSB | Input High Voltage for USB Buffer | 2.0 | — | — | V |  |
| USB318 | VDIFS | Differential Input Sensitivity | — | — | 0.2 | V | The difference between D+ and D- must exceed this value while VCM is met |
| USB319 | VCM | Differential Common-Mode Range | 0.8 | — | 2.5 | V |  |
| USB320 | ZOUT | Driver Output Impedance | 28.0 | — | 44.0 |  |  |
| USB321 | VOL | Voltage Output Low | 0.0 | — | 0.3 | V | 14.25 k load connected to 3.6V |
| USB322 | VOH | Voltage Output High | 2.8 | — | 3.6 | V | 14.25 k load connected to ground |

**Note 1:** These parameters are characterized but not tested in manufacturing.

# PACKAGING INFORMATION

### Package Marking Information

28-Lead SSOP (5.30 mm) Example



XXXXXXXXXXXX XXXXXXXXXXXX

YYWWNNN



PIC32MM0064 GPM028

1610017

28-Lead QFN (6x6 mm) Example



XXXXXXXX XXXXXXXX YYWWNNN



32MM0064 GPM028 1610017

28-Lead UQFN (4x4x0.6 mm) Example



XXXXXXXX XXXXXXXX YYWWNNN



32MM0064 GPM028 1610017

36-Lead VQFN (6x6x1.0 mm) Example



XXXXXXXX XXXXXXXX YYWWNNN



32MM0064 GPM036 1610017

**Note:** In the event the full Microchip part number cannot be marked on one line, it will be carried over to the next line, thus limiting the number of available characters for customer-specific information.

All packages are Pb-free

**\***

**Legend:** XX...X Customer-specific information

YY Year code (last 2 digits of calendar year) WW Week code (week of January 1 is week ‘01’) NNN Alphanumeric traceability code

### Package Marking Information (Continued)

40-Lead UQFN (5x5x0.5 mm)

Example



XXXXXXX XXXXXXX XXXXXXX YYWWNNN



32MM

0064

GPM036 1610017

48-Lead UQFN (6x6 mm) Example



XXXXXXXXXX XXXXXXXXXX XXXXXXXXXX YYWWNNN



32MM0064 GPM048

1610017

48-Lead TQFP (7x7x1.0 mm) Example

**1**

XXXXXXX

XXXYYWW NNN



0128GPM

0481610

017

64-Lead QFN (9x9x0.9 mm) Example




XXXXXXXXXXX XXXXXXXXXXX XXXXXXXXXXX YYWWNNN



PIC32MM0064 GPM064 1650017

64-Lead TQFP (10x10x1 mm) Example



XXXXXXXXX XXXXXXXXX XXXXXXXXX YYWWNNN



PIC32MM 0064GPM064

1620017

### Package Details

The following sections give the technical details of the packages.

##### 28-Lead Plastic Shrink Small Outline (SS) – 5.30 mm Body [SSOP]

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

D

N

E

E1

1 2

NOTE 1

b

e



c





L1

L

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| A |  | | | | | | | | | | | | | | | | | | | | | | | | | | | A2 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

A1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Units | | MILLIMETERS | | |
| Dimension Limits | | MIN | NOM | MAX |
| Number of Pins | N | 28 | | |
| Pitch | e | 0.65 BSC | | |
| Overall Height | A | – | – | 2.00 |
| Molded Package Thickness | A2 | 1.65 | 1.75 | 1.85 |
| Standoff | A1 | 0.05 | – | – |
| Overall Width | E | 7.40 | 7.80 | 8.20 |
| Molded Package Width | E1 | 5.00 | 5.30 | 5.60 |
| Overall Length | D | 9.90 | 10.20 | 10.50 |
| Foot Length | L | 0.55 | 0.75 | 0.95 |
| Footprint | L1 | 1.25 REF | | |
| Lead Thickness | c | 0.09 | – | 0.25 |
| Foot Angle |  | 0° | 4° | 8° |
| Lead Width | b | 0.22 | – | 0.38 |

**Notes:**

1. Pin 1 visual index feature may vary, but must be located within the hatched area.
2. Dimensions D and E1 do not include mold flash or protrusions. Mold flash or protrusions shall not exceed 0.20 mm per side.
3. Dimensioning and tolerancing per ASME Y14.5M.

BSC: Basic Dimension. Theoretically exact value shown without tolerances.

REF: Reference Dimension, usually without tolerance, for information purposes only.

Microchip Technology Drawing C04-073B







**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>





|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | |  |  | |
|  | |  |  |  |
|  |  |  | | |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |



















|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  |  | | | | |
|  |  |  |  | |  | |
|  |  |  | | | | |
|  |  |  | | | | |
|  |  |  | |  | |  |
|  |  |  | |  | |  |
|  |  |  | | | | |
|  |  |  | | | | |
|  |  |  | |  | |  |
|  |  |  | | | | |
|  |  |  | |  | |  |
|  |  |  | |  | |  |
|  |  |  | |  | |  |
|  |  |  | |  | |  |









##### 28-Lead Plastic Quad Flat, No Lead Package (ML) – 6x6 mm Body [QFN] with 0.55 mm Contact Length

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | |  | | |
|  | |  |  |  |
|  |  |  | | |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |





##### Lead Ultra Thin Plastic Quad Flat, No Lead Package (M6) - 4x4x0.6 mm Body [UQFN] With Corner Anchors

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

D A B

NOTE 1 N

1

2

SEATING PLANE

(DATUM B) (DATUM A)

2X

E

#### TOP VIEW

|  |  |  |  |
| --- | --- | --- | --- |
|  | 0.10 | C |  |

|  |  |  |
| --- | --- | --- |
| 2X | | |
|  | 0.10 | C |

A1



C

A

28X

(A3)

SIDE VIEW

B

A

C

0.10

C

0.08

|  |  |  |
| --- | --- | --- |
|  | 0.10 | C |



4x b1

D2

4x b2

4x b2

E2

NOTE 1

2

1

K

N

4x b1

L

28X b

e

2

e

B

A

C

0.10

#### BOTTOM VIEW

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | 0.07 | C | A | B |
| 0.05 | C |  | |

Microchip Technology Drawing C04-333-M6 Rev B Sheet 1 of 2

##### Lead Ultra Thin Plastic Quad Flat, No Lead Package (M6) - 4x4x0.6 mm Body [UQFN] With Corner Anchors

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Units | | MILLIMETERS | | |
| Dimension Limits | | MIN | NOM | MAX |
| Number of Pins | N | 28 | | |
| Pitch | e | 0.40 BSC | | |
| Overall Height | A | - | - | 0.60 |
| Standoff | A1 | 0.00 | 0.02 | 0.05 |
| Terminal Thickness | A3 | 0.152 REF | | |
| Overall Width | E | 4.00 BSC | | |
| Exposed Pad Width | E2 | 1.80 | 1.90 | 2.00 |
| Overall Length | D | 4.00 BSC | | |
| Exposed Pad Length | D2 | 1.80 | 1.90 | 2.00 |
| Terminal Width | b | 0.15 | 0.20 | 0.25 |
| Corner Anchor Pad | b1 | 0.40 | 0.45 | 0.50 |
| Corner Pad, Metal Free Zone | b2 | 0.18 | 0.23 | 0.28 |
| Terminal Length | L | 0.30 | 0.45 | 0.50 |
| Terminal-to-Exposed-Pad | K | - | 0.60 | - |

Notes:

* + - 1. Pin 1 visual index feature may vary, but must be located within the hatched area.
      2. Package is saw singulated
      3. Dimensioning and tolerancing per ASME Y14.5M

BSC: Basic Dimension. Theoretically exact value shown without tolerances.

REF: Reference Dimension, usually without tolerance, for information purposes only.

Microchip Technology Drawing C04-333-M6 Rev A Sheet 2 of 2

##### Lead Ultra Thin Plastic Quad Flat, No Lead Package (M6) - 4x4x0.6 mm Body [UQFN] With Corner Anchors

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>



C1 X2

EV

28

G3

1

2

ØV

G2

C2 Y2 EV

G1

Y1

Y3

X1

X3 SILK SCREEN

E

#### RECOMMENDED LAND PATTERN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Units | | MILLIMETERS | | |
| Dimension Limits | | MIN | NOM | MAX |
| Contact Pitch | E | 0.40 BSC | | |
| Center Pad Width | X2 |  |  | 2.00 |
| Center Pad Length | Y2 |  |  | 2.00 |
| Contact Pad Spacing | C1 |  | 3.90 |  |
| Contact Pad Spacing | C2 |  | 3.90 |  |
| Contact Pad Width (X28) | X1 |  |  | 0.20 |
| Contact Pad Length (X28) | Y1 |  |  | 0.85 |
| Contact Pad to Center Pad (X28) | G1 |  | 0.52 |  |
| Contact Pad to Pad (X24) | G2 | 0.20 |  |  |
| Contact Pad to Corner Pad (X8) | G3 | 0.20 |  |  |
| Corner Anchor Width (X4) | X3 |  |  | 0.78 |
| Corner Anchor Length (X4) | Y3 |  |  | 0.78 |
| Thermal Via Diameter | V |  | 0.30 |  |
| Thermal Via Pitch | EV |  | 1.00 |  |

Notes:


* 1. Dimensioning and tolerancing per ASME Y14.5M

BSC: Basic Dimension. Theoretically exact value shown without tolerances.

Microchip Technology Drawing C04-2333-M6 Rev B

### 36-Terminal Very Thin Plastic Quad Flatpack No-Lead (M2) - 6x6x1.0mm Body [VQFN] SMSC Legacy "Sawn Quad Flatpack No-Lead [SQFN]"

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

D A

B

NOTE 1 N

1

2

(DATUM B) (DATUM A)

2X

E

#### TOP VIEW

|  |  |  |  |
| --- | --- | --- | --- |
|  | 0.10 | C |  |

|  |  |  |
| --- | --- | --- |
| 2X | | |
|  | 0.10 | C |

A1

C

0.10

C

SEATING A

PLANE


#### SIDE VIEW

36X

C

0.08

(A3)



0.10 C A B

D2

0.10 C A B

E2

2

1

N

K

L 36X b

e

NOTE 1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | 0.10 | C | A | B |
| 0.05 | C |  | |

#### BOTTOM VIEW

Microchip Technology Drawing C04-272B-M2 Sheet 1 of 2

### Terminal Very Thin Plastic Quad Flatpack No-Lead (M2) - 6x6x1.0mm Body [VQFN] SMSC Legacy "Sawn Quad Flatpack No-Lead [SQFN]"

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Units | | MILLIMETERS | | |
| Dimension Limits | | MIN | NOM | MAX |
| Number of Terminals | N | 36 | | |
| Pitch | e | 0.50 BSC | | |
| Overall Height | A | 0.80 | 0.90 | 1.00 |
| Standoff | A1 | 0.00 | 0.02 | 0.05 |
| Terminal Thickness | A3 | 0.20 REF | | |
| Overall Width | E | 6.00 BSC | | |
| Exposed Pad Width | E2 | 3.60 | 3.70 | 3.80 |
| Overall Length | D | 6.00 BSC | | |
| Exposed Pad Length | D2 | 3.60 | 3.70 | 3.80 |
| Terminal Width | b | 0.18 | 0.25 | 0.30 |
| Terminal Length | L | 0.50 | 0.60 | 0.75 |
| Terminal-to-Exposed-Pad | K | 0.45 | 0.55 | - |

Notes:

* 1. Pin 1 visual index feature may vary, but must be located within the hatched area.
  2. Package is saw singulated
  3. Dimensioning and tolerancing per ASME Y14.5M

BSC: Basic Dimension. Theoretically exact value shown without tolerances.


REF: Reference Dimension, usually without tolerance, for information purposes only.

Microchip Technology Drawing C04-272B-M2 Sheet 2 of 2

### 36-Terminal Very Thin Plastic Quad Flatpack No-Lead (M2) - 6x6x0.9 mm Body [VQFN] SMSC Legacy "Sawn Quad Flatpack No-Lead [SQFN]"

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

C1 X2



EV

36

G2

1

2

Y2 ØV

C2 EV

G1

Y1

X1

E SILK SCREEN

#### RECOMMENDED LAND PATTERN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Units | | MILLIMETERS | | |
| Dimension Limits | | MIN | NOM | MAX |
| Contact Pitch | E | 0.50 BSC | | |
| Optional Center Pad Width | X2 |  |  | 3.80 |
| Optional Center Pad Length | Y2 |  |  | 3.80 |
| Contact Pad Spacing | C1 |  | 5.60 |  |
| Contact Pad Spacing | C2 |  | 5.60 |  |
| Contact Pad Width (X36) | X1 |  |  | 0.30 |
| Contact Pad Length (X36) | Y1 |  |  | 1.10 |
| Contact Pad to Center Pad (X36) | G1 | 0.35 |  |  |
| Space Between Contact Pads (X32) | G2 | 0.20 |  |  |
| Thermal Via Diameter | V |  | 0.30 |  |
| Thermal Via Pitch | EV |  | 1.00 |  |



Notes:

1. Dimensioning and tolerancing per ASME Y14.5M

BSC: Basic Dimension. Theoretically exact value shown without tolerances.

1. For best soldering results, thermal vias, if used, should be filled or tented to avoid solder loss during reflow process

Microchip Technology Drawing C04-2272B-M2



**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>




|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |






|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |






      

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>




|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | | |  |  | |
|  | | |  |  |  |
|  |  | |  | | |
|  |  | |  | | |
|  |  | |  | | |
|  |  | |  | | |
|  |  | |  | | |
|  |  | |  | | |
|  |  | |  |  | |
|  |  | |  | | |
|  |  | |  |  |  |
|  |  | |  |  |  |
|  |  | |  |  |  |
|  |  |  |  |  |  |









**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>





|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | |  | | |
|  | |  |  |  |
|  |  |  | | |
|  |  |  |  | |
|  |  |  |  | |
|  |  |  |  | |
|  |  |  |  | |
|  |  |  |  | |
|  |  |  |  | |
|  |  |  |  | |





### 48-Lead Ultra Thin Plastic Quad Flat, No Lead Package (M4) - 6x6 mm Body [UQFN] With Corner Anchors and 4.6x4.6 mm Exposed Pad

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

A1



52X

C

0.08

NOTE 1 D A B

|  |  |  |
| --- | --- | --- |
|  | 0.10 | C |
|  | | |

N

1

2

E

(DATUM B) (DATUM A)

2X

|  |  |  |
| --- | --- | --- |
| 2X | | |
|  | 0.10 | C |

|  |  |  |  |
| --- | --- | --- | --- |
|  | 0.10 | C |  |


8X (b1)

#### TOP VIEW

(A3)

A

SEATING PLANE



B

A

C

0.10

C

D2 SIDE VIEW

B

A

C

0.10

8X (b2)

E2

2

e

2

1

NOTE 1

L

N

e

#### BOTTOM VIEW

48X b

(K)




Microchip Technology Drawing C04-442A-M4 Sheet 1 of 2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | 0.07 | C | A | B |
| 0.05 | C |  | |

### Lead Ultra Thin Plastic Quad Flat, No Lead Package (M4) - 6x6 mm Body [UQFN] With Corner Anchors and 4.6x4.6 mm Exposed Pad

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Units | | MILLIMETERS | | |
| Dimension Limits | | MIN | NOM | MAX |
| Number of Terminals | N | 48 | | |
| Pitch | e | 0.40 BSC | | |
| Overall Height | A | 0.50 | 0.55 | 0.60 |
| Standoff | A1 | 0.00 | 0.02 | 0.05 |
| Terminal Thickness | A3 | 0.15 REF | | |
| Overall Length | D | 6.00 BSC | | |
| Exposed Pad Length | D2 | 4.50 | 4.60 | 4.70 |
| Overall Width | E | 6.00 BSC | | |
| Exposed Pad Width | E2 | 4.50 | 4.60 | 4.70 |
| Terminal Width | b | 0.15 | 0.20 | 0.25 |
| Corner Anchor Pad | b1 | 0.45 REF | | |
| Corner Anchor Pad, Metal-free Zone | b2 | 0.23 REF | | |
| Terminal Length | L | 0.35 | 0.40 | 0.45 |
| Terminal-to-Exposed-Pad | K | 0.30 REF | | |

Notes:

* 1. Pin 1 visual index feature may vary, but must be located within the hatched area.
  2. Package is saw singulated
  3. Dimensioning and tolerancing per ASME Y14.5M

BSC: Basic Dimension. Theoretically exact value shown without tolerances.

REF: Reference Dimension, usually without tolerance, for information purposes only.


Microchip Technology Drawing C04-442A-M4 Sheet 2 of 2

### Lead Ultra Thin Plastic Quad Flat, No Lead Package (M4) - 6x6 mm Body [UQFN] With Corner Anchors and 4.6x4.6 mm Exposed Pad

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

C1 X2

EV



R 48

Y3

1

2

Y2 EV

C2

ØV G2

G1 Y1

SILK SCREEN

X1

X3

E

#### RECOMMENDED LAND PATTERN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Units | | MILLIMETERS | | |
| Dimension Limits | | MIN | NOM | MAX |
| Contact Pitch | E | 0.40 BSC | | |
| Center Pad Width | X2 |  |  | 4.70 |
| Center Pad Length | Y2 |  |  | 4.70 |
| Contact Pad Spacing | C1 |  | 6.00 |  |
| Contact Pad Spacing | C2 |  | 6.00 |  |
| Contact Pad Width (X48) | X1 |  |  | 0.20 |
| Contact Pad Length (X48) | Y1 |  |  | 0.80 |
| Corner Anchor Pad Width (X4) | X3 |  |  | 0.90 |
| Corner Anchor Pad Length (X4) | Y3 |  |  | 0.90 |
| Pad Corner Radius (X 20) | R |  |  | 0.10 |
| Contact Pad to Center Pad (X48) | G1 | 0.25 |  |  |
| Contact Pad to Contact Pad | G2 | 0.20 |  |  |
| Thermal Via Diameter | V |  | 0.33 |  |
| Thermal Via Pitch | EV |  | 1.20 |  |

Notes:

* 1. Dimensioning and tolerancing per ASME Y14.5M

BSC: Basic Dimension. Theoretically exact value shown without tolerances.

* 1. For best soldering results, thermal vias, if used, should be filled or tented to avoid solder loss during reflow process

Microchip Technology Drawing C04-2442A-M4

##### Lead Thin Quad Flatpack (PT) - 7x7x1.0 mm Body [TQFP] With Exposed Pad

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | | | | |  |
| 4X | | | | | |
|  | 0.20 | H | A-B | D |  |

A

C

**SEATING PLANE**

#### TOP VIEW

H



D

D1

D

A

NOTE 1

E1 E

A

A

E1/2

E1/4 N

48X TIPS

1 2

D1/4

D

A-B

C

0.20

D1/2

B



|  |  |  |  |
| --- | --- | --- | --- |
|  |  | 0.10 | C |

#### SIDE VIEW

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | 0.08 | C |

A2 A1



D2

4X

1 2

E2

48x b

e/2

0.20

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | 0.20 | H | A-B | D |
| 4X | | | | |

N

e

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | 0.08 | C | A-B | D |

#### TOP VIEW

Microchip Technology Drawing C04-183A Sheet 1 of 2

##### Lead Thin Quad Flatpack (PT) - 7x7x1.0 mm Body [TQFP] With Exposed Pad

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>



D

H

c

E

L

T

(L1)

#### SECTION A-A

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Units | | MILLIMETERS | | |
| Dimension Limits | | MIN | NOM | MAX |
| Number of Leads | N | 48 | | |
| Lead Pitch | e | 0.50 BSC | | |
| Overall Height | A | - | - | 1.20 |
| Standoff | A1 | 0.05 | - | 0.15 |
| Molded Package Thickness | A2 | 0.95 | 1.00 | 1.05 |
| Foot Length | L | 0.45 | 0.60 | 0.75 |
| Footprint | L1 | 1.00 REF | | |
| Foot Angle | I | 0° | 3.5° | 7° |
| Overall Width | E | 9.00 BSC | | |
| Overall Length | D | 9.00 BSC | | |
| Molded Package Width | E1 | 7.00 BSC | | |
| Molded Package Length | D1 | 7.00 BSC | | |
| Exposed Pad Width | E2 | 3.50 BSC | | |
| Exposed Pad Length | D2 | 3.50 BSC | | |
| Lead Thickness | c | 0.09 | - | 0.16 |
| Lead Width | b | 0.17 | 0.22 | 0.27 |
| Mold Draft Angle Top | D | 11° | 12° | 13° |
| Mold Draft Angle Bottom | E | 11° | 12° | 13° |

Notes:

* + 1. Pin 1 visual index feature may vary, but must be located within the hatched area.
    2. Chamfers at corners are optional; size may vary.
    3. Dimensions D1 and E1 do not include mold flash or protrusions. Mold flash or protrusions shall not exceed 0.25mm per side.
    4. Dimensioning and tolerancing per ASME Y14.5M

BSC: Basic Dimension. Theoretically exact value shown without tolerances.

REF: Reference Dimension, usually without tolerance, for information purposes only.

Microchip Technology Drawing C04-183A Sheet 2 of 2

##### Lead Thin Quad Flatpack (PT) - 7x7x1.0 mm Body [TQFP] With Thermal Tab

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

C2

C1

X2

Y2

E

Y1

X1

#### RECOMMENDED LAND PATTERN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Units | | MILLIMETERS | | |
| Dimension Limits | | MIN | NOM | MAX |
| Contact Pitch | E | 0.50 BSC | | |
| Optional Center Tab Width | X2 |  | 3.50 |  |
| Optional Center Tab Length | Y2 |  | 3.50 |  |
| Contact Pad Spacing | C1 |  | 8.40 |  |
| Contact Pad Spacing | C2 |  | 8.40 |  |
| Contact Pad Width (X48) | X1 |  |  | 0.30 |
| Contact Pad Length (X48) | Y1 |  |  | 1.50 |

Notes:

* 1. Dimensioning and tolerancing per ASME Y14.5M


BSC: Basic Dimension. Theoretically exact value shown without tolerances.

Microchip Technology Drawing No. C04-2183A

##### 64-Lead Plastic Quad Flat, No Lead Package (MR) – 9x9x0.9 mm Body [QFN]

##### With 7.70 x 7.70 Exposed Pad [QFN]

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

D A B

N

1

2

NOTE 1

SEATING PLANE

(DATUM B) (DATUM A)

2X


E

#### TOP VIEW

|  |  |  |  |
| --- | --- | --- | --- |
|  | 0.25 | C |  |

|  |  |  |
| --- | --- | --- |
| 2X | | |
|  | 0.25 | C |

A1



A

C

64X

A3


SIDE VIEW

C

0.08

|  |  |  |
| --- | --- | --- |
|  | 0.10 | C |

NOTE 1



0.10 C A B

D2

0.10 C A B

E2

2

1

N

K

L 64X b

e

2

e


#### BOTTOM VIEW

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | 0.10 | C | A | B |
| 0.05 | C |  | |

Microchip Technology Drawing C04-213B Sheet 1 of 2

##### Lead Plastic Quad Flat, No Lead Package (MR) – 9x9x0.9 mm Body [QFN] With 7.70 x 7.70 Exposed Pad [QFN]

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Units | | MILLIMETERS | | |
| Dimension Limits | | MIN | NOM | MAX |
| Number of Pins | N | 64 | | |
| Pitch | e | 0.50 BSC | | |
| Overall Height | A | 0.80 | 0.85 | 0.90 |
| Standoff | A1 | 0.00 | 0.02 | 0.05 |
| Contact Thickness | A3 | 0.20 REF | | |
| Overall Width | E | 9.00 BSC | | |
| Exposed Pad Width | E2 | 7.60 | 7.70 | 7.80 |
| Overall Length | D | 9.00 BSC | | |
| Exposed Pad Length | D2 | 7.60 | 7.70 | 7.80 |
| Contact Width | b | 0.20 | 0.25 | 0.30 |
| Contact Length | L | 0.30 | 0.40 | 0.50 |
| Contact-to-Exposed Pad | K | 0.20 | - | - |

**Notes:**

* 1. Pin 1 visual index feature may vary, but must be located within the hatched area.
  2. Package is saw singulated.
  3. Dimensioning and tolerancing per ASME Y14.5M.

BSC: Basic Dimension. Theoretically exact value shown without tolerances.

REF: Reference Dimension, usually without tolerance, for information purposes only.


Microchip Technology Drawing C04-213B Sheet 2 of 2

###### 64-Lead Plastic Quad Flat, No Lead Package (MR) – 9x9x0.9 mm Body [QFN] With 0.40 mm Contact Length and 7.70x7.70mm Exposed Pad

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

C1 W2

EV



64

1

2 EV

C2 T2

G

ØV

Y1

X1

E SILK SCREEN

#### RECOMMENDED LAND PATTERN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Units | | MILLIMETERS | | |
| Dimension Limits | | MIN | NOM | MAX |
| Contact Pitch | E | 0.50 BSC | | |
| Optional Center Pad Width | W2 |  |  | 7.50 |
| Optional Center Pad Length | T2 |  |  | 7.50 |
| Contact Pad Spacing | C1 |  | 8.90 |  |
| Contact Pad Spacing | C2 |  | 8.90 |  |
| Contact Pad Width (X20) | X1 |  |  | 0.30 |
| Contact Pad Length (X20) | Y1 |  |  | 0.90 |
| Contact Pad to Center Pad (X20) | G | 0.20 |  |  |
| Thermal Via Diameter | V |  | 0.30 |  |
| Thermal Via Pitch | EV |  | 1.00 |  |

Notes:

1. Dimensioning and tolerancing per ASME Y14.5M

BSC: Basic Dimension. Theoretically exact value shown without tolerances.

1. For best soldering results, thermal vias, if used, should be filled or tented to avoid solder loss during reflow process

Microchip Technology Drawing No. C04-2213B

##### 64-Lead Plastic Thin Quad Flatpack (PT)-10x10x1 mm Body, 2.00 mm Footprint [TQFP]

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

D D1



D1/2

D

NOTE 2

A

E1/2

B

E1

E

A A

SEE DETAIL 1

N

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | | | | |  |
| 4X | | | | | |
|  | 0.20 | H | A-B | D |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 4X N/4 TIPS | | | | |
|  | 0.20 | C | A-B | D |

NOTE 1

1 2 3

#### TOP VIEW

A A2



0.05

C

**SEATING PLANE**

e

C

0.08

64 X b A1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | 0.08 | C | A-B | D |


#### SIDE VIEW

Microchip Technology Drawing C04-085C Sheet 1 of 2

##### 64-Lead Plastic Thin Quad Flatpack (PT)-10x10x1 mm Body, 2.00 mm Footprint [TQFP]

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

H



c

E

L

(L1)

T

X=A—B OR D

#### SECTION A-A X

e/2

#### DETAIL 1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Units | | MILLIMETERS | | |
| Dimension Limits | | MIN | NOM | MAX |
| Number of Leads | N | 64 | | |
| Lead Pitch | e | 0.50 BSC | | |
| Overall Height | A | - | - | 1.20 |
| Molded Package Thickness | A2 | 0.95 | 1.00 | 1.05 |
| Standoff | A1 | 0.05 | - | 0.15 |
| Foot Length | L | 0.45 | 0.60 | 0.75 |
| Footprint | L1 | 1.00 REF | | |
| Foot Angle | I | 0° | 3.5° | 7° |
| Overall Width | E | 12.00 BSC | | |
| Overall Length | D | 12.00 BSC | | |
| Molded Package Width | E1 | 10.00 BSC | | |
| Molded Package Length | D1 | 10.00 BSC | | |
| Lead Thickness | c | 0.09 | - | 0.20 |
| Lead Width | b | 0.17 | 0.22 | 0.27 |
| Mold Draft Angle Top | D | 11° | 12° | 13° |
| Mold Draft Angle Bottom | E | 11° | 12° | 13° |

Notes:

1. Pin 1 visual index feature may vary, but must be located within the hatched area.
2. Chamfers at corners are optional; size may vary.
3. Dimensions D1 and E1 do not include mold flash or protrusions. Mold flash or protrusions shall not exceed 0.25mm per side.
4. Dimensioning and tolerancing per ASME Y14.5M

BSC: Basic Dimension. Theoretically exact value shown without tolerances.

REF: Reference Dimension, usually without tolerance, for information purposes only.

Microchip Technology Drawing C04-085C Sheet 2 of 2

##### Lead Plastic Thin Quad Flatpack (PT)-10x10x1 mm Body, 2.00 mm Footprint [TQFP]

**Note:** For the most current package drawings, please see the Microchip Packaging Specification located at <http://www.microchip.com/packaging>

C1

C2

E

G

Y1

X1

#### RECOMMENDED LAND PATTERN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Units | | MILLIMETERS | | |
| Dimension Limits | | MIN | NOM | MAX |
| Contact Pitch | E | 0.50 BSC | | |
| Contact Pad Spacing | C1 |  | 11.40 |  |
| Contact Pad Spacing | C2 |  | 11.40 |  |
| Contact Pad Width (X28) | X1 |  |  | 0.30 |
| Contact Pad Length (X28) | Y1 |  |  | 1.50 |
| Distance Between Pads | G | 0.20 |  |  |

Notes:

* 1. Dimensioning and tolerancing per ASME Y14.5M

BSC: Basic Dimension. Theoretically exact value shown without tolerances.

Microchip Technology Drawing C04-2085B Sheet 1 of 1

# APPENDIX A: REVISION HISTORY

### Revision A (January 2016)

This is the initial version of the document.

### Revision B (March 2017)

This revision incorporates the following updates:

* Sections:
  + Updated the [**“Low-Power Modes”**](#_bookmark0), [**“Peripheral Features”**](#_bookmark2), [**“Microcontroller Features”**](#_bookmark1) and [**“Analog Features”**](#_bookmark3)sections.
  + Changed program row size to 128 32-bit words in [**Section 5.0 “Flash Program Memory”**](#_bookmark101).
  + Updated [**Section 4.2 “Bus Matrix (BMX)”**](#_bookmark82), [**Section 8.0 “Direct Memory Access (DMA) Controller”**](#_bookmark169), [**Section 9.0 “Oscillator Con- figuration”**](#_bookmark207), [**Section 9.2 “Clock Switching Operation”**](#_bookmark209), [**Section 9.3 “FRC Active Clock Tuning”**](#_bookmark215), [**Section 10.1 “CLR, SET and INV Registers”**](#_bookmark250), [**Section 10.5 “I/O Port Write/Read Timing”**](#_bookmark255), [**Section 10.6 “GPIO Port Merging”**](#_bookmark257), [**Section 20.1 “Introduc- tion”**](#_bookmark472), [**Section 26.5 “Band Gap Voltage Reference”**](#_bookmark577) and [**Section 26.7 “Unique Device Identifier (UDID)”**](#_bookmark580).
  + Added the 36-Lead VQFN (M2) and 48-Lead UQFN (M4) packaging diagrams to

[**Section 30.0 “Packaging Information”**](#_bookmark779).

* Tables:
  + Updated [Table 1-1](#_bookmark27), [Table 7-2](#_bookmark153), [Table 7-3](#_bookmark156), [Table 9-1](#_bookmark224), [Table 10-5](#_bookmark281), [Table 10-6](#_bookmark287), [Table 10-7](#_bookmark291),

[Table 10-8](#_bookmark296), [Table 20-1](#_bookmark478), [Table 26-3](#_bookmark584),

[Table 26-4](#_bookmark587), [Table 26-6](#_bookmark608), [Table 26-8](#_bookmark616), [Table 29-2](#_bookmark645),

[Table 29-3](#_bookmark648), [Table 29-4](#_bookmark650), [Table 29-5](#_bookmark653), [Table 29-6](#_bookmark657),

[Table 29-7](#_bookmark661), [Table 29-8](#_bookmark665), [Table 29-11](#_bookmark679),

[Table 29-14](#_bookmark684), [Table 29-20](#_bookmark703) and [Table 29-21](#_bookmark706).

* + Replaced Table 29-34 with [Table 29-34](#_bookmark761), [Table 29-35](#_bookmark763) and [Table 29-36](#_bookmark767).
  + Removed previously numbered Table 29-35.
* Examples:
  + Updated [Example 9-1](#_bookmark213).
* Figures:
  + Updated [Figure 1-1](#_bookmark24), [Figure 8-1](#_bookmark172), [Figure 9-1](#_bookmark218),

[Figure 9-2](#_bookmark221) and [Figure 22-1](#_bookmark526).

* + Added [Figure 9-2](#_bookmark221).
* Registers:
  + Updated [Register 6-4](#_bookmark141), [Register 9-1](#_bookmark228),

[Register 9-2](#_bookmark231), [Register 9-3](#_bookmark233), [Register 9-5](#_bookmark242),

[Register 14-1](#_bookmark341), [Register 19-1](#_bookmark463), [Register 19-2](#_bookmark466), [Register 26-1](#_bookmark589),[Register 26-5](#_bookmark594) and

[Register 26-10](#_bookmark612).

* + Removed Register 9-7.

### Revision C (May 2017)

This revision incorporates the following updates:

* Sections:
  + Updated the [**“Peripheral Features”**](#_bookmark2)

section.

* + Updated [**Section 2.3 ”Master Clear (MCLR) Pin”**](#_bookmark37) and [**Section 25.3 ”Retention Sleep Mode”**](#_bookmark554).
* Tables:
  + Updated [Table 29-4](#_bookmark650), [Table 29-5](#_bookmark653), [Table 29-6](#_bookmark657) and [Table 29-7](#_bookmark661).
* Registers:
  + Updated [Register 13-1](#_bookmark330).

NOTES:

# INDEX

A

AC Characteristics

[10-Bit ADC Accuracy and Conversion](#_bookmark768)

[Requirements 316](#_bookmark768)

[12-Bit ADC Accuracy and Conversion](#_bookmark764)

[Requirements 315](#_bookmark764)

[ADC Inputs Specifications 315](#_bookmark762)

[and Timing Parameters 298](#_bookmark690)

[Capacitive Loading on Output Pins 298](#_bookmark693)

[CLKO and I/O Timing Requirements 301](#_bookmark708)

[EJTAG Requirements 317](#_bookmark772)

[External Clock Timing Requirements 299](#_bookmark697)

[I2Cx Bus Data Requirements (Master Mode) 311](#_bookmark752)

[I2Cx Bus Data Requirements (Slave Mode) 313](#_bookmark759)

[Internal RC Accuracy 300](#_bookmark704)

[Load Conditions for Device Timing 298](#_bookmark692)

[MCCP/SCCP Input Capture Mode](#_bookmark718)

[Requirements 304](#_bookmark718)

[MCCP/SCCP Output Compare Mode](#_bookmark722)

[Requirements 304](#_bookmark722)

[MCCP/SCCP PWM Mode Requirements 305](#_bookmark724)

[PLL Clock Timing Specifications 300](#_bookmark701)

[RC Oscillator Start-up Time 300](#_bookmark706)

[Reset and Brown-out Reset Requirements 302](#_bookmark712)

[SPIx Master Mode (CKE = 0) Requirements 306](#_bookmark727)

[SPIx Master Mode (CKE = 1) Requirements 307](#_bookmark733)

[SPIx Slave Mode (CKE = 0) Requirements 308](#_bookmark739)

[SPIx Slave Mode (CKE = 1) Requirements 310](#_bookmark746)

[Timer1 External Clock Requirements 303](#_bookmark715)

[USB OTG Specifications 318](#_bookmark775)

ADC Converter

[Control Registers 218](#_bookmark476)

[Introduction 217](#_bookmark473)

Assembler

[MPASM Assembler 284](#_bookmark624)

B

[Band Gap Voltage Reference 264](#_bookmark578)

Block Diagrams

[ADC Module 217](#_bookmark475)

[CLCx Input Source Selection 231](#_bookmark515)

[CLCx Logic Function Combinatorial Options 230](#_bookmark513)

[CLCx Module 229](#_bookmark511)

[CPU Exceptions and Interrupt Controller 59](#_bookmark148)

[CPU Module 30](#_bookmark60)

[DMA Module 77](#_bookmark173)

[High/Low-Voltage Detect (HLVD) 253](#_bookmark544)

[I2Cx Circuit 168](#_bookmark376)

[MCCP/SCCP Module 142](#_bookmark336)

MCLR [Pin Connections 24](#_bookmark40)

[Multiplexing Remappable Output for RP0 118](#_bookmark277)

[Oscillator Circuit Placement 27](#_bookmark53)

[Oscillator System 100](#_bookmark219)

[PIC32MM0256GPM0064 Family 15](#_bookmark25)

[PIC32MM0256GPM0064 Family USB Interface 183](#_bookmark402)

[Recommended Minimum Connection 24](#_bookmark35)

[Remappable Input Example for U2RX 116](#_bookmark269)

[Reset System 53](#_bookmark129)

[RTCC Module 209](#_bookmark459)

SPI/I2[S Module 159](#_bookmark360)

[Three Dual Comparator Modules 243](#_bookmark527)

[Timer1 Module 127](#_bookmark306)

[Timer2/3 (Type A, 16-Bit) 131](#_bookmark314)

[Timer2/3 (Type B, 32-Bit) 132](#_bookmark315)

[Typical Shared Port Structure 113](#_bookmark249)

[UARTx Module 175](#_bookmark385)

[Voltage Reference 249](#_bookmark537)

[Watchdog Timer (WDT) 137](#_bookmark327)

C

C Compilers

[MPLAB XC Compilers 284](#_bookmark623)

[Capture/Compare/PWM/Timer Modules](#_bookmark334)

[(MCCP, SCCP) 141](#_bookmark334)

[CLC](#_bookmark508)

[Control Registers 232](#_bookmark516)

Code Examples

[Basic Clock Switching 98](#_bookmark214)

[System Unlock 263](#_bookmark573)

[System Unlock with DMA and](#_bookmark575)

[Interrupts Enabled 263](#_bookmark575)

[Code Execution from RAM 263](#_bookmark567)

[Comparator 243](#_bookmark524)

[Configurable Logic Cell (CLC) 229](#_bookmark509)

[Configurable Logic Cell.](#_bookmark508) *See* CLC.

[Configuration Bits 263](#_bookmark566)

CPU

[Architecture Overview 31](#_bookmark61)

[Coprocessor 0 Registers 33](#_bookmark65)

[Core Exception Types 60](#_bookmark151)

[EJTAG Debug Support 34](#_bookmark69)

[Power Management 34](#_bookmark68)

[CPU Module 29](#_bookmark58)

[Customer Change Notification Service 353](#_bookmark789)

[Customer Notification Service 353](#_bookmark789)

[Customer Support 353](#_bookmark791)

D

DC Characteristics

[Comparator Specifications 297](#_bookmark685)

 Current (BOR, WDT, HLVD, RTCC,

FRC, PLL, VREF[) 292](#_bookmark662)

[High/Low-Voltage Detect 296](#_bookmark683)

[I/O Pin Input Injection Current Specifications 294](#_bookmark670)

[I/O Pin Input Specifications 293](#_bookmark666)

[I/O Pin Output Specifications 295](#_bookmark677)

Idle Current (IIDLE[) 290](#_bookmark654)

[Internal Voltage Regulator Specifications 296](#_bookmark682)

Operating Current (IDD[) 289](#_bookmark650)

[Operating Voltage Specifications 289](#_bookmark648)

[Package Thermal Resistance 288](#_bookmark646)

Power-Down Current (IPD[) 291](#_bookmark658)

[Program Memory 295](#_bookmark679)

[Thermal Operating Conditions 288](#_bookmark644)

[Voltage Reference Specifications 297](#_bookmark688)

[Demo/Development Boards, Evaluation and](#_bookmark633)

[Starter Kits 286](#_bookmark633)

[Development Support 283](#_bookmark621)

[Third-Party Tools 286](#_bookmark634)

[Device IDs 263](#_bookmark568)

[Device Overview 15](#_bookmark22)

[Direct Memory Access (DMA) Controller 77](#_bookmark170)

[Direct Memory Access.](#_bookmark171) *See* DMA.

E

[Electrical Characteristics 287](#_bookmark636)

[Absolute Maximum Ratings 287](#_bookmark637)

[V/F Graph (Industrial) 288](#_bookmark642)

[Errata 12](#_bookmark21)

F

[Flash Program Memory 45](#_bookmark101)

[Flash Controller Registers Write Protection 45](#_bookmark103)

[Write Protection 45](#_bookmark102)

[MPLAB X SIM Software Simulator 285](#_bookmark628)

[MPLIB Object Librarian 284](#_bookmark625)

[MPLINK Object Linker 284](#_bookmark626)

[Multiply/Divide Unit Latencies and Repeat Rates 31](#_bookmark63)

O

[Oscillator Configuration 97](#_bookmark206)

[Clock Switching 97](#_bookmark210)

[Sequence 97](#_bookmark211)

[Fail-Safe Clock Monitor (FSCM) 97](#_bookmark208)

[FRC Self-Tuning 99](#_bookmark216)

G

[Getting Started with PIC32 MCUs 23](#_bookmark30)

[Connection Requirements 23](#_bookmark31)

[Decoupling Capacitors 23](#_bookmark33)

[External Oscillator Pins 27](#_bookmark55)

[ICSP Pins 26](#_bookmark50)

[JTAG 27](#_bookmark51)

Master Clear (MCLR[) Pin 24](#_bookmark38)

[Unused I/Os 27](#_bookmark56)

Voltage Regulator (VCAP[) 25](#_bookmark45)

H

[High/Low-Voltage Detect (HLVD) 253](#_bookmark542)

[High/Low-Voltage Detect.](#_bookmark543) *See* HLVD.

I

[I/O Ports 113](#_bookmark247)

[Analog/Digital Port Pins Configuration 114](#_bookmark254)

[CLR, SET and INV Registers 114](#_bookmark251)

[GPIO Port Merging 114](#_bookmark258)

[Open-Drain Configuration 114](#_bookmark253)

[Parallel I/O (PIO) 114](#_bookmark252)

[Pull-up/Pull-Down Pins 115](#_bookmark261)

[Write/Read Timing 114](#_bookmark256)

[Input Change Notification (ICN) 114](#_bookmark259)

[Instruction Set 281](#_bookmark619)

[Inter-IC Sound.](#_bookmark357) *See* I2S.

Inter-Integrated Circuit (I2[C 167](#_bookmark373)

[Inter-Integrated Circuit.](#_bookmark374) *See* I2C.

[Internet Address 353](#_bookmark787)

Interrupts

[Sources and Vector Names 62](#_bookmark154)

M

MCCP/SCCP

[Registers 142](#_bookmark337)

Memory Maps

[Devices with 128 Kbytes Program Memory 42](#_bookmark91)

[Devices with 256 Kbytes Program Memory 43](#_bookmark96)

[Devices with 64 Kbytes Program Memory 41](#_bookmark87)

[Memory Organization 39](#_bookmark79)

[Alternate Configuration Bits Space 39](#_bookmark81)

[Bus Matrix (BMX) 39](#_bookmark83)

[Flash Line Buffer 40](#_bookmark85)

[Microchip Internet Web Site 353](#_bookmark787)

MIPS32® [microAptiv™ UC Core Configuration 34](#_bookmark70)

[MPLAB Assembler, Linker, Librarian 284](#_bookmark627)

[MPLAB ICD 3 In-Circuit Debugger 285](#_bookmark630)

[MPLAB PM3 Device Programmer 285](#_bookmark632)

[MPLAB REAL ICE In-Circuit Emulator System 285](#_bookmark629)

[MPLAB X Integrated Development](#_bookmark622)

[Environment Software 283](#_bookmark622)

**P**

[Packaging 319](#_bookmark780)

[Details 321](#_bookmark782)

[Marking 319](#_bookmark781)

[Peripheral Pin Select (PPS) 115](#_bookmark263)

[PICkit 3 In-Circuit Debugger/Programmer 285](#_bookmark631)

[Pinout Description 16](#_bookmark28)

[Power-Saving Features 257](#_bookmark551)

[Idle Mode 257](#_bookmark556)

[Low-Power Brown-out Reset 261](#_bookmark562)

[On-Chip Voltage Regulator](#_bookmark561)

[(Low-Power Modes) 261](#_bookmark561)

[Peripheral Module Disable. 258](#_bookmark557)

[Retention Sleep Mode 257](#_bookmark555)

[Sleep Mode 257](#_bookmark552)

[Standby Sleep Mode 257](#_bookmark553)

PPS

[Available Peripherals 115](#_bookmark265)

[Available Pins 115](#_bookmark264)

[Controlling 115](#_bookmark266)

[Controlling Configuration Changes 118](#_bookmark278)

[Input Mapping 116](#_bookmark267)

[Input Pin Selection 116](#_bookmark271)

[Output Mapping 118](#_bookmark275)

[Output Pin Selection 119](#_bookmark280)

[Remappable Pin Input Source Assignments 117](#_bookmark273)

[Programming and Diagnostics 264](#_bookmark579)

R

[Real-Time Clock and Calendar (RTCC) 209](#_bookmark457)

[Real-Time Clock and Calendar.](#_bookmark458) *See* RTCC. Register Maps

[ADC 219](#_bookmark478)

[Alternate Configuration Words Summary 266](#_bookmark588)

[Band Gap 277](#_bookmark609)

[CLC1, CLC2 and CLC3 233](#_bookmark517)

[Comparator 1, 2 and 3 244](#_bookmark528)

[Configuration Words Summary 265](#_bookmark585)

[DMA Channels 0-3 79](#_bookmark176)

[DMA Controller 78](#_bookmark174)

[Flash Controller 46](#_bookmark105)

[High/Low Voltage Detect 254](#_bookmark545)

[I2C1, I2C2 and I2C3 169](#_bookmark377)

[Interrupts 66](#_bookmark157)

[MCCP/SCCP 143](#_bookmark338)

[Oscillator Configuration 102](#_bookmark225)

[Peripheral Module Disable. 260](#_bookmark559)

[Peripheral Pin Select 124](#_bookmark300)

[PORTA 120](#_bookmark282)

[PORTB 121](#_bookmark288)

[PORTC 122](#_bookmark292)

[PORTD 123](#_bookmark297)

[RAM Configuration, Device ID and](#_bookmark598)

[System Lock 274](#_bookmark598)

[Reserved Registers 279](#_bookmark617)

[Resets 54](#_bookmark130)

[RTCC 210](#_bookmark461)

[SPI1, SPI2 and SPI3 160](#_bookmark361)

[Timer1 128](#_bookmark307)

[Timer2/3 133](#_bookmark316)

[UART1, UART2 and UART3 176](#_bookmark386)

[UDID 279](#_bookmark614)

[USB OTG 184](#_bookmark403)

[Voltage Reference 250](#_bookmark538)

[Watchdog Timer 138](#_bookmark328)

Registers

[AD1CHIT (ADC Compare Hit) 228](#_bookmark503)

[AD1CHS (ADC Input Select) 226](#_bookmark493)

[AD1CON1 (ADC Control 1) 221](#_bookmark482)

[AD1CON2 (ADC Control 2) 223](#_bookmark486)

[AD1CON3 (ADC Control 3) 224](#_bookmark488)

[AD1CON5 (ADC Control 5) 225](#_bookmark490)

[AD1CSS (ADC Input Scan Select) 227](#_bookmark498)

[ANCFG (Band Gap Control) 278](#_bookmark612)

[CCPxCON1 (Capture/Compare/PWMx](#_bookmark342)

[Control 1) 149](#_bookmark342)

[CCPxCON2 (Capture/Compare/PWMx](#_bookmark347)

[Control 2) 152](#_bookmark347)

[CCPxCON3 (Capture/Compare/PWMx](#_bookmark351)

[Control 3) 154](#_bookmark351)

[CCPxSTAT (Capture/Compare/PWMx Status) 156](#_bookmark354)

[CFGCON (Configuration Control) 275](#_bookmark600)

[CLCxCON (CLCx Control) 234](#_bookmark519)

[CLCxGLS (CLCx Gate Logic Input Select) 240](#_bookmark522)

[CLCxSEL (CLCx Input MUX Select) 236](#_bookmark521)

[CLKSTAT (Clock Status) 109](#_bookmark243)

[CMSTAT (Comparator Status) 245](#_bookmark531)

[CMxCON (Comparator x Control) 246](#_bookmark533)

[CNCONx (Change Notification Control](#_bookmark303)

[for PORTx) 126](#_bookmark303)

[CONFIG (Configuration, CP0 Register 16,](#_bookmark72)

[Select 0) 35](#_bookmark72)

[CONFIG1 (Configuration 1, CP0 Register 16,](#_bookmark74)

[Select 1) 36](#_bookmark74)

[CONFIG3 (Configuration 3, CP0 Register 16,](#_bookmark75)

[Select 3) 37](#_bookmark75)

[CONFIG5 (Configuration 5, CP0 Register 16,](#_bookmark77)

[Select 5) 38](#_bookmark77)

[DAC1CON (Voltage Reference Control) 251](#_bookmark540)

[DCHxCON (DMA Channel x Control) 88](#_bookmark186)

[DCHxCPTR (DMA Channel x Cell Pointer) 95](#_bookmark202)

[DCHxCSIZ (DMA Channel x Cell Size) 95](#_bookmark201)

[DCHxDAT (DMA Channel x Pattern Data) 96](#_bookmark204)

[DCHxDPTR (DMA Channel x](#_bookmark200)

[Destination Pointer) 94](#_bookmark200)

[DCHxDSA (DMA Channel x](#_bookmark194)

[Destination Start Address) 92](#_bookmark194)

[DCHxDSIZ (DMA Channel x Destination Size) 93](#_bookmark197)

[DCHxECON (DMA Channel x Event Control) 89](#_bookmark189)

[DCHxINT (DMA Channel x Interrupt Control) 90](#_bookmark191)

[DCHxSPTR (DMA Channel x Source Pointer) 94](#_bookmark198)

[DCHxSSA (DMA Channel x](#_bookmark192)

[Source Start Address) 92](#_bookmark192)

[DCHxSSIZ (DMA Channel x Source Size) 93](#_bookmark196)

[DCRCCON (DMA CRC Control) 85](#_bookmark182)

[DCRCDATA (DMA CRC Data) 87](#_bookmark184)

[DCRCXOR (DMA CRCXOR Enable) 87](#_bookmark185)

[DEVID (Device ID) 276](#_bookmark603)

[DMAADDR (DMA Address) 84](#_bookmark181)

[DMACON (DMA Controller Control) 83](#_bookmark178)

[DMASTAT (DMA Status) 84](#_bookmark180)

[FDEVOPT/AFDEVOPT](#_bookmark589)

[(Device Options Configuration) 267](#_bookmark589)

[FICD/AFICD (ICD/Debug Configuration) 268](#_bookmark591)

[FOSCSEL/AFOSCSEL](#_bookmark594)

[(Oscillator Selection Configuration) 272](#_bookmark594)

[FPOR/AFPOR](#_bookmark592)

[(Power-up Settings Configuration) 269](#_bookmark592)

[FSEC/AFSEC (Code-Protect Configuration) 273](#_bookmark596)

[FWDT/AFWDT](#_bookmark593)

[(Watchdog Timer Configuration) 270](#_bookmark593)

[HLVDCON (High/Low Voltage Detect Control) 255](#_bookmark548)

[I2CxCON (I2Cx Control) 171](#_bookmark379)

[I2CxSTAT (I2Cx Status) 173](#_bookmark380)

[IECx (Interrupt Enable Control x) 73](#_bookmark166)

[IFSx (Interrupt Flag Status x) 73](#_bookmark165)

[INTCON (Interrupt Control) 69](#_bookmark159)

[INTSTAT (Interrupt Status) 72](#_bookmark162)

[IPCx (Interrupt Priority Control x) 74](#_bookmark167)

[IPTMR (Interrupt Proximity Timer) 72](#_bookmark164)

[NVMADDR (Flash Address) 49](#_bookmark113)

[NVMBWP (Boot Flash (Page) Write-Protect) 52](#_bookmark118)

[NVMCON (Programming Control) 47](#_bookmark108)

[NVMDATAx (Flash Data x) 50](#_bookmark115)

[NVMKEY (Programming Unlock) 48](#_bookmark112)

[NVMPWP (Program Flash Write-Protect) 51](#_bookmark117)

[NVMSRCADDR (Source Data Address) 50](#_bookmark116)

[OSCCON (Oscillator Control) 103](#_bookmark229)

[OSCTUN (FRC Tuning) 110](#_bookmark244)

[PRISS (Priority Shadow Select) 70](#_bookmark160)

[PWRCON (Power Control) 58](#_bookmark142)

[RCON (Reset Control) 55](#_bookmark132)

[REFO1CON (Reference Oscillator Control) 106](#_bookmark234)

[REFO1TRIM (Reference Oscillator Trim) 108](#_bookmark238)

[RNMICON (Non-Maskable Interrupt (NMI) Control) 57](#_bookmark138)

[RSWRST (Software Reset) 56](#_bookmark135)

[RTCCON1 (RTCC Control 1) 211](#_bookmark464)

[RTCCON2 (RTCC Control 2) 213](#_bookmark467)

[RTCDATE/ALMDATE (RTCC/Alarm Date) 216](#_bookmark470)

[RTCSTAT (RTCC Status Register) 214](#_bookmark468)

[RTCTIME/ALMTIME (RTCC/Alarm Time) 215](#_bookmark469)

[SPIxCON (SPIx Control) 161](#_bookmark363)

[SPIxCON2 (SPIx Control 2) 164](#_bookmark368)

[SPIxSTAT (SPIx Status) 165](#_bookmark371)

[SPLLCON (System PLL Control) 105](#_bookmark232)

[SYSKEY (System Unlock) 276](#_bookmark605)

[T1CON (Timer1 (Type A) Control) 129](#_bookmark310)

[T2CON (Timer2 Control) 134](#_bookmark319)

[T3CON (Timer3 Control) 136](#_bookmark324)

[U1ADDR (USB Address) 201](#_bookmark444)

[U1BDTP1 (USB BDT Page 1) 204](#_bookmark451)

[U1BDTP2 (USB BDT Page 2) 204](#_bookmark452)

[U1BDTP3 (USB BDT Page 3) 205](#_bookmark453)

[U1CNFG1 (USB Configuration 1) 206](#_bookmark454)

[U1CON (USB Control) 199](#_bookmark438)

[U1EIE (USB Error Interrupt Enable) 197](#_bookmark432)

[U1EIR (USB Error Interrupt Status) 195](#_bookmark426)

[U1EP0-U1EP15 (USB Endpoint Control) 207](#_bookmark455)

[U1FRMH (USB Frame Number High) 202](#_bookmark446)

[U1FRML (USB Frame Number Low) 202](#_bookmark445)

[U1IE (USB Interrupt Enable) 194](#_bookmark422)

[U1IR (USB Interrupt) 192](#_bookmark415)

[U1OTGCON (USB OTG Control) 190](#_bookmark411)

[U1OTGIE (USB OTG Interrupt Enable) 188](#_bookmark409)

[U1OTGIR (USB OTG Interrupt Status) 187](#_bookmark408)

[U1OTGSTAT (USB OTG Status) 189](#_bookmark410)

[U1PWRC (USB Power Control) 191](#_bookmark413)

[U1SOF (USB SOF Threshold) 203](#_bookmark450)

[U1STAT (USB Status) 198](#_bookmark435)

[U1TOK (USB Token) 203](#_bookmark448)

[UxMODE (UARTx Mode) 177](#_bookmark388)

[UxSTA (UARTx Status and Control) 179](#_bookmark390)

[WDTCON (Watchdog Timer Control) 139](#_bookmark331)

[Reserved Registers 264](#_bookmark582)

[Resets 53](#_bookmark121)

[Brown-out Reset (BOR) 53](#_bookmark124)

[Configuration Mismatch Reset (CMR) 53](#_bookmark126)

Master Clear Reset Pin (MCLR[) 53](#_bookmark127)

[Power-on Reset (POR) 53](#_bookmark122)

[Software Reset (SWR) 53](#_bookmark123)

[Watchdog Timer Reset (WDTR) 53](#_bookmark125)

[Revision History 347](#_bookmark784)

S

[Serial Peripheral Interface (SPI) 159](#_bookmark358)

[Serial Peripheral Interface.](#_bookmark359) *See* SPI.

[Special Features 263](#_bookmark564)

T

[Timer1 Module 127](#_bookmark305)

[Timer2/3 Modules 131](#_bookmark312)

[Additional Supported Features 131](#_bookmark313)

Timing Diagrams

[CLKO and I/O Characteristics 301](#_bookmark707)

[EJTAG 317](#_bookmark771)

[External Clock 299](#_bookmark696)

[I2Cx Bus Data (Master Mode) 311](#_bookmark751)

[I2Cx Bus Data (Slave Mode) 313](#_bookmark758)

[I2Cx Bus Start/Stop Bits (Master Mode) 311](#_bookmark753)

[I2Cx Bus Start/Stop Bits (Slave Mode) 313](#_bookmark757)

[MCCP/SCCP Input Capture Mode 304](#_bookmark719)

[MCCP/SCCP Output Compare Mode 304](#_bookmark721)

[MCCP/SCCP PWM Mode Characteristics 305](#_bookmark725)

[SPIx Master Mode (CKE = 0) 306](#_bookmark728)

[SPIx Master Mode (CKE = 1) 307](#_bookmark734)

[SPIx Slave Mode (CKE = 0) 308](#_bookmark740)

[SPIx Slave Mode (CKE = 1) 309](#_bookmark745)

[Timer1 External Clock 303](#_bookmark714)

U

[UART](#_bookmark382) [175](#_bookmark383)

[Unique Device Identifier (UDID) 264](#_bookmark581)

[Universal Asynchronous Receiver Transmitter.](#_bookmark382) *See* UART. [USB On-The-Go (OTG) 181](#_bookmark392)

USB OTG

[Introduction 181](#_bookmark396)

[Operation of Port Pins Shared with](#_bookmark400)

[USB Transceiver 182](#_bookmark400)

[Powering the USB Transceiver 182](#_bookmark399)

[Reclaiming USB Pins When USB is Disabled 181](#_bookmark395)

[Reclaiming USB Pins When USB is Operating 181](#_bookmark394)

V

Voltage Reference (CVREF[) 249](#_bookmark535)

W

[Watchdog Timer (WDT) 137](#_bookmark326)

Write Protection

[System Registers 263](#_bookmark571)

[WWW Address 353](#_bookmark787)

[WWW, On-Line Support 12](#_bookmark20)

# THE MICROCHIP WEB SITE

[Microchip provides online support via our WWW site at](http://www.microchip.com/) [w](http://www.microchip.com/)ww.microchip.com. This web site is used as a means to make files and information easily available to customers. Accessible by using your favorite Internet browser, the web site contains the following informa- tion:

* **Product Support** – Data sheets and errata, appli- cation notes and sample programs, design resources, user’s guides and hardware support documents, latest software releases and archived software
* **General Technical Support** – Frequently Asked Questions (FAQ), technical support requests, online discussion groups, Microchip consultant program member listing
* **Business of Microchip** – Product selector and ordering guides, latest Microchip press releases, listing of seminars and events, listings of Micro- chip sales offices, distributors and factory repre- sentatives

# CUSTOMER CHANGE NOTIFICATION SERVICE

Microchip’s customer notification service helps keep customers current on Microchip products. Subscribers will receive e-mail notification whenever there are changes, updates, revisions or errata related to a spec- ified product family or development tool of interest.

[To register, access the Microchip web site at](http://www.microchip.com/) [w](http://www.microchip.com/)ww.microchip.com. Under “Support”, click on “Cus- tomer Change Notification” and follow the registration instructions.

# CUSTOMER SUPPORT

Users of Microchip products can receive assistance through several channels:

* Distributor or Representative
* Local Sales Office
* Field Application Engineer (FAE)
* Technical Support

Customers should contact their distributor, representa- tive or Field Application Engineer (FAE) for support. Local sales offices are also available to help custom- ers. A listing of sales offices and locations is included in the back of this document.

[**Technical support is available through the web site**](http://www.microchip.com/)[**at:**](http://www.microchip.com/) [**http://microchip.com/support**](http://microchip.com/support)

NOTES:

Three-digit QTP, SQTP, Code or Special Requirements (blank otherwise)

ES = Engineering Sample

Pattern

M = Up to 25 MHz operating frequency with basic peripheral set of 3 UARTs, 3 SPIs, 3 I2C modules and USB

Key Feature

GP = General Purpose Family

Family

Flash Memory Size 0064 = 64 Kbytes

0128 = 128 Kbytes

0256 = 256 Kbytes

MM = MIPS32® microAptiv™ UC CPU Core

Architecture

# PRODUCT IDENTIFICATION SYSTEM

To order or obtain information, e.g., on pricing or delivery, refer to the factory or the listed sales office.

**Example:**

PIC32MM0064GPM028-I/MV:

PIC32 General Purpose Device with MIPS32® microAptiv™ UC

Core, 64-Kbyte Program Memory, 28-Pin, Industrial Temp.,

UQFN Package.

**PIC32 MM XXXX GP M XXX T - XXX**

**Microchip Brand Architecture**

**Flash Memory Size**

**Family Key Feature Set Pin Count**

**Tape and Reel Flag (if applicable)**

**Pattern**

|  |  |  |
| --- | --- | --- |
| Pin Count | 028 | = 28-pin |
|  | 036 | = 36/40-pin |
|  | 048 | = 48-pin |
|  | 064 | = 64-pin |

NOTES:

**Note the following details of the code protection feature on Microchip devices:**

* + Microchip products meet the specification contained in their particular Microchip Data Sheet.
  + Microchip believes that its family of products is one of the most secure families of its kind on the market today, when used in the intended manner and under normal conditions.
  + There are dishonest and possibly illegal methods used to breach the code protection feature. All of these methods, to our knowledge, require using the Microchip products in a manner outside the operating specifications contained in Microchip’s Data Sheets. Most likely, the person doing so is engaged in theft of intellectual property.
  + Microchip is willing to work with the customer who is concerned about the integrity of their code.
  + Neither Microchip nor any other semiconductor manufacturer can guarantee the security of their code. Code protection does not mean that we are guaranteeing the product as “unbreakable.”

Code protection is constantly evolving. We at Microchip are committed to continuously improving the code protection features of our products. Attempts to break Microchip’s code protection feature may be a violation of the Digital Millennium Copyright Act. If such acts allow unauthorized access to your software or other copyrighted work, you may have a right to sue for relief under that Act.

Information contained in this publication regarding device applications and the like is provided only for your convenience and may be superseded by updates. It is your responsibility to ensure that your application meets with your specifications. MICROCHIP MAKES NO REPRESENTATIONS OR WARRANTIES OF ANY KIND WHETHER EXPRESS OR IMPLIED, WRITTEN OR ORAL, STATUTORY OR OTHERWISE, RELATED TO THE INFORMATION, INCLUDING BUT NOT LIMITED TO ITS CONDITION, QUALITY, PERFORMANCE, MERCHANTABILITY OR

FITNESS FOR PURPOSE**.** Microchip disclaims all liability arising from this information and its use. Use of Microchip devices in life support and/or safety applications is entirely at the buyer’s risk, and the buyer agrees to defend, indemnify and hold harmless Microchip from any and all damages, claims, suits, or expenses resulting from such use. No licenses are conveyed, implicitly or otherwise, under any Microchip intellectual property rights unless otherwise stated.

*Microchip received ISO/TS-16949:2009 certification for its worldwide headquarters, design and wafer fabrication facilities in Chandler and Tempe, Arizona; Gresham, Oregon and design centers in California and India. The Company’s quality system processes and procedures are for its PIC® MCUs and dsPIC® DSCs, KEELOQ® code hopping devices, Serial EEPROMs, microperipherals, nonvolatile memory and analog products. In addition, Microchip’s quality system for the design and manufacture of development systems is ISO 9001:2000 certified.*

**QUALITY MANAGEMENT SYSTEM CERTIFIED BY DNV**

== **ISO/TS 16949** ==

**Trademarks**

The Microchip name and logo, the Microchip logo, AnyRate, AVR, AVR logo, AVR Freaks, BeaconThings, BitCloud, CryptoMemory, CryptoRF, dsPIC, FlashFlex, flexPWR, Heldo, JukeBlox, KEELOQ, KEELOQ logo, Kleer, LANCheck, LINK MD, maXStylus, maXTouch, MediaLB, megaAVR, MOST, MOST logo, MPLAB, OptoLyzer, PIC, picoPower, PICSTART, PIC32 logo, Prochip Designer, QTouch, RightTouch, SAM-BA, SpyNIC, SST, SST Logo, SuperFlash, tinyAVR, UNI/O, and XMEGA are registered trademarks of Microchip Technology Incorporated in the U.S.A. and other countries.

ClockWorks, The Embedded Control Solutions Company, EtherSynch, Hyper Speed Control, HyperLight Load, IntelliMOS, mTouch, Precision Edge, and Quiet-Wire are registered trademarks of Microchip Technology Incorporated in the U.S.A.

Adjacent Key Suppression, AKS, Analog-for-the-Digital Age, Any Capacitor, AnyIn, AnyOut, BodyCom, chipKIT, chipKIT logo, CodeGuard, CryptoAuthentication, CryptoCompanion, CryptoController, dsPICDEM, dsPICDEM.net, Dynamic Average Matching, DAM, ECAN, EtherGREEN, In-Circuit Serial Programming, ICSP, Inter-Chip Connectivity, JitterBlocker, KleerNet, KleerNet logo, Mindi, MiWi, motorBench, MPASM, MPF, MPLAB Certified logo, MPLIB, MPLINK, MultiTRAK, NetDetach, Omniscient Code Generation, PICDEM, PICDEM.net, PICkit, PICtail, PureSilicon, QMatrix, RightTouch logo, REAL ICE, Ripple Blocker, SAM-ICE, Serial Quad I/O, SMART-I.S., SQI, SuperSwitcher, SuperSwitcher II, Total Endurance, TSHARC, USBCheck, VariSense, ViewSpan, WiperLock, Wireless DNA, and ZENA are trademarks of Microchip Technology Incorporated in the

U.S.A. and other countries.

SQTP is a service mark of Microchip Technology Incorporated in the U.S.A.

Silicon Storage Technology is a registered trademark of Microchip Technology Inc. in other countries.

GestIC is a registered trademark of Microchip Technology Germany II GmbH & Co. KG, a subsidiary of Microchip Technology Inc., in other countries.

All other trademarks mentioned herein are property of their respective companies.

© 2016-2017, Microchip Technology Incorporated, All Rights Reserved.

ISBN: 978-1-5224-1752-1



**Worldwide Sales and Service**

AMERICAS

**Corporate Office**

2355 West Chandler Blvd. Chandler, AZ 85224-6199

Tel: 480-792-7200

Fax: 480-792-7277

Technical Support: [http://www.microchip.com/ support](http://support.microchip.com/)

Web Address: [www](http://www.microchip.com/).microchip.com

**Atlanta**

Duluth, GA

Tel: 678-957-9614

Fax: 678-957-1455

**Austin, TX**

Tel: 512-257-3370

**Boston** Westborough, MA Tel: 774-760-0087

Fax: 774-760-0088

**Chicago**

Itasca, IL

Tel: 630-285-0071

Fax: 630-285-0075

**Dallas**

Addison, TX

Tel: 972-818-7423

Fax: 972-818-2924

**Detroit**

Novi, MI

Tel: 248-848-4000

**Houston, TX**

Tel: 281-894-5983

**Indianapolis** Noblesville, IN Tel: 317-773-8323

Fax: 317-773-5453

Tel: 317-536-2380

**Los Angeles** Mission Viejo, CA Tel: 949-462-9523

Fax: 949-462-9608

Tel: 951-273-7800

**Raleigh, NC**

Tel: 919-844-7510

**New York, NY**

Tel: 631-435-6000

**San Jose, CA**

Tel: 408-735-9110

Tel: 408-436-4270

**Canada - Toronto**

Tel: 905-695-1980

Fax: 905-695-2078

ASIA/PACIFIC

**Asia Pacific Office** Suites 3707-14, 37th Floor Tower 6, The Gateway Harbour City, Kowloon

**Hong Kong**

Tel: 852-2943-5100

Fax: 852-2401-3431

**Australia - Sydney**

Tel: 61-2-9868-6733

Fax: 61-2-9868-6755

**China - Beijing**

Tel: 86-10-8569-7000

Fax: 86-10-8528-2104

**China - Chengdu**

Tel: 86-28-8665-5511

Fax: 86-28-8665-7889

**China - Chongqing**

Tel: 86-23-8980-9588

Fax: 86-23-8980-9500

**China - Dongguan**

Tel: 86-769-8702-9880

**China - Guangzhou**

Tel: 86-20-8755-8029

**China - Hangzhou**

Tel: 86-571-8792-8115

Fax: 86-571-8792-8116

**China - Hong Kong SAR**

Tel: 852-2943-5100

Fax: 852-2401-3431

**China - Nanjing**

Tel: 86-25-8473-2460

Fax: 86-25-8473-2470

**China - Qingdao**

Tel: 86-532-8502-7355

Fax: 86-532-8502-7205

**China - Shanghai**

Tel: 86-21-3326-8000

Fax: 86-21-3326-8021

**China - Shenyang**

Tel: 86-24-2334-2829

Fax: 86-24-2334-2393

**China - Shenzhen**

Tel: 86-755-8864-2200

Fax: 86-755-8203-1760

**China - Wuhan**

Tel: 86-27-5980-5300

Fax: 86-27-5980-5118

**China - Xian**

Tel: 86-29-8833-7252

Fax: 86-29-8833-7256

ASIA/PACIFIC

**China - Xiamen**

Tel: 86-592-2388138

Fax: 86-592-2388130

**China - Zhuhai**

Tel: 86-756-3210040

Fax: 86-756-3210049

**India - Bangalore**

Tel: 91-80-3090-4444

Fax: 91-80-3090-4123

**India - New Delhi**

Tel: 91-11-4160-8631

Fax: 91-11-4160-8632

**India - Pune**

Tel: 91-20-3019-1500

**Japan - Osaka**

Tel: 81-6-6152-7160

Fax: 81-6-6152-9310

**Japan - Tokyo**

Tel: 81-3-6880- 3770

Fax: 81-3-6880-3771

**Korea - Daegu**

Tel: 82-53-744-4301

Fax: 82-53-744-4302

**Korea - Seoul**

Tel: 82-2-554-7200

Fax: 82-2-558-5932 or

82-2-558-5934

**Malaysia - Kuala Lumpur**

Tel: 60-3-6201-9857

Fax: 60-3-6201-9859

**Malaysia - Penang**

Tel: 60-4-227-8870

Fax: 60-4-227-4068

**Philippines - Manila**

Tel: 63-2-634-9065

Fax: 63-2-634-9069

**Singapore**

Tel: 65-6334-8870

Fax: 65-6334-8850

**Taiwan - Hsin Chu**

Tel: 886-3-5778-366

Fax: 886-3-5770-955

**Taiwan - Kaohsiung**

Tel: 886-7-213-7830

**Taiwan - Taipei**

Tel: 886-2-2508-8600

Fax: 886-2-2508-0102

**Thailand - Bangkok**

Tel: 66-2-694-1351

Fax: 66-2-694-1350

EUROPE

**Austria - Wels**

Tel: 43-7242-2244-39

Fax: 43-7242-2244-393

**Denmark - Copenhagen**

Tel: 45-4450-2828

Fax: 45-4485-2829

**Finland - Espoo**

Tel: 358-9-4520-820

**France - Paris**

Tel: 33-1-69-53-63-20

Fax: 33-1-69-30-90-79

**France - Saint Cloud**

Tel: 33-1-30-60-70-00

**Germany - Garching**

Tel: 49-8931-9700

**Germany - Haan**

Tel: 49-2129-3766400

**Germany - Heilbronn**

Tel: 49-7131-67-3636

**Germany - Karlsruhe**

Tel: 49-721-625370

**Germany - Munich**

Tel: 49-89-627-144-0

Fax: 49-89-627-144-44

**Germany - Rosenheim**

Tel: 49-8031-354-560

**Israel - Ra’anana**

Tel: 972-9-744-7705

**Italy - Milan**

Tel: 39-0331-742611

Fax: 39-0331-466781

**Italy - Padova**

Tel: 39-049-7625286

**Netherlands - Drunen**

Tel: 31-416-690399

Fax: 31-416-690340

**Norway - Trondheim**

Tel: 47-7289-7561

**Poland - Warsaw**

Tel: 48-22-3325737

**Romania - Bucharest**

Tel: 40-21-407-87-50

**Spain - Madrid**

Tel: 34-91-708-08-90

Fax: 34-91-708-08-91

**Sweden - Gothenberg**

Tel: 46-31-704-60-40

**Sweden - Stockholm**

Tel: 46-8-5090-4654

**UK - Wokingham**

Tel: 44-118-921-5800

Fax: 44-118-921-5820

**Mouser Electronics**

## Authorized Distributor

Click to View Pricing, Inventory, Delivery & Lifecycle Information:

[Microchip](https://www.mouser.com/microchip):

PIC32MM0128GPM028-I/ML PIC32MM0128GPM048T-I/M4 PIC32MM0128GPM048-I/PT PIC32MM0128GPM048- I/M4 PIC32MM0128GPM036-I/MV PIC32MM0064GPM028-I/SS PIC32MM0064GPM064T-I/PT PIC32MM0256GPM028-I/SS PIC32MM0064GPM048-I/M4 PIC32MM0256GPM028-I/ML PIC32MM0064GPM036-I/M2

PIC32MM0256GPM036-I/MV PIC32MM0128GPM064T-I/PT PIC32MM0256GPM036T-I/M2 PIC32MM0256GPM048- I/M4 PIC32MM0128GPM028T-I/SS PIC32MM0256GPM036-I/M2 PIC32MM0064GPM036T-I/MV PIC32MM0128GPM036-I/M2 PIC32MM0128GPM048T-I/PT PIC32MM0064GPM028T-I/ML PIC32MM0064GPM048T- I/M4 PIC32MM0064GPM028-I/ML PIC32MM0256GPM064T-I/PT PIC32MM0064GPM048-I/PT PIC32MM0064GPM064-I/PT PIC32MM0128GPM028T-I/ML PIC32MM0128GPM036T-I/M2 PIC32MM0064GPM036T- I/M2 PIC32MM0256GPM048T-I/M4 PIC32MM0256GPM028T-I/ML PIC32MM0256GPM048T-I/PT PIC32MM0256GPM028T-I/SS PIC32MM0064GPM036-I/MV PIC32MM0128GPM064-I/PT PIC32MM0128GPM028- I/SS PIC32MM0064GPM048T-I/PT PIC32MM0256GPM036T-I/MV PIC32MM0064GPM028T-I/SS PIC32MM0128GPM036T-I/MV PIC32MM0256GPM064-I/PT PIC32MM0256GPM048-I/PT PIC32MM0256GPM028T- I/M6 PIC32MM0256GPM028-I/M6 PIC32MM0128GPM028T-I/M6 PIC32MM0128GPM064T-I/MR PIC32MM0128GPM028-I/M6 PIC32MM0128GPM064-I/MR PIC32MM0064GPM028-I/M6 PIC32MM0256GPM064T- I/MR PIC32MM0256GPM064-I/MR PIC32MM0064GPM028T-I/M6 PIC32MM0064GPM064T-I/MR PIC32MM0064GPM064-I/MR PIC32MM0256GPM036-E/MV PIC32MM0128GPM028-E/ML PIC32MM0256GPM028- E/SS PIC32MM0128GPM028-E/SS PIC32MM0256GPM028-E/M6 PIC32MM0128GPM028-E/M6 PIC32MM0256GPM028-E/ML PIC32MM0128GPM036-E/MV PIC32MM0128GPM036-E/M2 PIC32MM0128GPM064- E/MR PIC32MM0128GPM048-E/PT PIC32MM0128GPM064-E/PT PIC32MM0256GPM048-E/PT PIC32MM0256GPM064-E/PT PIC32MM0256GPM064-E/MR PIC32MM0256GPM036-E/M2